MSP430™CapTIvateSoftwareLibraryAPIGuide 1_70_00_03

Macros | Functions
CAPT_EMC.h File Reference
`#include <stdlib.h>`
`#include <stdbool.h>`
`#include <stdint.h>`
Include dependency graph for CAPT_EMC.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | CAPT_EMC_STDFREQ_CNT (0x01)
#define | CAPT_EMC_MULTIFREQ_CNT (0x04)
#define | CAPT_EMC_SAMPLE_ERROR_CODE (0x00000)

## Functions
bool | CAPT_loadEMCConfig (const tEMCConfig *pConfig)
uint16_t | CAPT_getGlobalFilteredNoiseLevel (void)
void | CAPT_resetGlobalFilteredNoiseLevel (void)
void | CAPT_updateGlobalFilteredNoiseLevel (tElement *pElement, uint16_t ui16RelNoiseLevel)
void | CAPT_getEMCConversionSettings (tSenseTechnology method, tRawConversionStyle *pConversion, tOversamplingStyle *pOversampling)
uint8_t | CAPT_getRelNoiseStatusThreshold (void)
| Get the relative noise threshold parameter. More...
uint8_t | CAPT_getMaxRelThreshold (void)
bool | CAPT_testConversionFrequencyForNoise (tSensor *pSensor, uint8_t ui8Freq)
bool | CAPT_correctInvalidMultiFreqCalibration (tSensor *pSensor, uint8_t ui8NoiseMask)
void | CAPT_replaceFrequencyWithError (uint16_t *pNewSet, uint16_t ui16Replacement)
void | CAPT_resolveMultiFreqSet (const uint16_t *pNewSet, uint16_t *pResult, uint16_t *pNoiseLevel, bool bRemoveOutlier)
uint16_t | CAPT_computeJitterFilter (uint16_t ui16Prev, uint16_t ui16Curr)
| This function applies a basic single-level jitter filter to a sample. More...
uint8_t | CAPT_computeRelNoiseComp (void)

© Copyright 1995-2018, Texas Instruments Incorporated. All rights reserved.
Trademarks | Privacy policy | Terms of use | Terms of sale