MSP430™CapTIvateSoftwareLibraryAPIGuide 1_70_00_03

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - b -

- bBISTFail : tElement
- bCalibrationError : tSensor
- bCounterOVF : tSensor
- bCountFilterEnable : tSensor
- bCsDischarge : tSensor
- bDetect : tElement
- bElementDataTxEnable : tCaptivateApplication
- bElementHalt : tElement
- bEnableDynamicThresholdAdjustment : tEMCConfig
- bGestureEnable : tTrackPadSensorParams
- bIdleState : tSensor
- bJitterFilterEnable : tEMCConfig
- bLpmControl : tSensor
- bMaxCountError : tSensor
- bModEnable : tSensor
- bNegativeTouch : tElement
- bNoiseDetected : tElement
- bPresentTouch : tTrackPadSensorParams
- bProx : tElement
- bPTElementHalt : tSensor
- bPTSensorHalt : tSensor
- bReCalibrateEnable : tSensor
- bReseed : tElement , tTrackPadSensorParams
- bSendReadLengthFirst : tI2CSlavePort
- bSensorDataTxEnable : tCaptivateApplication
- bSensorDetect : tSensor
- bSensorHalt : tSensor
- bSensorNegativeTouch : tSensor
- bSensorNoiseState : tSensor
- bSensorPrevTouch : tSensor
- bSensorProx : tSensor
- bSensorTouch : tSensor
- bSensorUpdating : tSensor
- bStuffedByteDetected : tTLProtocolProcessingVariables
- bTimerSyncControl : tSensor
- bTouch : tElement
- bTrackPadFilterEnable : tTrackPadSensorParams
- bTrackPadFilterType : tTrackPadSensorParams

### - c -

- coeffA : tEMCConfig
- coeffB : tEMCConfig

### - d -

- DbIn : tDeBounceSettings
- DbOut : tDeBounceSettings
- DirectionOfInterest : tSensor

### - f -

- filterCount : tElement

### - i -

- i8currPacketIndex : tTLProtocolProcessingVariables

### - l -

- LTA : tElement

### - p -

- pbErrorCallback : tUARTPort
- pbFunction_A : tFunctionTimer
- pbFunction_B : tFunctionTimer
- pbReceiveCallback : tI2CSlavePort , tUARTPort
- pCycle : tSensor
- pEditBuffer : tPingPongBuffer
- pElements : tCycle
- peripheralParameters : tUARTPort
- pMatrix : tTrackPadSensorParams
- Position_X : tTrackPadSensorParams
- Position_Y : tTrackPadSensorParams
- pRawCount : tElement
- pReceiveBuffer : tI2CSlavePort
- projModeConversionStyle : tEMCConfig
- projModeOversamplingStyle : tEMCConfig
- ProxDbCounter : tElement
- ProxDbThreshold : tSensor
- pSensor : tButtonSensorParams , tProxSensorParams
- pSensorList : tCaptivateApplication
- pSensorParams : tSensor
- pSumX : tTrackPadSensorParams
- pSumY : tTrackPadSensorParams
- pTransmitBuffer : tPingPongBuffer
- pTuning : tElement
- pvCallback : tSensor
- pvErrorCallback : tI2CSlavePort
- pvProcessGesture : tTrackPadSensorParams
- pvProcessSensor : tTrackPadSensorParams

### - q -

- QueueArray : tByteQueue

### - r -

- Reseed : tSliderSensorParams

### - s -

- selfModeConversionStyle : tEMCConfig
- selfModeOversamplingStyle : tEMCConfig
- SensingMethod : tSensor
- SliderAlgorithm : tSliderSensorParams
- SliderBeta : tSliderSensorParams
- SliderFilterEnable : tSliderSensorParams
- SliderLower : tSliderSensorParams
- SliderPosition : tSliderSensorParams
- SliderUpper : tSliderSensorParams
- state : tCaptivateApplication

### - t -

- TouchDbCounter : tElement
- TouchDbThreshold : tSensor
- TypeOfSensor : tSensor

### - u -

- ui16ActiveModeScanPeriod : tCaptivateApplication
- ui16BottomSpeed : tTrackPadSensorParams
- ui16CalibrationNoiseLimit : tEMCConfig
- ui16Checksum : tParameterPacket
- ui16CompositeRawCount : tElement
- ui16ConversionCount : tSensor
- ui16ConversionGain : tSensor
- ui16Decimal : IQ16_t
- ui16DominantElement : tButtonSensorParams
- ui16DoubleTapTime_Max : tTrackPadSensorParams
- ui16ErrorThreshold : tSensor
- ui16FunctionDelay_A : tFunctionTimer
- ui16FunctionDelay_B : tFunctionTimer
- ui16InactivityTimeout : tCaptivateApplication
- ui16LowerTrim_X : tTrackPadSensorParams
- ui16LowerTrim_Y : tTrackPadSensorParams
- ui16Natural : IQ16_t
- ui16NegativeTouchThreshold : tSensor
- ui16NoiseCount : tElement
- ui16OffsetTap : tCaptivateElementTuning
- ui16Parameter : tGenericSensorParams
- ui16PrevCompositeRawCount : tElement
- ui16PrevDominantElement : tButtonSensorParams
- ui16PrevRaw_X : tTrackPadSensorParams
- ui16PrevRaw_Y : tTrackPadSensorParams
- ui16ProxThreshold : tSensor
- ui16QueueArraySize : tByteQueue
- ui16QueueHead : tByteQueue
- ui16QueueTail : tByteQueue
- ui16Raw_X : tTrackPadSensorParams
- ui16Raw_Y : tTrackPadSensorParams
- ui16ReceiveBufferSize : tI2CSlavePort
- ui16Resolution : tSliderSensorParams
- ui16Resolution_X : tTrackPadSensorParams
- ui16Resolution_Y : tTrackPadSensorParams
- ui16SwipeDistance_Min : tTrackPadSensorParams
- ui16SwipeTime_Max : tTrackPadSensorParams
- ui16TapHoldTime_Min : tTrackPadSensorParams
- ui16TapTime_Max : tTrackPadSensorParams
- ui16TapTime_Min : tTrackPadSensorParams
- ui16Timeout : tSensor
- ui16TimeoutThreshold : tSensor
- ui16TopSpeed : tTrackPadSensorParams
- ui16UpperTrim_X : tTrackPadSensorParams
- ui16UpperTrim_Y : tTrackPadSensorParams
- ui16Value : tGenericSensorParams
- ui16WakeOnProxModeScanPeriod : tCaptivateApplication
- ui32Full : IQ16_t
- ui8AppLPM : tCaptivateApplication
- ui8BiasControl : tSensor
- ui8Blank : tParameterPacket
- ui8CalibrationTestSampleSize : tEMCConfig
- ui8ChargeLength : tSensor
- ui8CntBeta : tSensor
- ui8CoarseGainRatio : tCaptivateElementTuning
- ui8Command : tParameterPacket
- ui8FineGainRatio : tCaptivateElementTuning
- ui8FreqDiv : tSensor
- ui8Gesture : tTrackPadSensorParams
- ui8InputSyncControl : tSensor
- ui8Length : tParameterPacket
- ui8LowerBeta : tTrackPadSensorParams
- ui8LTABeta : tSensor
- ui8MaxRelThreshAdj : tEMCConfig
- ui8NoiseLevelFilterDown : tEMCConfig
- ui8NoiseLevelFilterEntryThresh : tEMCConfig
- ui8NoiseLevelFilterExitThresh : tEMCConfig
- ui8NoiseLevelFilterUp : tEMCConfig
- ui8NoiseThreshold : tEMCConfig
- ui8NrOfCycles : tSensor
- ui8NrOfElements : tCycle
- ui8NrOfSensors : tCaptivateApplication
- ui8NumberOfSensors : tButtonSensorParams , tProxSensorParams
- ui8Packet : tParameterPacket
- ui8Param0 : tParameterPacket
- ui8Param1 : tParameterPacket
- ui8Param2 : tParameterPacket
- ui8Param3 : tParameterPacket
- ui8RxBlock : tElement
- ui8RxPin : tElement
- ui8SensorID : tParameterPacket
- ui8Sync : tParameterPacket
- ui8TotalColumns : tTrackPadSensorParams
- ui8TotalElements : tSliderSensorParams
- ui8TotalRows : tTrackPadSensorParams
- ui8TouchThreshold : tElement
- ui8TrackPadSensorBeta : tTrackPadSensorParams
- ui8TransferLength : tSensor
- ui8TxBlock : tElement
- ui8TxPin : tElement
- ui8WakeupInterval : tCaptivateApplication
- ui8Write : tParameterPacket

© Copyright 1995-2018, Texas Instruments Incorporated. All rights reserved.
Trademarks | Privacy policy | Terms of use | Terms of sale