MSP430™CapTIvateSoftwareLibraryAPIGuide 1_70_00_03

Data Fields
tDeBounceSettings Struct Reference
CAPT_TYPE

typedef tDeBounceSettings More...

`#include <CAPT_Type.h>`

## Data Fields
uint8_t | DbIn: 4
uint8_t | DbOut: 4

## Detailed Description

typedef tDeBounceSettings

The de-bounce structure holds de-bounce up/down information, and can be used for storing de-bounce thresholds or counts.

## Field Documentation

## § DbIn

uint8_t tDeBounceSettings::DbIn

De-bounce into a Touch/Prox State May hold the threshold or the current de-bounce count

## § DbOut

uint8_t tDeBounceSettings::DbOut

De-bounce out of a Touch/Prox State May hold the threshold or the current de-bounce count

The documentation for this struct was generated from the following file:

- CAPT_Type.h

© Copyright 1995-2018, Texas Instruments Incorporated. All rights reserved.
Trademarks | Privacy policy | Terms of use | Terms of sale