MSP430™CapTIvateSoftwareLibraryAPIGuide 1_70_00_03

Data Fields
tProxSensorParams Struct Reference
CAPT_TYPE

`#include <CAPT_Type.h>`

Collaboration diagram for tProxSensorParams:
[legend]

## Data Fields
tSensor ** | pSensor
uint8_t | ui8NumberOfSensors

## Detailed Description

typedef tProxSensorParams

Proximity sensor specific parameters. One instance must be created and tied to every proximity sensor.

## Field Documentation

## § pSensor

tSensor** tProxSensorParams::pSensor

Pointer to an array of sensor pointers that should be activated as Tx electrodes during the proximity measurement (if in projected capacitance mode).

## § ui8NumberOfSensors

uint8_t tProxSensorParams::ui8NumberOfSensors

Indicates how many sensors are activated as Tx electrodes during the proximity measurement (if in projected capacitance mode).

The documentation for this struct was generated from the following file:

- CAPT_Type.h

© Copyright 1995-2018, Texas Instruments Incorporated. All rights reserved.
Trademarks | Privacy policy | Terms of use | Terms of sale