VIN_SENSE P1.2 ADC Input Switching Waveform
See scope shot below.  This should be a flat line DC.  Why does this signal appear during ADC reads?  Is our ADC interface circuit incorrect?  Would this have something to do with the ADC related register settings?  We are reading the voltage of a battery.
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