# MSP430 DriverLib 2.00.00.16

# List of APIs removed in this version

MSP430F5xx_6xx Family

Old API | New API
ADC10_A_memoryConfigure | ADC10_A_configureMemory
ADC12_A_memoryConfigure | ADC12_A_configureMemory
AES_clearInterruptFlag | AES_clearInterrupt
AES_generateFirstRoundKey | AES_setDecipherKey
AES_getInterruptFlagStatus | AES_getInterruptStatus
AES_startGenerateFirstRoundKey | AES_startSetDecipherKey
AES256_clearInterruptFlag | AES256_clearInterrupt
AES256_getInterruptFlagStatus | AES256_getInterruptStatus
BAK_BATT_chargerInitAndEnable | BattBak_initAndEnableCharger
BAK_BATT_disable | BattBak_disable
BAK_BATT_disableBackupSupplyToADC | BattBak_disableBackupSupplyToADC
BAK_BATT_disableCharger | BattBak_disableCharger
BAK_BATT_enableBackupSupplyToADC | BattBak_enableBackupSupplyToADC
BAK_BATT_getBackupRAMData | BattBak_getBackupRAMData
BAK_BATT_manuallySwitchToBackupSupply | BattBak_manuallySwitchToBackupSupply
BAK_BATT_setBackupRAMData | BattBak_setBackupRAMData
BAK_BATT_unlockBackupSubSystem | BattBak_unlockBackupSubSystem
BattBak_chargerInitAndEnable | BattBak_initAndEnableCharger
BattBak_manuallySwitchToBackupSupply | BattBak_switchToBackupSupplyManually
COMP_B_clearInterrupt | Comp_B_clearInterrupt
COMP_B_configureReferenceVoltage | Comp_B_configureReferenceVoltage
COMP_B_disable | Comp_B_disable
COMP_B_disableInputBuffer | Comp_B_disableInputBuffer
COMP_B_disableInterrupt | Comp_B_disableInterrupt
COMP_B_enable | Comp_B_enable
COMP_B_enableInputBuffer | Comp_B_enableInputBuffer
COMP_B_enableInterrupt | Comp_B_enableInterrupt
COMP_B_getInterruptStatus | Comp_B_getInterruptStatus
COMP_B_init | Comp_B_init
COMP_B_initialize | Comp_B_init
COMP_B_interruptSetEdgeDirection | Comp_B_setInterruptEdgeDirection
Comp_B_interruptSetEdgeDirection | Comp_B_setInterruptEdgeDirection
COMP_B_interruptToggleEdgeDirection | Comp_B_interruptToggleEdgeDirection
Comp_B_interruptToggleEdgeDirection | Comp_B_toggleInterruptEdgeDirection
COMP_B_IOSwap | Comp_B_swapIO
Comp_B_IOSwap | Comp_B_swapIO
COMP_B_outputValue | Comp_B_outputValue
Comp_B_setReferenceVoltage | Comp_B_configureReferenceVoltage
COMP_B_setReferenceVoltage | Comp_B_setReferenceVoltage
COMP_B_shortInputs | Comp_B_shortInputs
COMP_B_unshortInputs | Comp_B_unshortInputs
CRC_setData | CRC_set16BitData
CRC_setDataByteBitsReversed | CRC_set16BitDataReversed
DAC12_A_initialize | DAC12_A_init
DMA_initialize | DMA_init
DMA_NMIAbortStatus | DMA_getNMIAbortStatus
EUSCI_A_SPI_clearInterruptFlag | EUSCI_A_SPI_clearInterrupt
EUSCI_A_SPI_getReceiveBufferAddressForDMA | EUSCI_A_SPI_getReceiveBufferAddress
EUSCI_A_SPI_getTransmitBufferAddressForDMA | EUSCI_A_SPI_getTransmitBufferAddress
EUSCI_A_SPI_masterChangeClock | EUSCI_A_SPI_changeMasterClock
EUSCI_A_SPI_masterInit | EUSCI_A_SPI_initMaster
EUSCI_A_SPI_slaveInit | EUSCI_A_SPI_initSlave
EUSCI_A_UART_clearInterruptFlag | EUSCI_A_UART_clearInterrupt
EUSCI_A_UART_getReceiveBufferAddressForDMA | EUSCI_A_UART_getReceiveBufferAddress
EUSCI_A_UART_getTransmitBufferAddressForDMA | EUSCI_A_UART_getTransmitBufferAddress
EUSCI_A_UART_initAdvance | EUSCI_A_UART_init
EUSCI_B_I2C_clearInterruptFlag | EUSCI_B_I2C_clearInterrupt
EUSCI_B_I2C_getReceiveBufferAddressForDMA | EUSCI_B_I2C_getReceiveBufferAddress
EUSCI_B_I2C_getTransmitBufferAddressForDMA | EUSCI_B_I2C_getTransmitBufferAddress
EUSCI_B_I2C_masterInit | EUSCI_B_I2C_initMaster
EUSCI_B_I2C_masterIsSTOPSent | EUSCI_B_I2C_masterIsStopSent
EUSCI_B_I2C_masterMultiByteReceiveFinish | EUSCI_B_I2C_masterReceiveMultiByteFinish
EUSCI_B_I2C_masterMultiByteReceiveFinishWithTimeout | EUSCI_B_I2C_masterReceiveMultiByteFinishWithTimeout
EUSCI_B_I2C_masterMultiByteReceiveNext | EUSCI_B_I2C_masterReceiveMultiByteNext
EUSCI_B_I2C_masterMultiByteReceiveStop | EUSCI_B_I2C_masterReceiveMultiByteStop
EUSCI_B_I2C_masterMultiByteSendFinish | EUSCI_B_I2C_masterSendMultiByteFinish
EUSCI_B_I2C_masterMultiByteSendFinishWithTimeout | EUSCI_B_I2C_masterSendMultiByteFinishWithTimeout
EUSCI_B_I2C_masterMultiByteSendNext | EUSCI_B_I2C_masterSendMultiByteNext
EUSCI_B_I2C_masterMultiByteSendNextWithTimeout | EUSCI_B_I2C_masterSendMultiByteNextWithTimeout
EUSCI_B_I2C_masterMultiByteSendStart | EUSCI_B_I2C_masterSendMultiByteStart
EUSCI_B_I2C_masterMultiByteSendStartWithTimeout | EUSCI_B_I2C_masterSendMultiByteStartWithTimeout
EUSCI_B_I2C_masterMultiByteSendStop | EUSCI_B_I2C_masterSendMultiByteStop
EUSCI_B_I2C_masterMultiByteSendStopWithTimeout | EUSCI_B_I2C_masterSendMultiByteStopWithTimeout
EUSCI_B_I2C_masterSingleReceive | EUSCI_B_I2C_masterReceiveSingle
EUSCI_B_I2C_slaveDataGet | EUSCI_B_I2C_slaveGetData
EUSCI_B_I2C_slaveDataPut | EUSCI_B_I2C_slavePutData
EUSCI_B_I2C_slaveInit | EUSCI_B_I2C_initSlave
EUSCI_B_SPI_clearInterruptFlag | EUSCI_B_SPI_clearInterrupt
EUSCI_B_SPI_getReceiveBufferAddressForDMA | EUSCI_B_SPI_getReceiveBufferAddress
EUSCI_B_SPI_getTransmitBufferAddressForDMA | EUSCI_B_SPI_getTransmitBufferAddress
EUSCI_B_SPI_masterChangeClock | EUSCI_B_SPI_changeMasterClock
EUSCI_B_SPI_masterInit | EUSCI_B_SPI_initMaster
EUSCI_B_SPI_slaveInit | EUSCI_B_SPI_initSlave
FLASH_bankErase | FlashCtl_eraseBank
FLASH_eraseCheck | FlashCtl_eraseCheck
FLASH_lockInfoA | FlashCtl_lockInfoA
FLASH_massErase | FlashCtl_performMassErase
FLASH_memoryFill32 | FlashCtl_fillMemory32
FLASH_segmentErase | FlashCtl_eraseSegment
FLASH_status | FlashCtl_status
FLASH_unlockInfoA | FlashCtl_unlockInfoA
FLASH_write16 | FlashCtl_write16
FLASH_write32 | FlashCtl_write32
FLASH_write8 | FlashCtl_write8
FlashCtl_bankErase | FlashCtl_eraseBank
FlashCtl_eraseCheck | FlashCtl_performEraseCheck
FlashCtl_massErase | FlashCtl_performMassErase
FlashCtl_memoryFill32 | FlashCtl_fillMemory32
FlashCtl_segmentErase | FlashCtl_eraseSegment
FlashCtl_status | FlashCtl_getStatus
GPIO_clearInterruptFlag | GPIO_clearInterrupt
GPIO_interruptEdgeSelect | GPIO_selectInterruptEdge
GPIO_setAsInputPinWithPullDownresistor | GPIO_setAsInputPinWithPullDownResistor
GPIO_setAsInputPinWithPullUpresistor | GPIO_setAsInputPinWithPullUpResistor
LCD_C_setMemoryCharacter | [REMOVED]
LDOPWR_clearInterruptStatus | LDOPWR_clearInterrupt
MPU_clearAllInterruptFlags | MPU_clearAllInterrupts
MPU_clearInterruptFlag | MPU_clearInterrupt
MPY32_getResult16Bit | MPY32_getResult
MPY32_getResult24Bit | MPY32_getResult
MPY32_getResult32Bit | MPY32_getResult
MPY32_getResult64Bit | MPY32_getResult
MPY32_getResult8Bit | MPY32_getResult
MPY32_resetFractionMode | MPY32_disableFractionalMode
MPY32_resetSaturationMode | MPY32_disableSaturationMode
MPY32_setFractionMode | MPY32_enableFractionalMode
MPY32_setSaturationMode | MPY32_enableSaturationMode
PMAP_configurePorts | PMAP_initPorts
PMM_regOff | PMM_turnOffRegulator
PMM_regOn | PMM_turnOnRegulator
PMM_SvsHDisabledInLPMFullPerf | PMM_disableSvsHInLPMFullPerf
PMM_SvsHDisabledInLPMNormPerf | PMM_disableSvsHInLPMNormPerf
PMM_SvsHEnabledInLPMFullPerf | PMM_enableSvsHInLPMFullPerf
PMM_SvsHEnabledInLPMNormPerf | PMM_enableSvsHInLPMNormPerf
PMM_SvsHOptimizedInLPMFullPerf | PMM_optimizeSvsHInLPMFullPerf
PMM_SvsLDisabledInLPMFastWake | PMM_disableSvsLInLPMFastWake
PMM_SvsLDisabledInLPMSlowWake | PMM_disableSvsLInLPMSlowWake
PMM_SvsLEnabledInLPMFastWake | PMM_enableSvsLInLPMFastWake
PMM_SvsLEnabledInLPMSlowWake | PMM_enableSvsLInLPMSlowWake
PMM_SvsLOptimizedInLPMFastWake | PMM_optimizeSvsLInLPMFastWake
REF_A_disableReferenceVoltage | Ref_A_disableReferenceVoltage
REF_A_disableReferenceVoltageOutput | Ref_A_disableReferenceVoltageOutput
REF_A_disableTempSensor | Ref_A_disableTempSensor
REF_A_enableReferenceVoltage | Ref_A_enableReferenceVoltage
REF_A_enableReferenceVoltageOutput | Ref_A_enableReferenceVoltageOutput
REF_A_enableTempSensor | Ref_A_enableTempSensor
REF_A_getBandgapMode | Ref_A_getBandgapMode
REF_A_getBufferedBandgapVoltageStatus | Ref_A_isBufferedBandgapVoltageReady
REF_A_getVariableReferenceVoltageStatus | Ref_A_isVariableReferenceVoltageOutputReady
REF_A_isBandgapActive | Ref_A_isBandgapActive
REF_A_isBufferedBandgapVoltageReady | Ref_A_isBufferedBandgapVoltageReady
REF_A_isRefGenActive | Ref_A_isRefGenActive
REF_A_isRefGenBusy | Ref_A_isRefGenBusy
REF_A_isVariableReferenceVoltageOutputReady | Ref_A_isVariableReferenceVoltageOutputReady
REF_A_setBufferedBandgapVoltageOneTimeTrigger | Ref_A_setBufferedBandgapVoltageOneTimeTrigger
REF_A_setReferenceVoltage | Ref_A_setReferenceVoltage
REF_A_setReferenceVoltageOneTimeTrigger | Ref_A_setReferenceVoltageOneTimeTrigger
RTC_A_calendarInit | RTC_A_initCalendar
RTC_A_CounterInit | RTC_A_initCounter
RTC_A_counterPrescaleHold | RTC_A_holdCounterPrescale
RTC_A_counterPrescaleInit | RTC_A_initCounterPrescale
RTC_A_counterPrescaleStart | RTC_A_startCounterPrescale
RTC_A_setCalendarAlarm | RTC_A_configureCalendarAlarm
RTC_A_setPrescaleCounterValue | RTC_A_setPrescaleValue
SD24_B_configureConverter | SD24_B_initConverter
SD24_B_configureConverterAdvanced | SD24_B_initConverterAdvanced
SD24_B_initialize | SD24_B_init
SYS_clearJTAGMailboxFlagStatus | SysCtl_clearJTAGMailboxFlagStatus
SYS_disableBSLMemory | SysCtl_disableBSLMemory
SYS_disableBSLProtect | SysCtl_disableBSLProtect
SYS_disableRAMBasedInterruptVectors | SysCtl_disableRAMBasedInterruptVectors
SYS_enableBSLMemory | SysCtl_enableBSLMemory
SYS_enableBSLProtect | SysCtl_enableBSLProtect
SYS_enableDedicatedJTAGPins | SysCtl_enableDedicatedJTAGPins
SYS_enablePMMAccessProtect | SysCtl_enablePMMAccessProtect
SYS_enableRAMBasedInterruptVectors | SysCtl_enableRAMBasedInterruptVectors
SYS_getBSLEntryIndication | SysCtl_getBSLEntryIndication
SYS_getJTAGInboxMessage16Bit | SysCtl_getJTAGInboxMessage16Bit
SYS_getJTAGInboxMessage32Bit | SysCtl_getJTAGInboxMessage32Bit
SYS_getJTAGMailboxFlagStatus | SysCtl_getJTAGMailboxFlagStatus
SYS_JTAGMailboxInit | SysCtl_initJTAGMailbox
SYS_setBSLSize | SysCtl_setBSLSize
SYS_setJTAGOutgoingMessage16Bit | SysCtl_setJTAGOutgoingMessage16Bit
SYS_setJTAGOutgoingMessage32Bit | SysCtl_setJTAGOutgoingMessage32Bit
SYS_setRAMAssignedToBSL | SysCtl_setRAMAssignedToBSL
SysCtl_JTAGMailboxInit | SysCtl_initJTAGMailbox
TEC_clearInterruptFlag | TEC_clearInterrupt
TEC_configureExternalClearInput | TEC_initExternalClearInput
TEC_configureExternalFaultInput | TEC_initExternalFaultInput
TIMER_A_clear | Timer_A_clear
TIMER_A_clearCaptureCompareInterruptFlag | Timer_A_clearCaptureCompareInterrupt
Timer_A_clearCaptureCompareInterruptFlag | Timer_A_clearCaptureCompareInterrupt
TIMER_A_clearTimerInterruptFlag | Timer_A_clearTimerInterrupt
Timer_A_clearTimerInterruptFlag | Timer_A_clearTimerInterrupt
Timer_A_configureContinuousMode | Timer_A_initContinuousMode
TIMER_A_configureContinuousMode | Timer_A_initContinuousMode
Timer_A_configureUpDownMode | Timer_A_initUpDownMode
TIMER_A_configureUpDownMode | Timer_A_initUpDownMode
Timer_A_configureUpMode | Timer_A_initUpMode
TIMER_A_configureUpMode | Timer_A_initUpMode
TIMER_A_disableCaptureCompareInterrupt | Timer_A_disableCaptureCompareInterrupt
TIMER_A_disableInterrupt | Timer_A_disableInterrupt
TIMER_A_enableCaptureCompareInterrupt | Timer_A_enableCaptureCompareInterrupt
TIMER_A_enableInterrupt | Timer_A_enableInterrupt
Timer_A_generatePWM | Timer_A_outputPWM
TIMER_A_generatePWM | Timer_A_outputPWM
TIMER_A_getCaptureCompareCount | Timer_A_getCaptureCompareCount
TIMER_A_getCaptureCompareInterruptStatus | Timer_A_getCaptureCompareInterruptStatus
TIMER_A_getCounterValue | Timer_A_getCounterValue
TIMER_A_getInterruptStatus | Timer_A_getInterruptStatus
TIMER_A_getOutputForOutputModeOutBitValue | Timer_A_getOutputForOutputModeOutBitValue
TIMER_A_getSynchronizedCaptureCompareInput | Timer_A_getSynchronizedCaptureCompareInput
Timer_A_initCapture | Timer_A_initCaptureMode
TIMER_A_initCapture | Timer_A_initCaptureMode
TIMER_A_initCaptureMode | Timer_A_initCaptureMode
Timer_A_initCompare | Timer_A_initCompareMode
TIMER_A_initCompare | Timer_A_initCompareMode
TIMER_A_initCompareMode | Timer_A_initCompareMode
TIMER_A_initContinuousMode | Timer_A_initContinuousMode
TIMER_A_initUpDownMode | Timer_A_initUpDownMode
TIMER_A_initUpMode | Timer_A_initUpMode
TIMER_A_outputPWM | Timer_A_outputPWM
TIMER_A_setCompareValue | Timer_A_setCompareValue
TIMER_A_setOutputForOutputModeOutBitValue | Timer_A_setOutputForOutputModeOutBitValue
Timer_A_startContinousMode | Timer_A_startCounter
TIMER_A_startContinousMode | Timer_A_startCounter
Timer_A_startContinuousMode | Timer_A_startCounter
TIMER_A_startContinuousMode | Timer_A_startCounter
TIMER_A_startCounter | Timer_A_startCounter
Timer_A_startUpDownMode | Timer_A_startCounter
TIMER_A_startUpDownMode | Timer_A_startCounter
Timer_A_startUpMode | Timer_A_startCounter
TIMER_A_startUpMode | Timer_A_startUpMode
TIMER_A_stop | Timer_A_stop
TIMER_B_clear | Timer_B_clear
TIMER_B_clearCaptureCompareInterruptFlag | Timer_B_clearCaptureCompareInterrupt
Timer_B_clearCaptureCompareInterruptFlag | Timer_B_clearCaptureCompareInterrupt
TIMER_B_clearTimerInterruptFlag | Timer_B_clearTimerInterrupt
Timer_B_clearTimerInterruptFlag | Timer_B_clearTimerInterrupt
Timer_B_configureContinuousMode | Timer_B_initContinuousMode
TIMER_B_configureContinuousMode | Timer_B_initContinuousMode
Timer_B_configureUpDownMode | Timer_B_initUpDownMode
TIMER_B_configureUpDownMode | Timer_B_initUpDownMode
Timer_B_configureUpMode | Timer_B_initUpMode
TIMER_B_configureUpMode | Timer_B_initUpMode
TIMER_B_disableCaptureCompareInterrupt | Timer_B_disableCaptureCompareInterrupt
TIMER_B_disableInterrupt | Timer_B_disableInterrupt
TIMER_B_enableCaptureCompareInterrupt | Timer_B_enableCaptureCompareInterrupt
TIMER_B_enableInterrupt | Timer_B_enableInterrupt
Timer_B_generatePWM | Timer_B_outputPWM
TIMER_B_generatePWM | Timer_B_outputPWM
TIMER_B_getCaptureCompareCount | Timer_B_getCaptureCompareCount
TIMER_B_getCaptureCompareInterruptStatus | Timer_B_getCaptureCompareInterruptStatus
TIMER_B_getCounterValue | Timer_B_getCounterValue
TIMER_B_getInterruptStatus | Timer_B_getInterruptStatus
TIMER_B_getOutputForOutputModeOutBitValue | Timer_B_getOutputForOutputModeOutBitValue
TIMER_B_getSynchronizedCaptureCompareInput | Timer_B_getSynchronizedCaptureCompareInput
Timer_B_initCapture | Timer_B_initCaptureMode
TIMER_B_initCapture | Timer_B_initCaptureMode
TIMER_B_initCaptureMode | Timer_B_initCaptureMode
Timer_B_initCompare | Timer_B_initCompareMode
TIMER_B_initCompare | Timer_B_initCompareMode
TIMER_B_initCompareLatchLoadEvent | Timer_B_initCompareLatchLoadEvent
TIMER_B_initCompareMode | Timer_B_initCompareMode
TIMER_B_initContinuousMode | Timer_B_initContinuousMode
TIMER_B_initUpDownMode | Timer_B_initUpDownMode
TIMER_B_initUpMode | Timer_B_initUpMode
TIMER_B_outputPWM | Timer_B_outputPWM
TIMER_B_selectCounterLength | Timer_B_selectCounterLength
TIMER_B_selectLatchingGroup | Timer_B_selectLatchingGroup
TIMER_B_setCompareValue | Timer_B_setCompareValue
TIMER_B_setOutputForOutputModeOutBitValue | Timer_B_setOutputForOutputModeOutBitValue
Timer_B_startContinousMode | Timer_B_startCounter
TIMER_B_startContinousMode | Timer_B_startCounter
Timer_B_startContinuousMode | Timer_B_startCounter
TIMER_B_startContinuousMode | Timer_B_startCounter
TIMER_B_startCounter | Timer_B_startCounter
Timer_B_startUpDownMode | Timer_B_startCounter
TIMER_B_startUpDownMode | Timer_B_startCounter
Timer_B_startUpMode | Timer_B_startCounter
TIMER_B_startUpMode | Timer_B_startCounter
TIMER_B_stop | Timer_B_stop
TIMER_D_clear | Timer_D_clear
TIMER_D_clearCaptureCompareInterruptFlag | Timer_D_clearCaptureCompareInterrupt
Timer_D_clearCaptureCompareInterruptFlag | Timer_D_clearCaptureCompareInterrupt
TIMER_D_clearHighResInterruptStatus | Timer_D_clearHighResInterrupt
Timer_D_clearHighResInterruptStatus | Timer_D_clearHighResInterrupt
TIMER_D_clearTimerInterruptFlag | Timer_D_clearTimerInterrupt
Timer_D_clearTimerInterruptFlag | Timer_D_clearTimerInterrupt
Timer_D_combineTDCCRToGeneratePWM | Timer_D_combineTDCCRToOuputPWM
TIMER_D_combineTDCCRToGeneratePWM | Timer_D_combineTDCCRToOuputPWM
TIMER_D_combineTDCCRToOutputPWM | Timer_D_combineTDCCRToOutputPWM
Timer_D_configureContinuousMode | Timer_D_initContinuousMode
TIMER_D_configureContinuousMode | Timer_D_initContinuousMode
TIMER_D_configureHighResGeneratorInFreeRunningMode | Timer_D_initHighResGeneratorInFreeRunningMode
Timer_D_configureHighResGeneratorInRegulatedMode | Timer_D_initHighResGeneratorInRegulatedMode
TIMER_D_configureHighResGeneratorInRegulatedMode | Timer_D_initHighResGeneratorInRegulatedMode
Timer_D_configureUpDownMode | Timer_D_initUpDownMode
TIMER_D_configureUpDownMode | Timer_D_initUpDownMode
Timer_D_configureUpMode | Timer_D_initUpMode
TIMER_D_configureUpMode | Timer_D_initUpMode
TIMER_D_disableCaptureCompareInterrupt | Timer_D_disableCaptureCompareInterrupt
TIMER_D_disableHighResClockEnhancedAccuracy | Timer_D_disableHighResClockEnhancedAccuracy
TIMER_D_disableHighResFastWakeup | Timer_D_disableHighResFastWakeup
TIMER_D_DisableHighResGeneratorForceON | Timer_D_disableHighResGeneratorForceON
TIMER_D_disableHighResGeneratorForceON | Timer_D_disableHighResGeneratorForceON
TIMER_D_disableHighResInterrupt | Timer_D_disableHighResInterrupt
TIMER_D_disableTimerInterrupt | Timer_D_disableTimerInterrupt
TIMER_D_enableCaptureCompareInterrupt | Timer_D_enableCaptureCompareInterrupt
TIMER_D_enableHighResClockEnhancedAccuracy | Timer_D_enableHighResClockEnhancedAccuracy
TIMER_D_enableHighResFastWakeup | Timer_D_enableHighResFastWakeup
TIMER_D_EnableHighResGeneratorForceON | Timer_D_enableHighResGeneratorForceON
TIMER_D_enableHighResGeneratorForceON | Timer_D_enableHighResGeneratorForceON
TIMER_D_enableHighResInterrupt | Timer_D_enableHighResInterrupt
TIMER_D_enableTimerInterrupt | Timer_D_enableTimerInterrupt
Timer_D_generatePWM | Timer_D_outputPWM
TIMER_D_generatePWM | Timer_D_outputPWM
TIMER_D_getCaptureCompareCount | Timer_D_getCaptureCompareCount
TIMER_D_getCaptureCompareInputSignal | Timer_D_getCaptureCompareInputSignal
TIMER_D_getCaptureCompareInterruptStatus | Timer_D_getCaptureCompareInterruptStatus
TIMER_D_getCaptureCompareLatchCount | Timer_D_getCaptureCompareLatchCount
TIMER_D_getCounterValue | Timer_D_getCounterValue
TIMER_D_getHighResInterruptStatus | Timer_D_getHighResInterruptStatus
TIMER_D_getOutputForOutputModeOutBitValue | Timer_D_getOutputForOutputModeOutBitValue
TIMER_D_getSynchronizedCaptureCompareInput | Timer_D_getSynchronizedCaptureCompareInput
TIMER_D_getTimerInterruptStatus | Timer_D_getTimerInterruptStatus
Timer_D_initCapture | Timer_D_initCaptureMode
TIMER_D_initCapture | Timer_D_initCaptureMode
TIMER_D_initCaptureMode | Timer_D_initCaptureMode
Timer_D_initCompare | Timer_D_initCompareMode
TIMER_D_initCompare | Timer_D_initCompareMode
TIMER_D_initCompareLatchLoadEvent | Timer_D_initCompareLatchLoadEvent
TIMER_D_initCompareMode | Timer_D_initCompareMode
TIMER_D_initContinuousMode | Timer_D_initContinuousMode
TIMER_D_initHighResGeneratorInFreeRunningMode | Timer_D_initHighResGeneratorInFreeRunningMode
TIMER_D_initHighResGeneratorInRegulatedMode | Timer_D_initHighResGeneratorInRegulatedMode
TIMER_D_initUpDownMode | Timer_D_initUpDownMode
TIMER_D_initUpMode | Timer_D_initUpMode
TIMER_D_outputPWM | Timer_D_outputPWM
TIMER_D_selectCounterLength | Timer_D_selectCounterLength
TIMER_D_selectHighResClockRange | Timer_D_selectHighResClockRange
TIMER_D_selectHighResCoarseClockRange | Timer_D_selectHighResCoarseClockRange
TIMER_D_selectLatchingGroup | Timer_D_selectLatchingGroup
TIMER_D_setCompareValue | Timer_D_setCompareValue
TIMER_D_setOutputForOutputModeOutBitValue | Timer_D_setOutputForOutputModeOutBitValue
TIMER_D_startCounter | Timer_D_startCounter
TIMER_D_stop | Timer_D_stop
UCS_clockSignalInit | UCS_initClockSignal
UCS_faultFlagStatus | UCS_getFaultFlagStatus
UCS_HFXT1Start | UCS_turnOnHFXT1
UCS_HFXT1StartWithTimeout | UCS_turnOnHFXT1WithTimeout
UCS_LFXT1Start | UCS_turnOnLFXT1
UCS_LFXT1StartWithTimeout | UCS_turnOnLFXT1WithTimeout
UCS_SMCLKOff | UCS_turnOffSMCLK
UCS_SMCLKOn | UCS_turnOnSMCLK
UCS_XT1Off | UCS_turnOffXT1
UCS_XT2Off | UCS_turnOffXT2
UCS_XT2Start | UCS_turnOnXT2
UCS_XT2StartWithTimeout | UCS_turnOnXT2WithTimeout
USCI_A_SPI_clearInterruptFlag | USCI_A_SPI_clearInterrupt
USCI_A_SPI_masterChangeClock | USCI_A_SPI_changeMasterClock
USCI_A_SPI_masterInit | USCI_A_SPI_initMaster
USCI_A_SPI_slaveInit | USCI_A_SPI_initSlave
USCI_A_UART_clearInterruptFlag | USCI_A_UART_clearInterrupt
USCI_A_UART_initAdvance | USCI_A_UART_init
USCI_B_I2C_clearInterruptFlag | USCI_B_I2C_clearInterrupt
USCI_B_I2C_masterInit | USCI_B_I2C_initMaster
USCI_B_I2C_masterIsSTOPSent | USCI_B_I2C_masterIsStopSent
USCI_B_I2C_masterMultiByteReceiveFinish | USCI_B_I2C_masterReceiveMultiByteFinish
USCI_B_I2C_masterMultiByteReceiveFinishWithTimeout | USCI_B_I2C_masterReceiveMultiByteFinishWithTimeout
USCI_B_I2C_masterMultiByteReceiveNext | USCI_B_I2C_masterReceiveMultiByteNext
USCI_B_I2C_masterMultiByteReceiveStart | USCI_B_I2C_masterReceiveMultiByteStart
USCI_B_I2C_masterMultiByteReceiveStop | USCI_B_I2C_masterReceiveMultiByteStop
USCI_B_I2C_masterMultiByteSendFinish | USCI_B_I2C_masterSendMultiByteFinish
USCI_B_I2C_masterMultiByteSendFinishWithTimeout | USCI_B_I2C_masterSendMultiByteFinishWithTimeout
USCI_B_I2C_masterMultiByteSendNext | USCI_B_I2C_masterSendMultiByteNext
USCI_B_I2C_masterMultiByteSendNextWithTimeout | USCI_B_I2C_masterSendMultiByteNextWithTimeout
USCI_B_I2C_masterMultiByteSendStart | USCI_B_I2C_masterSendMultiByteStart
USCI_B_I2C_masterMultiByteSendStartWithTimeout | USCI_B_I2C_masterSendMultiByteStartWithTimeout
USCI_B_I2C_masterMultiByteSendStop | USCI_B_I2C_masterSendMultiByteStop
USCI_B_I2C_masterMultiByteSendStopWithTimeout | USCI_B_I2C_masterSendMultiByteStopWithTimeout
USCI_B_I2C_masterSingleReceive | USCI_B_I2C_masterReceiveSingle
USCI_B_I2C_masterSingleReceiveStart | USCI_B_I2C_masterReceiveSingleStart
USCI_B_I2C_masterSingleReceiveStartWithTimeout | USCI_B_I2C_masterReceiveSingleStartWithTimeout
USCI_B_I2C_slaveDataGet | USCI_B_I2C_slaveGetData
USCI_B_I2C_slaveDataPut | USCI_B_I2C_slavePutData
USCI_B_I2C_slaveInit | USCI_B_I2C_initSlave
USCI_B_SPI_clearInterruptFlag | USCI_B_SPI_clearInterrupt
USCI_B_SPI_masterChangeClock | USCI_B_SPI_changeMasterClock
USCI_B_SPI_masterInit | USCI_B_SPI_initMaster
USCI_B_SPI_slaveInit | USCI_B_SPI_initSlave
WDT_A_intervalTimerInit | WDT_A_initIntervalTimer
WDT_A_watchdogTimerInit | WDT_A_initWatchdogTimer

eusci_i2c.c/eusci_i2c.h files are replaced with eusci_b_i2c.c/eusci_b_i2c.h
eusci_spi.c/eusci_spi.h files are replaced with eusci_a_spi.c/eusci_a_spi.h/eusci_b_spi.c/eusci_b_spi.h
eusci_uart.c/eusci_uart.h files are replaced with eusci_a_uart.c/eusci_a_uart.h
usci_i2c.c/usci_i2c.h files are replaced with usci_b_i2c.c/usci_b_i2c.h
usci_spi.c/usci_spi.h files are replaced with usci_a_spi.c/usci_a_spi.h/usci_b_spi.c/usci_b_spi.h
usci_uart.c/usci_uart.h files are replaced with usci_a_uart.c/usci_a_uart.h
MSP430FR5xx_6xx Family

Old API | New API
ADC12_B_initialize | ADC12_B_init
ADC12_B_memoryConfigure | ADC12_B_configureMemory
AES256_clearInterruptFlag | AES256_clearInterrupt
AES256_getInterruptFlagStatus | AES256_getInterruptStatus
COMP_E_clearInterrupt | Comp_E_clearInterrupt
COMP_E_disable | Comp_E_disable
COMP_E_disableInputBuffer | Comp_E_disableInputBuffer
COMP_E_disableInterrupt | Comp_E_disableInterrupt
COMP_E_enable | Comp_E_enable
COMP_E_enableInputBuffer | Comp_E_enableInputBuffer
COMP_E_enableInterrupt | Comp_E_enableInterrupt
COMP_E_getInterruptStatus | Comp_E_getInterruptStatus
COMP_E_init | Comp_E_init
COMP_E_initialize | COMP_E_init
COMP_E_interruptSetEdgeDirection | Comp_E_setInterruptEdgeDirection
Comp_E_interruptSetEdgeDirection | Comp_E_setInterruptEdgeDirection
COMP_E_interruptToggleEdgeDirection | Comp_E_toggleInterruptEdgeDirection
Comp_E_interruptToggleEdgeDirection | Comp_E_toggleInterruptEdgeDirection
COMP_E_IOSwap | Comp_E_swapIO
Comp_E_IOSwap | Comp_E_swapIO
COMP_E_outputValue | Comp_E_outputValue
COMP_E_setPowerMode | Comp_E_setPowerMode
COMP_E_setReferenceAccuracy | Comp_E_setReferenceAccuracy
COMP_E_setReferenceVoltage | Comp_E_setReferenceVoltage
COMP_E_shortInputs | Comp_E_shortInputs
COMP_E_unshortInputs | Comp_E_unshortInputs
CRC_setData | CRC_set16BitData
CRC_setDataByteBitsReversed | CRC_set16BitDataReversed
CS_clockSignalInit | CS_initClockSignal
CS_faultFlagStatus | CS_getFaultFlagStatus
CS_HFXTOff | CS_turnOffHFXT
CS_HFXTStart | CS_turnOnHFXT
CS_HFXTStartWithTimeout | CS_turnOnHFXTWithTimeout
CS_LFXTOff | CS_turnOffLFXT
CS_LFXTStart | CS_turnOnLFXT
CS_LFXTStartWithTimeout | CS_turnOnLFXTWithTimeout
CS_VLOoff | CS_turnOffVLO
DMA_initialize | DMA_init
DMA_NMIAbortStatus | DMA_getNMIAbortStatus
ESI_clearInterruptFlag | ESI_clearInterrupt
EUSCI_A_SPI_clearInterruptFlag | EUSCI_A_SPI_clearInterrupt
EUSCI_A_SPI_getReceiveBufferAddressForDMA | EUSCI_A_SPI_getReceiveBufferAddress
EUSCI_A_SPI_getTransmitBufferAddressForDMA | EUSCI_A_SPI_getTransmitBufferAddress
EUSCI_A_SPI_masterChangeClock | EUSCI_A_SPI_changeMasterClock
EUSCI_A_SPI_masterInit | EUSCI_A_SPI_initMaster
EUSCI_A_SPI_slaveInit | EUSCI_A_SPI_initSlave
EUSCI_A_UART_clearInterruptFlag | EUSCI_A_UART_clearInterrupt
EUSCI_A_UART_getReceiveBufferAddressForDMA | EUSCI_A_UART_getReceiveBufferAddress
EUSCI_A_UART_getTransmitBufferAddressForDMA | EUSCI_A_UART_getTransmitBufferAddress
EUSCI_A_UART_initAdvance | EUSCI_A_UART_init
EUSCI_B_I2C_clearInterruptFlag | EUSCI_B_I2C_clearInterrupt
EUSCI_B_I2C_getReceiveBufferAddressForDMA | EUSCI_B_I2C_getReceiveBufferAddress
EUSCI_B_I2C_getTransmitBufferAddressForDMA | EUSCI_B_I2C_getTransmitBufferAddress
EUSCI_B_I2C_masterInit | EUSCI_B_I2C_initMaster
EUSCI_B_I2C_masterIsSTOPSent | EUSCI_B_I2C_masterIsStopSent
EUSCI_B_I2C_masterMultiByteReceiveFinish | EUSCI_B_I2C_masterReceiveMultiByteFinish
EUSCI_B_I2C_masterMultiByteReceiveFinishWithTimeout | EUSCI_B_I2C_masterReceiveMultiByteFinishWithTimeout
EUSCI_B_I2C_masterMultiByteReceiveNext | EUSCI_B_I2C_masterReceiveMultiByteNext
EUSCI_B_I2C_masterMultiByteReceiveStop | EUSCI_B_I2C_masterReceiveMultiByteStop
EUSCI_B_I2C_masterMultiByteSendFinish | EUSCI_B_I2C_masterSendMultiByteFinish
EUSCI_B_I2C_masterMultiByteSendFinishWithTimeout | EUSCI_B_I2C_masterSendMultiByteFinishWithTimeout
EUSCI_B_I2C_masterMultiByteSendNext | EUSCI_B_I2C_masterSendMultiByteNext
EUSCI_B_I2C_masterMultiByteSendNextWithTimeout | EUSCI_B_I2C_masterSendMultiByteNextWithTimeout
EUSCI_B_I2C_masterMultiByteSendStart | EUSCI_B_I2C_masterSendMultiByteStart
EUSCI_B_I2C_masterMultiByteSendStartWithTimeout | EUSCI_B_I2C_masterSendMultiByteStartWithTimeout
EUSCI_B_I2C_masterMultiByteSendStop | EUSCI_B_I2C_masterSendMultiByteStop
EUSCI_B_I2C_masterMultiByteSendStopWithTimeout | EUSCI_B_I2C_masterSendMultiByteStopWithTimeout
EUSCI_B_I2C_masterSingleReceive | EUSCI_B_I2C_masterReceiveSingle
EUSCI_B_I2C_slaveDataGet | EUSCI_B_I2C_slaveGetData
EUSCI_B_I2C_slaveDataPut | EUSCI_B_I2C_slavePutData
EUSCI_B_I2C_slaveInit | EUSCI_B_I2C_initSlave
EUSCI_B_SPI_clearInterruptFlag | EUSCI_B_SPI_clearInterrupt
EUSCI_B_SPI_getReceiveBufferAddressForDMA | EUSCI_B_SPI_getReceiveBufferAddress
EUSCI_B_SPI_getTransmitBufferAddressForDMA | EUSCI_B_SPI_getTransmitBufferAddress
EUSCI_B_SPI_masterChangeClock | EUSCI_B_SPI_changeMasterClock
EUSCI_B_SPI_masterInit | EUSCI_B_SPI_initMaster
EUSCI_B_SPI_slaveInit | EUSCI_B_SPI_initSlave
FRAM_configureWaitStateControl | FRAMCtl_configureWaitStateControl
FRAM_delayPowerUpFromLPM | FRAMCtl_delayPowerUpFromLPM
FRAM_disableInterrupt | FRAMCtl_disableInterrupt
FRAM_enableInterrupt | FRAMCtl_enableInterrupt
FRAM_getInterruptStatus | FRAMCtl_getInterruptStatus
FRAM_memoryFill32 | FRAMCtl_memoryFill32
FRAM_write16 | FRAMCtl_write16
FRAM_write32 | FRAMCtl_write32
FRAM_write8 | FRAMCtl_write8
GPIO_clearInterruptFlag | GPIO_clearInterrupt
GPIO_interruptEdgeSelect | GPIO_selectInterruptEdge
GPIO_setAsInputPinWithPullDownresistor | GPIO_setAsInputPinWithPullDownResistor
GPIO_setAsInputPinWithPullUpresistor | GPIO_setAsInputPinWithPullUpResistor
LCD_C_setMemoryCharacter | [REMOVED]
MPU_clearAllInterruptFlags | MPU_clearAllInterrupts
MPU_clearInterruptFlag | MPU_clearInterrupt
MPU_createThreeSegments | MPU_initThreeSegments
MPU_createTwoSegments | MPU_initTwoSegments
MPY32_getResult16Bit | MPY32_getResult
MPY32_getResult24Bit | MPY32_getResult
MPY32_getResult32Bit | MPY32_getResult
MPY32_getResult64Bit | MPY32_getResult
MPY32_getResult8Bit | MPY32_getResult
MPY32_resetFractionMode | MPY32_disableFractionalMode
MPY32_resetSaturationMode | MPY32_disableSaturationMode
MPY32_setFractionMode | MPY32_enableFractionalMode
MPY32_setSaturationMode | MPY32_enableSaturationMode
PMAP_configurePorts | PMAP_initPorts
PMM_regOff | PMM_turnOffRegulator
PMM_regOn | PMM_turnOnRegulator
REF_A_disableReferenceVoltage | Ref_A_disableReferenceVoltage
REF_A_disableReferenceVoltageOutput | Ref_A_disableReferenceVoltageOutput
REF_A_disableTempSensor | Ref_A_disableTempSensor
REF_A_enableReferenceVoltage | Ref_A_enableReferenceVoltage
REF_A_enableReferenceVoltageOutput | Ref_A_enableReferenceVoltageOutput
REF_A_enableTempSensor | Ref_A_enableTempSensor
REF_A_getBandgapMode | Ref_A_getBandgapMode
REF_A_getBufferedBandgapVoltageStatus | Ref_A_isBufferedBandgapVoltageReady
REF_A_getVariableReferenceVoltageStatus | Ref_A_isVariableReferenceVoltageOutputReady
REF_A_isBandgapActive | Ref_A_isBandgapActive
REF_A_isBufferedBandgapVoltageReady | Ref_A_isBufferedBandgapVoltageReady
REF_A_isRefGenActive | Ref_A_isRefGenActive
REF_A_isRefGenBusy | Ref_A_isRefGenBusy
REF_A_isVariableReferenceVoltageOutputReady | Ref_A_isVariableReferenceVoltageOutputReady
REF_A_setBufferedBandgapVoltageOneTimeTrigger | Ref_A_setBufferedBandgapVoltageOneTimeTrigger
REF_A_setReferenceVoltage | Ref_A_setReferenceVoltage
REF_A_setReferenceVoltageOneTimeTrigger | Ref_A_setReferenceVoltageOneTimeTrigger
RTC_B_calendarInit | RTC_B_initCalendar
RTC_B_setCalendarAlarm | RTC_B_configureCalendarAlarm
RTC_B_setPrescaleCounterValue | RTC_B_setPrescaleValue
RTC_C_calendarInit | RTC_C_initCalendar
RTC_C_counterInit | RTC_C_initCounter
RTC_C_counterPrescaleHold | RTC_C_holdCounterPrescale
RTC_C_counterPrescaleInit | RTC_C_initCounterPrescale
RTC_C_counterPrescaleStart | RTC_C_startCounterPrescale
RTC_C_setCalendarAlarm | RTC_C_configureCalendarAlarm
SYS_clearJTAGMailboxFlagStatus | SysCtl_clearJTAGMailboxFlagStatus
SYS_disableBSLMemory | [REMOVED]
SYS_disableBSLProtect | [REMOVED]
SYS_disableRAMBasedInterruptVectors | SysCtl_disableRAMBasedInterruptVectors
SYS_enableBSLMemory | [REMOVED]
SYS_enableBSLProtect | [REMOVED]
SYS_enableDedicatedJTAGPins | SysCtl_enableDedicatedJTAGPins
SYS_enablePMMAccessProtect | SysCtl_enablePMMAccessProtect
SYS_enableRAMBasedInterruptVectors | SysCtl_enableRAMBasedInterruptVectors
SYS_getBSLEntryIndication | SysCtl_getBSLEntryIndication
SYS_getJTAGInboxMessage16Bit | SysCtl_getJTAGInboxMessage16Bit
SYS_getJTAGInboxMessage32Bit | SysCtl_getJTAGInboxMessage32Bit
SYS_getJTAGMailboxFlagStatus | SysCtl_getJTAGMailboxFlagStatus
SYS_JTAGMailboxInit | SysCtl_initJTAGMailbox
SYS_setBSLSize | SysCtl_setBSLSize
SYS_setJTAGOutgoingMessage16Bit | SysCtl_setJTAGOutgoingMessage16Bit
SYS_setJTAGOutgoingMessage32Bit | SysCtl_setJTAGOutgoingMessage32Bit
SYS_setRAMAssignedToBSL | SysCtl_setRAMAssignedToBSL
SysCtl_disableBSLMemory | [REMOVED]
SysCtl_disableBSLProtect | [REMOVED]
SysCtl_enableBSLMemory | [REMOVED]
SysCtl_enableBSLProtect | [REMOVED]
SysCtl_JTAGMailboxInit | SysCtl_initJTAGMailbox
SysCtl_setBSLSize | [REMOVED]
SysCtl_setRAMAssignedToBSL | [REMOVED]
TIMER_A_clear | Timer_A_clear
TIMER_A_clearCaptureCompareInterruptFlag | Timer_A_clearCaptureCompareInterrupt
Timer_A_clearCaptureCompareInterruptFlag | Timer_A_clearCaptureCompareInterrupt
Timer_A_clearCaptureCompareInterruptFlag | Timer_A_clearCaptureCompareInterrupt
Timer_A_clearTimerInterruptFlag | Timer_A_clearTimerInterrupt
TIMER_A_clearTimerInterruptFlag | Timer_A_clearTimerInterrupt
Timer_A_clearTimerInterruptFlag | Timer_A_clearTimerInterrupt
Timer_A_configureContinuousMode | Timer_A_initContinuousMode
TIMER_A_configureContinuousMode | Timer_A_initContinuousMode
Timer_A_configureUpDownMode | Timer_A_initUpDownMode
TIMER_A_configureUpDownMode | Timer_A_initUpDownMode
Timer_A_configureUpMode | Timer_A_initUpMode
TIMER_A_configureUpMode | Timer_A_initUpMode
TIMER_A_disableCaptureCompareInterrupt | Timer_A_disableCaptureCompareInterrupt
TIMER_A_disableInterrupt | Timer_A_disableInterrupt
TIMER_A_enableCaptureCompareInterrupt | Timer_A_enableCaptureCompareInterrupt
TIMER_A_enableInterrupt | Timer_A_enableInterrupt
Timer_A_generatePWM | Timer_A_outputPWM
TIMER_A_generatePWM | Timer_A_outputPWM
TIMER_A_getCaptureCompareCount | Timer_A_getCaptureCompareCount
TIMER_A_getCaptureCompareInterruptStatus | Timer_A_getCaptureCompareInterruptStatus
TIMER_A_getCounterValue | Timer_A_getCounterValue
TIMER_A_getInterruptStatus | Timer_A_getInterruptStatus
TIMER_A_getOutputForOutputModeOutBitValue | Timer_A_getOutputForOutputModeOutBitValue
TIMER_A_getSynchronizedCaptureCompareInput | Timer_A_getSynchronizedCaptureCompareInput
Timer_A_initCapture | Timer_A_initCaptureMode
TIMER_A_initCapture | Timer_A_initCaptureMode
TIMER_A_initCaptureMode | Timer_A_initCaptureMode
Timer_A_initCompare | Timer_A_initCompareMode
TIMER_A_initCompare | Timer_A_initCompareMode
TIMER_A_initCompareMode | Timer_A_initCompareMode
TIMER_A_initContinuousMode | Timer_A_initContinuousMode
TIMER_A_initUpDownMode | Timer_A_initUpDownMode
TIMER_A_initUpMode | Timer_A_initUpMode
TIMER_A_outputPWM | Timer_A_outputPWM
TIMER_A_setCompareValue | Timer_A_setCompareValue
TIMER_A_setOutputForOutputModeOutBitValue | Timer_A_setOutputForOutputModeOutBitValue
Timer_A_startContinousMode | Timer_A_startCounter
TIMER_A_startContinousMode | Timer_A_startCounter
Timer_A_startContinuousMode | Timer_A_startCounter
TIMER_A_startContinuousMode | Timer_A_startCounter
TIMER_A_startCounter | Timer_A_startCounter
Timer_A_startUpDownMode | Timer_A_startCounter
TIMER_A_startUpDownMode | Timer_A_startCounter
Timer_A_startUpMode | Timer_A_startCounter
TIMER_A_startUpMode | Timer_A_startUpMode
TIMER_A_stop | Timer_A_stop
TIMER_B_clear | Timer_B_clear
TIMER_B_clearCaptureCompareInterruptFlag | Timer_B_clearCaptureCompareInterrupt
Timer_B_clearCaptureCompareInterruptFlag | Timer_B_clearCaptureCompareInterrupt
Timer_B_clearCaptureCompareInterruptFlag | Timer_B_clearCaptureCompareInterrupt
Timer_B_clearTimerInterruptFlag | Timer_B_clearTimerInterrupt
TIMER_B_clearTimerInterruptFlag | Timer_B_clearTimerInterrupt
Timer_B_clearTimerInterruptFlag | Timer_B_clearTimerInterrupt
Timer_B_configureContinuousMode | Timer_B_initContinuousMode
TIMER_B_configureContinuousMode | Timer_B_initContinuousMode
Timer_B_configureUpDownMode | Timer_B_initUpDownMode
TIMER_B_configureUpDownMode | Timer_B_initUpDownMode
Timer_B_configureUpMode | Timer_B_initUpMode
TIMER_B_configureUpMode | Timer_B_initUpMode
TIMER_B_disableCaptureCompareInterrupt | Timer_B_disableCaptureCompareInterrupt
TIMER_B_disableInterrupt | Timer_B_disableInterrupt
TIMER_B_enableCaptureCompareInterrupt | Timer_B_enableCaptureCompareInterrupt
TIMER_B_enableInterrupt | Timer_B_enableInterrupt
Timer_B_generatePWM | Timer_B_outputPWM
TIMER_B_generatePWM | Timer_B_outputPWM
TIMER_B_getCaptureCompareCount | Timer_B_getCaptureCompareCount
TIMER_B_getCaptureCompareInterruptStatus | Timer_B_getCaptureCompareInterruptStatus
TIMER_B_getCounterValue | Timer_B_getCounterValue
TIMER_B_getInterruptStatus | Timer_B_getInterruptStatus
TIMER_B_getOutputForOutputModeOutBitValue | Timer_B_getOutputForOutputModeOutBitValue
TIMER_B_getSynchronizedCaptureCompareInput | Timer_B_getSynchronizedCaptureCompareInput
Timer_B_initCapture | Timer_B_initCaptureMode
TIMER_B_initCapture | Timer_B_initCaptureMode
TIMER_B_initCaptureMode | Timer_B_initCaptureMode
Timer_B_initCompare | Timer_B_initCompareMode
TIMER_B_initCompare | Timer_B_initCompareMode
TIMER_B_initCompareLatchLoadEvent | Timer_B_initCompareLatchLoadEvent
TIMER_B_initCompareMode | Timer_B_initCompareMode
TIMER_B_initContinuousMode | Timer_B_initContinuousMode
TIMER_B_initUpDownMode | Timer_B_initUpDownMode
TIMER_B_initUpMode | Timer_B_initUpMode
TIMER_B_outputPWM | Timer_B_outputPWM
TIMER_B_selectCounterLength | Timer_B_selectCounterLength
TIMER_B_selectLatchingGroup | Timer_B_selectLatchingGroup
TIMER_B_setCompareValue | Timer_B_setCompareValue
TIMER_B_setOutputForOutputModeOutBitValue | Timer_B_setOutputForOutputModeOutBitValue
Timer_B_startContinousMode | Timer_B_startCounter
TIMER_B_startContinousMode | Timer_B_startCounter
Timer_B_startContinuousMode | Timer_B_startCounter
TIMER_B_startContinuousMode | Timer_B_startCounter
TIMER_B_startCounter | Timer_B_startCounter
Timer_B_startUpDownMode | Timer_B_startCounter
TIMER_B_startUpDownMode | Timer_B_startCounter
Timer_B_startUpMode | Timer_B_startCounter
TIMER_B_startUpMode | Timer_B_startCounter
TIMER_B_stop | Timer_B_stop
WDT_A_intervalTimerInit | WDT_A_initIntervalTimer
WDT_A_watchdogTimerInit | WDT_A_initWatchdogTimer

MSP430FR57xx Family

Old API | New API
ADC10_B_memoryConfgiure | ADC10_B_configureMemory
AES256_clearInterruptFlag | AES256_clearInterrupt
AES256_getInterruptFlagStatus | AES256_getInterruptStatus
COMP_D_clearInterrupt | Comp_D_clearInterrupt
COMP_D_disable | Comp_D_disable
COMP_D_disableInputBuffer | Comp_D_disableInputBuffer
COMP_D_disableInterrupt | Comp_D_disableInterrupt
COMP_D_enable | Comp_D_enable
COMP_D_enableInputBuffer | Comp_D_enableInputBuffer
COMP_D_enableInterrupt | Comp_D_enableInterrupt
COMP_D_getInterruptStatus | Comp_D_getInterruptStatus
COMP_D_init | Comp_D_init
COMP_D_initialize | Comp_D_init
COMP_D_interruptSetEdgeDirection | Comp_D_setInterruptEdgeDirection
COMP_D_interruptToggleEdgeDirection | Comp_D_toggleInterruptEdgeDirection
Comp_D_interruptSetEdgeDirection | Comp_D_setInterruptEdgeDirection
Comp_D_interruptToggleEdgeDirection | Comp_D_toggleInterruptEdgeDirection
COMP_D_IOSwap | Comp_D_swapIO
Comp_D_IOSwap | Comp_D_swapIO
COMP_D_outputValue | Comp_D_outputValue
COMP_D_setReferenceAccuracy | Comp_D_setReferenceAccuracy
COMP_D_setReferenceVoltage | Comp_D_setReferenceVoltage
COMP_D_shortInputs | Comp_D_shortInputs
COMP_D_unshortInputs | Comp_D_unshortInputs
CRC_setData | CRC_set16BitData
CRC_setDataByteBitsReversed | CRC_set16BitDataReversed
CS_clockSignalInit | CS_initClockSignal
CS_faultFlagStatus | CS_getFaultFlagStatus
CS_XT1Off | CS_turnOffXT1
CS_XT1Start | CS_turnOnXT1
CS_XT1StartWithTimeout | CS_turnOnXT1WithTimeout
CS_XT2Off | CS_turnOffXT2
CS_XT2Start | CS_turnOnXT2
CS_XT2StartWithTimeout | CS_turnOnXT2WithTimeout
DMA_initialize | DMA_init
DMA_NMIAbortStatus | DMA_getNMIAbortStatus
EUSCI_A_SPI_clearInterruptFlag | EUSCI_A_SPI_clearInterrupt
EUSCI_A_SPI_getReceiveBufferAddressForDMA | EUSCI_A_SPI_getReceiveBufferAddress
EUSCI_A_SPI_getTransmitBufferAddressForDMA | EUSCI_A_SPI_getTransmitBufferAddress
EUSCI_A_SPI_masterChangeClock | EUSCI_A_SPI_changeMasterClock
EUSCI_A_SPI_masterInit | EUSCI_A_SPI_initMaster
EUSCI_A_SPI_slaveInit | EUSCI_A_SPI_initSlave
EUSCI_A_UART_clearInterruptFlag | EUSCI_A_UART_clearInterrupt
EUSCI_A_UART_getReceiveBufferAddressForDMA | EUSCI_A_UART_getReceiveBufferAddress
EUSCI_A_UART_getTransmitBufferAddressForDMA | EUSCI_A_UART_getTransmitBufferAddress
EUSCI_A_UART_initAdvance | EUSCI_A_UART_init
EUSCI_B_I2C_clearInterruptFlag | EUSCI_B_I2C_clearInterrupt
EUSCI_B_I2C_getReceiveBufferAddressForDMA | EUSCI_B_I2C_getReceiveBufferAddress
EUSCI_B_I2C_getTransmitBufferAddressForDMA | EUSCI_B_I2C_getTransmitBufferAddress
EUSCI_B_I2C_masterInit | EUSCI_B_I2C_initMaster
EUSCI_B_I2C_masterIsSTOPSent | EUSCI_B_I2C_masterIsStopSent
EUSCI_B_I2C_masterMultiByteReceiveFinish | EUSCI_B_I2C_masterReceiveMultiByteFinish
EUSCI_B_I2C_masterMultiByteReceiveFinishWithTimeout | EUSCI_B_I2C_masterReceiveMultiByteFinishWithTimeout
EUSCI_B_I2C_masterMultiByteReceiveNext | EUSCI_B_I2C_masterReceiveMultiByteNext
EUSCI_B_I2C_masterMultiByteReceiveStop | EUSCI_B_I2C_masterReceiveMultiByteStop
EUSCI_B_I2C_masterMultiByteSendFinish | EUSCI_B_I2C_masterSendMultiByteFinish
EUSCI_B_I2C_masterMultiByteSendFinishWithTimeout | EUSCI_B_I2C_masterSendMultiByteFinishWithTimeout
EUSCI_B_I2C_masterMultiByteSendNext | EUSCI_B_I2C_masterSendMultiByteNext
EUSCI_B_I2C_masterMultiByteSendNextWithTimeout | EUSCI_B_I2C_masterSendMultiByteNextWithTimeout
EUSCI_B_I2C_masterMultiByteSendStart | EUSCI_B_I2C_masterSendMultiByteStart
EUSCI_B_I2C_masterMultiByteSendStartWithTimeout | EUSCI_B_I2C_masterSendMultiByteStartWithTimeout
EUSCI_B_I2C_masterMultiByteSendStop | EUSCI_B_I2C_masterSendMultiByteStop
EUSCI_B_I2C_masterMultiByteSendStopWithTimeout | EUSCI_B_I2C_masterSendMultiByteStopWithTimeout
EUSCI_B_I2C_masterSingleReceive | EUSCI_B_I2C_masterReceiveSingle
EUSCI_B_I2C_slaveDataGet | EUSCI_B_I2C_slaveGetData
EUSCI_B_I2C_slaveDataPut | EUSCI_B_I2C_slavePutData
EUSCI_B_I2C_slaveInit | EUSCI_B_I2C_initSlave
EUSCI_B_SPI_clearInterruptFlag | EUSCI_B_SPI_clearInterrupt
EUSCI_B_SPI_getReceiveBufferAddressForDMA | EUSCI_B_SPI_getReceiveBufferAddress
EUSCI_B_SPI_getTransmitBufferAddressForDMA | EUSCI_B_SPI_getTransmitBufferAddress
EUSCI_B_SPI_masterChangeClock | EUSCI_B_SPI_changeMasterClock
EUSCI_B_SPI_masterInit | EUSCI_B_SPI_initMaster
EUSCI_B_SPI_slaveInit | EUSCI_B_SPI_initSlave
FRAM_configureWaitStateControl | FRAMCtl_configureWaitStateControl
FRAM_disableInterrupt | FRAMCtl_disableInterrupt
FRAM_enableInterrupt | FRAMCtl_enableInterrupt
FRAM_getInterruptStatus | FRAMCtl_getInterruptStatus
FRAM_memoryFill32 | FRAMCtl_memoryFill32
FRAM_write16 | FRAMCtl_write16
FRAM_write32 | FRAMCtl_write32
FRAM_write8 | FRAMCtl_write8
GPIO_clearInterruptFlag | GPIO_clearInterrupt
GPIO_interruptEdgeSelect | GPIO_selectInterruptEdge
GPIO_setAsInputPinWithPullDownresistor | GPIO_setAsInputPinWithPullDownResistor
GPIO_setAsInputPinWithPullUpresistor | GPIO_setAsInputPinWithPullUpResistor
MPU_clearAllInterruptFlags | MPU_clearAllInterrupts
MPU_clearInterruptFlag | MPU_clearInterrupt
MPU_createThreeSegments | MPU_initThreeSegments
MPU_createTwoSegments | MPU_initTwoSegments
MPY32_getResult16Bit | MPY32_getResult
MPY32_getResult24Bit | MPY32_getResult
MPY32_getResult32Bit | MPY32_getResult
MPY32_getResult64Bit | MPY32_getResult
MPY32_getResult8Bit | MPY32_getResult
MPY32_resetFractionMode | MPY32_disableFractionalMode
MPY32_resetSaturationMode | MPY32_disableSaturationMode
MPY32_setFractionMode | MPY32_enableFractionalMode
MPY32_setSaturationMode | MPY32_enableSaturationMode
PMM_regOff | PMM_turnOffRegulator
PMM_regOn | PMM_turnOnRegulator
REF_disableReferenceVoltage | Ref_disableReferenceVoltage
REF_disableTempSensor | Ref_disableTempSensor
REF_enableReferenceVoltage | Ref_enableReferenceVoltage
REF_enableTempSensor | Ref_enableTempSensor
REF_getBandgapMode | Ref_getBandgapMode
REF_isBandgapActive | Ref_isBandgapActive
REF_isRefGenActive | Ref_isRefGenActive
REF_isRefGenBusy | Ref_isRefGenBusy
REF_setReferenceVoltage | Ref_setReferenceVoltage
RTC_B_calendarInit | RTC_B_initCalendar
RTC_B_setCalendarAlarm | RTC_B_configureCalendarAlarm
RTC_B_setPrescaleCounterValue | RTC_B_setPrescaleValue
RTC_C_calendarInit | RTC_C_initCalendar
RTC_C_counterInit | RTC_C_initCounter
RTC_C_counterPrescaleHold | RTC_C_holdCounterPrescale
RTC_C_counterPrescaleInit | RTC_C_initCounterPrescale
RTC_C_counterPrescaleStart | RTC_C_startCounterPrescale
RTC_C_setCalendarAlarm | RTC_C_configureCalendarAlarm
SYS_clearJTAGMailboxFlagStatus | SysCtl_clearJTAGMailboxFlagStatus
SYS_disableBSLMemory | SysCtl_disableBSLMemory
SYS_disableBSLProtect | SysCtl_disableBSLProtect
SYS_disableRAMBasedInterruptVectors | SysCtl_disableRAMBasedInterruptVectors
SYS_enableBSLMemory | SysCtl_enableBSLMemory
SYS_enableBSLProtect | SysCtl_enableBSLProtect
SYS_enableDedicatedJTAGPins | SysCtl_enableDedicatedJTAGPins
SYS_enablePMMAccessProtect | SysCtl_enablePMMAccessProtect
SYS_enableRAMBasedInterruptVectors | SysCtl_enableRAMBasedInterruptVectors
SYS_getBSLEntryIndication | SysCtl_getBSLEntryIndication
SYS_getJTAGInboxMessage16Bit | SysCtl_getJTAGInboxMessage16Bit
SYS_getJTAGInboxMessage32Bit | SysCtl_getJTAGInboxMessage32Bit
SYS_getJTAGMailboxFlagStatus | SysCtl_getJTAGMailboxFlagStatus
SYS_JTAGMailboxInit | SysCtl_initJTAGMailbox
SYS_setBSLSize | SysCtl_setBSLSize
SYS_setJTAGOutgoingMessage16Bit | SysCtl_setJTAGOutgoingMessage16Bit
SYS_setJTAGOutgoingMessage32Bit | SysCtl_setJTAGOutgoingMessage32Bit
SYS_setRAMAssignedToBSL | SysCtl_setRAMAssignedToBSL
SysCtl_disableBSLMemory | [REMOVED]
SysCtl_disableBSLProtect | [REMOVED]
SysCtl_enableBSLMemory | [REMOVED]
SysCtl_enableBSLProtect | [REMOVED]
SysCtl_JTAGMailboxInit | SysCtl_initJTAGMailbox
SysCtl_setBSLSize | [REMOVED]
SysCtl_setRAMAssignedToBSL | [REMOVED]
TIMER_A_clear | Timer_A_clear
TIMER_A_clearCaptureCompareInterruptFlag | Timer_A_clearCaptureCompareInterrupt
Timer_A_clearCaptureCompareInterruptFlag | Timer_A_clearCaptureCompareInterrupt
Timer_A_clearCaptureCompareInterruptFlag | Timer_A_clearCaptureCompareInterrupt
Timer_A_clearCaptureCompareInterruptFlag | Timer_A_clearCaptureCompareInterrupt
Timer_A_clearTimerInterruptFlag | Timer_A_clearTimerInterrupt
TIMER_A_clearTimerInterruptFlag | Timer_A_clearTimerInterrupt
Timer_A_clearTimerInterruptFlag | Timer_A_clearTimerInterrupt
Timer_A_clearTimerInterruptFlag | Timer_A_clearTimerInterrupt
Timer_A_configureContinuousMode | Timer_A_initContinuousMode
TIMER_A_configureContinuousMode | Timer_A_initContinuousMode
Timer_A_configureUpDownMode | Timer_A_initUpDownMode
TIMER_A_configureUpDownMode | Timer_A_initUpDownMode
Timer_A_configureUpMode | Timer_A_initUpMode
TIMER_A_configureUpMode | Timer_A_initUpMode
TIMER_A_disableCaptureCompareInterrupt | Timer_A_disableCaptureCompareInterrupt
TIMER_A_disableInterrupt | Timer_A_disableInterrupt
TIMER_A_enableCaptureCompareInterrupt | Timer_A_enableCaptureCompareInterrupt
TIMER_A_enableInterrupt | Timer_A_enableInterrupt
Timer_A_generatePWM | Timer_A_outputPWM
TIMER_A_generatePWM | Timer_A_outputPWM
TIMER_A_getCaptureCompareCount | Timer_A_getCaptureCompareCount
TIMER_A_getCaptureCompareInterruptStatus | Timer_A_getCaptureCompareInterruptStatus
TIMER_A_getCounterValue | Timer_A_getCounterValue
TIMER_A_getInterruptStatus | Timer_A_getInterruptStatus
TIMER_A_getOutputForOutputModeOutBitValue | Timer_A_getOutputForOutputModeOutBitValue
TIMER_A_getSynchronizedCaptureCompareInput | Timer_A_getSynchronizedCaptureCompareInput
Timer_A_initCapture | Timer_A_initCaptureMode
TIMER_A_initCapture | Timer_A_initCaptureMode
TIMER_A_initCaptureMode | Timer_A_initCaptureMode
Timer_A_initCompare | Timer_A_initCompareMode
TIMER_A_initCompare | Timer_A_initCompareMode
TIMER_A_initCompareMode | Timer_A_initCompareMode
TIMER_A_initContinuousMode | Timer_A_initContinuousMode
TIMER_A_initUpDownMode | Timer_A_initUpDownMode
TIMER_A_initUpMode | Timer_A_initUpMode
TIMER_A_outputPWM | Timer_A_outputPWM
TIMER_A_setCompareValue | Timer_A_setCompareValue
TIMER_A_setOutputForOutputModeOutBitValue | Timer_A_setOutputForOutputModeOutBitValue
Timer_A_startContinousMode | Timer_A_startCounter
TIMER_A_startContinousMode | Timer_A_startCounter
Timer_A_startContinuousMode | Timer_A_startCounter
TIMER_A_startContinuousMode | Timer_A_startCounter
TIMER_A_startCounter | Timer_A_startCounter
Timer_A_startUpDownMode | Timer_A_startCounter
TIMER_A_startUpDownMode | Timer_A_startCounter
Timer_A_startUpMode | Timer_A_startCounter
TIMER_A_startUpMode | Timer_A_startUpMode
TIMER_A_stop | Timer_A_stop
TIMER_B_clear | Timer_B_clear
TIMER_B_clearCaptureCompareInterruptFlag | Timer_B_clearCaptureCompareInterrupt
Timer_B_clearCaptureCompareInterruptFlag | Timer_B_clearCaptureCompareInterrupt
Timer_B_clearCaptureCompareInterruptFlag | Timer_B_clearCaptureCompareInterrupt
Timer_B_clearCaptureCompareInterruptFlag | Timer_B_clearCaptureCompareInterrupt
Timer_B_clearTimerInterruptFlag | Timer_B_clearTimerInterrupt
TIMER_B_clearTimerInterruptFlag | Timer_B_clearTimerInterrupt
Timer_B_clearTimerInterruptFlag | Timer_B_clearTimerInterrupt
Timer_B_clearTimerInterruptFlag | Timer_B_clearTimerInterrupt
Timer_B_configureContinuousMode | Timer_B_initContinuousMode
TIMER_B_configureContinuousMode | Timer_B_initContinuousMode
Timer_B_configureUpDownMode | Timer_B_initUpDownMode
TIMER_B_configureUpDownMode | Timer_B_initUpDownMode
Timer_B_configureUpMode | Timer_B_initUpMode
TIMER_B_configureUpMode | Timer_B_initUpMode
TIMER_B_disableCaptureCompareInterrupt | Timer_B_disableCaptureCompareInterrupt
TIMER_B_disableInterrupt | Timer_B_disableInterrupt
TIMER_B_enableCaptureCompareInterrupt | Timer_B_enableCaptureCompareInterrupt
TIMER_B_enableInterrupt | Timer_B_enableInterrupt
Timer_B_generatePWM | Timer_B_outputPWM
TIMER_B_generatePWM | Timer_B_outputPWM
TIMER_B_getCaptureCompareCount | Timer_B_getCaptureCompareCount
TIMER_B_getCaptureCompareInterruptStatus | Timer_B_getCaptureCompareInterruptStatus
TIMER_B_getCounterValue | Timer_B_getCounterValue
TIMER_B_getInterruptStatus | Timer_B_getInterruptStatus
TIMER_B_getOutputForOutputModeOutBitValue | Timer_B_getOutputForOutputModeOutBitValue
TIMER_B_getSynchronizedCaptureCompareInput | Timer_B_getSynchronizedCaptureCompareInput
Timer_B_initCapture | Timer_B_initCaptureMode
TIMER_B_initCapture | Timer_B_initCaptureMode
TIMER_B_initCaptureMode | Timer_B_initCaptureMode
Timer_B_initCompare | Timer_B_initCompareMode
TIMER_B_initCompare | Timer_B_initCompareMode
TIMER_B_initCompareLatchLoadEvent | Timer_B_initCompareLatchLoadEvent
TIMER_B_initCompareMode | Timer_B_initCompareMode
TIMER_B_initContinuousMode | Timer_B_initContinuousMode
TIMER_B_initUpDownMode | Timer_B_initUpDownMode
TIMER_B_initUpMode | Timer_B_initUpMode
TIMER_B_outputPWM | Timer_B_outputPWM
TIMER_B_selectCounterLength | Timer_B_selectCounterLength
TIMER_B_selectLatchingGroup | Timer_B_selectLatchingGroup
TIMER_B_setCompareValue | Timer_B_setCompareValue
TIMER_B_setOutputForOutputModeOutBitValue | Timer_B_setOutputForOutputModeOutBitValue
Timer_B_startContinousMode | Timer_B_startCounter
TIMER_B_startContinousMode | Timer_B_startCounter
Timer_B_startContinuousMode | Timer_B_startCounter
TIMER_B_startContinuousMode | Timer_B_startCounter
TIMER_B_startCounter | Timer_B_startCounter
Timer_B_startUpDownMode | Timer_B_startCounter
TIMER_B_startUpDownMode | Timer_B_startCounter
Timer_B_startUpMode | Timer_B_startCounter
TIMER_B_startUpMode | Timer_B_startCounter
TIMER_B_stop | Timer_B_stop
WDT_A_intervalTimerInit | WDT_A_initIntervalTimer
WDT_A_watchdogTimerInit | WDT_A_initWatchdogTimer

eusci_i2c.c/eusci_i2c.h files are replaced with eusci_b_i2c.c/eusci_b_i2c.h
eusci_spi.c/eusci_spi.h files are replaced with eusci_a_spi.c/eusci_a_spi.h/eusci_b_spi.c/eusci_b_spi.h
eusci_uart.c/eusci_uart.h files are replaced with eusci_a_uart.c/eusci_a_uart.h
MSP430FR2xx_4xx Family

Old API | New API
CS_clockSignalInit | CS_initClockSignal
CS_faultFlagStatus | CS_getFaultFlagStatus
CS_XT1AutoOff | CS_turnOffXT1
CS_XT1Start | CS_turnOnXT1
CS_XT1StartWithTimeout | CS_turnOnXT1WithTimeout
EUSCI_A_SPI_clearInterruptFlag | EUSCI_A_SPI_clearInterrupt
EUSCI_A_SPI_getReceiveBufferAddressForDMA | EUSCI_A_SPI_getReceiveBufferAddress
EUSCI_A_SPI_getTransmitBufferAddressForDMA | EUSCI_A_SPI_getTransmitBufferAddress
EUSCI_A_SPI_masterChangeClock | EUSCI_A_SPI_changeMasterClock
EUSCI_A_SPI_masterInit | EUSCI_A_SPI_initMaster
EUSCI_A_SPI_slaveInit | EUSCI_A_SPI_initSlave
EUSCI_A_UART_clearInterruptFlag | EUSCI_A_UART_clearInterrupt
EUSCI_A_UART_getReceiveBufferAddressForDMA | EUSCI_A_UART_getReceiveBufferAddress
EUSCI_A_UART_getTransmitBufferAddressForDMA | EUSCI_A_UART_getTransmitBufferAddress
EUSCI_A_UART_initAdvance | EUSCI_A_UART_init
EUSCI_B_I2C_clearInterruptFlag | EUSCI_B_I2C_clearInterrupt
EUSCI_B_I2C_getReceiveBufferAddressForDMA | EUSCI_B_I2C_getReceiveBufferAddress
EUSCI_B_I2C_getTransmitBufferAddressForDMA | EUSCI_B_I2C_getTransmitBufferAddress
EUSCI_B_I2C_masterInit | EUSCI_B_I2C_initMaster
EUSCI_B_I2C_masterIsSTOPSent | EUSCI_B_I2C_masterIsStopSent
EUSCI_B_I2C_masterMultiByteReceiveFinish | EUSCI_B_I2C_masterReceiveMultiByteFinish
EUSCI_B_I2C_masterMultiByteReceiveFinishWithTimeout | EUSCI_B_I2C_masterReceiveMultiByteFinishWithTimeout
EUSCI_B_I2C_masterMultiByteReceiveNext | EUSCI_B_I2C_masterReceiveMultiByteNext
EUSCI_B_I2C_masterMultiByteReceiveStop | EUSCI_B_I2C_masterReceiveMultiByteStop
EUSCI_B_I2C_masterMultiByteSendFinish | EUSCI_B_I2C_masterSendMultiByteFinish
EUSCI_B_I2C_masterMultiByteSendFinishWithTimeout | EUSCI_B_I2C_masterSendMultiByteFinishWithTimeout
EUSCI_B_I2C_masterMultiByteSendNext | EUSCI_B_I2C_masterSendMultiByteNext
EUSCI_B_I2C_masterMultiByteSendNextWithTimeout | EUSCI_B_I2C_masterSendMultiByteNextWithTimeout
EUSCI_B_I2C_masterMultiByteSendStart | EUSCI_B_I2C_masterSendMultiByteStart
EUSCI_B_I2C_masterMultiByteSendStartWithTimeout | EUSCI_B_I2C_masterSendMultiByteStartWithTimeout
EUSCI_B_I2C_masterMultiByteSendStop | EUSCI_B_I2C_masterSendMultiByteStop
EUSCI_B_I2C_masterMultiByteSendStopWithTimeout | EUSCI_B_I2C_masterSendMultiByteStopWithTimeout
EUSCI_B_I2C_masterSingleReceive | EUSCI_B_I2C_masterReceiveSingle
EUSCI_B_I2C_slaveDataGet | EUSCI_B_I2C_slaveGetData
EUSCI_B_I2C_slaveDataPut | EUSCI_B_I2C_slavePutData
EUSCI_B_I2C_slaveInit | EUSCI_B_I2C_initSlave
EUSCI_B_SPI_clearInterruptFlag | EUSCI_B_SPI_clearInterrupt
EUSCI_B_SPI_getReceiveBufferAddressForDMA | EUSCI_B_SPI_getReceiveBufferAddress
EUSCI_B_SPI_getTransmitBufferAddressForDMA | EUSCI_B_SPI_getTransmitBufferAddress
EUSCI_B_SPI_masterChangeClock | EUSCI_B_SPI_changeMasterClock
EUSCI_B_SPI_masterInit | EUSCI_B_SPI_initMaster
EUSCI_B_SPI_slaveInit | EUSCI_B_SPI_initSlave
FRAMCtl_memoryFill32 | FRAMCtl_fillMemory32
GPIO_clearInterruptFlag | GPIO_clearInterrupt
GPIO_interruptEdgeSelect | GPIO_selectInterruptEdge
PMM_regOff | PMM_turnOffRegulator
PMM_regOn | PMM_turnOnRegulator
SysCtl_JTAGMailboxInit | SysCtl_initJTAGMailbox
Timer_A_clearCaptureCompareInterruptFlag | Timer_A_clearCaptureCompareInterrupt
Timer_A_clearTimerInterruptFlag | Timer_A_clearTimerInterrupt
WDT_A_intervalTimerInit | WDT_A_initIntervalTimer
WDT_A_watchdogTimerInit | WDT_A_initWatchdogTimer

MSP430I2xx Family

Old API | New API
CS_clockSignalInit | CS_initClockSignal
CS_faultFlagStatus | CS_getFaultFlagStatus
DMA_NMIAbortStatus | DMA_getNMIAbortStatus
EUSCI_A_SPI_clearInterruptFlag | EUSCI_A_SPI_clearInterrupt
EUSCI_A_SPI_getReceiveBufferAddressForDMA | EUSCI_A_SPI_getReceiveBufferAddress
EUSCI_A_SPI_getTransmitBufferAddressForDMA | EUSCI_A_SPI_getTransmitBufferAddress
EUSCI_A_SPI_masterChangeClock | EUSCI_A_SPI_changeMasterClock
EUSCI_A_SPI_masterInit | EUSCI_A_SPI_initMaster
EUSCI_A_SPI_slaveInit | EUSCI_A_SPI_initSlave
EUSCI_A_UART_clearInterruptFlag | EUSCI_A_UART_clearInterrupt
EUSCI_A_UART_getReceiveBufferAddressForDMA | EUSCI_A_UART_getReceiveBufferAddress
EUSCI_A_UART_getTransmitBufferAddressForDMA | EUSCI_A_UART_getTransmitBufferAddress
EUSCI_A_UART_initAdvance | EUSCI_A_UART_init
EUSCI_B_I2C_clearInterruptFlag | EUSCI_B_I2C_clearInterrupt
EUSCI_B_I2C_getReceiveBufferAddressForDMA | EUSCI_B_I2C_getReceiveBufferAddress
EUSCI_B_I2C_getTransmitBufferAddressForDMA | EUSCI_B_I2C_getTransmitBufferAddress
EUSCI_B_I2C_masterInit | EUSCI_B_I2C_initMaster
EUSCI_B_I2C_masterIsSTOPSent | EUSCI_B_I2C_masterIsStopSent
EUSCI_B_I2C_masterMultiByteReceiveFinish | EUSCI_B_I2C_masterReceiveMultiByteFinish
EUSCI_B_I2C_masterMultiByteReceiveFinishWithTimeout | EUSCI_B_I2C_masterReceiveMultiByteFinishWithTimeout
EUSCI_B_I2C_masterMultiByteReceiveNext | EUSCI_B_I2C_masterReceiveMultiByteNext
EUSCI_B_I2C_masterMultiByteReceiveStop | EUSCI_B_I2C_masterReceiveMultiByteStop
EUSCI_B_I2C_masterMultiByteSendFinish | EUSCI_B_I2C_masterSendMultiByteFinish
EUSCI_B_I2C_masterMultiByteSendFinishWithTimeout | EUSCI_B_I2C_masterSendMultiByteFinishWithTimeout
EUSCI_B_I2C_masterMultiByteSendNext | EUSCI_B_I2C_masterSendMultiByteNext
EUSCI_B_I2C_masterMultiByteSendNextWithTimeout | EUSCI_B_I2C_masterSendMultiByteNextWithTimeout
EUSCI_B_I2C_masterMultiByteSendStart | EUSCI_B_I2C_masterSendMultiByteStart
EUSCI_B_I2C_masterMultiByteSendStartWithTimeout | EUSCI_B_I2C_masterSendMultiByteStartWithTimeout
EUSCI_B_I2C_masterMultiByteSendStop | EUSCI_B_I2C_masterSendMultiByteStop
EUSCI_B_I2C_masterMultiByteSendStopWithTimeout | EUSCI_B_I2C_masterSendMultiByteStopWithTimeout
EUSCI_B_I2C_masterSingleReceive | EUSCI_B_I2C_masterReceiveSingle
EUSCI_B_I2C_slaveDataGet | EUSCI_B_I2C_slaveGetData
EUSCI_B_I2C_slaveDataPut | EUSCI_B_I2C_slavePutData
EUSCI_B_I2C_slaveInit | EUSCI_B_I2C_initSlave
EUSCI_B_SPI_clearInterruptFlag | EUSCI_B_SPI_clearInterrupt
EUSCI_B_SPI_getReceiveBufferAddressForDMA | EUSCI_B_SPI_getReceiveBufferAddress
EUSCI_B_SPI_getTransmitBufferAddressForDMA | EUSCI_B_SPI_getTransmitBufferAddress
EUSCI_B_SPI_masterChangeClock | EUSCI_B_SPI_changeMasterClock
EUSCI_B_SPI_masterInit | EUSCI_B_SPI_initMaster
EUSCI_B_SPI_slaveInit | EUSCI_B_SPI_initSlave
FlashCtl_bankErase | FlashCtl_eraseBank
FlashCtl_eraseCheck | FlashCtl_performEraseCheck
FlashCtl_massErase | FlashCtl_performMassErase
FlashCtl_memoryFill32 | FlashCtl_fillMemory32
FlashCtl_segmentErase | FlashCtl_eraseSegment
FlashCtl_status | FlashCtl_getStatus
GPIO_clearInterruptFlag | GPIO_clearInterrupt
GPIO_interruptEdgeSelect | GPIO_selectInterruptEdge
GPIO_interruptEdgeSelect | GPIO_selectInterruptEdge
PMM_regOff | PMM_turnOffRegulator
PMM_regOn | PMM_turnOnRegulator
SysCtl_JTAGMailboxInit | SysCtl_initJTAGMailbox
TIMER_A_clear | Timer_A_clear
TIMER_A_clearCaptureCompareInterruptFlag | Timer_A_clearCaptureCompareInterrupt
Timer_A_clearCaptureCompareInterruptFlag | Timer_A_clearCaptureCompareInterrupt
Timer_A_clearCaptureCompareInterruptFlag | Timer_A_clearCaptureCompareInterrupt
Timer_A_clearTimerInterruptFlag | Timer_A_clearTimerInterrupt
TIMER_A_clearTimerInterruptFlag | Timer_A_clearTimerInterrupt
Timer_A_clearTimerInterruptFlag | Timer_A_clearTimerInterrupt
Timer_A_configureContinuousMode | Timer_A_initContinuousMode
TIMER_A_configureContinuousMode | Timer_A_initContinuousMode
Timer_A_configureUpDownMode | Timer_A_initUpDownMode
TIMER_A_configureUpDownMode | Timer_A_initUpDownMode
Timer_A_configureUpMode | Timer_A_initUpMode
TIMER_A_configureUpMode | Timer_A_initUpMode
TIMER_A_disableCaptureCompareInterrupt | Timer_A_disableCaptureCompareInterrupt
TIMER_A_disableInterrupt | Timer_A_disableInterrupt
TIMER_A_enableCaptureCompareInterrupt | Timer_A_enableCaptureCompareInterrupt
TIMER_A_enableInterrupt | Timer_A_enableInterrupt
Timer_A_generatePWM | Timer_A_outputPWM
TIMER_A_generatePWM | Timer_A_outputPWM
TIMER_A_getCaptureCompareCount | Timer_A_getCaptureCompareCount
TIMER_A_getCaptureCompareInterruptStatus | Timer_A_getCaptureCompareInterruptStatus
TIMER_A_getCounterValue | Timer_A_getCounterValue
TIMER_A_getInterruptStatus | Timer_A_getInterruptStatus
TIMER_A_getOutputForOutputModeOutBitValue | Timer_A_getOutputForOutputModeOutBitValue
TIMER_A_getSynchronizedCaptureCompareInput | Timer_A_getSynchronizedCaptureCompareInput
Timer_A_initCapture | Timer_A_initCaptureMode
TIMER_A_initCapture | Timer_A_initCaptureMode
TIMER_A_initCaptureMode | Timer_A_initCaptureMode
Timer_A_initCompare | Timer_A_initCompareMode
TIMER_A_initCompare | Timer_A_initCompareMode
TIMER_A_initCompareMode | Timer_A_initCompareMode
TIMER_A_initContinuousMode | Timer_A_initContinuousMode
TIMER_A_initUpDownMode | Timer_A_initUpDownMode
TIMER_A_initUpMode | Timer_A_initUpMode
TIMER_A_outputPWM | Timer_A_outputPWM
TIMER_A_setCompareValue | Timer_A_setCompareValue
TIMER_A_setOutputForOutputModeOutBitValue | Timer_A_setOutputForOutputModeOutBitValue
Timer_A_startContinousMode | Timer_A_startCounter
TIMER_A_startContinousMode | Timer_A_startCounter
Timer_A_startContinuousMode | Timer_A_startCounter
TIMER_A_startContinuousMode | Timer_A_startCounter
TIMER_A_startCounter | Timer_A_startCounter
Timer_A_startUpDownMode | Timer_A_startCounter
TIMER_A_startUpDownMode | Timer_A_startCounter
Timer_A_startUpMode | Timer_A_startCounter
TIMER_A_startUpMode | Timer_A_startUpMode
TIMER_A_stop | Timer_A_stop
WDT_A_intervalTimerInit | WDT_A_initIntervalTimer
WDT_A_watchdogTimerInit | WDT_A_initWatchdogTimer

## Additional Resources

For more information, visit www.ti.com.