#

## Table of Contents

## Example Summary

This example is intended to be a starting point for new development where a minimal footprint is needed.

## Peripherals Exercised

- `Board_LED0` - Indicates that the board was initialized within `main()`

## Example Usage

- The example lights `Board_LED0` as part of the initialization in `main()`. Then a heartBeat task toggles the LED at a rate determined by the `arg0` parameter for the constructed Task instance in the .c file.

## Application Design Details

This examples is the same as the Empty example except many development and debug features are disabled. For example:

- No logging is enabled
- No assert checking is enabled
- No Kernel Idle task
- Non-Instrumented driver modules are used
- No stack overflow checking

> Please refer to the Memory Footprint Reduction section in the TI-RTOS User Guide spruhd4.pdf for a complete and detailed list of the differences between the empty minimal and empty projects.

## References

- For GNU and IAR users, please read the following website for details about enabling semi-hosting in order to view console output.

- For more help, search either the SYS/BIOS User Guide or the TI-RTOS Getting Started Guide within your TI-RTOS installation.