# Ucglib

Color graphics library for embedded systems with focus on Arduino Environment.

Supported display controller: ST7735, ILI9341, PCF8833, SSD1351, LD50T6160, ILI9163

Features: Graphics primitives with 18 bit color depth, filled polygon draw, >300, landscape/portrait mode.

See the [github wiki](https://github.com/olikraus/ucglib/wiki) for reference manual and tutorials.


[//]: # ([Download Ucglib Arduino Library](https://github.com/olikraus/Ucglib_Arduino/releases/latest))

[Download Ucglib Arduino Library v1.2 (Arduino IDE 1.5 or higher)](https://github.com/olikraus/Ucglib_Arduino/releases/latest)

Version v1.01 for Arduino IDE 1.0.x [![](https://api.bintray.com/packages/olikraus/Ucglib/Arduino/images/download.png)](https://bintray.com/olikraus/Ucglib/Arduino/_latestVersion)

<a href='http://www.youtube.com/watch?feature=player_embedded&v=GSpYY0AMtEU' target='_blank'><img src='http://img.youtube.com/vi/GSpYY0AMtEU/0.jpg' width='425' height=344 /></a>
