lwIP 2.1.2 Lightweight IP stack

Data Structures | Macros | Functions | Variables
ip.h File Reference
`#include "lwip/opt.h"`
`#include "lwip/def.h"`
`#include "lwip/pbuf.h"`
`#include "lwip/ip_addr.h"`
`#include "lwip/err.h"`
`#include "lwip/netif.h"`
`#include "lwip/ip4.h"`
`#include "lwip/ip6.h"`
`#include "lwip/prot/ip.h"`

## Data Structures
struct | ip_globals

## Macros
#define | LWIP_IP_CHECK_PBUF_REF_COUNT_FOR_TX(p) LWIP_ASSERT("p->ref == 1", (p)->ref == 1)
#define | IP_PCB
#define | ip_current_netif() (ip_data.current_netif)
#define | ip_current_input_netif() (ip_data.current_input_netif)
#define | ip_current_header_tot_len() (ip_data.current_ip_header_tot_len)
#define | ip_current_src_addr() (&ip_data.current_iphdr_src)
#define | ip_current_dest_addr() (&ip_data.current_iphdr_dest)
#define | ip4_current_header() ip_data.current_ip4_header
#define | ip6_current_header() ((const struct ip6_hdr*)(ip_data.current_ip6_header))
#define | ip_current_is_v6() (ip6_current_header() != NULL)
#define | ip6_current_src_addr() (ip_2_ip6(&ip_data.current_iphdr_src))
#define | ip6_current_dest_addr() (ip_2_ip6(&ip_data.current_iphdr_dest))
#define | ip_current_header_proto()
#define | ip_next_header_ptr()
#define | ip4_current_src_addr() (ip_2_ip4(&ip_data.current_iphdr_src))
#define | ip4_current_dest_addr() (ip_2_ip4(&ip_data.current_iphdr_dest))
#define | ip_current_src_addr() (&ip_data.current_iphdr_src)
#define | ip_current_dest_addr() (&ip_data.current_iphdr_dest)
#define | ip_get_option(pcb, opt) ((pcb)->so_options & (opt))
#define | ip_set_option(pcb, opt) ((pcb)->so_options = (u8_t)((pcb)->so_options | (opt)))
#define | ip_reset_option(pcb, opt) ((pcb)->so_options = (u8_t)((pcb)->so_options & ~(opt)))
#define | ip_output(p, src, dest, ttl, tos, proto)
#define | ip_output_if(p, src, dest, ttl, tos, proto, netif)
#define | ip_output_if_src(p, src, dest, ttl, tos, proto, netif)
#define | ip_output_if_hdrincl(p, src, dest, netif)
#define | ip_output_hinted(p, src, dest, ttl, tos, proto, netif_hint)
#define | ip_route(src, dest)
#define | ip_netif_get_local_ip(netif, dest)

## Functions
err_t | ip_input (struct pbuf *p, struct netif *inp)

## Variables
struct ip_globals | ip_data

## Detailed Description

IP API

## Macro Definition Documentation

## ◆ ip4_current_dest_addr

#define ip4_current_dest_addr | ( |  | ) | (ip_2_ip4(&ip_data.current_iphdr_dest))

Destination IP4 address of current_header

## ◆ ip4_current_header

#define ip4_current_header | ( |  | ) | ip_data.current_ip4_header

Get the IPv4 header of the current packet. This function must only be called from a receive callback (udp_recv, raw_recv, tcp_accept). It will return NULL otherwise.

## ◆ ip4_current_src_addr

#define ip4_current_src_addr | ( |  | ) | (ip_2_ip4(&ip_data.current_iphdr_src))

Source IP4 address of current_header

## ◆ ip6_current_dest_addr

#define ip6_current_dest_addr | ( |  | ) | (ip_2_ip6(&ip_data.current_iphdr_dest))

Destination IPv6 address of current_header

## ◆ ip6_current_header

#define ip6_current_header | ( |  | ) | ((const struct ip6_hdr*)(ip_data.current_ip6_header))

Get the IPv6 header of the current packet. This function must only be called from a receive callback (udp_recv, raw_recv, tcp_accept). It will return NULL otherwise.

## ◆ ip6_current_src_addr

#define ip6_current_src_addr | ( |  | ) | (ip_2_ip6(&ip_data.current_iphdr_src))

Source IPv6 address of current_header

## ◆ ip_current_dest_addr [1/2]

#define ip_current_dest_addr | ( |  | ) | (&ip_data.current_iphdr_dest)

Destination IP address of current_header

Union destination address of current_header

## ◆ ip_current_dest_addr [2/2]

#define ip_current_dest_addr | ( |  | ) | (&ip_data.current_iphdr_dest)

Destination IP address of current_header

Union destination address of current_header

## ◆ ip_current_header_proto

#define ip_current_header_proto | ( |  | ) |

Value:
(ip_current_is_v6() ? \
IP6H_NEXTH(ip6_current_header()) :\
IPH_PROTO(ip4_current_header()))
ip_current_is_v6
#define ip_current_is_v6()
Definition: ip.h:157
ip6_current_header
#define ip6_current_header()
Definition: ip.h:155
ip4_current_header
#define ip4_current_header()
Definition: ip.h:151

Get the transport layer protocol

## ◆ ip_current_header_tot_len

#define ip_current_header_tot_len | ( |  | ) | (ip_data.current_ip_header_tot_len)

Total header length of ip(6)_current_header() (i.e. after this, the UDP/TCP header starts)

## ◆ ip_current_input_netif

#define ip_current_input_netif | ( |  | ) | (ip_data.current_input_netif)

Get the interface that received the current packet. This function must only be called from a receive callback (udp_recv, raw_recv, tcp_accept). It will return NULL otherwise.

## ◆ ip_current_is_v6

#define ip_current_is_v6 | ( |  | ) | (ip6_current_header() != NULL)

Returns TRUE if the current IP input packet is IPv6, FALSE if it is IPv4

## ◆ ip_current_netif

#define ip_current_netif | ( |  | ) | (ip_data.current_netif)

Get the interface that accepted the current packet. This may or may not be the receiving netif, depending on your netif/network setup. This function must only be called from a receive callback (udp_recv, raw_recv, tcp_accept). It will return NULL otherwise.

## ◆ ip_current_src_addr [1/2]

#define ip_current_src_addr | ( |  | ) | (&ip_data.current_iphdr_src)

Source IP address of current_header

Union source address of current_header

## ◆ ip_current_src_addr [2/2]

#define ip_current_src_addr | ( |  | ) | (&ip_data.current_iphdr_src)

Source IP address of current_header

Union source address of current_header

## ◆ ip_get_option

#define ip_get_option | ( |  | pcb,
|  |  | opt
| ) |  | ((pcb)->so_options & (opt))

Gets an IP pcb option (SOF_* flags)

## ◆ ip_next_header_ptr

#define ip_next_header_ptr | ( |  | ) |

Value:
((const void*)((ip_current_is_v6() ? \
(const u8_t*)ip6_current_header() : (const u8_t*)ip4_current_header()) + ip_current_header_tot_len()))
ip_current_is_v6
#define ip_current_is_v6()
Definition: ip.h:157
ip_current_header_tot_len
#define ip_current_header_tot_len()
Definition: ip.h:141
ip6_current_header
#define ip6_current_header()
Definition: ip.h:155
ip4_current_header
#define ip4_current_header()
Definition: ip.h:151

Get the transport layer header

## ◆ ip_output_hinted

#define ip_output_hinted | ( |  | p,
|  |  | src,
|  |  | dest,
|  |  | ttl,
|  |  | tos,
|  |  | proto,
|  |  | netif_hint
| ) |  |

Value:
(IP_IS_V6(dest) ? \
ip6_output_hinted(p, ip_2_ip6(src), ip_2_ip6(dest), ttl, tos, proto, netif_hint) : \
ip4_output_hinted(p, ip_2_ip4(src), ip_2_ip4(dest), ttl, tos, proto, netif_hint))
ip_2_ip4
#define ip_2_ip4(ipaddr)
Definition: ip_addr.h:120
IP_IS_V6
#define IP_IS_V6(ipaddr)
Definition: ip_addr.h:102
ip_2_ip6
#define ip_2_ip6(ipaddr)
Definition: ip_addr.h:116

Output IP packet with netif_hint

## ◆ ip_output_if_hdrincl

#define ip_output_if_hdrincl | ( |  | p,
|  |  | src,
|  |  | dest,
|  |  | netif
| ) |  |

Value:
(IP_IS_V6(dest) ? \
ip6_output_if(p, ip_2_ip6(src), LWIP_IP_HDRINCL, 0, 0, 0, netif) : \
ip4_output_if(p, ip_2_ip4(src), LWIP_IP_HDRINCL, 0, 0, 0, netif))
ip_2_ip4
#define ip_2_ip4(ipaddr)
Definition: ip_addr.h:120
IP_IS_V6
#define IP_IS_V6(ipaddr)
Definition: ip_addr.h:102
netif
Definition: netif.h:260
ip4_output_if
err_t ip4_output_if(struct pbuf *p, const ip4_addr_t *src, const ip4_addr_t *dest, u8_t ttl, u8_t tos, u8_t proto, struct netif *netif)
Definition: ip4.c:787
ip_2_ip6
#define ip_2_ip6(ipaddr)
Definition: ip_addr.h:116

Output IP packet that already includes an IP header.

## ◆ IP_PCB

#define IP_PCB

Value:
/* ip addresses in network byte order */ \
ip_addr_t local_ip; \
ip_addr_t remote_ip; \
/* Bound netif index */ \
u8_t netif_idx; \
/* Socket options */ \
u8_t so_options; \
/* Type Of Service */ \
u8_t tos; \
/* Time To Live */ \
u8_t ttl \
/* link layer address resolution hint */ \
IP_PCB_NETIFHINT

This is the common part of all PCB types. It needs to be at the beginning of a PCB type definition. It is located here so that changes to this common part are made in one location instead of having to change all PCB structs.

## ◆ ip_reset_option

#define ip_reset_option | ( |  | pcb,
|  |  | opt
| ) |  | ((pcb)->so_options = (u8_t)((pcb)->so_options & ~(opt)))

Resets an IP pcb option (SOF_* flags)

## ◆ ip_set_option

#define ip_set_option | ( |  | pcb,
|  |  | opt
| ) |  | ((pcb)->so_options = (u8_t)((pcb)->so_options | (opt)))

Sets an IP pcb option (SOF_* flags)

## ◆ LWIP_IP_CHECK_PBUF_REF_COUNT_FOR_TX

#define LWIP_IP_CHECK_PBUF_REF_COUNT_FOR_TX | ( |  | p | ) | LWIP_ASSERT("p->ref == 1", (p)->ref == 1)

pbufs passed to IP must have a ref-count of 1 as their payload pointer gets altered as the packet is passed down the stack

## Variable Documentation

## ◆ ip_data

struct ip_globals ip_data

Global data for both IPv4 and IPv6