# TCPIP Echoserver with SysBios and TI Ethernet Stack
- FW can be compiled for Flash and is running without emulator
- CPU1 sets pinout and let CM boot also for Ethernet. Toggles LED1
- CM is running with SYSBIOS and TI NDK stack