# SDFM Module

The Sigma-Delta Filter Module (SDFM) API provides a set of functions for configuring and using the SDFM module. The functions provided allow the user to setup and configure the Input data type to SDFM filters, the Primary (data) and Secondary (comparator) filters, Data FIFO, the PWM - SDFM sync signals, comparator threshold values and interrupt sources. Functions are also provided to read the filter data and the status of the SDFM module components.

Note that the Secondary (comparator) Filter configuration APIs have the “Comp” key word embedded to represent access to the Comparator sub-module. For example the function SDFM_setComparatorFilterType() sets the comparator filter type while SDFM_setFilterType() sets the primary filter type.

APIs providing higher level abstraction are also available in the sdfm.c source file. These APIs can be used to configure the Comparator, Data Filter and the Data filter FIFO.

{color{red} textsc{Note: The Manchester modulator clock mode is no longer supported in SDFM for this device. The required software changes are scoped for next C2000Ware release and are not supported in this release. Users are advised to not use this feature on this device.}}

group `sdfm_api`

  Defines

  `SDFM_GET_LOW_THRESHOLD`(C) ((uint16_t)(C))

    Macro to get the low threshold

  `SDFM_GET_HIGH_THRESHOLD`(C) ((uint16_t)((uint32_t)(C) >> 16U))

    Macro to get the high threshold

  `SDFM_GET_LOW_THRESHOLD_BOTH`(C1, C2) ((((uint32_t)(SDFM_GET_LOW_THRESHOLD

  (C2))) << 16U) | \

  ((uint32_t)(

  SDFM_GET_LOW_THRESHOLD(C1))))

    Macro to get the high threshold 1 & 2 to be passed as lowThreshold parameter to SDFM_setCompFilterLowThreshold().

  `SDFM_GET_HIGH_THRESHOLD_BOTH`(C1, C2) ((((uint32_t)(SDFM_GET_HIGH_THRESHOLD

  (C2))) << 16U) | \

  ((uint32_t)(

  SDFM_GET_HIGH_THRESHOLD(C1))))

    Macro to get the high threshold 1 & 2 to be passed as highThreshold parameter to SDFM_setCompFilterHighThreshold().

  `SDFM_SET_OSR`(X) (((X) - 1) << 8U)

    Macro to convert comparator over sampling ratio to acceptable bit location

  `SDFM_SHIFT_VALUE`(X) ((X) << 2U)

    Macro to convert the data shift bit values to acceptable bit location

  `SDFM_THRESHOLD`(H, L) ((((uint32_t)(H)) << 16U) | (L))

    Macro to combine high threshold and low threshold values

  `SDFM_SET_FIFO_LEVEL`(X) ((X) << 7U)

    Macro to set the FIFO level to acceptable bit location

  `SDFM_SET_ZERO_CROSS_THRESH_VALUE`(X) (0x8000 | (X))

    Macro to set and enable the zero cross threshold value.

  `SDFM_FILTER_DISABLE` 0x0U

    Macros to enable or disable filter.

  `SDFM_FILTER_ENABLE` 0x2U
  `SDFM_SDFIL_OFFSET` (SDFM_O_SDCTLPARM2 - SDFM_O_SDCTLPARM1)

    < SD filter offset

    Event Digital filter offset

  `SDFM_DIGFIL_OFFSET` (SDFM_O_SDCOMP2CTL - SDFM_O_SDCOMP1CTL)

    Offset between high threshold 1 & 2 registers.

  `SDFM_SDFLT1CMPHx_OFFSET` (SDFM_O_SDFLT1CMPH2 - SDFM_O_SDFLT1CMPH1)

    Offset between low threshold 1 & 2 registers.

  `SDFM_SDFLT1CMPLx_OFFSET` (SDFM_O_SDFLT1CMPL2 - SDFM_O_SDFLT1CMPL1)
  `SDFM_COMPEVT_FILTER_CONFIG_M` (SDFM_SDCOMP1EVT1FLTCTL_SAMPWIN_M

  | \

  SDFM_SDCOMP1EVT1FLTCTL_THRESH_M)
  `SDFM_COMPEVT_FILTER_LOCK_M`

  (SDFM_SDCOMPLOCK_SDCOMPCTL | \

  SDFM_SDCOMPLOCK_COMP)

  `SDFM_CLOCK_SYNCHRONIZER` SDFM_SDCTLPARM1_SDCLKSYNC

    Define for Clock synchronizer Configuration.

  `SDFM_DATA_SYNCHRONIZER` SDFM_SDCTLPARM1_SDDATASYNC

    Define for Data Synchronizer Configuration.

  `SDFM_MODULATOR_FAILURE_INTERRUPT` 0x200U

    Interrupt is generated if Modulator fails.

  `SDFM_LOW_LEVEL_THRESHOLD_INTERRUPT` 0x40U

    Interrupt on Comparator low-level threshold.

  `SDFM_HIGH_LEVEL_THRESHOLD_INTERRUPT` 0x20U

    Interrupt on Comparator high-level threshold.

  `SDFM_DATA_FILTER_ACKNOWLEDGE_INTERRUPT` 0x1U

    Interrupt on Acknowledge flag

  `SDFM_FIFO_INTERRUPT` 0x1000U

    Interrupt on FIFO level

  `SDFM_FIFO_OVERFLOW_INTERRUPT` 0x8000U

    Interrupt on FIFO overflow

  `SDFM_MAIN_INTERRUPT_FLAG` 0x80000000U

    Main interrupt flag

  `SDFM_FILTER_1_HIGH_THRESHOLD_FLAG` 0x1U

    Filter 1 high -level threshold flag

  `SDFM_FILTER_1_LOW_THRESHOLD_FLAG` 0x2U

    Filter 1 low -level threshold flag

  `SDFM_FILTER_2_HIGH_THRESHOLD_FLAG` 0x4U

    Filter 2 high -level threshold flag

  `SDFM_FILTER_2_LOW_THRESHOLD_FLAG` 0x8U

    Filter 2 low -level threshold flag

  `SDFM_FILTER_3_HIGH_THRESHOLD_FLAG` 0x10U

    Filter 3 high -level threshold flag

  `SDFM_FILTER_3_LOW_THRESHOLD_FLAG` 0x20U

    Filter 3 low -level threshold flag

  `SDFM_FILTER_4_HIGH_THRESHOLD_FLAG` 0x40U

    Filter 4 high -level threshold flag

  `SDFM_FILTER_4_LOW_THRESHOLD_FLAG` 0x80U

    Filter 4 low -level threshold flag

  `SDFM_FILTER_1_MOD_FAILED_FLAG` 0x100U

    Filter 1 modulator failed flag

  `SDFM_FILTER_2_MOD_FAILED_FLAG` 0x200U

    Filter 2 modulator failed flag

  `SDFM_FILTER_3_MOD_FAILED_FLAG` 0x400U

    Filter 3 modulator failed flag

  `SDFM_FILTER_4_MOD_FAILED_FLAG` 0x800U

    Filter 4 modulator failed flag

  `SDFM_FILTER_1_NEW_DATA_FLAG` 0x1000U

    Filter 1 new data flag

  `SDFM_FILTER_2_NEW_DATA_FLAG` 0x2000U

    Filter 2 new data flag

  `SDFM_FILTER_3_NEW_DATA_FLAG` 0x4000U

    Filter 3 new data flag

  `SDFM_FILTER_4_NEW_DATA_FLAG` 0x8000U

    Filter 4 new data flag

  `SDFM_FILTER_1_FIFO_OVERFLOW_FLAG` 0x10000U

    Filter 1 FIFO overflow flag

  `SDFM_FILTER_2_FIFO_OVERFLOW_FLAG` 0x20000U

    Filter 2 FIFO overflow flag

  `SDFM_FILTER_3_FIFO_OVERFLOW_FLAG` 0x40000U

    Filter 3 FIFO overflow flag

  `SDFM_FILTER_4_FIFO_OVERFLOW_FLAG` 0x80000U

    Filter 4 FIFO overflow flag

  `SDFM_FILTER_1_FIFO_INTERRUPT_FLAG` 0x100000U

    Filter 1 FIFO overflow flag

  `SDFM_FILTER_2_FIFO_INTERRUPT_FLAG` 0x200000U

    Filter 2 FIFO overflow flag

  `SDFM_FILTER_3_FIFO_INTERRUPT_FLAG` 0x400000U

    Filter 3 FIFO overflow flag

  `SDFM_FILTER_4_FIFO_INTERRUPT_FLAG` 0x800000U

    Filter 4 FIFO overflow flag

  Enums

  enum `SDFM_OutputThresholdStatus`

    Values that can be returned from SDFM_getThresholdStatus()

    Values:

    enumerator `SDFM_OUTPUT_WITHIN_THRESHOLD` = 0

      SDFM output is within threshold.

    enumerator `SDFM_OUTPUT_ABOVE_THRESHOLD` = 1

      SDFM output is above threshold.

    enumerator `SDFM_OUTPUT_BELOW_THRESHOLD` = 2

      SDFM output is below threshold.

  enum `SDFM_FilterNumber`

    Values that can be passed to all functions as the filterNumber parameter.

    Values:

    enumerator `SDFM_FILTER_1` = 0

      Digital filter 1.

    enumerator `SDFM_FILTER_2` = 1

      Digital filter 2.

    enumerator `SDFM_FILTER_3` = 2

      Digital filter 3.

    enumerator `SDFM_FILTER_4` = 3

      Digital filter 4.

  enum `SDFM_FilterType`

    Values that can be passed to SDFM_setFilterType(), SDFM_setComparatorFilterType() as the filterType parameter.

    Values:

    enumerator `SDFM_FILTER_SINC_FAST` = 0x00

      Digital filter with SincFast structure.

    enumerator `SDFM_FILTER_SINC_1` = 0x10

      Digital filter with Sinc1 structure.

    enumerator `SDFM_FILTER_SINC_2` = 0x20

      Digital filter with Sinc3 structure.

    enumerator `SDFM_FILTER_SINC_3` = 0x30

      Digital filter with Sinc4 structure.

  enum `SDFM_ModulatorClockMode`

    Values that can be passed to SDFM_setupModulatorClock(),as the clockMode parameter.

    Values:

    enumerator `SDFM_MODULATOR_CLK_EQUAL_DATA_RATE` = 0

      Modulator clock is identical to the data rate.

  enum `SDFM_OutputDataFormat`

    Values that can be passed to SDFM_setOutputDataFormat(),as the dataFormat parameter.

    Values:

    enumerator `SDFM_DATA_FORMAT_16_BIT` = 0

      Filter output is in 16 bits 2’s complement format.

    enumerator `SDFM_DATA_FORMAT_32_BIT` = 1

      Filter output is in 32 bits 2’s complement format.

  enum `SDFM_DataReadyInterruptSource`

    Values that can be passed to SDFM_setDataReadyInterruptSource(),as the dataReadySource parameter.

    Values:

    enumerator `SDFM_DATA_READY_SOURCE_DIRECT` = 0

      Data ready interrupt source is direct (non -FIFO).

    enumerator `SDFM_DATA_READY_SOURCE_FIFO` = 1

      Data ready interrupt source is FIFO.

  enum `SDFM_PWMSyncSource`

    Values that can be passed to SDFM_setPWMSyncSource(),as the syncSource parameter.

    Values:

    enumerator `SDFM_SYNC_PWM1_SOCA` = 0

      SDFM sync source is PWM1 SOCA.

    enumerator `SDFM_SYNC_PWM1_SOCB` = 1

      SDFM sync source is PWM1 SOCB.

    enumerator `SDFM_SYNC_PWM2_SOCA` = 4

      SDFM sync source is PWM2 SOCA.

    enumerator `SDFM_SYNC_PWM2_SOCB` = 5

      SDFM sync source is PWM2 SOCB.

    enumerator `SDFM_SYNC_PWM3_SOCA` = 8

      SDFM sync source is PWM3 SOCA.

    enumerator `SDFM_SYNC_PWM3_SOCB` = 9

      SDFM sync source is PWM3 SOCB.

    enumerator `SDFM_SYNC_PWM4_SOCA` = 12

      SDFM sync source is PWM4 SOCA.

    enumerator `SDFM_SYNC_PWM4_SOCB` = 13

      SDFM sync source is PWM4 SOCB.

    enumerator `SDFM_SYNC_PWM5_SOCA` = 16

      SDFM sync source is PWM5 SOCA.

    enumerator `SDFM_SYNC_PWM5_SOCB` = 17

      SDFM sync source is PWM5 SOCB.

    enumerator `SDFM_SYNC_PWM6_SOCA` = 20

      SDFM sync source is PWM6 SOCA.

    enumerator `SDFM_SYNC_PWM6_SOCB` = 21

      SDFM sync source is PWM6 SOCB.

    enumerator `SDFM_SYNC_PWM7_SOCA` = 24

      SDFM sync source is PWM7 SOCA.

    enumerator `SDFM_SYNC_PWM7_SOCB` = 25

      SDFM sync source is PWM7 SOCB.

    enumerator `SDFM_SYNC_PWM8_SOCA` = 28

      SDFM sync source is PWM8 SOCA.

    enumerator `SDFM_SYNC_PWM8_SOCB` = 29

      SDFM sync source is PWM8 SOCB.

    enumerator `SDFM_SYNC_PWM9_SOCA` = 32

      SDFM sync source is PWM9 SOCA.

    enumerator `SDFM_SYNC_PWM9_SOCB` = 33

      SDFM sync source is PWM9 SOCB.

    enumerator `SDFM_SYNC_PWM10_SOCA` = 36

      SDFM sync source is PWM10 SOCA.

    enumerator `SDFM_SYNC_PWM10_SOCB` = 37

      SDFM sync source is PWM10 SOCB.

    enumerator `SDFM_SYNC_PWM11_SOCA` = 40

      SDFM sync source is PWM11 SOCA.

    enumerator `SDFM_SYNC_PWM11_SOCB` = 41

      SDFM sync source is PWM11 SOCB.

    enumerator `SDFM_SYNC_PWM12_SOCA` = 44

      SDFM sync source is PWM12 SOCA.

    enumerator `SDFM_SYNC_PWM12_SOCB` = 45

      SDFM sync source is PWM12 SOCB.

    enumerator `SDFM_SYNC_PWM13_SOCA` = 48

      SDFM sync source is PWM13 SOCA.

    enumerator `SDFM_SYNC_PWM13_SOCB` = 49

      SDFM sync source is PWM13 SOCB.

    enumerator `SDFM_SYNC_PWM14_SOCA` = 52

      SDFM sync source is PWM14 SOCA.

    enumerator `SDFM_SYNC_PWM14_SOCB` = 53

      SDFM sync source is PWM14 SOCB.

    enumerator `SDFM_SYNC_PWM15_SOCA` = 56

      SDFM sync source is PWM15 SOCA.

    enumerator `SDFM_SYNC_PWM15_SOCB` = 57

      SDFM sync source is PWM15 SOCB.

    enumerator `SDFM_SYNC_PWM16_SOCA` = 60

      SDFM sync source is PWM16 SOCA.

    enumerator `SDFM_SYNC_PWM16_SOCB` = 61

      SDFM sync source is PWM16 SOCB.

  enum `SDFM_FIFOClearSyncMode`

    Values that can be passed to SDFM_setFIFOClearOnSyncMode(),as the fifoClearSyncMode parameter.

    Values:

    enumerator `SDFM_FIFO_NOT_CLEARED_ON_SYNC` = 0

      SDFM FIFO buffer is not cleared on Sync signal.

    enumerator `SDFM_FIFO_CLEARED_ON_SYNC` = 1

      SDFM FIFO buffer is cleared on Sync signal.

  enum `SDFM_WaitForSyncClearMode`

    Values that can be passed to SDFM_setWaitForSyncClearMode(),as the syncClearMode parameter.

    Values:

    enumerator `SDFM_MANUAL_CLEAR_WAIT_FOR_SYNC` = 0

      Wait for sync cleared using software.

    enumerator `SDFM_AUTO_CLEAR_WAIT_FOR_SYNC` = 1

      Wait for sync cleared automatically.

  enum `SDFM_CompEventNumber`

    Values that can be passed to SDFM_selectCompEventSource() as the compEventNum parameter.

    Values:

    enumerator `SDFM_COMP_EVENT_1` = 11U

      Selects CEVT1.

    enumerator `SDFM_COMP_EVENT_2` = 14U

      Selects CEVT2.

  enum `SDFM_CompEventSource`

    Values that can be passed to SDFM_selectCompEventSource() as the compEventSource parameter.

    Values:

    enumerator `SDFM_COMP_EVENT_SRC_COMPH1` = 0

      COMPH1 event is the source.

    enumerator `SDFM_COMP_EVENT_SRC_COMPH1_L1` = 1

      Either of COMPH1 or COMPL1 event can be the source

    enumerator `SDFM_COMP_EVENT_SRC_COMPH2` = 2

      COMPH2 event is the source.

    enumerator `SDFM_COMP_EVENT_SRC_COMPH2_L2` = 3

      Either of COMPH2 or COMPL2 event can be the source

    enumerator `SDFM_COMP_EVENT_SRC_COMPL1` = 0

      COMPL1 event is the source.

    enumerator `SDFM_COMP_EVENT_SRC_COMPL2` = 2

      COMPL2 event is the source.

  enum `SDFM_ClockSource`

    Values that can be passed to SDFM_selectClockSource() as the clkSource parameter.

    Values:

    enumerator `SDFM_CLK_SOURCE_CHANNEL_CLK` = 0x0

      Source is respective channel clock.

    enumerator `SDFM_CLK_SOURCE_SD1_CLK` = 0x8U

      Source is SD1 channel clock is the source.

  enum `SDFM_CompEventHighSource`

    Values that can be passed to SDFM_selectCompEventHighSource() as the source parameter.

    Values:

    enumerator `SDFM_COMPHOUT_SOURCE_COMPHIN` = 0x0

      Comparator event high source is unfiltered event.

    enumerator `SDFM_COMPHOUT_SOURCE_FILTER` = 0x8

      Comparator event high source is filtered event.

  enum `SDFM_CompEventLowSource`

    Values that can be passed to SDFM_selectCompEventLowSource() as the source parameter.

    Values:

    enumerator `SDFM_COMPLOUT_SOURCE_COMPLIN` = 0x000

      Comparator event low source is unfiltered event.

    enumerator `SDFM_COMPLOUT_SOURCE_FILTER` = 0x800

      Comparator event low source is filtered event.

  Functions

  void `SDFM_enableExternalReset`(uint32_t base, SDFM_FilterNumber filterNumber)

    Enable external reset

    This function enables data filter to be reset by an external source (PWM compare output).

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_disableExternalReset`(uint32_t base, SDFM_FilterNumber filterNumber)

    Disable external reset

    This function disables data filter from being reset by an external source (PWM compare output).

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_enableFilter`(uint32_t base, SDFM_FilterNumber filterNumber)

    Enable filter

    This function enables the filter specified by the

    filterNumber variable.
    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_disableFilter`(uint32_t base, SDFM_FilterNumber filterNumber)

    Disable filter

    This function disables the filter specified by the

    filterNumber variable.
    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_enableFIFOBuffer`(uint32_t base, SDFM_FilterNumber filterNumber)

    Enable FIFO buffer

    This function enables the filter FIFO buffer specified by the

    filterNumber variable.
    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_disableFIFOBuffer`(uint32_t base, SDFM_FilterNumber filterNumber)

    Disable FIFO buffer

    This function disables the filter FIFO buffer specified by the

    filterNumber variable.
    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  bool `SDFM_getZeroCrossTripStatus`(uint32_t base, SDFM_FilterNumber filterNumber)

    Return the Zero Cross Trip status

    This function returns the Zero Cross Trip status for the filter specified by filterNumber variable.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      true if Comparator filter output >= High-level threshold (Z) false if Comparator filter output < High-level threshold (Z)

  void `SDFM_clearZeroCrossTripStatus`(uint32_t base, SDFM_FilterNumber filterNumber)

    Clear the Zero Cross Trip status

    This function clears the Zero Cross Trip status for the filter specified by filterNumber variable.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_enableComparator`(uint32_t base, SDFM_FilterNumber filterNumber)

    Enable Comparator.

    This function enables the Comparator for the selected filter.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_disableComparator`(uint32_t base, SDFM_FilterNumber filterNumber)

    Disable Comparator.

    This function disables the Comparator for the selected filter.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_selectCompEventSource`(uint32_t base, SDFM_FilterNumber filterNumber, SDFM_CompEventNumber compEventNum, SDFM_CompEventSource compEventSource)

    Selects Comparator Event Source.

    This function selects the comparator event source. Valid values for

    compEventNum are:

    - SDFM_COMP_EVENT_1 - Selects comparator event 1

    - SDFM_COMP_EVENT_2 - Selects comparator event 2 Valid values for SDFM_COMP_EVENT_1 are:

    - SDFM_COMP_EVENT_SRC_COMPH1 - COMPH1 event is the source for selected event

    - SDFM_COMP_EVENT_SRC_COMPH1_L1 - Either of COMPH1 or COMPL1 event can be the source for selected event

    - SDFM_COMP_EVENT_SRC_COMPH2 - COMPH2 event is the source for selected event

    - SDFM_COMP_EVENT_SRC_COMPH2_L2 - Either of COMPH2 or COMPL2 event can be the source for selected event

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number

      - `compEventNum`: is the event number

      - `compEventSource`: is the event source

    Valid values for SDFM_COMP_EVENT_2 are:

    - SDFM_COMP_EVENT_SRC_COMPL1 - COMPL1 event is the source for selected event

    - SDFM_COMP_EVENT_SRC_COMPH1_L1 - Either of COMPH1 or COMPL1 event can be the source for selected event

    - SDFM_COMP_EVENT_SRC_COMPL2 - COMPL2 event is the source for selected event

    - SDFM_COMP_EVENT_SRC_COMPH2_L2 - Either of COMPH2 or COMPL2 event can be the source for selected event

    Return

      None.

  void `SDFM_setFilterType`(uint32_t base, SDFM_FilterNumber filterNumber, SDFM_FilterType filterType)

    Set filter type.

    This function sets the filter type or structure to be used as specified by filterType for the selected filter number as specified by filterNumber.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `filterType`: is the filter type or structure.

    Return

      None.

  void `SDFM_setFilterOverSamplingRatio`(uint32_t base, SDFM_FilterNumber filterNumber, uint16_t overSamplingRatio)

    Set data filter over sampling ratio.

    This function sets the filter oversampling ratio for the filter specified by the filterNumber variable.Valid values for the variable overSamplingRatio are 0 to 255 inclusive. The actual oversampling ratio will be this value plus one.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `overSamplingRatio`: is the data filter over sampling ratio.

    Return

      None.

  void `SDFM_setupModulatorClock`(uint32_t base, SDFM_FilterNumber filterNumber, SDFM_ModulatorClockMode clockMode)

    Set modulator clock mode.

    This function sets the modulator clock mode specified by clockMode for the filter specified by filterNumber.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `clockMode`: is the modulator clock mode.

    Note

      This function also enables the data and clock synchronizers for the specified filter.

    Return

      None.

  void `SDFM_setOutputDataFormat`(uint32_t base, SDFM_FilterNumber filterNumber, SDFM_OutputDataFormat dataFormat)

    Set the output data format

    This function sets the output data format for the filter specified by filterNumber.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `dataFormat`: is the output data format.

    Return

      None.

  void `SDFM_setDataShiftValue`(uint32_t base, SDFM_FilterNumber filterNumber, uint16_t shiftValue)

    Set data shift value.

    This function sets the shift value for the 16 bit 2’s complement data format. The valid maximum value for shiftValue is 31.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `shiftValue`: is the data shift value.

    Note: Use this function with 16 bit 2’s complement data format only.

    Return

      None.

  void `SDFM_setCompFilterHighThreshold`(uint32_t base, SDFM_FilterNumber filterNumber, uint32_t highThreshold)

    Set Filter output high-level threshold.

    This function sets the unsigned high-level threshold value for the Comparator filter output. If the output value of the filter exceeds highThreshold and interrupt generation is enabled, an interrupt will be issued. The param

    highThreshold takes both high threshold 1 & 2 values. The upper 16-bits represent the high threshold 2 value while lower 16-bits represent the threshold 1 values.
    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `highThreshold`: is the high-level threshold 1 & 2.

    Return

      None.

  void `SDFM_setCompFilterLowThreshold`(uint32_t base, SDFM_FilterNumber filterNumber, uint32_t lowThreshold)

    Set Filter output low-level threshold.

    This function sets the unsigned low-level threshold value 1 or 2 for the Comparator filter output. If the output value of the filter gets below lowThreshold and interrupt generation is enabled, an interrupt will be issued. The param

    lowThreshold takes both low threshold 1 & 2 values. The upper 16-bits represent the low threshold 2 value while lower 16-bits represent the threshold 1 values.
    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number

      - `lowThreshold`: is the low-level threshold

    Return

      None.

  void `SDFM_setCompFilterZeroCrossThreshold`(uint32_t base, SDFM_FilterNumber filterNumber, uint16_t zeroCrossThreshold)

    Set Filter output zero-cross threshold.

    This function sets the unsigned zero-cross threshold value for the Comparator filter output.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `zeroCrossThreshold`: is the zero-cross threshold.

    Return

      None.

  void `SDFM_enableZeroCrossEdgeDetect`(uint32_t base, SDFM_FilterNumber filterNumber)

    Enable zero-cross Edge detect mode.

    This function enables Zero Cross Edge detection.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_disableZeroCrossEdgeDetect`(uint32_t base, SDFM_FilterNumber filterNumber)

    Disable zero-cross Edge detect mode.

    This function disables Zero Cross Edge detection.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_enableInterrupt`(uint32_t base, SDFM_FilterNumber filterNumber, uint16_t intFlags)

    Enable SDFM interrupts.

    This function enables the low threshold , high threshold or modulator failure interrupt as determined by intFlags for the filter specified by filterNumber. Valid values for intFlags are: SDFM_MODULATOR_FAILURE_INTERRUPT , SDFM_LOW_LEVEL_THRESHOLD_INTERRUPT, SDFM_HIGH_LEVEL_THRESHOLD_INTERRUPT, SDFM_FIFO_INTERRUPT, SDFM_FIFO_OVERFLOW_INTERRUPT,SDFM_DATA_FILTER_ACKNOWLEDGE_INTERRUPT

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `intFlags`: is the interrupt source.

    Return

      None.

  void `SDFM_disableInterrupt`(uint32_t base, SDFM_FilterNumber filterNumber, uint16_t intFlags)

    Disable SDFM interrupts.

    This function disables the low threshold , high threshold or modulator failure interrupt as determined by intFlags for the filter specified by filterNumber. Valid values for intFlags are: SDFM_MODULATOR_FAILURE_INTERRUPT , SDFM_LOW_LEVEL_THRESHOLD_INTERRUPT, SDFM_HIGH_LEVEL_THRESHOLD_INTERRUPT, SDFM_FIFO_INTERRUPT, SDFM_FIFO_OVERFLOW_INTERRUPT,SDFM_DATA_FILTER_ACKNOWLEDGE_INTERRUPT

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `intFlags`: is the interrupt source.

    Return

      None.

  void `SDFM_setComparatorFilterType`(uint32_t base, SDFM_FilterNumber filterNumber, SDFM_FilterType filterType)

    Set the comparator filter type.

    This function sets the Comparator filter type or structure to be used as specified by filterType for the selected filter number as specified by filterNumber.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `filterType`: is the comparator filter type or structure.

    Return

      None.

  void `SDFM_setCompFilterOverSamplingRatio`(uint32_t base, SDFM_FilterNumber filterNumber, uint16_t overSamplingRatio)

    Set Comparator filter over sampling ratio.

    This function sets the comparator filter oversampling ratio for the filter specified by the filterNumber.Valid values for the variable overSamplingRatio are 0 to 31 inclusive. The actual oversampling ratio will be this value plus one.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `overSamplingRatio`: is the comparator filter over sampling ration.

    Return

      None.

  uint32_t `SDFM_getFilterData`(uint32_t base, SDFM_FilterNumber filterNumber)

    Get the filter data output.

    This function returns the latest data filter output. Depending on the filter data output format selected, the valid value will be the lower 16 bits or the whole 32 bits of the returned value.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      Returns the latest data filter output.

  SDFM_OutputThresholdStatus `SDFM_getThresholdStatus`(uint32_t base, SDFM_FilterNumber filterNumber)

    Get the Comparator threshold status.

    This function returns the Comparator output threshold status for the given filterNumber.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      Returns the following status flags.

      - SDFM_OUTPUT_WITHIN_THRESHOLD if the output is within the specified threshold.

      - SDFM_OUTPUT_ABOVE_THRESHOLD if the output is above the high threshold

      - SDFM_OUTPUT_BELOW_THRESHOLD if the output is below the low threshold.

  bool `SDFM_getModulatorStatus`(uint32_t base, SDFM_FilterNumber filterNumber)

    Get the Modulator status.

    This function returns the Modulator status.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      Returns true if the Modulator is operating normally Returns false if the Modulator has failed

  bool `SDFM_getNewFilterDataStatus`(uint32_t base, SDFM_FilterNumber filterNumber)

    Check if new Filter data is available.

    This function returns new filter data status.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      Returns true if new filter data is available Returns false if no new filter data is available

  bool `SDFM_getFIFOOverflowStatus`(uint32_t base, SDFM_FilterNumber filterNumber)

    Check if FIFO buffer is overflowed.

    This function returns the status of the FIFO buffer overflow for the given filter value.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      Returns true if FIFO buffer is overflowed Returns false if FIFO buffer is not overflowed

  bool `SDFM_getFIFOISRStatus`(uint32_t base, SDFM_FilterNumber filterNumber)

    Check FIFO buffer interrupt status.

    This function returns the status of the FIFO buffer interrupt for the given filter.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      Returns true if FIFO buffer interrupt has occurred. Returns false if FIFO buffer interrupt has not occurred.

  bool `SDFM_getIsrStatus`(uint32_t base)

    Get pending interrupt.

    This function returns any pending interrupt status.

    Parameters

      - `base`: is the base address of the SDFM module

    Return

      Returns true if there is a pending interrupt. Returns false if no interrupt is pending.

  void `SDFM_clearInterruptFlag`(uint32_t base, uint32_t flag)

    Clear pending flags.

    This function clears the specified pending interrupt flag. Valid values are SDFM_MAIN_INTERRUPT_FLAG,SDFM_FILTER_1_NEW_DATA_FLAG, SDFM_FILTER_2_NEW_DATA_FLAG,SDFM_FILTER_3_NEW_DATA_FLAG, SDFM_FILTER_4_NEW_DATA_FLAG,SDFM_FILTER_1_MOD_FAILED_FLAG, SDFM_FILTER_2_MOD_FAILED_FLAG,SDFM_FILTER_3_MOD_FAILED_FLAG, SDFM_FILTER_4_MOD_FAILED_FLAG,SDFM_FILTER_1_HIGH_THRESHOLD_FLAG, SDFM_FILTER_1_LOW_THRESHOLD_FLAG,SDFM_FILTER_2_HIGH_THRESHOLD_FLAG, SDFM_FILTER_2_LOW_THRESHOLD_FLAG,SDFM_FILTER_3_HIGH_THRESHOLD_FLAG, SDFM_FILTER_3_LOW_THRESHOLD_FLAG,SDFM_FILTER_4_HIGH_THRESHOLD_FLAG, SDFM_FILTER_4_LOW_THRESHOLD_FLAG,SDFM_FILTER_1_FIFO_OVERFLOW_FLAG, SDFM_FILTER_2_FIFO_OVERFLOW_FLAG,SDFM_FILTER_3_FIFO_OVERFLOW_FLAG SDFM_FILTER_4_FIFO_OVERFLOW_FLAG,SDFM_FILTER_1_FIFO_INTERRUPT_FLAG, SDFM_FILTER_2_FIFO_INTERRUPT_FLAG,SDFM_FILTER_3_FIFO_INTERRUPT_FLAG SDFM_FILTER_4_FIFO_INTERRUPT_FLAG or any combination of the above flags.

    Parameters

      - `base`: is the base address of the SDFM module

      - `flag`: is the SDFM status

    Return

      None

  void `SDFM_enableMainInterrupt`(uint32_t base)

    Enable main interrupt.

    This function enables the main SDFM interrupt.

    Parameters

      - `base`: is the base address of the SDFM module

    Return

      None

  void `SDFM_disableMainInterrupt`(uint32_t base)

    Disable main interrupt.

    This function disables the main SDFM interrupt.

    Parameters

      - `base`: is the base address of the SDFM module

    Return

      None

  void `SDFM_enableMainFilter`(uint32_t base)

    Enable main filter.

    This function enables main filter.

    Parameters

      - `base`: is the base address of the SDFM module

    Return

      None

  void `SDFM_disableMainFilter`(uint32_t base)

    Disable main filter.

    This function disables main filter.

    Parameters

      - `base`: is the base address of the SDFM module

    Return

      None

  uint16_t `SDFM_getFIFODataCount`(uint32_t base, SDFM_FilterNumber filterNumber)

    Return the FIFO data count

    This function returns the FIFO data count.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      Returns the number of data words available in FIFO buffer.

  uint16_t `SDFM_getComparatorSincData`(uint32_t base, SDFM_FilterNumber filterNumber)

    Return the Comparator sinc filter data

    This function returns the Comparator sinc filter data output.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      Returns the Comparator sinc filter data output.

  uint32_t `SDFM_getFIFOData`(uint32_t base, SDFM_FilterNumber filterNumber)

    Return the FIFO data

    This function returns the latest FIFO data.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      Returns the latest FIFO data.

    Note

      Discard the upper 16 bits if the output data format is 16bits.

  void `SDFM_setFIFOInterruptLevel`(uint32_t base, SDFM_FilterNumber filterNumber, uint16_t fifoLevel)

    Set the FIFO interrupt level.

    This function sets the FIFO interrupt level. Interrupt is generated when the FIFO buffer word count gets to or exceeds the value of

    fifoLevel. Maximum value for fifoLevel is 16.
    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `fifoLevel`: is the FIFO interrupt level.

    Return

      None.

  void `SDFM_setDataReadyInterruptSource`(uint32_t base, SDFM_FilterNumber filterNumber, SDFM_DataReadyInterruptSource dataReadySource)

    Set data ready interrupt source.

    This function sets the data ready interrupt source. Valid values for

    dataReadySource:

    - SDFM_DATA_READY_SOURCE_DIRECT - Direct data ready

    - SDFM_DATA_READY_SOURCE_FIFO - FIFO data ready.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `dataReadySource`: is the data ready interrupt source.

    Return

      None.

  bool `SDFM_getWaitForSyncStatus`(uint32_t base, SDFM_FilterNumber filterNumber)

    Get the wait-for-sync event status.

    This function returns the Wait-for-Sync event status.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      Returns true if sync event has occurred. Returns false if sync event has not occurred.

  void `SDFM_clearWaitForSyncFlag`(uint32_t base, SDFM_FilterNumber filterNumber)

    Clear the Wait-for-sync event status.

    This function clears the Wait-for-sync event status.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_enableWaitForSync`(uint32_t base, SDFM_FilterNumber filterNumber)

    Enable wait for sync mode.

    This function enables the wait for sync mode. Data to FIFO will be written only after PWM sync event.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_disableWaitForSync`(uint32_t base, SDFM_FilterNumber filterNumber)

    Disable wait for sync mode.

    This function disables the wait for sync mode. Data to FIFO will be written every Data ready event.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_setPWMSyncSource`(uint32_t base, SDFM_FilterNumber filterNumber, SDFM_PWMSyncSource syncSource)

    Set the PWM sync mode.

    This function sets the PWM sync source for the specific SDFM filter. Valid values for syncSource are SDFM_SYNC_PWMx_CMPy. Where x ranges from 1 to 8 Representing PWM1 to PWM8 respectively and y ranges from A to D representing PWM comparators A to D.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `syncSource`: is the PWM sync source.

    Return

      None.

  void `SDFM_setFIFOClearOnSyncMode`(uint32_t base, SDFM_FilterNumber filterNumber, SDFM_FIFOClearSyncMode fifoClearSyncMode)

    Set FIFO clear on sync mode.

    This function sets the FIFO clear mode for the specified filter when a sync happens depending on the value of fifoClearSyncMode. Valid values for fifoClearSyncMode are:

    - SDFM_FIFO_NOT_CLEARED_ON_SYNC - FIFO is not cleared on sync.

    - SDFM_FIFO_CLEARED_ON_SYNC - FIFO is cleared on sync.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `fifoClearSyncMode`: is the FIFO clear on sync mode.

    Return

      None.

  void `SDFM_setWaitForSyncClearMode`(uint32_t base, SDFM_FilterNumber filterNumber, SDFM_WaitForSyncClearMode syncClearMode)

    Set Wait-for-sync clear mode.

    This function sets the Wait-For-sync clear mode depending on the value of syncClearMode. Valid values for syncClearMode are:

    - SDFM_MANUAL_CLEAR_WAIT_FOR_SYNC - Wait-for-sync flag is cleared by invoking SDFM_clearWaitForSyncFlag().

    - SDFM_AUTO_CLEAR_WAIT_FOR_SYNC - Wait-for-sync flag is cleared automatically on FIFO interrupt.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `syncClearMode`: is the wait-for-sync clear mode.

    Return

      None.

  void `SDFM_selectClockSource`(uint32_t base, SDFM_FilterNumber filterNumber, SDFM_ClockSource clkSource)

    Selects clock source for SDFM channels.

    This function selects the clock for SDFM module filter channels. Valid values for clkSource are:

    - SDFM_CLK_SOURCE_CHANNEL_CLK - Respective channel’s clk is the source

    - SDFM_CLK_SOURCE_SD1_CLK - Filter 1 clock is the source

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `clkSource`: is the clock source

    Return

      None.

  void `SDFM_enableSynchronizer`(uint32_t base, SDFM_FilterNumber filterNumber, uint16_t syncConfig)

    Enables Input Synchronizer.

    This function enables either data or clock or both synchronizer. Valid values for syncConfig can be the logical OR of any of the values:

    - SDFM_CLOCK_SYNCHRONIZER - Enable SDFM input clock synchronizer

    - SDFM_DATA_SYNCHRONIZER - Enable SDFM input data synchronizer

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `syncConfig`: defines which synchronizer to be enabled

    Return

      None.

  void `SDFM_disableSynchronizer`(uint32_t base, SDFM_FilterNumber filterNumber, uint16_t syncConfig)

    Disables Input Synchronizer.

    This function disables either data or clock or both synchronizer. Valid values for syncConfig can be the logical OR of any of the values:

    - SDFM_CLOCK_SYNCHRONIZER - Disable SDFM input clock synchronizer

    - SDFM_DATA_SYNCHRONIZER - Disable SDFM input data synchronizer

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `syncConfig`: defines which synchronizer to be disabled

    Return

      None.

  void `SDFM_selectCompEventHighSource`(uint32_t base, SDFM_FilterNumber filterNumber, SDFM_CompEventHighSource source)

    Selects comparator event high source.

    This function selects the source for comparator event high. Valid values for source are:

    - SDFM_COMPHOUT_SOURCE_COMPHIN - Original COMPHIN/CEVT1 signal is source

    - SDFM_COMPHOUT_SOURCE_FILTER - Filtered COMPHIN/CEVT1 signal is source

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `source`: is the comparator event high source

    Return

      None.

  void `SDFM_selectCompEventLowSource`(uint32_t base, SDFM_FilterNumber filterNumber, SDFM_CompEventLowSource source)

    Selects comparator event low source.

    This function selects the source for comparator event low. Valid values for source are:

    - SDFM_COMPLOUT_SOURCE_COMPLIN - Original COMPLIN/CEVT2 signal is source

    - SDFM_COMPHOUT_SOURCE_FILTER - Filtered COMPLIN/CEVT2 signal is source

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `source`: is the comparator event low source

    Return

      None.

  void `SDFM_initCompEventLowFilter`(uint32_t base, SDFM_FilterNumber filterNumber)

    Initializes Comparator Event Low Filter.

    This function initializes Comparator Event Low Filter.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_initCompEventHighFilter`(uint32_t base, SDFM_FilterNumber filterNumber)

    Initializes Comparator Event High Filter.

    This function initializes Comparator Event High Filter.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

    Return

      None.

  void `SDFM_lockCompEventFilterConfig`(uint32_t base, SDFM_FilterNumber filterNumber, uint16_t lockConfig)

    Lock Comparator Event Filter Configurations

    This function locks the comparator event filter configurations. Valid values of the lockConfig can be logical OR of any of the following values:

    - SDFM_SDCOMPLOCK_SDCOMPCTL - Locks write access to SDCOMPCTL register

    - SDFM_SDCOMPLOCK_COMP - Locks write access to SDCOMPxFILCTL & SDCOMPxFILCLKCTL register

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `lockConfig`: defines the configurations to be locked

    Return

      None.

  void `SDFM_configComparator`(uint32_t base, uint16_t config1, uint32_t config2, uint16_t config3)

    Configures SDFM comparator for filter config & threshold values

    This function configures the comparator filter for filter config and threshold values based on provided inputs.

    Parameters

      - `base`: is the base address of the SDFM module

      - `config1`: is the filter number, filter type and over sampling ratio.

      - `config2`: is high-level and low-level threshold 1 values.

    The config1 parameter is the logical OR of the filter number, filter type and oversampling ratio. The bit definitions for config1 are as follow:

    - config1.[3:0] filter number

    - config1.[7:4] filter type

    - config1.[15:8] Over sampling Ratio Valid values for filter number and filter type are defined in SDFM_FilterNumber and SDFM_FilterType enumerations respectively. SDFM_SET_OSR(X) macro can be used to set the value of the oversampling ratio ,which ranges [1,32] inclusive, in the appropriate bit location. For example the value (SDFM_FILTER_1 | SDFM_FILTER_SINC_2 | SDFM_SET_OSR(16)) will select Filter 1, SINC 2 type with an oversampling ratio of 16.

    The config2 parameter is the logical OR of the filter high and low threshold 1 values. The bit definitions for config2 are as follow:

    - config2.[15:0] low threshold 1

    - config2.[31:16] high threshold 1 The upper 16 bits define the high threshold 1 and the lower 16 bits define the low threshold 1. SDFM_THRESHOLD(H,L) can be used to combine the high and low thresholds. The config3 parameter is the logical OR of the zero cross threshold enable flag and the zero-cross threshold value. The bit definitions for config3 are as follow:

    - config3.[15] - Enable or disable zero cross threshold. Valid values are 1 or 0 to enable or disable the zero cross threshold respectively. -config3.[14:0] - Zero Cross Threshold value. The SDFM_SET_ZERO_CROSS_THRESH_VALUE(X) macro can be used to specify the zero-cross threshold value and OR the 1 to enable it.

    Return

      None.

  void `SDFM_configEnhancedComparator`(uint32_t base, uint16_t filterConfig, uint32_t highLowThreshold1, uint32_t highLowThreshold2, uint16_t zeroCrossThreshold)

    Configure SDFM enhanced comparator for filter config & threshold values

    This function configures the comparator filter for filter config and threshold values based on input parameters.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterConfig`: is the filter number, filter type & over sampling ratio.

      - `highLowThreshold1`: is high-level and low-level threshold 1 values.

      - `highLowThreshold2`: is high-level and low-level threshold 2 values.

      - `zeroCrossThreshold`: is the zero-cross threshold value.

    The filterConfig parameter is the logical OR of the filter number, filter type and oversampling ratio. The bit definitions for filterConfig are as follow:

    - filterConfig.[3:0] filter number

    - filterConfig.[7:4] filter type

    - filterConfig.[15:8] Over sampling Ratio Valid values for filter number and filter type are defined in SDFM_FilterNumber and SDFM_FilterType enumerations respectively. SDFM_SET_OSR(X) macro can be used to set the value of the oversampling ratio ,which ranges [1,32] inclusive, in the appropriate bit location. For example the value (SDFM_FILTER_1 | SDFM_FILTER_SINC_2 | SDFM_SET_OSR(16)) will select Filter 1, SINC 2 type with an oversampling ratio of 16.

    The highLowThreshold1 parameter is the logical OR of the filter high & low threshold 1 values. The bit definitions for highLowThreshold1 are as follow:

    - highLowThreshold1.[15:0] low threshold 1

    - highLowThreshold1.[31:16] high threshold 1 The upper 16 bits define the high threshold and the lower 16 bits define the low threshold. SDFM_THRESHOLD(H,L) can be used to combine the high and low thresholds.

    The highLowThreshold2 parameter is the logical OR of the filter high & low threshold 2 values. The bit definitions for highLowThreshold2 are as follow:

    - highLowThreshold2.[15:0] low threshold 2

    - highLowThreshold2.[31:16] high threshold 2 The upper 16 bits define the high threshold and the lower 16 bits define the low threshold. SDFM_THRESHOLD(H,L) can be used to combine the high & low thresholds.

    The zeroCrossThreshold parameter is the logical OR of the zero cross threshold enable flag and the zero-cross threshold value. The bit definitions for zeroCrossThreshold are as follows:

    - zeroCrossThreshold.[15] - Enable or disable zero cross threshold. Valid values are 1 or 0 to enable or disable the zero cross threshold respectively.

    - zeroCrossThreshold.[14:0] - Zero Cross Threshold value. The SDFM_SET_ZERO_CROSS_THRESH_VALUE(X) macro can be used as parameter zeroCrossThreshold to enable & specify the zero-cross threshold value.

    Return

      None.

  void `SDFM_configDataFilter`(uint32_t base, uint16_t config1, uint16_t config2)

    Configure SDFM data filter

    This function configures the data filter based on configurations config1 and config2.

    Parameters

      - `base`: is the base address of the SDFM module

      - `config1`: is the filter number, filter type and over sampling ratio configuration.

      - `config2`: is filter switch, data representation and data shift values configuration.

    The config1 parameter is the logical OR of the filter number, filter type and oversampling ratio. The bit definitions for config1 are as follow:

    - config1.[3:0] Filter number

    - config1.[7:4] Filter type

    - config1.[15:8] Over sampling Ratio Valid values for filter number and filter type are defined in SDFM_FilterNumber and SDFM_FilterType enumerations respectively. SDFM_SET_OSR(X) macro can be used to set the value of the oversampling ratio , which ranges [1,256] inclusive , in the appropriate bit location for config1. For example the value (SDFM_FILTER_2 | SDFM_FILTER_SINC_3 | SDFM_SET_OSR(64)) will select Filter 2 , SINC 3 type with an oversampling ratio of 64.

    The config2 parameter is the logical OR of data representation, filter switch, and data shift values The bit definitions for config2 are as follow:

    - config2.[0] Data representation

    - config2.[1] Filter switch

    - config2.[15:2] Shift values Valid values for data representation are given in SDFM_OutputDataFormat enumeration. SDFM_FILTER_DISABLE or SDFM_FILTER_ENABLE will define the filter switch values.SDFM_SHIFT_VALUE(X) macro can be used to set the value of the data shift value,which ranges [0,31] inclusive, in the appropriate bit location for config2. The shift value is valid only in SDFM_DATA_FORMAT_16_BIT data representation format.

    Return

      None.

  void `SDFM_configZeroCrossComparator`(uint32_t base, uint16_t config1, uint16_t config2)

    Configure SDFM comparator Zero Cross threshold

    This function configures the comparator filter zero cross threshold values based on configurations config1 and config2.

    Parameters

      - `base`: is the base address of the SDFM module

      - `config1`: is the filter number, filter type and over sampling ratio.

      - `config2`: is the zero cross threshold value.

    The config1 parameter is the logical OR of the filter number, filter type and oversampling ratio. The bit definitions for config1 are as follow:

    - config1.[3:0] filter number

    - config1.[7:4] filter type

    - config1.[15:8] Over sampling Ratio Valid values for filter number and filter type are defined in SDFM_FilterNumber and SDFM_FilterType enumerations respectively. SDFM_SET_OSR(X) macro can be used to set the value of the oversampling ratio ,which ranges [1,32] inclusive, in the appropriate bit location. For example the value (SDFM_FILTER_1 | SDFM_FILTER_SINC_2 | SDFM_SET_OSR(16)) will select Filter 1 , SINC 2 type with an oversampling ratio of 16.

    The config2 parameter is the value of the zero cross threshold. The maximum acceptable value is 32767.

    Return

      None.

  void `SDFM_configDataFilterFIFO`(uint32_t base, uint16_t config1, uint16_t config2)

    Configure SDFM data filter FIFO

    This function enables and configures the data filter FIFO based on configurations config1 and config2.

    Parameters

      - `base`: is the base address of the SDFM module

      - `config1`: is the filter number, filter type and over sampling ratio configuration.

      - `config2`: is filter switch, data representation and data shift values and FIFO level configuration.

    The config1 parameter is the logical OR of the filter number, filter type and oversampling ratio. The bit definitions for config1 are as follow:

    - config1.[3:0] filter number

    - config1.[7:4] filter type

    - config1.[15:8] Over sampling Ratio Valid values for filter number and filter type are defined in SDFM_FilterNumber and SDFM_FilterType enumerations respectively. SDFM_SET_OSR(X) macro can be used to set the value of the oversampling ratio , which ranges [1,256] inclusive , in the appropriate bit location for config1. For example the value (SDFM_FILTER_2 | SDFM_FILTER_SINC_3 | SDFM_SET_OSR(64)) will select Filter 2 , SINC 3 type with an oversampling ratio of 64.

    The config2 parameter is the logical OR of data representation, filter switch, data shift value, and FIFO level The bit definitions for config2 are as follow:

    - config2.[0] Data representation

    - config2.[1] filter switch.

    - config2.[6:2] shift values.

    - config2.[15:7] FIFO level Valid values for data representation are given in SDFM_OutputDataFormat enumeration. SDFM_FILTER_DISABLE or SDFM_FILTER_ENABLE will define the filter switch values.SDFM_SHIFT_VALUE(X) macro can be used to set the value of the data shift value,which ranges [0,31] inclusive, in the appropriate bit location for config2. The value of FIFO level ranges [1,16] inclusive. The macro SDFM_SET_FIFO_LEVEL(X) can be used to set the value of the FIFO level.

    Return

      None.

  void `SDFM_configCompEventLowFilter`(uint32_t base, SDFM_FilterNumber filterNumber, const SDFM_CompEventFilterConfig *config)

    Configure Comparator Event Low Filter

    This function configures the sample window, threshold and clock prescale configurations for the comparator event low filter.

    Parameters

      - `base`: is the base address of the SDFM module

      - `filterNumber`: is the filter number.

      - `config`: is the comparator event low source

    Return

      None.

  void `SDFM_configCompEventHighFilter`(uint32_t base, SDFM_FilterNumber filterNumber, const SDFM_CompEventFilterConfig *config)

    Configure Comparator Event High Filter

    This function configures the sample window, threshold and clock prescale configurations for the comparator event high filter.

    Parameters

      - `base`: is the base address of the SDFM module.

      - `filterNumber`: is the filter number.

      - `config`: is the comparator event high source

    Return

      None.

  struct `SDFM_CompEventFilterConfig`
    #include <sdfm.h>

    Values that can be passed to SDFM_configCompEventLowFilter() & SDFM_configCompEventHighFilter() as the filterNumber.

The code for this module is contained in driverlib/sdfm.c, with driverlib/sdfm.h containing the API declarations for use by applications.