ADC input in PGAx_OF group used as CMP input
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Figure 12.4（P1453 in TRM）shows that the PGAx_OF is the source of CMPx_HP0 and CMPx_LP0. While take Analog Group1 for example, in Table 12-1（P1454 in TRM）, if pin A2/B6/PGA1_OF is used as normal ADC input A2 and B6 (not as PGA1_OF), can this pin be used as CMP1_HP0 at the same time?
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