# ASysCtl Module

The ASysCtl or Analog System Control driver provides functions to enable, disable and lock the temperature sensor on the device. It will also provide additional functionality if available for that device.

group `asysctl_api`

  Functions

  void `ASysCtl_enableTemperatureSensor`(void)

    Enable temperature sensor.

    This function enables the temperature sensor output to the ADC.

    Return

      None.

  void `ASysCtl_disableTemperatureSensor`(void)

    Disable temperature sensor.

    This function disables the temperature sensor output to the ADC.

    Return

      None.

  void `ASysCtl_lockTemperatureSensor`(void)

    Locks the temperature sensor control register.

    Return

      None.

The code for this module is contained in driverlib/asysctl.c, with driverlib/asysctl.h containing the API declarations for use by applications.