# Code Interface Report for Inverter_000_test

### Table of Contents

- Entry-Point Functions
- Inports
- Outports
- Interface Parameters
- Data Stores

### Entry-Point Functions

Function: Inverter_000_test_initialize

Prototype | void Inverter_000_test_initialize(void)
Description | Initialization entry point of generated code
Timing | Must be called exactly once
Arguments | None
Return value | None
Header file | Inverter_000_test.h

Function: Inverter_000_test_step0

Prototype | void Inverter_000_test_step0(void)
Description | Output entry point of generated code
Timing | Must be called periodically, every 5e-05 seconds
Arguments | None
Return value | None
Header file | Inverter_000_test.h

Function: Inverter_000_test_step1

Prototype | void Inverter_000_test_step1(void)
Description | Output entry point of generated code
Timing | Must be called periodically, every 0.0001 seconds
Arguments | None
Return value | None
Header file | Inverter_000_test.h

Function: Inverter_000_test_terminate

Prototype | void Inverter_000_test_terminate(void)
Description | Termination entry point of generated code
Timing | Must be called exactly once
Arguments | None
Return value | None
Header file | Inverter_000_test.h

### Inports

No Inports in model.

### Outports

No Outports in model.

### Interface Parameters

[-]

Parameter Source | Code Identifier | Data Type | Scaling | Dimension
--- | --- | --- | --- | ---
<S4>/Float to IQN2 | Inverter_000_test_P.FloattoIQN2_P1 | real_T |  | 1
<S4>/Float to IQN | Inverter_000_test_P.FloattoIQN_P1 | real_T |  | 1
<S4>/Float to IQN1 | Inverter_000_test_P.FloattoIQN1_P1 | real_T |  | 1
<S11>/Float to IQN | Inverter_000_test_P.FloattoIQN_P1_j | real_T |  | 1
<S2>/Float to IQN1 | Inverter_000_test_P.FloattoIQN1_P1_b | real_T |  | 1
<Root>/Constant | Inverter_000_test_P.Constant_Value | real_T |  | 1
<Root>/Saturation4 | Inverter_000_test_P.Saturation4_UpperSat | int32_T | sfix32_En10 | 1
<Root>/Saturation4 | Inverter_000_test_P.Saturation4_LowerSat | int32_T | sfix32_En10 | 1
<Root>/Constant8 | Inverter_000_test_P.Constant8_Value | int32_T | sfix32_En10 | 1
<Root>/Saturation5 | Inverter_000_test_P.Saturation5_UpperSat | int32_T | sfix32_En10 | 1
<Root>/Saturation5 | Inverter_000_test_P.Saturation5_LowerSat | int32_T | sfix32_En10 | 1
<Root>/Constant3 | Inverter_000_test_P.Constant3_Value | int32_T | sfix32_En10 | 1
<S4>/Constant11 | Inverter_000_test_P.Constant11_Value | int32_T | sfix32_En29 | 1
<S4>/Constant8 | Inverter_000_test_P.Constant8_Value_e | int32_T | sfix32_En29 | 1
<S4>/Constant9 | Inverter_000_test_P.Constant9_Value | int32_T | sfix32_En29 | 1
<S12>/Unit Delay | Inverter_000_test_P.UnitDelay_InitialCondition | int32_T | sfix32_En29 | 1
<S14>/1 | Inverter_000_test_P.u_Value | int32_T | sfix32_En29 | 1
<S14>/-1 | Inverter_000_test_P.u_Value_e | int32_T | sfix32_En29 | 1
<S15>/1 | Inverter_000_test_P.u_Value_f | int32_T | sfix32_En29 | 1
<S15>/-1 | Inverter_000_test_P.u_Value_c | int32_T | sfix32_En29 | 1
<S2>/Gain | Inverter_000_test_P.Gain_Gain | int32_T | sfix32_En31 | 1
<S5>/Gain | Inverter_000_test_P.Gain_Gain_h | int32_T | sfix32_En32 | 1
<S5>/Gain1 | Inverter_000_test_P.Gain1_Gain | int32_T | sfix32_En32 | 1
<Root>/Rate Transition1 | Inverter_000_test_P.RateTransition1_InitialConditio | real32_T |  | 1
<S4>/Gain3 | Inverter_000_test_P.Gain3_Gain | real32_T |  | 1
<S4>/Constant13 | Inverter_000_test_P.Constant13_Value | real32_T |  | 1
<S4>/Constant14 | Inverter_000_test_P.Constant14_Value | real32_T |  | 1
<S4>/Constant10 | Inverter_000_test_P.Constant10_Value | real32_T |  | 1
<S4>/Gain2 | Inverter_000_test_P.Gain2_Gain | real32_T |  | 1
<S11>/Constant | Inverter_000_test_P.Constant_Value_j | real32_T |  | 1
<Root>/Gain2 | Inverter_000_test_P.Gain2_Gain_f | real32_T |  | 1
<Root>/Bias1 | Inverter_000_test_P.Bias1_Bias | real32_T |  | 1
<S1>/Constant15 | Inverter_000_test_P.Constant15_Value | real32_T |  | 1
<S1>/Constant13 | Inverter_000_test_P.Constant13_Value_a | real32_T |  | 1
<S1>/Constant14 | Inverter_000_test_P.Constant14_Value_m | real32_T |  | 1
<Root>/Constant2 | Inverter_000_test_P.Constant2_Value | real32_T |  | 1
<Root>/Bias2 | Inverter_000_test_P.Bias2_Bias | real32_T |  | 1
<Root>/Constant14 | Inverter_000_test_P.Constant14_Value_mo | real32_T |  | 1

### Data Stores

No data stores in the model; note that this report lists only data stores with non-auto storage class and global data stores