    1#ifndef PORTABLE_WORDSIZES

    2#ifdef __MW_TARGET_USE_HARDWARE_RESOURCES_H__

    3#ifndef __MW_TARGET_HARDWARE_RESOURCES_H__

    4#define __MW_TARGET_HARDWARE_RESOURCES_H__

    5

    6#define MW_MULTI_TASKING_MODE 1

    7#include "c2000BoardSupport.h"

    8#include "F2837xD_device.h"

    9#include "F2837xD_Examples.h"

    10#include "F2837xD_GlobalPrototypes.h"

    11#include "F2837xD_cputimer.h"

    12#include "c2000SchedulerTimer.h"

    13

    14#define MW_USECODERTARGET 1

    15#define MW_TARGETHARDWARE TI Delfino F2837xD

    16#define MW_CONNECTIONINFO_SERIAL_IPADDRESS codertarget.registry.getLoopbackIP;

    17#define MW_CONNECTIONINFO_SERIAL_PORT 17725

    18#define MW_CONNECTIONINFO_SERIAL_VERBOSE 1

    19#define MW_CONNECTIONINFO_CAN_MEXARGS

    20#define MW_EXTMODE_CONFIGURATION serial

    21#define MW_RTOS Baremetal

    22#define MW_SCHEDULER_INTERRUPT_SOURCE 0

    23#define MW_RUNTIME_BUILDACTION 1

    24#define MW_RUNTIME_DEVICEID 0

    25#define MW_RUNTIME_FLASHLOAD 1

    26#define MW_RUNTIME_CPU 0

    27#define MW_RUNTIME_LOADCOMMANDARG C:/ProgramData/MATLAB/SupportPackages/R2018a/toolbox/target/supportpackages/tic2000/CCS_Config/f28379D_test.ccxml

    28#define MW_RUNTIME_CPU2MODELENABLE 102

    29#define MWalse #define MW_RUNTIME_CPU2MODEL

    30#define MW_TARGETLINKOBJ_USECUSTOMLINKER 0

    31#define MW_TARGETLINKOBJ_NAME $(TARGET_ROOT)/src/c28377D.cmd

    32#define MW_CLOCKING_CPUCLOCKRATEMHZ 200

    33#define MW_CLOCKING_USEINTERNALOSC 0

    34#define MW_CLOCKING_OSCCLK 20

    35#define MW_CLOCKING_AUTOSETPLLSETTINGS 1

    36#define MW_CLOCKING_PLLCR 20

    37#define MW_CLOCKING_DIVSEL 2

    38#define MW_CLOCKING_CLOSESTCPUCLOCK 200

    39#define MW_CLOCKING_LSPCLKDIV 0

    40#define MW_CLOCKING_LSPCLK 200

    41#define MW_ADCA_CPUCORE 0

    42#define MW_ADCA_CLOCKDIV 7

    43#define MW_ADCA_CLOCKFREQUENCY 40.000000

    44#define MW_ADCA_OFFSETCORRECTIONVALUE AdcaRegs.ADCOFFTRIM.bit.OFFTRIM

    45#define MW_ADCA_EXTERNALREFERENCESELECTOR 0

    46#define MW_ADCA_EXTERNALREFERENCEVREFHI 3.3

    47#define MW_ADCA_EXTERNALREFERENCEVREFLO 0

    48#define MW_ADCA_INTPULSEGENERATION 0

    49#define MW_ADCA_SOCPRIORITY 0

    50#define MW_ADCA_XINT2GPIO GPIO0

    51#define MW_ADCB_CPUCORE 0

    52#define MW_ADCB_CLOCKDIV 7

    53#define MW_ADCB_CLOCKFREQUENCY 40.000000

    54#define MW_ADCB_OFFSETCORRECTIONVALUE AdcbRegs.ADCOFFTRIM.bit.OFFTRIM

    55#define MW_ADCB_EXTERNALREFERENCESELECTOR 0

    56#define MW_ADCB_EXTERNALREFERENCEVREFHI 3.3

    57#define MW_ADCB_EXTERNALREFERENCEVREFLO 0

    58#define MW_ADCB_INTPULSEGENERATION 0

    59#define MW_ADCB_SOCPRIORITY 0

    60#define MW_ADCB_XINT2GPIO GPIO0

    61#define MW_ADCC_CPUCORE 0

    62#define MW_ADCC_CLOCKDIV 7

    63#define MW_ADCC_CLOCKFREQUENCY 40.000000

    64#define MW_ADCC_OFFSETCORRECTIONVALUE AdccRegs.ADCOFFTRIM.bit.OFFTRIM

    65#define MW_ADCC_EXTERNALREFERENCESELECTOR 0

    66#define MW_ADCC_EXTERNALREFERENCEVREFHI 3.3

    67#define MW_ADCC_EXTERNALREFERENCEVREFLO 0

    68#define MW_ADCC_INTPULSEGENERATION 0

    69#define MW_ADCC_SOCPRIORITY 0

    70#define MW_ADCC_XINT2GPIO GPIO0

    71#define MW_ADCD_CPUCORE 0

    72#define MW_ADCD_CLOCKDIV 7

    73#define MW_ADCD_CLOCKFREQUENCY 40.000000

    74#define MW_ADCD_OFFSETCORRECTIONVALUE AdcdRegs.ADCOFFTRIM.bit.OFFTRIM

    75#define MW_ADCD_EXTERNALREFERENCESELECTOR 0

    76#define MW_ADCD_EXTERNALREFERENCEVREFHI 3.3

    77#define MW_ADCD_EXTERNALREFERENCEVREFLO 0

    78#define MW_ADCD_INTPULSEGENERATION 0

    79#define MW_ADCD_SOCPRIORITY 0

    80#define MW_ADCD_XINT2GPIO GPIO0

    81#define MW_DACA_VOLTAGE 0

    82#define MW_DACA_LOADMODE 0

    83#define MW_DACB_VOLTAGE 0

    84#define MW_DACB_LOADMODE 0

    85#define MW_DACC_VOLTAGE 0

    86#define MW_DACC_LOADMODE 0

    87#define MW_EPWM_CLOCKDIV 1

    88#define MW_EPWM_PINASSIGNMENT_TZ1 None

    89#define MW_EPWM_PINASSIGNMENT_TZ2 None

    90#define MW_EPWM_PINASSIGNMENT_TZ3 None

    91#define MW_EPWM_PINASSIGNMENT_SYNCI None

    92#define MW_EPWM_PINASSIGNMENT_SYNCO None

    93#define MW_EPWM_PINASSIGNMENT_PWM1A 1

    94#define MW_EPWM_PINASSIGNMENT_PWM1B 1

    95#define MW_EPWM_PINASSIGNMENT_PWM2A 1

    96#define MW_EPWM_PINASSIGNMENT_PWM2B 1

    97#define MW_EPWM_PINASSIGNMENT_PWM3A 1

    98#define MW_EPWM_PINASSIGNMENT_PWM3B 1

    99#define MW_EPWM_PINASSIGNMENT_PWM4A 1

    100#define MW_EPWM_PINASSIGNMENT_PWM4B 1

    101#define MW_EPWM_PINASSIGNMENT_PWM5A 1

    102#define MW_EPWM_PINASSIGNMENT_PWM5B 1

    103#define MW_EPWM_PINASSIGNMENT_PWM6A 1

    104#define MW_EPWM_PINASSIGNMENT_PWM6B 1

    105#define MW_EPWM_PINASSIGNMENT_PWM7A 1

    106#define MW_EPWM_PINASSIGNMENT_PWM7B 1

    107#define MW_EPWM_PINASSIGNMENT_PWM8A 1

    108#define MW_EPWM_PINASSIGNMENT_PWM8B 1

    109#define MW_EPWM_PINASSIGNMENT_PWM9A 1

    110#define MW_EPWM_PINASSIGNMENT_PWM9B 1

    111#define MW_EPWM_PINASSIGNMENT_PWM10A 1

    112#define MW_EPWM_PINASSIGNMENT_PWM10B 1

    113#define MW_EPWM_PINASSIGNMENT_PWM11A 1

    114#define MW_EPWM_PINASSIGNMENT_PWM11B 1

    115#define MW_EPWM_PINASSIGNMENT_PWM12A 1

    116#define MW_EPWM_PINASSIGNMENT_PWM12B 1

    117#define MW_ECAP_PINASSIGNMENT_ECAP1 GPIO24

    118#define MW_ECAP_PINASSIGNMENT_ECAP2 GPIO25

    119#define MW_ECAP_PINASSIGNMENT_ECAP3 GPIO26

    120#define MW_ECAP_PINASSIGNMENT_ECAP4 GPIO20

    121#define MW_ECAP_PINASSIGNMENT_ECAP5 GPIO21

    122#define MW_ECAP_PINASSIGNMENT_ECAP6 GPIO23

    123#define MW_ECAP_PINASSIGNMENT_APWM1 13

    124#define MW_ECAP_PINASSIGNMENT_APWM2 14

    125#define MW_ECAP_PINASSIGNMENT_APWM3 15

    126#define MW_ECAP_PINASSIGNMENT_APWM4 16

    127#define MW_ECAP_PINASSIGNMENT_APWM5 17

    128#define MW_ECAP_PINASSIGNMENT_APWM6 18

    129#define MW_EQEP_PINASSIGNMENT_EQEP1A 2

    130#define MW_EQEP_PINASSIGNMENT_EQEP1B 2

    131#define MW_EQEP_PINASSIGNMENT_EQEP1S 2

    132#define MW_EQEP_PINASSIGNMENT_EQEP1I 2

    133#define MW_EQEP_PINASSIGNMENT_EQEP2A 1

    134#define MW_EQEP_PINASSIGNMENT_EQEP2B 1

    135#define MW_EQEP_PINASSIGNMENT_EQEP2S 1

    136#define MW_EQEP_PINASSIGNMENT_EQEP2I 1

    137#define MW_EQEP_PINASSIGNMENT_EQEP3A 2

    138#define MW_EQEP_PINASSIGNMENT_EQEP3B 2

    139#define MW_EQEP_PINASSIGNMENT_EQEP3S 2

    140#define MW_EQEP_PINASSIGNMENT_EQEP3I 2

    141#define MW_I2C_MODE 0

    142#define MW_I2C_ADDRDATAFORMAT 0

    143#define MW_I2C_OWNADDRESS 1

    144#define MW_I2C_BITCOUNT 0

    145#define MW_I2C_MODULECLOCKPRESCALER 9

    146#define MW_I2C_MODULECLOCKFREQUENCY 20000000.000000

    147#define MW_I2C_MASTERCLKLOWTIME 20

    148#define MW_I2C_MASTERCLKHIGHTIME 20

    149#define MW_I2C_MASTERCLOCKFREQUENCY 400000.000000

    150#define MW_I2C_MASTERCLOCKFREQUENCY_1 400000.000000

    151#define MW_I2C_MASTERCLOCKFREQUENCY_2 400000.000000

    152#define MW_I2C_ENABLELOOPBACK 0

    153#define MW_I2C_PINASSIGNMENT_SDAA 1

    154#define MW_I2C_PINASSIGNMENT_SCLA 1

    155#define MW_I2C_ENABLETXINT 0

    156#define MW_I2C_TXFIFOLEVEL 16

    157#define MW_I2C_ENABLERXINT 0

    158#define MW_I2C_RXFIFOLEVEL 16

    159#define MW_I2C_ENABLESYSINT 0

    160#define MW_I2C_AAS 0

    161#define MW_I2C_SCD 0

    162#define MW_I2C_ARDY 0

    163#define MW_I2C_NACK 0

    164#define MW_I2C_AL 0

    165#define MW_I2C_B_MODE 0

    166#define MW_I2C_B_ADDRDATAFORMAT 0

    167#define MW_I2C_B_OWNADDRESS 1

    168#define MW_I2C_B_BITCOUNT 0

    169#define MW_I2C_B_MODULECLOCKPRESCALER 9

    170#define MW_I2C_B_MODULECLOCKFREQUENCY 20000000.000000

    171#define MW_I2C_B_MASTERCLKLOWTIME 20

    172#define MW_I2C_B_MASTERCLKHIGHTIME 20

    173#define MW_I2C_B_MASTERCLOCKFREQUENCY 400000.000000

    174#define MW_I2C_B_MASTERCLOCKFREQUENCY_1 400000.000000

    175#define MW_I2C_B_MASTERCLOCKFREQUENCY_2 400000.000000

    176#define MW_I2C_B_ENABLELOOPBACK 0

    177#define MW_I2C_B_PINASSIGNMENT_SDAA 1

    178#define MW_I2C_B_PINASSIGNMENT_SCLA 1

    179#define MW_I2C_B_ENABLETXINT 0

    180#define MW_I2C_B_TXFIFOLEVEL 16

    181#define MW_I2C_B_ENABLERXINT 0

    182#define MW_I2C_B_RXFIFOLEVEL 16

    183#define MW_I2C_B_ENABLESYSINT 0

    184#define MW_I2C_B_AAS 0

    185#define MW_I2C_B_SCD 0

    186#define MW_I2C_B_ARDY 0

    187#define MW_I2C_B_NACK 0

    188#define MW_I2C_B_AL 0

    189#define MW_SCI_A_ENABLELOOPBACK 0

    190#define MW_SCI_A_SUSPENSIONMODE 2

    191#define MW_SCI_A_NUMBEROFSTOPBITS 0

    192#define MW_SCI_A_PARITYMODE 0

    193#define MW_SCI_A_CHARACTERLENGTHBITS 0

    194#define MW_SCI_A_USERBAUDRATE 115200

    195#define MW_SCI_A_BAUDRATEPRESCALER 216.000000

    196#define MW_SCI_A_BAUDRATE 115207.000000

    197#define MW_SCI_A_COMMUNICATIONMODE 0

    198#define MW_SCI_A_BLOCKINGMODE 0

    199#define MW_SCI_A_DATABYTEORDER 0

    200#define MW_SCI_A_DATASWAPWIDTH 0

    201#define MW_SCI_A_PINASSIGNMENT_TX 2

    202#define MW_SCI_A_PINASSIGNMENT_RX 2

    203#define MW_SCI_B_ENABLELOOPBACK 0

    204#define MW_SCI_B_SUSPENSIONMODE 2

    205#define MW_SCI_B_NUMBEROFSTOPBITS 0

    206#define MW_SCI_B_PARITYMODE 0

    207#define MW_SCI_B_CHARACTERLENGTHBITS 0

    208#define MW_SCI_B_USERBAUDRATE 115200

    209#define MW_SCI_B_BAUDRATEPRESCALER 216.000000

    210#define MW_SCI_B_BAUDRATE 115207.000000

    211#define MW_SCI_B_COMMUNICATIONMODE 0

    212#define MW_SCI_B_BLOCKINGMODE 0

    213#define MW_SCI_B_DATABYTEORDER 0

    214#define MW_SCI_B_DATASWAPWIDTH 0

    215#define MW_SCI_B_PINASSIGNMENT_TX 1

    216#define MW_SCI_B_PINASSIGNMENT_RX 1

    217#define MW_SCI_C_ENABLELOOPBACK 0

    218#define MW_SCI_C_SUSPENSIONMODE 2

    219#define MW_SCI_C_NUMBEROFSTOPBITS 0

    220#define MW_SCI_C_PARITYMODE 0

    221#define MW_SCI_C_CHARACTERLENGTHBITS 0

    222#define MW_SCI_C_USERBAUDRATE 115200

    223#define MW_SCI_C_BAUDRATEPRESCALER 216.000000

    224#define MW_SCI_C_BAUDRATE 115207.000000

    225#define MW_SCI_C_COMMUNICATIONMODE 0

    226#define MW_SCI_C_BLOCKINGMODE 0

    227#define MW_SCI_C_DATABYTEORDER 0

    228#define MW_SCI_C_DATASWAPWIDTH 0

    229#define MW_SCI_C_PINASSIGNMENT_TX 1

    230#define MW_SCI_C_PINASSIGNMENT_RX 1

    231#define MW_SCI_D_ENABLELOOPBACK 0

    232#define MW_SCI_D_SUSPENSIONMODE 2

    233#define MW_SCI_D_NUMBEROFSTOPBITS 0

    234#define MW_SCI_D_PARITYMODE 0

    235#define MW_SCI_D_CHARACTERLENGTHBITS 0

    236#define MW_SCI_D_USERBAUDRATE 115200

    237#define MW_SCI_D_BAUDRATEPRESCALER 216.000000

    238#define MW_SCI_D_BAUDRATE 115207.000000

    239#define MW_SCI_D_COMMUNICATIONMODE 0

    240#define MW_SCI_D_BLOCKINGMODE 0

    241#define MW_SCI_D_DATABYTEORDER 0

    242#define MW_SCI_D_DATASWAPWIDTH 0

    243#define MW_SCI_D_PINASSIGNMENT_TX 1

    244#define MW_SCI_D_PINASSIGNMENT_RX 1

    245#define MW_SPI_A_MODE 0

    246#define MW_SPI_A_USERBAUDRATE 1843200

    247#define MW_SPI_A_BAUDRATEFACTOR 108.000000

    248#define MW_SPI_A_BAUDRATE 1834862.000000

    249#define MW_SPI_A_DATABITS 15

    250#define MW_SPI_A_CLOCKPOLARITY 0

    251#define MW_SPI_A_CLOCKPHASE 0

    252#define MW_SPI_A_SUSPENSIONMODE 2

    253#define MW_SPI_A_ENABLELOOPBACK 0

    254#define MW_SPI_A_ENABLETHREEWIRE 0

    255#define MW_SPI_A_TXINTERRUPTENABLE 0

    256#define MW_SPI_A_FIFOINTERRUPTLEVEL_TX 0

    257#define MW_SPI_A_RXINTERRUPTENABLE 0

    258#define MW_SPI_A_FIFOINTERRUPTLEVEL_RX 16

    259#define MW_SPI_A_FIFOENABLE 1

    260#define MW_SPI_A_FIFOTRANSMITDELAY 0

    261#define MW_SPI_A_PINASSIGNMENT_SIMO 1

    262#define MW_SPI_A_PINASSIGNMENT_SOMI 1

    263#define MW_SPI_A_PINASSIGNMENT_CLK 1

    264#define MW_SPI_A_PINASSIGNMENT_STE 1

    265#define MW_SPI_A_PINVALUE_SIMO 16

    266#define MW_SPI_A_PINVALUE_SOMI 17

    267#define MW_SPI_A_PINVALUE_CLK 18

    268#define MW_SPI_A_PINVALUE_STE 19

    269#define MW_SPI_A_PINMUX_SIMO 1

    270#define MW_SPI_A_PINMUX_SOMI 1

    271#define MW_SPI_A_PINMUX_CLK 1

    272#define MW_SPI_A_PINMUX_STE 1

    273#define MW_SPI_A_FIFO_LEVEL 16.000000

    274#define MW_SPI_B_MODE 0

    275#define MW_SPI_B_USERBAUDRATE 1843200

    276#define MW_SPI_B_BAUDRATEFACTOR 108.000000

    277#define MW_SPI_B_BAUDRATE 1834862.000000

    278#define MW_SPI_B_DATABITS 15

    279#define MW_SPI_B_CLOCKPOLARITY 0

    280#define MW_SPI_B_CLOCKPHASE 0

    281#define MW_SPI_B_SUSPENSIONMODE 2

    282#define MW_SPI_B_ENABLELOOPBACK 0

    283#define MW_SPI_B_ENABLETHREEWIRE 0

    284#define MW_SPI_B_TXINTERRUPTENABLE 0

    285#define MW_SPI_B_FIFOINTERRUPTLEVEL_TX 0

    286#define MW_SPI_B_RXINTERRUPTENABLE 0

    287#define MW_SPI_B_FIFOINTERRUPTLEVEL_RX 16

    288#define MW_SPI_B_FIFOENABLE 1

    289#define MW_SPI_B_FIFOTRANSMITDELAY 0

    290#define MW_SPI_B_PINASSIGNMENT_SIMO 1

    291#define MW_SPI_B_PINASSIGNMENT_SOMI 1

    292#define MW_SPI_B_PINASSIGNMENT_CLK 2

    293#define MW_SPI_B_PINASSIGNMENT_STE 2

    294#define MW_SPI_B_PINVALUE_SIMO 24

    295#define MW_SPI_B_PINVALUE_SOMI 25

    296#define MW_SPI_B_PINVALUE_CLK 26

    297#define MW_SPI_B_PINVALUE_STE 27

    298#define MW_SPI_B_PINMUX_SIMO 6

    299#define MW_SPI_B_PINMUX_SOMI 6

    300#define MW_SPI_B_PINMUX_CLK 6

    301#define MW_SPI_B_PINMUX_STE 6

    302#define MW_SPI_B_FIFO_LEVEL 16.000000

    303#define MW_SPI_C_MODE 0

    304#define MW_SPI_C_USERBAUDRATE 1843200

    305#define MW_SPI_C_BAUDRATEFACTOR 108.000000

    306#define MW_SPI_C_BAUDRATE 1834862.000000

    307#define MW_SPI_C_DATABITS 15

    308#define MW_SPI_C_CLOCKPOLARITY 0

    309#define MW_SPI_C_CLOCKPHASE 0

    310#define MW_SPI_C_SUSPENSIONMODE 2

    311#define MW_SPI_C_ENABLELOOPBACK 0

    312#define MW_SPI_C_ENABLETHREEWIRE 0

    313#define MW_SPI_C_TXINTERRUPTENABLE 0

    314#define MW_SPI_C_FIFOINTERRUPTLEVEL_TX 0

    315#define MW_SPI_C_RXINTERRUPTENABLE 0

    316#define MW_SPI_C_FIFOINTERRUPTLEVEL_RX 16

    317#define MW_SPI_C_FIFOENABLE 1

    318#define MW_SPI_C_FIFOTRANSMITDELAY 0

    319#define MW_SPI_C_PINASSIGNMENT_SIMO 1

    320#define MW_SPI_C_PINASSIGNMENT_SOMI 1

    321#define MW_SPI_C_PINASSIGNMENT_CLK 1

    322#define MW_SPI_C_PINASSIGNMENT_STE 1

    323#define MW_SPI_C_PINVALUE_SIMO 50

    324#define MW_SPI_C_PINVALUE_SOMI 51

    325#define MW_SPI_C_PINVALUE_CLK 52

    326#define MW_SPI_C_PINVALUE_STE 53

    327#define MW_SPI_C_PINMUX_SIMO 6

    328#define MW_SPI_C_PINMUX_SOMI 6

    329#define MW_SPI_C_PINMUX_CLK 6

    330#define MW_SPI_C_PINMUX_STE 6

    331#define MW_SPI_C_FIFO_LEVEL 16.000000

    332#define MW_ECAN_A_MODULECLOCKFREQUENCY 200

    333#define MW_ECAN_A_BAUDRATEPRESCALER 20.000000

    334#define MW_ECAN_A_TSEG1 4

    335#define MW_ECAN_A_TSEG2 3

    336#define MW_ECAN_A_BAUDRATE 1000000

    337#define MW_ECAN_A_SBG 0

    338#define MW_ECAN_A_SJW 1

    339#define MW_ECAN_A_SAM 0

    340#define MW_ECAN_A_ENHANCEDCANMODE 1

    341#define MW_ECAN_A_SELFTESTMODE 0

    342#define MW_ECAN_A_PINASSIGNMENT_TX 3

    343#define MW_ECAN_A_PINASSIGNMENT_RX 3

    344#define MW_ECAN_B_MODULECLOCKFREQUENCY 200

    345#define MW_ECAN_B_BAUDRATEPRESCALER 20.000000

    346#define MW_ECAN_B_TSEG1 4

    347#define MW_ECAN_B_TSEG2 3

    348#define MW_ECAN_B_BAUDRATE 1000000

    349#define MW_ECAN_B_SBG 0

    350#define MW_ECAN_B_SJW 1

    351#define MW_ECAN_B_SAM 0

    352#define MW_ECAN_B_ENHANCEDCANMODE 1

    353#define MW_ECAN_B_SELFTESTMODE 0

    354#define MW_ECAN_B_PINASSIGNMENT_TX 2

    355#define MW_ECAN_B_PINASSIGNMENT_RX 2

    356#define MW_WATCHDOG_ENABLE_WATCHDOG 0

    357#define MW_WATCHDOG_WATCHDOGCLOCK 0

    358#define MW_WATCHDOG_TIME_PERIOD 0.013107

    359#define MW_WATCHDOG_WATCHDOGEVENT 0

    360#define MW_GPIO0_7_GPIOQUALSEL0 0

    361#define MW_GPIO0_7_GPIOQUALSEL1 0

    362#define MW_GPIO0_7_GPIOQUALSEL2 0

    363#define MW_GPIO0_7_GPIOQUALSEL3 0

    364#define MW_GPIO0_7_GPIOQUALSEL4 0

    365#define MW_GPIO0_7_GPIOQUALSEL5 0

    366#define MW_GPIO0_7_GPIOQUALSEL6 0

    367#define MW_GPIO0_7_GPIOQUALSEL7 0

    368#define MW_GPIO0_7_QUALPRD 0

    369#define MW_GPIO8_15_GPIOQUALSEL8 0

    370#define MW_GPIO8_15_GPIOQUALSEL9 0

    371#define MW_GPIO8_15_GPIOQUALSEL10 0

    372#define MW_GPIO8_15_GPIOQUALSEL11 0

    373#define MW_GPIO8_15_GPIOQUALSEL12 0

    374#define MW_GPIO8_15_GPIOQUALSEL13 0

    375#define MW_GPIO8_15_GPIOQUALSEL14 0

    376#define MW_GPIO8_15_GPIOQUALSEL15 0

    377#define MW_GPIO8_15_QUALPRD 0

    378#define MW_GPIO16_23_GPIOQUALSEL16 0

    379#define MW_GPIO16_23_GPIOQUALSEL17 0

    380#define MW_GPIO16_23_GPIOQUALSEL18 0

    381#define MW_GPIO16_23_GPIOQUALSEL19 0

    382#define MW_GPIO16_23_GPIOQUALSEL20 0

    383#define MW_GPIO16_23_GPIOQUALSEL21 0

    384#define MW_GPIO16_23_GPIOQUALSEL22 0

    385#define MW_GPIO16_23_GPIOQUALSEL23 0

    386#define MW_GPIO16_23_QUALPRD 0

    387#define MW_GPIO24_31_GPIOQUALSEL24 0

    388#define MW_GPIO24_31_GPIOQUALSEL25 0

    389#define MW_GPIO24_31_GPIOQUALSEL26 0

    390#define MW_GPIO24_31_GPIOQUALSEL27 0

    391#define MW_GPIO24_31_GPIOQUALSEL28 0

    392#define MW_GPIO24_31_GPIOQUALSEL29 0

    393#define MW_GPIO24_31_GPIOQUALSEL30 0

    394#define MW_GPIO24_31_GPIOQUALSEL31 0

    395#define MW_GPIO24_31_QUALPRD 0

    396#define MW_GPIO32_39_GPIOQUALSEL32 0

    397#define MW_GPIO32_39_GPIOQUALSEL33 0

    398#define MW_GPIO32_39_GPIOQUALSEL34 0

    399#define MW_GPIO32_39_GPIOQUALSEL35 0

    400#define MW_GPIO32_39_GPIOQUALSEL36 0

    401#define MW_GPIO32_39_GPIOQUALSEL37 0

    402#define MW_GPIO32_39_GPIOQUALSEL38 0

    403#define MW_GPIO32_39_GPIOQUALSEL39 0

    404#define MW_GPIO32_39_QUALPRD 0

    405#define MW_GPIO40_47_GPIOQUALSEL40 0

    406#define MW_GPIO40_47_GPIOQUALSEL41 0

    407#define MW_GPIO40_47_GPIOQUALSEL42 0

    408#define MW_GPIO40_47_GPIOQUALSEL43 0

    409#define MW_GPIO40_47_GPIOQUALSEL44 0

    410#define MW_GPIO40_47_GPIOQUALSEL45 0

    411#define MW_GPIO40_47_GPIOQUALSEL46 0

    412#define MW_GPIO40_47_GPIOQUALSEL47 0

    413#define MW_GPIO40_47_QUALPRD 0

    414#define MW_GPIO48_55_GPIOQUALSEL48 0

    415#define MW_GPIO48_55_GPIOQUALSEL49 0

    416#define MW_GPIO48_55_GPIOQUALSEL50 0

    417#define MW_GPIO48_55_GPIOQUALSEL51 0

    418#define MW_GPIO48_55_GPIOQUALSEL52 0

    419#define MW_GPIO48_55_GPIOQUALSEL53 0

    420#define MW_GPIO48_55_GPIOQUALSEL54 0

    421#define MW_GPIO48_55_GPIOQUALSEL55 0

    422#define MW_GPIO48_55_QUALPRD 0

    423#define MW_GPIO56_63_GPIOQUALSEL56 0

    424#define MW_GPIO56_63_GPIOQUALSEL57 0

    425#define MW_GPIO56_63_GPIOQUALSEL58 0

    426#define MW_GPIO56_63_GPIOQUALSEL59 0

    427#define MW_GPIO56_63_GPIOQUALSEL60 0

    428#define MW_GPIO56_63_GPIOQUALSEL61 0

    429#define MW_GPIO56_63_GPIOQUALSEL62 0

    430#define MW_GPIO56_63_GPIOQUALSEL63 0

    431#define MW_GPIO56_63_QUALPRD 0

    432#define MW_GPIO64_71_GPIOQUALSEL64 0

    433#define MW_GPIO64_71_GPIOQUALSEL65 0

    434#define MW_GPIO64_71_GPIOQUALSEL66 0

    435#define MW_GPIO64_71_GPIOQUALSEL67 0

    436#define MW_GPIO64_71_GPIOQUALSEL68 0

    437#define MW_GPIO64_71_GPIOQUALSEL69 0

    438#define MW_GPIO64_71_GPIOQUALSEL70 0

    439#define MW_GPIO64_71_GPIOQUALSEL71 0

    440#define MW_GPIO64_71_QUALPRD 0

    441#define MW_GPIO72_79_GPIOQUALSEL72 0

    442#define MW_GPIO72_79_GPIOQUALSEL73 0

    443#define MW_GPIO72_79_GPIOQUALSEL74 0

    444#define MW_GPIO72_79_GPIOQUALSEL75 0

    445#define MW_GPIO72_79_GPIOQUALSEL76 0

    446#define MW_GPIO72_79_GPIOQUALSEL77 0

    447#define MW_GPIO72_79_GPIOQUALSEL78 0

    448#define MW_GPIO72_79_GPIOQUALSEL79 0

    449#define MW_GPIO72_79_QUALPRD 0

    450#define MW_GPIO80_87_GPIOQUALSEL80 0

    451#define MW_GPIO80_87_GPIOQUALSEL81 0

    452#define MW_GPIO80_87_GPIOQUALSEL82 0

    453#define MW_GPIO80_87_GPIOQUALSEL83 0

    454#define MW_GPIO80_87_GPIOQUALSEL84 0

    455#define MW_GPIO80_87_GPIOQUALSEL85 0

    456#define MW_GPIO80_87_GPIOQUALSEL86 0

    457#define MW_GPIO80_87_GPIOQUALSEL87 0

    458#define MW_GPIO80_87_QUALPRD 0

    459#define MW_GPIO88_95_GPIOQUALSEL88 0

    460#define MW_GPIO88_95_GPIOQUALSEL89 0

    461#define MW_GPIO88_95_GPIOQUALSEL90 0

    462#define MW_GPIO88_95_GPIOQUALSEL91 0

    463#define MW_GPIO88_95_GPIOQUALSEL92 0

    464#define MW_GPIO88_95_GPIOQUALSEL93 0

    465#define MW_GPIO88_95_GPIOQUALSEL94 0

    466#define MW_GPIO88_95_GPIOQUALSEL95 0

    467#define MW_GPIO88_95_QUALPRD 0

    468#define MW_GPIO96_103_GPIOQUALSEL96 0

    469#define MW_GPIO96_103_GPIOQUALSEL97 0

    470#define MW_GPIO96_103_GPIOQUALSEL98 0

    471#define MW_GPIO96_103_GPIOQUALSEL99 0

    472#define MW_GPIO96_103_GPIOQUALSEL100 0

    473#define MW_GPIO96_103_GPIOQUALSEL101 0

    474#define MW_GPIO96_103_GPIOQUALSEL102 0

    475#define MW_GPIO96_103_GPIOQUALSEL103 0

    476#define MW_GPIO96_103_QUALPRD 0

    477#define MW_GPIO104_111_GPIOQUALSEL104 0

    478#define MW_GPIO104_111_GPIOQUALSEL105 0

    479#define MW_GPIO104_111_GPIOQUALSEL106 0

    480#define MW_GPIO104_111_GPIOQUALSEL107 0

    481#define MW_GPIO104_111_GPIOQUALSEL108 0

    482#define MW_GPIO104_111_GPIOQUALSEL109 0

    483#define MW_GPIO104_111_GPIOQUALSEL110 0

    484#define MW_GPIO104_111_GPIOQUALSEL111 0

    485#define MW_GPIO104_111_QUALPRD 0

    486#define MW_GPIO112_119_GPIOQUALSEL112 0

    487#define MW_GPIO112_119_GPIOQUALSEL113 0

    488#define MW_GPIO112_119_GPIOQUALSEL114 0

    489#define MW_GPIO112_119_GPIOQUALSEL115 0

    490#define MW_GPIO112_119_GPIOQUALSEL116 0

    491#define MW_GPIO112_119_GPIOQUALSEL117 0

    492#define MW_GPIO112_119_GPIOQUALSEL118 0

    493#define MW_GPIO112_119_GPIOQUALSEL119 0

    494#define MW_GPIO112_119_QUALPRD 0

    495#define MW_GPIO120_127_GPIOQUALSEL120 0

    496#define MW_GPIO120_127_GPIOQUALSEL121 0

    497#define MW_GPIO120_127_GPIOQUALSEL122 0

    498#define MW_GPIO120_127_GPIOQUALSEL123 0

    499#define MW_GPIO120_127_GPIOQUALSEL124 0

    500#define MW_GPIO120_127_GPIOQUALSEL125 0

    501#define MW_GPIO120_127_GPIOQUALSEL126 0

    502#define MW_GPIO120_127_GPIOQUALSEL127 0

    503#define MW_GPIO120_127_QUALPRD 0

    504#define MW_GPIO128_135_GPIOQUALSEL128 0

    505#define MW_GPIO128_135_GPIOQUALSEL129 0

    506#define MW_GPIO128_135_GPIOQUALSEL130 0

    507#define MW_GPIO128_135_GPIOQUALSEL131 0

    508#define MW_GPIO128_135_GPIOQUALSEL132 0

    509#define MW_GPIO128_135_GPIOQUALSEL133 0

    510#define MW_GPIO128_135_GPIOQUALSEL134 0

    511#define MW_GPIO128_135_GPIOQUALSEL135 0

    512#define MW_GPIO128_135_QUALPRD 0

    513#define MW_GPIO136_143_GPIOQUALSEL136 0

    514#define MW_GPIO136_143_GPIOQUALSEL137 0

    515#define MW_GPIO136_143_GPIOQUALSEL138 0

    516#define MW_GPIO136_143_GPIOQUALSEL139 0

    517#define MW_GPIO136_143_GPIOQUALSEL140 0

    518#define MW_GPIO136_143_GPIOQUALSEL141 0

    519#define MW_GPIO136_143_GPIOQUALSEL142 0

    520#define MW_GPIO136_143_GPIOQUALSEL143 0

    521#define MW_GPIO136_143_QUALPRD 0

    522#define MW_GPIO144_151_GPIOQUALSEL144 0

    523#define MW_GPIO144_151_GPIOQUALSEL145 0

    524#define MW_GPIO144_151_GPIOQUALSEL146 0

    525#define MW_GPIO144_151_GPIOQUALSEL147 0

    526#define MW_GPIO144_151_GPIOQUALSEL148 0

    527#define MW_GPIO144_151_GPIOQUALSEL149 0

    528#define MW_GPIO144_151_GPIOQUALSEL150 0

    529#define MW_GPIO144_151_GPIOQUALSEL151 0

    530#define MW_GPIO144_151_QUALPRD 0

    531#define MW_GPIO152_159_GPIOQUALSEL152 0

    532#define MW_GPIO152_159_GPIOQUALSEL153 0

    533#define MW_GPIO152_159_GPIOQUALSEL154 0

    534#define MW_GPIO152_159_GPIOQUALSEL155 0

    535#define MW_GPIO152_159_GPIOQUALSEL156 0

    536#define MW_GPIO152_159_GPIOQUALSEL157 0

    537#define MW_GPIO152_159_GPIOQUALSEL158 0

    538#define MW_GPIO152_159_GPIOQUALSEL159 0

    539#define MW_GPIO152_159_QUALPRD 0

    540#define MW_GPIO160_167_GPIOQUALSEL160 0

    541#define MW_GPIO160_167_GPIOQUALSEL161 0

    542#define MW_GPIO160_167_GPIOQUALSEL162 0

    543#define MW_GPIO160_167_GPIOQUALSEL163 0

    544#define MW_GPIO160_167_GPIOQUALSEL164 0

    545#define MW_GPIO160_167_GPIOQUALSEL165 0

    546#define MW_GPIO160_167_GPIOQUALSEL166 0

    547#define MW_GPIO160_167_GPIOQUALSEL167 0

    548#define MW_GPIO160_167_QUALPRD 0

    549#define MW_GPIO168_175_GPIOQUALSEL168 0

    550#define MW_GPIO168_175_GPIOQUALSEL169 0

    551#define MW_GPIO168_175_GPIOQUALSEL170 0

    552#define MW_GPIO168_175_GPIOQUALSEL171 0

    553#define MW_GPIO168_175_GPIOQUALSEL172 0

    554#define MW_GPIO168_175_GPIOQUALSEL173 0

    555#define MW_GPIO168_175_GPIOQUALSEL174 0

    556#define MW_GPIO168_175_GPIOQUALSEL175 0

    557#define MW_GPIO168_175_QUALPRD 0

    558#define MW_XINT_GPIOXINT1SEL 0

    559#define MW_XINT_GPIOXINT2SEL 0

    560#define MW_XINT_GPIOXINT3SEL 0

    561#define MW_XINT_GPIOXINT4SEL 0

    562#define MW_XINT_GPIOXINT5SEL 0

    563#define MW_XINT_POLARITY1 0

    564#define MW_XINT_POLARITY2 0

    565#define MW_XINT_POLARITY3 0

    566#define MW_XINT_POLARITY4 0

    567#define MW_XINT_POLARITY5 0

    568#define MW_EXTMODECOMPORT COM7

    569#define MW_EXECUTIONPROFILEBUFFERLEN 50.000000

    570#define MW_DATAVERSION 2016.02

    571

    572#endif /* __MW_TARGET_HARDWARE_RESOURCES_H__ */

    573

    574#endif

    575

    576#endif

    577