[2]Building file: "../ClaTasks.asm"
[3]Invoking: C2000 Compiler
[4]"/Applications/ti/ccs2040/ccs/tools/compiler/ti-cgt-c2000_22.6.3.LTS/bin/cl2000" -v28 -ml -mt --cla_support=cla2 --float_support=fpu32 --tmu_support=tmu1 -Ooff --fp_mode=relaxed --include_path="/Users/dennisjarc/workspace_ccstheia/spe1053_28P55x" --include_path="/Applications/ti/c2000/C2000Ware_6_00_01_00" --include_path="/Users/dennisjarc/workspace_ccstheia/spe1053_28P55x/device" --include_path="/Applications/ti/c2000/C2000Ware_6_00_01_00/driverlib/f28p55x/driverlib/" --include_path="/Applications/ti/c2000/C2000Ware_6_00_01_00/device_support/f28p55x/headers/include" --include_path="/Applications/ti/ccs2040/ccs/tools/compiler/ti-cgt-c2000_22.6.3.LTS/include" --define=_DUAL_HEADERS --define=DEBUG --define=CMD_FLASH --define=_FLASH --diag_suppress=10063 --diag_warning=225 --diag_wrap=off --display_error_number --gen_func_subsections=on --abi=eabi --cla_background_task=off --cla_signed_compare_workaround=on --preproc_with_compile --preproc_dependency="ClaTasks.d_raw" --include_path="/Users/dennisjarc/workspace_ccstheia/spe1053_28P55x/CPU1_FLASH/syscfg" --cmd_file="syscfg/board.opt" --cmd_file="syscfg/device_cmd.opt" --cmd_file="syscfg/c2000ware_libraries.opt"  "../ClaTasks.asm"
[5]"/Applications/ti/c2000/C2000Ware_6_00_01_00/driverlib/f28p55x/driverlib/interrupt.h", line 483: warning #1853-D: declaration hides built-in function "__disable_interrupts"
[6]"/Applications/ti/c2000/C2000Ware_6_00_01_00/driverlib/f28p55x/driverlib/interrupt.h", line 484: warning #1853-D: declaration hides built-in function "__enable_interrupts"
[7]"/Applications/ti/c2000/C2000Ware_6_00_01_00/driverlib/f28p55x/driverlib/lin.h", line 696: warning #169-D: argument of type "int16_t *" is incompatible with parameter of type "int *"
[8]"/var/tmp/TI7wZmIyZc0", WARNING! at line 4299: [E0004] Cannot redefine existing opcode 'EALLOW' with .define. Assembler ignoring .define.
[9]	           .define "__eallow()",EALLOW

[10]"/var/tmp/TI7wZmIyZc0", WARNING! at line 4390: [E0004] Cannot redefine existing opcode 'EDIS' with .define. Assembler ignoring .define.
[11]	           .define "__edis()",EDIS

[12]"/var/tmp/TI7wZmIyZc0", WARNING! at line 13726: [E0004] Cannot redefine existing opcode 'Reset' with .define. Assembler ignoring .define.
[13]	           .define "49",Reset

[14]"/var/tmp/TI7wZmIyZc0", ERROR!   at line 43246: [E0003] Only labels and comments may begin in the first column. Make sure that the label name is not a reserved keyword.
[15]	MCANSS_REGS                                  .struct 0,4          ; struct size=(44 bytes|704 bits), alignment=4

[16]"/var/tmp/TI7wZmIyZc0", REMARK   at line 43246: [R0001] After symbol substitution the line became:
[17]	(0x1400U)                                  .struct 0,4          ; struct size=(44 bytes|704 bits), alignment=4

[18]"/var/tmp/TI7wZmIyZc0", ERROR!   at line 43246: [E0002] Invalid mnemonic specification
[19]	MCANSS_REGS                                  .struct 0,4          ; struct size=(44 bytes|704 bits), alignment=4

[20]"/var/tmp/TI7wZmIyZc0", REMARK   at line 43246: [R0001] After symbol substitution the line became:
[21]	(0x1400U)                                  .struct 0,4          ; struct size=(44 bytes|704 bits), alignment=4

[22]"/var/tmp/TI7wZmIyZc0", ERROR!   at line 43247: [E0300] Can't tag an undefined symbol
[23]	MCANSS_PID                                   .tag MCANSS_PID_REG  ; union MCANSS_PID_REG MCANSS_PID - offset 0 bytes, size (4 bytes|64 bits)

[24]"/var/tmp/TI7wZmIyZc0", ERROR!   at line 43248: [E0300] Can't tag an undefined symbol
[25]	MCANSS_CTRL                                  .tag MCANSS_CTRL_REG ; union MCANSS_CTRL_REG MCANSS_CTRL - offset 4 bytes, size (4 bytes|64 bits)

[26]"/var/tmp/TI7wZmIyZc0", ERROR!   at line 43249: [E0300] Can't tag an undefined symbol
[27]	MCANSS_STAT                                  .tag MCANSS_STAT_REG ; union MCANSS_STAT_REG MCANSS_STAT - offset 8 bytes, size (4 bytes|64 bits)

[28]"/var/tmp/TI7wZmIyZc0", ERROR!   at line 43250: [E0300] Can't tag an undefined symbol
[29]	MCANSS_ICS                                   .tag MCANSS_ICS_REG  ; union MCANSS_ICS_REG MCANSS_ICS - offset 12 bytes, size (4 bytes|64 bits)

[30]"/var/tmp/TI7wZmIyZc0", ERROR!   at line 43251: [E0300] Can't tag an undefined symbol
[31]	MCANSS_IRS                                   .tag MCANSS_IRS_REG  ; union MCANSS_IRS_REG MCANSS_IRS - offset 16 bytes, size (4 bytes|64 bits)

[32]"/var/tmp/TI7wZmIyZc0", ERROR!   at line 43252: [E0300] Can't tag an undefined symbol
[33]	MCANSS_IECS                                  .tag MCANSS_IECS_REG ; union MCANSS_IECS_REG MCANSS_IECS - offset 20 bytes, size (4 bytes|64 bits)

[34]"/var/tmp/TI7wZmIyZc0", ERROR!   at line 43253: [E0300] Can't tag an undefined symbol
[35]	MCANSS_IE                                    .tag MCANSS_IE_REG   ; union MCANSS_IE_REG MCANSS_IE - offset 24 bytes, size (4 bytes|64 bits)

[36]"/var/tmp/TI7wZmIyZc0", ERROR!   at line 43254: [E0300] Can't tag an undefined symbol
[37]	MCANSS_IES                                   .tag MCANSS_IES_REG  ; union MCANSS_IES_REG MCANSS_IES - offset 28 bytes, size (4 bytes|64 bits)

[38]"/var/tmp/TI7wZmIyZc0", ERROR!   at line 43255: [E0300] Can't tag an undefined symbol
[39]	MCANSS_EOI                                   .tag MCANSS_EOI_REG  ; union MCANSS_EOI_REG MCANSS_EOI - offset 32 bytes, size (4 bytes|64 bits)

[40]"/var/tmp/TI7wZmIyZc0", ERROR!   at line 43256: [E0300] Can't tag an undefined symbol
[41]	MCANSS_EXT_TS_PRESCALER                      .tag MCANSS_EXT_TS_PRESCALER_REG ; union MCANSS_EXT_TS_PRESCALER_REG MCANSS_EXT_TS_PRESCALER - offset 36 bytes, size (4 bytes|64 bits)