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B Console 23

NewTargetConfiguration.coxml

2B CPUL: Writing Flash @ Address @x00082000 of Length ex00000016 (page ) -
Erasing Flash Bank @, Sector

Erasing Flash Bank @, Sector

Erasing Flash Bank @, Sector

Erasing Flash Bank @, Sector

Erasing Flash Bank @, Sector

Erasing Flash Bank @, Sector

Erasing Flash Bank @, Sector

Erasing Flash Bank @, Sector

Erasing Flash Bank @, Sector

Erasing Flash Bank @, Sector

Erasing Flash Bank @, Sector

Erasing Flash Bank @, Sector

Erasing Flash Bank @, Sector

Erasing Flash Bank @, Sector

Data has been buffered at the end of the current data block for 64-bit aligned writes.

Error during Flash programming (Flash algorithm returned error code). Operation cancelled.

Error iriting Flash @ Address 0x0052000 of Length 0x00000016 (page @)

Writing buffered data @ Address @x00082014 of Length @x00000004

Error during Flash programming (Flash algorithm returned error code). Operation cancelled.

Y Please make sure the memory location you are programming have not already been programmed.

€28 CPUL: GEL: File: E:\Project\PDSOD\F2837xD\F2837xD\V150\F2837xD_exanples_Cpul\aa_cpu_timers\cpudl\ccs\CPUL_FLASH\cpu_tiners_cpudl.out: Load failed.
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i BB -PHRS @i B3RP iEEr D Quick Access i B | B cos edit (B CCS bebug )
35 Debug 52 ¥ = 0O - Variables 53 6 Expressions i1t Registers 0| @ §
4 ¥ NewTargetConfiguration.coxml [Code Composer Studio - Device Debugging] Name Type Value

4 P Texas Instruments XDS2xx USB Debug Probe_0/C28xx CPUI (Suspended - SW Breakpoint)
= 0x00C696 (no symbols are defined for 0x00C696)
4 Texas Instruments XDS2xx USB Debug Probe_0/CPU1_CLA1 (Disconnected : Unknown)

@ Texas Instruments XDS2xx USB Debug Probe_0/C28xx_CPU2 (Disconnected : Unknown)
@ Texas Instruments XDS2xx USB Debug Probe_0/CPU2_CLA1 (Disconnected : Unknown) < = I
[E] 0xc696 52 = B @ MemoryBrowser 32 He@-e-PH(ris Y0

No source available for "0xc696" Data ~| 0x00082000

'Data0,82000 - 000082000 <Memory Rendering 1> £3
16-Bit Hex - T1 Style

R FFF FFEF FEEF FEFF FEFF FEFF FEFF FEFF FEFF FEFF FEFF FEFF FEFF FEFF FFFF FEFF FFE FEFEFEFE o
©x0002014  FFFF FFFF FFFF FFFF FFFF FFFF FEFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFRF FFRE
©x00082028  FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FEFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FEFF FFRE
Ox000B203C  FFFF FFFF FFEF FEFF FRFF FFFF FEFF FEFF FEFF FRFF FFEF FEFF FRFF FFCF FEFF FREF FFEF FEFE FRFF FEFE [
©x00082050  FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFRF FFRF FFRF FFAF FFFE
©x0002064  FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFRE
©x0002078  FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFFF FFRF FFFF FFFF FFFF FFFF

= Console 2 bl B -9y = O | @ onChipFlash 3 =g

NewTargetConfigurstion.ccaml e . 3
ter text System PLLCR Integer Mulipler (SPLUIMULT) (15-50) 15

a0 CPUL: Error during Flash progranming (Flash slgorithn returned error x| 2P = it LEEED T

code). Operation cancelled. Memory Map System PLLCR Fractional Multipler (SPLLEMULT)  [0.10] il

2 CPUL: Error lriting Flash § Address of Length 6x00000016 GEL Fles

(page @) i System Clock Divide Select (SYSDIVSEL) 01 2

C2830c CPUL: Wiriting buffered data @ Address 0x00052014 of Length 0x00000004 On-Chip Flash o flstem Clock Divide Select (YSDIVSEL)__ iz 3

280 CPUL: Error during Flash programming (Flash slgorithn returned error Program/Memory Load Options

code) Operation cancelled. " Auto Run and Launch Options Remember My Settings

280 CPUL: Please make sure the memory location you are programming have not " >

already been programmed. Misc/Other Options The changed setting will take immediate effect for the current debug session. If
C28xx CPUL: GEL: Fils C28xx Disassembly Style Options. you would like to persist your changes for subsequent debug sessions, you'll
£:\Project\PDBOO\F2837XD\F2837xD\v150\F2837xD_examples_Cpul\aa_cpu_timers\cpuo| need to click on Remember My Settings' button. Click here to hide this
1\ces\CPUL_FLASH\cpu_timers_cpudl.out: Load failed. m e e
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2B CPUL: GEL Output:
Memory Map Initialization

Flash
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memory...
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C28x0_CPUL: If erase/program (E/P) operation is being done on one core, the B

other core should not execute from shared-RAM (SR) as they are used for the £/P
Also, CPUL will be halted to determine SR ownership for the CPU which

will run the Flash Plugin code, after which CPUL will be set to run its

application. User code execution from SR could commence after both flash banks

ZErmunzammonar

ot CPUL: Operation completed successfully.

[ype filter text
Memory Map
GEL Files
On-Chip Flash
Program/Memory Load Options
Auto Run and Launch Options
Misc/Other Options
2B Disassembly Style Options

Quick Access | B cesedit
==
E
Erase Setings “ (lloe=
Entire Flash i

Necessary Sectors Only (for Program Load)
© Selected Sectors Only

Sector B (0xB2000 - 0XB3FFR) |
Sector C (0x84000 - Ox8SFFF) W

Sector D (0486000 - 0XB7FFF)
Sector E (0488000 - OXBFFFF)
Sector F (0x90000 - 0:7FFF)
Sector G (0498000 - OXOFFF)
Sector H (0xADO0O - OxATFFF)
Sector I (0xAB0OO - OxAFFFF)
Sector J (0xB000D - OXBTFFF)
Sector K (0xB8000 - 0xBIFFF)
Sector L (0xBADDO - OxBBFFF)
Sector M (0xBCO0O - 0BDFFF)
Sector N (0xBEODD - OXBFFFF)

Sector A (0x80000 - OxB1FFF) ‘ ‘

Remember My Setiings

The changed setting will take immediate effect for the current debug
session. If you would like to persist your changes for subsequent
debug sessions, youll need to click on ‘Remember My Settings'
button. Click here to hide this message.





image2.png
File Edit View Project Tools Scripts Run Window Help
Cingg TRERS @i OiB ik

%5 Debug 52
4 ¥ NewTargetConfiguration.coml [Code Composer Studio - Device Debugging]
4 P Texas Instruments XDS2xx USB Debug Probe_0/C28xx CPUI (Suspended)
= 0x3FE494 (no symbols are defined for 0x3FE494)
& Texas Instruments XDS2xx USB Debug Probe_0/CPU1_CLA1 (Disconnected : Unknown)
& Texas Instruments XDS2xx USB Debug Probe_0/C280x CPU2 (Disconnected : Unknown)
& Texas Instruments XDS2xx USB Debug Probe_0/CPU2_CLA1 (Disconnected : Unknown)

PT—— Quckheeers | 28| 1 cos e (g oS omag)
5 Load Program i - ) R

Program file EA\Project\PDB00\F28374D\F2837xD\ISO\ 283740 ¢ + | Browse..|

Code offset
Data offset

<o
B Console 2 4@ B 2 D5 = 0 TN =a
i?:s"‘i‘ix'(‘,"‘e [epu_timers_cpu01] [type filter text Core Selection: [CPUL (Master) =
e Memory Map o
“Building target: cpu_tiners_cpuol.out’ L Filoe Clock/PLL Settings
JInvoling: 2000 Linker’ i Backup/Restore clock register settings during Flash operations
i 3000.6-3.11)bin/12000" 28 -l -nt --cla_support-clal --Float_support-fpus2 On-Chip Flash 7 egi ngs during Flash oper

~-tmu_support=tmu@ --vcu_support=vcu2 -g --define=CPUL --define=_FLASH

--diag_warning=225 --display_error_number -z -m"cpu_timers_cpuel
tack_size=0x100 --warn_sections -i"c:/ti/c2000_6.2.11/13b"
't1/c2000_6.2.11/ include’
Project/PD866/F2837xD/F2837xD/v156/F2837xD_common/cnd”
Project/PD8e8/F2837xD/F2837xD/V156/F2837xD_headers/cnd
~display_error_number --xml_link_info="cpu_timers_cpu@l_linkInfo.xr] 0
cpu_timers_cpubl.out” "./F2837xD_CodeStartBranch.obj" "./F2837xD_CpuTimers.obj
./F2837xD_DefaultIsR.obj" "./F2837xD_GlobalVariableDefs.obj" "./F2837xD_Gpio.obj"
./F2837xD_Tpc.obj" *./F2837xD_PieCtr /F2837xD_PieVect.obj"
/F2837x0_sysCtrl. . /F2837xD_usDelay.obj" "./cpu_timers_cpudl.obj’
rts2800_fpu32.1ib" -1"2837xD_FLASH_Lnk_cpul.cmd
F2837xD_Headers_nonBI0S_cpul.crd” -1"1ibc.a”
<Linking>
“Finished building target: cpu_timers_cpuel.out’

=== Build Finished ****

Full License.

Program/Memory Load Options
Auto Run and Launch Options
Misc/Other Options

2B Disassembly Style Options

OSCCLK (MHZ)INTOSC2) 10

System PLLCR Integer Multiplier (SPLUMULT) (15-50) 15

User PLLSYSCLK (MHz) (2-190) 1%

System PLLCR Fractional Multiplier (SPLLFMULT)

System Clock Divide Select (SYSDIVSEL)

Ll —— ’

The changed setting will take immediate effect for the current debug
session. If you would like to persist your changes for subsequent debug
sessions, you'll need to click on "Remember My Settings' button. Click here
to hide this message.
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Cing TRHDES O iR in B3RP iG G D Quick Access B | B ces edit (B cCs Debug )
%5 Debug 52 T = B @ Veriables 53 Gf Expressions I Registers B3] |t =1
4 ¥ NewTargetConfiguration.coxml [Code Composer Studio - Device Debugging] Name Type Value Location

4 P Texas Instruments XDS2xx USB Debug Probe_0/C28xx CPUI (Suspended - SW Breakpoint)
= 0x00C696 (no symbols are defined for 0x00C696)
4 Texas Instruments XDS2xx USB Debug Probe_0/CPU1_CLA1 (Disconnected : Unknown)
& Texas Instruments XDS2xx USB Debug Probe_0/C280x CPU2 (Disconnected : Unknown)
& Texas Instruments XDS2xx USB Debug Probe_0/CPU2_CLA1 (Disconnected : Unknown)

[l 0af6a 52 & Load Prograr Failed == ==
No sanrce available for *0s3ff16a" B

& Console 3 . EAProject\PDBO0\F2837xD\F2837xD\V150\F2837xD_examples_ Cpul\aa_cpu_ti =8
NewTargetConfiguration com mer\cPUOI\Ces\CPUIFLASH\cputimers cpu0Lout Load faed. P s .

C28xx_CPUL: Erasing Flash Bank @, Sector

Erasing Flash Bank @, Sector
Erasing Flash Bank @, Sector
Erasing Flash Bank @, Sector
Erasing Flash Bank @, Sector
Erasing Flash Bank @, Sector
Erasing Flash Bank @, Sector
Erasing Flash Bank @, Sector

Auto Run and Launch Options

zzrmunzamm

e T e s Misc/Other Options System PLLCR Integer Multiplier (SPLLIMULT) (15-50) 15
Erasing Flash Bank @, Sector . (C28xx Disassembly Style Options System PLLCR Fractional Multiplier (SPLLFMULT) 0 [0]
CCPUL: Data has been buffered at the end of the current data block for 64-bit
aligned writes. i X X System Clock Divide Select (SYSDIVSEL) ov1
280 CPUL: Error during Flash programming (Flash algorithm returned error code).
Operation cancelled. User PLLSYSCLK (MHz) (2-190) 190
C2Broc_CPUL: Error iriting Flash @ Address 0x00052000 of Length 0x00000016 (page @) >

280 CPUL: Writing buffered data @ Address @x00082014 of Length @x00000004

C28xx_CPUL: Error during Flash programming (Flash algorithm returned error code). 0 L t

Operation cancelled. = [Remember My Settings|
C28xx_CPUL: Please make sure the memory location you are programming have not already |- L
been programmed. The changed setting will take immediate effect for the current debug

C2B CPUL: GEL: Fils
£:\Project\PD8BB\F2837xD\F2837xD\V156\F2837xD_examples_Cpul\aa_cpu_timers\cpubl\ccs\CP
U1_FLASH\cpu_tiners_cpuel.out: Load failed. 4

session. If you would like to persist your changes for subsequent debug
sessions, you'll need to click on "Remember My Settings' button. Click here
to hide this message.
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