C28xx_CPU1: Trouble Reading Register PC: (Error -1137 @ 0x0) Device is held in reset. Take the device out of reset, and retry the operation. (Emulation package 9.5.0.00143) 
C28xx_CPU1: Trouble Writing Memory Block at 0x5f412 on Page 1 of Length 0x1: (Error -1156 @ 0x800) Device may be operating in low-power mode. Do you want to bring it out of this mode? Choose 'Yes' to force the device to wake up and retry the operation. Choose 'No' to retry the operation without waking the device. (Emulation package 9.5.0.00143) 
C28xx_CPU1: Trouble Writing Memory Block at 0x5f412 on Page 1 of Length 0x1: (Error -1137 @ 0x5F413) Device is held in reset. Take the device out of reset, and retry the operation. (Emulation package 9.5.0.00143) 
C28xx_CPU1: GEL: Error while executing OnTargetConnect(): Target failed to write 0x0005F412@Data
	 at *((int*) (0x0005F400+0x12))=0x0003 [f280025c.gel:185]
	 at OnTargetConnect()
C28xx_CPU1: Trouble Reading Register PC: (Error -1137 @ 0x0) Device is held in reset. Take the device out of reset, and retry the operation. (Emulation package 9.5.0.00143) 
C28xx_CPU1: Trouble Writing Memory Block at 0x5fb00 on Page 0 of Length 0x2: (Error -1137 @ 0x6) Device is held in reset. Take the device out of reset, and retry the operation. (Emulation package 9.5.0.00143) 
C28xx_CPU1: Error occurred during flash operation: Target failed to write 0x5FB00@Program
C28xx_CPU1: Trouble Writing Memory Block at 0x5f800 on Page 1 of Length 0x2: (Error -1137 @ 0x5F802) Device is held in reset. Take the device out of reset, and retry the operation. (Emulation package 9.5.0.00143) 
C28xx_CPU1: Error occurred during flash operation: Target failed to write 0x0005F800@Data
C28xx_CPU1: Trouble Writing Memory Block at 0x5fb00 on Page 0 of Length 0x2: (Error -1137 @ 0x6) Device is held in reset. Take the device out of reset, and retry the operation. (Emulation package 9.5.0.00143) 
C28xx_CPU1: Error occurred during flash operation: Target failed to write 0x5FB00@Program
C28xx_CPU1: Trouble Writing Memory Block at 0x5f800 on Page 1 of Length 0x2: (Error -1137 @ 0x5F802) Device is held in reset. Take the device out of reset, and retry the operation. (Emulation package 9.5.0.00143) 
C28xx_CPU1: Error occurred during flash operation: Target failed to write 0x0005F800@Data
C28xx_CPU1: Error initializing flash programming: Interface returned from dll, but flash is not available on this device.
C28xx_CPU1: Failed CPU Reset: (Error -1137 @ 0x0) Device is held in reset. Take the device out of reset, and retry the operation. (Emulation package 9.5.0.00143) 
C28xx_CPU1: Trouble Reading Register PC: (Error -1137 @ 0x0) Device is held in reset. Take the device out of reset, and retry the operation. (Emulation package 9.5.0.00143) 
C28xx_CPU1: Trouble Writing Memory Block at 0x5fb00 on Page 1 of Length 0x1: (Error -1137 @ 0x5FB01) Device is held in reset. Take the device out of reset, and retry the operation. (Emulation package 9.5.0.00143) 
C28xx_CPU1: GEL: Error while executing OnReset(-1): Target failed to write 0x0005FB00@Data
	 at *((int*) 0x5FB00)=0 [f280025c.gel:131]
	 at OnReset(-(1))
C28xx_CPU1: GEL: Error calling OnPreFileLoaded(): Reset failed: retcode=-1
C28xx_CPU1: Trouble Writing Memory Block at 0x80000 on Page 0 of Length 0x2: (Error -1137 @ 0x6) Device is held in reset. Take the device out of reset, and retry the operation. (Emulation package 9.5.0.00143) 
C28xx_CPU1: File Loader: Verification failed: Target failed to write 0x80000@Program
C28xx_CPU1: GEL: File: D:\PROJECTS_G21\adc_ex6_soc_continuous_dma\CPU1_FLASH\adc_ex6_soc_continuous_dma.out: Load failed.