******************************************************************************
             TMS320C2000 Linker PC v15.12.1                    
******************************************************************************
>> Linked Thu Jan 10 14:19:08 2019

OUTPUT FILE NAME:   <F28377S_RunTime_FlashUpdate_Example.out>
ENTRY POINT SYMBOL: "code_start"  address: 00080000

MEMORY CONFIGURATION

         name            origin    length      used     unused   attr    fill
----------------------  --------  ---------  --------  --------  ----  --------
PAGE 0:
  BOOT_RSVD             00000002   00000120  00000000  00000120  RWIX
  RAMM0                 00000122   000006de  00000200  000004de  RWIX
  RAMLS0_5_CODE         00008000   00010000  00007c9c  00008364  RWIX
  BEGIN                 00080000   00000002  00000002  00000000  RWIX
  FLASHA                00080002   0003fffe  000051f1  0003ae0d  RWIX
  RESET                 003fffc0   00000002  00000000  00000002  RWIX

PAGE 1:
  ADCA_RESULT           00000b00   00000020  00000018  00000008  RWIX
  ADCB_RESULT           00000b20   00000020  00000018  00000008  RWIX
  ADCC_RESULT           00000b40   00000020  00000018  00000008  RWIX
  ADCD_RESULT           00000b60   00000020  00000018  00000008  RWIX
  CPU_TIMER0            00000c00   00000008  00000008  00000000  RWIX
  CPU_TIMER1            00000c08   00000008  00000008  00000000  RWIX
  CPU_TIMER2            00000c10   00000008  00000008  00000000  RWIX
  PIE_CTRL              00000ce0   00000020  0000001a  00000006  RWIX
  PIE_VECT              00000d00   00000200  000001c0  00000040  RWIX
  DMA                   00001000   00000200  000000e0  00000120  RWIX
  CLA1                  00001400   00000040  0000003e  00000002  RWIX
  EPWM1                 00004000   00000100  00000100  00000000  RWIX
  EPWM2                 00004100   00000100  00000100  00000000  RWIX
  EPWM3                 00004200   00000100  00000100  00000000  RWIX
  EPWM4                 00004300   00000100  00000100  00000000  RWIX
  EPWM5                 00004400   00000100  00000100  00000000  RWIX
  EPWM6                 00004500   00000100  00000100  00000000  RWIX
  EPWM7                 00004600   00000100  00000100  00000000  RWIX
  EPWM8                 00004700   00000100  00000100  00000000  RWIX
  EPWM9                 00004800   00000100  00000100  00000000  RWIX
  EPWM10                00004900   00000100  00000100  00000000  RWIX
  EPWM11                00004a00   00000100  00000100  00000000  RWIX
  EPWM12                00004b00   00000100  00000100  00000000  RWIX
  ECAP1                 00005000   00000020  00000020  00000000  RWIX
  ECAP2                 00005020   00000020  00000020  00000000  RWIX
  ECAP3                 00005040   00000020  00000020  00000000  RWIX
  ECAP4                 00005060   00000020  00000020  00000000  RWIX
  ECAP5                 00005080   00000020  00000020  00000000  RWIX
  ECAP6                 000050a0   00000020  00000020  00000000  RWIX
  EQEP1                 00005100   00000040  00000022  0000001e  RWIX
  EQEP2                 00005140   00000040  00000022  0000001e  RWIX
  EQEP3                 00005180   00000040  00000022  0000001e  RWIX
  DACA                  00005c00   00000010  00000008  00000008  RWIX
  DACB                  00005c10   00000010  00000008  00000008  RWIX
  DACC                  00005c20   00000010  00000008  00000008  RWIX
  CMPSS1                00005c80   00000020  00000020  00000000  RWIX
  CMPSS2                00005ca0   00000020  00000020  00000000  RWIX
  CMPSS3                00005cc0   00000020  00000020  00000000  RWIX
  CMPSS4                00005ce0   00000020  00000020  00000000  RWIX
  CMPSS5                00005d00   00000020  00000020  00000000  RWIX
  CMPSS6                00005d20   00000020  00000020  00000000  RWIX
  CMPSS7                00005d40   00000020  00000020  00000000  RWIX
  CMPSS8                00005d60   00000020  00000020  00000000  RWIX
  SDFM1                 00005e00   00000080  00000080  00000000  RWIX
  SDFM2                 00005e80   00000080  00000080  00000000  RWIX
  MCBSPA                00006000   00000040  00000024  0000001c  RWIX
  MCBSPB                00006040   00000040  00000024  0000001c  RWIX
  SPIA                  00006100   00000010  00000010  00000000  RWIX
  SPIB                  00006110   00000010  00000010  00000000  RWIX
  SPIC                  00006120   00000010  00000010  00000000  RWIX
  SPID                  00006130   00000010  00000000  00000010  RWIX
  UPP                   00006200   00000100  00000048  000000b8  RWIX
  WD                    00007000   00000040  0000002b  00000015  RWIX
  NMIINTRUPT            00007060   00000010  00000007  00000009  RWIX
  XINT                  00007070   00000010  0000000b  00000005  RWIX
  SCIA                  00007200   00000010  00000010  00000000  RWIX
  SCIB                  00007210   00000010  00000010  00000000  RWIX
  SCIC                  00007220   00000010  00000010  00000000  RWIX
  SCID                  00007230   00000010  00000010  00000000  RWIX
  I2CA                  00007300   00000040  00000022  0000001e  RWIX
  I2CB                  00007340   00000040  00000022  0000001e  RWIX
  ADCA                  00007400   00000080  00000080  00000000  RWIX
  ADCB                  00007480   00000080  00000080  00000000  RWIX
  ADCC                  00007500   00000080  00000080  00000000  RWIX
  ADCD                  00007580   00000080  00000080  00000000  RWIX
  INPUT_XBAR            00007900   00000020  00000020  00000000  RWIX
  XBAR                  00007920   00000020  00000020  00000000  RWIX
  SYNC_SOC              00007940   00000010  00000006  0000000a  RWIX
  DMACLASRCSEL          00007980   00000040  0000001a  00000026  RWIX
  EPWM_XBAR             00007a00   00000040  00000040  00000000  RWIX
  CLB_XBAR              00007a40   00000040  00000000  00000040  RWIX
  OUTPUT_XBAR           00007a80   00000040  00000040  00000000  RWIX
  GPIOCTRL              00007c00   00000180  00000180  00000000  RWIX
  GPIODAT               00007f00   00000030  00000030  00000000  RWIX
  EMIF1                 00047000   00000800  00000070  00000790  RWIX
  EMIF2                 00047800   00000800  00000070  00000790  RWIX
  CANA                  00048000   00000800  00000000  00000800  RWIX
  CANB                  0004a000   00000800  00000000  00000800  RWIX
  FLASHPUMPSEMAPHORE    00050024   00000002  00000002  00000000  RWIX
  DEV_CFG               0005d000   00000180  0000012e  00000052  RWIX
  ANALOG_SUBSYS         0005d180   00000080  00000048  00000038  RWIX
  CLK_CFG               0005d200   00000100  00000032  000000ce  RWIX
  CPU_SYS               0005d300   00000100  00000082  0000007e  RWIX
  ROMPREFETCH           0005e608   00000002  00000002  00000000  RWIX
  DCSM_Z1               0005f000   00000030  00000024  0000000c  RWIX
  DCSM_Z2               0005f040   00000030  00000024  0000000c  RWIX
  DCSM_COMMON           0005f070   00000010  00000008  00000008  RWIX
  MEMCFG                0005f400   00000080  00000080  00000000  RWIX
  EMIF1CONFIG           0005f480   00000020  00000020  00000000  RWIX
  EMIF2CONFIG           0005f4a0   00000020  00000020  00000000  RWIX
  ACCESSPROTECTION      0005f4c0   00000040  00000040  00000000  RWIX
  MEMORYERROR           0005f500   00000040  00000040  00000000  RWIX
  ROMWAITSTATE          0005f540   00000002  00000002  00000000  RWIX
  FLASH0_CTRL           0005f800   00000300  00000182  0000017e  RWIX
  FLASH0_ECC            0005fb00   00000040  00000028  00000018  RWIX
  FLASH1_CTRL           0005fc00   00000300  00000182  0000017e  RWIX
  FLASH1_ECC            0005ff00   00000040  00000028  00000018  RWIX

SECTION ALLOCATION MAP

 output                                  attributes/
section   page    origin      length       input sections
--------  ----  ----------  ----------   ----------------
.stack     0    00000122    00000200     UNINITIALIZED
                  00000122    00000200     --HOLE--

.pinit     0    00008000    00000000     UNINITIALIZED

.ebss      0    0000ca1e    00002af0     UNINITIALIZED
                  0000ca1e    00000020     I2c_Eeprom.obj (.ebss)
                  0000ca3e    00000002     rts2800_fpu32.lib : _lock.obj (.ebss:__lock)
                  0000ca40    00001900     I2c_Eeprom_func.obj (.ebss)
                  0000e340    00000562     t.obj (.ebss)
                  0000e8a2    0000001c     protect_sw.obj (.ebss)
                  0000e8be    00000002     rts2800_fpu32.lib : _lock.obj (.ebss:__unlock)
                  0000e8c0    000004c0     SCIC_Uart.obj (.ebss)
                  0000ed80    00000358     SCIA_Uart.obj (.ebss)
                  0000f0d8    00000026     ti.obj (.ebss)
                  0000f0fe    00000001     F2837xS_EPwm.obj (.ebss)
                  0000f0ff    00000001     --HOLE--
                  0000f100    00000298     Global_Def.obj (.ebss)
                  0000f398    00000018     F2837xS_CpuTimers.obj (.ebss)
                  0000f3b0    0000000c     F021_API_F2837xS_FPU32.lib : Init.obj (.ebss)
                  0000f3bc    00000004     --HOLE--
                  0000f3c0    000000a4     adc.obj (.ebss)
                  0000f464    00000018     easy2837xS_sci_v8.5.obj (.ebss)
                  0000f47c    00000004     --HOLE--
                  0000f480    00000040     ntc_cal.obj (.ebss)
                  0000f4c0    00000035     RingBuff.obj (.ebss)
                  0000f4f5    00000009     init_test_func.obj (.ebss)
                  0000f4fe    00000002     --HOLE--
                  0000f500    00000007     protect_hw.obj (.ebss)
                  0000f507    00000001     --HOLE--
                  0000f508    00000006     rts2800_fpu32.lib : exit.obj (.ebss)

codestart 
*          0    00080000    00000002     
                  00080000    00000002     DSP28xxx_CodeStartBranch.obj (codestart)

.text      0    00080004    00004a1e     RUN ADDR = 00008000
                  00080004    00000d81     I2c_Eeprom_func.obj (.text)
                  00080d85    00000b14     I2c_Eeprom.obj (.text)
                  00081899    00000585     F2837xS_DefaultISR.obj (.text:retain)
                  00081e1e    000004b2     Global_Def.obj (.text)
                  000822d0    0000048d     F2837xS_SysCtrl.obj (.text)
                  0008275d    00000475     protect_sw.obj (.text)
                  00082bd2    000003c1     easy2837xS_sci_v8.5.obj (.text:retain)
                  00082f93    0000027b     adc.obj (.text)
                  0008320e    00000276     F021_API_F2837xS_FPU32.lib : FlashStateMachine.obj (.text:__Fapi_setupFlashStateMachine)
                  00083484    00000240     F2837xS_Gpio.obj (.text)
                  000836c4    000001c9     init_test_func.obj (.text)
                  0008388d    0000019e     F021_API_F2837xS_FPU32.lib : Program.obj (.text:_Fapi_issueProgrammingCommand)
                  00083a2b    0000016c     ntc_cal.obj (.text)
                  00083b97    0000016a     t.obj (.text)
                  00083d01    00000143     ti.obj (.text)
                  00083e44    0000013a     SCIA_Uart.obj (.text)
                  00083f7e    0000011f     protect_hw.obj (.text)
                  0008409d    000000dd     F2837xS_Adc.obj (.text)
                  0008417a    0000008d     ti.obj (.text:retain)
                  00084207    0000008a     F2837xS_EPwm.obj (.text)
                  00084291    00000088     rts2800_fpu32.lib : fs_div.obj (.text)
                  00084319    00000085     RingBuff.obj (.text)
                  0008439e    00000082     F021_API_F2837xS_FPU32.lib : Read.obj (.text:__Fapi_loopRegionForValue)
                  00084420    0000007c     F2837xS_CpuTimers.obj (.text)
                  0008449c    0000005f     F021_API_F2837xS_FPU32.lib : Init.obj (.text:_Fapi_initializeAPI)
                  000844fb    00000056     rts2800_fpu32.lib : boot.obj (.text)
                  00084551    00000055     F021_API_F2837xS_FPU32.lib : FlashStateMachine.obj (.text:_Fapi_setupEepromSectorEnable)
                  000845a6    00000050     easy2837xS_sci_v8.5.obj (.text)
                  000845f6    00000046     rts2800_fpu32.lib : cpy_tbl.obj (.text)
                  0008463c    0000003d     F021_API_F2837xS_FPU32.lib : BlankCheck.obj (.text:_Fapi_doBlankCheck)
                  00084679    00000039                                : Read.obj (.text:__Fapi_loopRegionForValueBy16bits)
                  000846b2    00000038     adc.obj (.text:retain)
                  000846ea    00000036     F021_API_F2837xS_FPU32.lib : FlashStateMachine.obj (.text:_Fapi_isAddressEcc)
                  00084720    00000032                                : Read.obj (.text:__Fapi_checkRegionForValueBy16bits)
                  00084752    0000002f                                : FlashStateMachine.obj (.text:__Fapi_issueFsmCommand)
                  00084781    0000002c                                : Utilities.obj (.text:_Fapi_calculateFletcherChecksum)
                  000847ad    0000002a                                : Utilities.obj (.text:__Fapi_divideUnsignedLong)
                  000847d7    0000002a     rts2800_fpu32.lib : l_div.obj (.text)
                  00084801    00000029     F021_API_F2837xS_FPU32.lib : FlashStateMachine.obj (.text:__Fapi_setupSectorsForWrite)
                  0008482a    00000029     rts2800_fpu32.lib : exit.obj (.text)
                  00084853    00000028     F2837xS_PieCtrl.obj (.text)
                  0008487b    00000026     F2837xS_PieVect.obj (.text)
                  000848a1    00000026     F021_API_F2837xS_FPU32.lib : Read.obj (.text:_Fapi_flushPipeline)
                  000848c7    00000026                                : FlashStateMachine.obj (.text:_Fapi_setActiveFlashBank)
                  000848ed    00000025                                : FlashStateMachine.obj (.text:_Fapi_setupBankSectorEnable)
                  00084912    00000024                                : Async.obj (.text:_Fapi_issueAsyncCommandWithAddress)
                  00084936    0000001e     rts2800_fpu32.lib : ll_cmp.obj (.text)
                  00084954    0000001e                       : memcpy.obj (.text)
                  00084972    0000001a     F021_API_F2837xS_FPU32.lib : Utilities.obj (.text:_Fapi_waitDelay)
                  0008498c    0000001a     rts2800_fpu32.lib : cpy_utils.obj (.text)
                  000849a6    00000019                       : args_main.obj (.text)
                  000849bf    00000018                       : ll_aox.obj (.text)
                  000849d7    00000011     F021_API_F2837xS_FPU32.lib : Verify.obj (.text:_Fapi_doVerifyBy16bits)
                  000849e8    0000000f                                : Utilities.obj (.text:__Fapi_scaleCycleValues)
                  000849f7    0000000b                                : FlashStateMachine.obj (.text:_Fapi_checkFsmForReady)
                  00084a02    0000000b                                : Utilities.obj (.text:__Fapi_calculateOtpChecksum)
                  00084a0d    00000009     rts2800_fpu32.lib : _lock.obj (.text)
                  00084a16    00000007     F021_API_F2837xS_FPU32.lib : FlashStateMachine.obj (.text:_Fapi_getFsmStatus)
                  00084a1d    00000002                                : Fapi_UserDefinedFunctions.obj (.text:_Fapi_serviceWatchdogTimer)
                  00084a1f    00000002     rts2800_fpu32.lib : pre_init.obj (.text)
                  00084a21    00000001                       : startup.obj (.text)

.cinit     0    00084a24    00000441     RUN ADDR = 0000f510
                  00084a24    000000d7     SCIC_Uart.obj (.cinit)
                  00084afb    000000a2     adc.obj (.cinit)
                  00084b9d    00000087     ntc_cal.obj (.cinit)
                  00084c24    00000077     ti.obj (.cinit)
                  00084c9b    00000056     I2c_Eeprom.obj (.cinit)
                  00084cf1    0000004e     easy2837xS_sci_v8.5.obj (.cinit)
                  00084d3f    00000048     protect_sw.obj (.cinit)
                  00084d87    0000003c     I2c_Eeprom_func.obj (.cinit)
                  00084dc3    00000024     init_test_func.obj (.cinit)
                  00084de7    0000001c     protect_hw.obj (.cinit)
                  00084e03    00000018     t.obj (.cinit)
                  00084e1b    00000014     SCIA_Uart.obj (.cinit)
                  00084e2f    0000000e     rts2800_fpu32.lib : exit.obj (.cinit)
                  00084e3d    0000000c     Global_Def.obj (.cinit)
                  00084e49    0000000c     RingBuff.obj (.cinit)
                  00084e55    00000005     rts2800_fpu32.lib : _lock.obj (.cinit:__lock)
                  00084e5a    00000005                       : _lock.obj (.cinit:__unlock)
                  00084e5f    00000004     F2837xS_EPwm.obj (.cinit)
                  00084e63    00000002     --HOLE-- [fill = 0]

.econst    0    00084e68    00000230     RUN ADDR = 0000f954
                  00084e68    000001c0     F2837xS_PieVect.obj (.econst:_PieVectTableInit)
                  00085028    00000070     Global_Def.obj (.econst:_FlashBankInfo)

.TI.ramfunc 
*          0    00085098    000000fd     RUN ADDR = 0000fb84
                  00085098    0000008b     SCIA_Uart.obj (.TI.ramfunc:retain)
                  00085123    0000006e     F2837xS_SysCtrl.obj (.TI.ramfunc)
                  00085191    00000004     F2837xS_usDelay.obj (.TI.ramfunc)

.switch    0    00085198    00000020     RUN ADDR = 0000fc84
                  00085198    00000020     I2c_Eeprom_func.obj (.switch:_Read_Event_Array_Data)

copysections 
*          0    000851b8    0000003d     
                  000851b8    0000003d     DSP28xxx_SectionCopy_nonBIOS.obj (copysections)

wddisable 
*          0    000851f8    00000008     
                  000851f8    00000008     DSP28xxx_CodeStartBranch.obj (wddisable)

.reset     0    003fffc0    00000002     DSECT
                  003fffc0    00000002     rts2800_fpu32.lib : boot.obj (.reset)

AdcaResultFile 
*          1    00000b00    00000018     UNINITIALIZED
                  00000b00    00000018     F2837xS_GlobalVariableDefs.obj (AdcaResultFile)

AdcbResultFile 
*          1    00000b20    00000018     UNINITIALIZED
                  00000b20    00000018     F2837xS_GlobalVariableDefs.obj (AdcbResultFile)

AdccResultFile 
*          1    00000b40    00000018     UNINITIALIZED
                  00000b40    00000018     F2837xS_GlobalVariableDefs.obj (AdccResultFile)

AdcdResultFile 
*          1    00000b60    00000018     UNINITIALIZED
                  00000b60    00000018     F2837xS_GlobalVariableDefs.obj (AdcdResultFile)

CpuTimer0RegsFile 
*          1    00000c00    00000008     UNINITIALIZED
                  00000c00    00000008     F2837xS_GlobalVariableDefs.obj (CpuTimer0RegsFile)

CpuTimer1RegsFile 
*          1    00000c08    00000008     UNINITIALIZED
                  00000c08    00000008     F2837xS_GlobalVariableDefs.obj (CpuTimer1RegsFile)

CpuTimer2RegsFile 
*          1    00000c10    00000008     UNINITIALIZED
                  00000c10    00000008     F2837xS_GlobalVariableDefs.obj (CpuTimer2RegsFile)

PieCtrlRegsFile 
*          1    00000ce0    0000001a     UNINITIALIZED
                  00000ce0    0000001a     F2837xS_GlobalVariableDefs.obj (PieCtrlRegsFile)

PieVectTableFile 
*          1    00000d00    000001c0     UNINITIALIZED
                  00000d00    000001c0     F2837xS_GlobalVariableDefs.obj (PieVectTableFile)

EmuBModeVar 
*          1    00000d00    00000001     UNINITIALIZED
                  00000d00    00000001     F2837xS_GlobalVariableDefs.obj (EmuBModeVar)

EmuBootPinsVar 
*          1    00000d01    00000001     UNINITIALIZED
                  00000d01    00000001     F2837xS_GlobalVariableDefs.obj (EmuBootPinsVar)

DmaRegsFile 
*          1    00001000    000000e0     UNINITIALIZED
                  00001000    000000e0     F2837xS_GlobalVariableDefs.obj (DmaRegsFile)

Cla1RegsFile 
*          1    00001400    0000003e     UNINITIALIZED
                  00001400    0000003e     F2837xS_GlobalVariableDefs.obj (Cla1RegsFile)

EPwm1RegsFile 
*          1    00004000    00000100     UNINITIALIZED
                  00004000    00000100     F2837xS_GlobalVariableDefs.obj (EPwm1RegsFile)

EPwm2RegsFile 
*          1    00004100    00000100     UNINITIALIZED
                  00004100    00000100     F2837xS_GlobalVariableDefs.obj (EPwm2RegsFile)

EPwm3RegsFile 
*          1    00004200    00000100     UNINITIALIZED
                  00004200    00000100     F2837xS_GlobalVariableDefs.obj (EPwm3RegsFile)

EPwm4RegsFile 
*          1    00004300    00000100     UNINITIALIZED
                  00004300    00000100     F2837xS_GlobalVariableDefs.obj (EPwm4RegsFile)

EPwm5RegsFile 
*          1    00004400    00000100     UNINITIALIZED
                  00004400    00000100     F2837xS_GlobalVariableDefs.obj (EPwm5RegsFile)

EPwm6RegsFile 
*          1    00004500    00000100     UNINITIALIZED
                  00004500    00000100     F2837xS_GlobalVariableDefs.obj (EPwm6RegsFile)

EPwm7RegsFile 
*          1    00004600    00000100     UNINITIALIZED
                  00004600    00000100     F2837xS_GlobalVariableDefs.obj (EPwm7RegsFile)

EPwm8RegsFile 
*          1    00004700    00000100     UNINITIALIZED
                  00004700    00000100     F2837xS_GlobalVariableDefs.obj (EPwm8RegsFile)

EPwm9RegsFile 
*          1    00004800    00000100     UNINITIALIZED
                  00004800    00000100     F2837xS_GlobalVariableDefs.obj (EPwm9RegsFile)

EPwm10RegsFile 
*          1    00004900    00000100     UNINITIALIZED
                  00004900    00000100     F2837xS_GlobalVariableDefs.obj (EPwm10RegsFile)

EPwm11RegsFile 
*          1    00004a00    00000100     UNINITIALIZED
                  00004a00    00000100     F2837xS_GlobalVariableDefs.obj (EPwm11RegsFile)

EPwm12RegsFile 
*          1    00004b00    00000100     UNINITIALIZED
                  00004b00    00000100     F2837xS_GlobalVariableDefs.obj (EPwm12RegsFile)

ECap1RegsFile 
*          1    00005000    00000020     UNINITIALIZED
                  00005000    00000020     F2837xS_GlobalVariableDefs.obj (ECap1RegsFile)

ECap2RegsFile 
*          1    00005020    00000020     UNINITIALIZED
                  00005020    00000020     F2837xS_GlobalVariableDefs.obj (ECap2RegsFile)

ECap3RegsFile 
*          1    00005040    00000020     UNINITIALIZED
                  00005040    00000020     F2837xS_GlobalVariableDefs.obj (ECap3RegsFile)

ECap4RegsFile 
*          1    00005060    00000020     UNINITIALIZED
                  00005060    00000020     F2837xS_GlobalVariableDefs.obj (ECap4RegsFile)

ECap5RegsFile 
*          1    00005080    00000020     UNINITIALIZED
                  00005080    00000020     F2837xS_GlobalVariableDefs.obj (ECap5RegsFile)

ECap6RegsFile 
*          1    000050a0    00000020     UNINITIALIZED
                  000050a0    00000020     F2837xS_GlobalVariableDefs.obj (ECap6RegsFile)

EQep1RegsFile 
*          1    00005100    00000022     UNINITIALIZED
                  00005100    00000022     F2837xS_GlobalVariableDefs.obj (EQep1RegsFile)

EQep2RegsFile 
*          1    00005140    00000022     UNINITIALIZED
                  00005140    00000022     F2837xS_GlobalVariableDefs.obj (EQep2RegsFile)

EQep3RegsFile 
*          1    00005180    00000022     UNINITIALIZED
                  00005180    00000022     F2837xS_GlobalVariableDefs.obj (EQep3RegsFile)

DacaRegsFile 
*          1    00005c00    00000008     UNINITIALIZED
                  00005c00    00000008     F2837xS_GlobalVariableDefs.obj (DacaRegsFile)

DacbRegsFile 
*          1    00005c10    00000008     UNINITIALIZED
                  00005c10    00000008     F2837xS_GlobalVariableDefs.obj (DacbRegsFile)

DaccRegsFile 
*          1    00005c20    00000008     UNINITIALIZED
                  00005c20    00000008     F2837xS_GlobalVariableDefs.obj (DaccRegsFile)

Cmpss1RegsFile 
*          1    00005c80    00000020     UNINITIALIZED
                  00005c80    00000020     F2837xS_GlobalVariableDefs.obj (Cmpss1RegsFile)

Cmpss2RegsFile 
*          1    00005ca0    00000020     UNINITIALIZED
                  00005ca0    00000020     F2837xS_GlobalVariableDefs.obj (Cmpss2RegsFile)

Cmpss3RegsFile 
*          1    00005cc0    00000020     UNINITIALIZED
                  00005cc0    00000020     F2837xS_GlobalVariableDefs.obj (Cmpss3RegsFile)

Cmpss4RegsFile 
*          1    00005ce0    00000020     UNINITIALIZED
                  00005ce0    00000020     F2837xS_GlobalVariableDefs.obj (Cmpss4RegsFile)

Cmpss5RegsFile 
*          1    00005d00    00000020     UNINITIALIZED
                  00005d00    00000020     F2837xS_GlobalVariableDefs.obj (Cmpss5RegsFile)

Cmpss6RegsFile 
*          1    00005d20    00000020     UNINITIALIZED
                  00005d20    00000020     F2837xS_GlobalVariableDefs.obj (Cmpss6RegsFile)

Cmpss7RegsFile 
*          1    00005d40    00000020     UNINITIALIZED
                  00005d40    00000020     F2837xS_GlobalVariableDefs.obj (Cmpss7RegsFile)

Cmpss8RegsFile 
*          1    00005d60    00000020     UNINITIALIZED
                  00005d60    00000020     F2837xS_GlobalVariableDefs.obj (Cmpss8RegsFile)

AdcaRegsFile 
*          1    00007400    00000080     UNINITIALIZED
                  00007400    00000080     F2837xS_GlobalVariableDefs.obj (AdcaRegsFile)

AdcbRegsFile 
*          1    00007480    00000080     UNINITIALIZED
                  00007480    00000080     F2837xS_GlobalVariableDefs.obj (AdcbRegsFile)

AdccRegsFile 
*          1    00007500    00000080     UNINITIALIZED
                  00007500    00000080     F2837xS_GlobalVariableDefs.obj (AdccRegsFile)

AdcdRegsFile 
*          1    00007580    00000080     UNINITIALIZED
                  00007580    00000080     F2837xS_GlobalVariableDefs.obj (AdcdRegsFile)

AnalogSubsysRegsFile 
*          1    0005d180    00000048     UNINITIALIZED
                  0005d180    00000048     F2837xS_GlobalVariableDefs.obj (AnalogSubsysRegsFile)

Cla1SoftIntRegsFile 
*          1    00000ce0    00000004     DSECT
                  00000ce0    00000004     F2837xS_GlobalVariableDefs.obj (Cla1SoftIntRegsFile)

Sdfm1RegsFile 
*          1    00005e00    00000080     UNINITIALIZED
                  00005e00    00000080     F2837xS_GlobalVariableDefs.obj (Sdfm1RegsFile)

Sdfm2RegsFile 
*          1    00005e80    00000080     UNINITIALIZED
                  00005e80    00000080     F2837xS_GlobalVariableDefs.obj (Sdfm2RegsFile)

McbspaRegsFile 
*          1    00006000    00000024     UNINITIALIZED
                  00006000    00000024     F2837xS_GlobalVariableDefs.obj (McbspaRegsFile)

McbspbRegsFile 
*          1    00006040    00000024     UNINITIALIZED
                  00006040    00000024     F2837xS_GlobalVariableDefs.obj (McbspbRegsFile)

SpiaRegsFile 
*          1    00006100    00000010     UNINITIALIZED
                  00006100    00000010     F2837xS_GlobalVariableDefs.obj (SpiaRegsFile)

SpibRegsFile 
*          1    00006110    00000010     UNINITIALIZED
                  00006110    00000010     F2837xS_GlobalVariableDefs.obj (SpibRegsFile)

SpicRegsFile 
*          1    00006120    00000010     UNINITIALIZED
                  00006120    00000010     F2837xS_GlobalVariableDefs.obj (SpicRegsFile)

UppRegsFile 
*          1    00006200    00000048     UNINITIALIZED
                  00006200    00000048     F2837xS_GlobalVariableDefs.obj (UppRegsFile)

WdRegsFile 
*          1    00007000    0000002b     UNINITIALIZED
                  00007000    0000002b     F2837xS_GlobalVariableDefs.obj (WdRegsFile)

NmiIntruptRegsFile 
*          1    00007060    00000007     UNINITIALIZED
                  00007060    00000007     F2837xS_GlobalVariableDefs.obj (NmiIntruptRegsFile)

XintRegsFile 
*          1    00007070    0000000b     UNINITIALIZED
                  00007070    0000000b     F2837xS_GlobalVariableDefs.obj (XintRegsFile)

SciaRegsFile 
*          1    00007200    00000010     UNINITIALIZED
                  00007200    00000010     F2837xS_GlobalVariableDefs.obj (SciaRegsFile)

ScibRegsFile 
*          1    00007210    00000010     UNINITIALIZED
                  00007210    00000010     F2837xS_GlobalVariableDefs.obj (ScibRegsFile)

ScicRegsFile 
*          1    00007220    00000010     UNINITIALIZED
                  00007220    00000010     F2837xS_GlobalVariableDefs.obj (ScicRegsFile)

ScidRegsFile 
*          1    00007230    00000010     UNINITIALIZED
                  00007230    00000010     F2837xS_GlobalVariableDefs.obj (ScidRegsFile)

I2caRegsFile 
*          1    00007300    00000022     UNINITIALIZED
                  00007300    00000022     F2837xS_GlobalVariableDefs.obj (I2caRegsFile)

I2cbRegsFile 
*          1    00007340    00000022     UNINITIALIZED
                  00007340    00000022     F2837xS_GlobalVariableDefs.obj (I2cbRegsFile)

InputXbarRegsFile 
*          1    00007900    00000020     UNINITIALIZED
                  00007900    00000020     F2837xS_GlobalVariableDefs.obj (InputXbarRegsFile)

XbarRegsFile 
*          1    00007920    00000020     UNINITIALIZED
                  00007920    00000020     F2837xS_GlobalVariableDefs.obj (XbarRegsFile)

SyncSocRegsFile 
*          1    00007940    00000006     UNINITIALIZED
                  00007940    00000006     F2837xS_GlobalVariableDefs.obj (SyncSocRegsFile)

DmaClaSrcSelRegsFile 
*          1    00007980    0000001a     UNINITIALIZED
                  00007980    0000001a     F2837xS_GlobalVariableDefs.obj (DmaClaSrcSelRegsFile)

EPwmXbarRegsFile 
*          1    00007a00    00000040     UNINITIALIZED
                  00007a00    00000040     F2837xS_GlobalVariableDefs.obj (EPwmXbarRegsFile)

OutputXbarRegsFile 
*          1    00007a80    00000040     UNINITIALIZED
                  00007a80    00000040     F2837xS_GlobalVariableDefs.obj (OutputXbarRegsFile)

GpioCtrlRegsFile 
*          1    00007c00    00000180     UNINITIALIZED
                  00007c00    00000180     F2837xS_GlobalVariableDefs.obj (GpioCtrlRegsFile)

GpioDataRegsFile 
*          1    00007f00    00000030     UNINITIALIZED
                  00007f00    00000030     F2837xS_GlobalVariableDefs.obj (GpioDataRegsFile)

Emif1RegsFile 
*          1    00047000    00000070     UNINITIALIZED
                  00047000    00000070     F2837xS_GlobalVariableDefs.obj (Emif1RegsFile)

Emif2RegsFile 
*          1    00047800    00000070     UNINITIALIZED
                  00047800    00000070     F2837xS_GlobalVariableDefs.obj (Emif2RegsFile)

FlashPumpSemaphoreRegsFile 
*          1    00050024    00000002     UNINITIALIZED
                  00050024    00000002     F2837xS_GlobalVariableDefs.obj (FlashPumpSemaphoreRegsFile)

DevCfgRegsFile 
*          1    0005d000    0000012e     UNINITIALIZED
                  0005d000    0000012e     F2837xS_GlobalVariableDefs.obj (DevCfgRegsFile)

ClkCfgRegsFile 
*          1    0005d200    00000032     UNINITIALIZED
                  0005d200    00000032     F2837xS_GlobalVariableDefs.obj (ClkCfgRegsFile)

CpuSysRegsFile 
*          1    0005d300    00000082     UNINITIALIZED
                  0005d300    00000082     F2837xS_GlobalVariableDefs.obj (CpuSysRegsFile)

RomPrefetchRegsFile 
*          1    0005e608    00000002     UNINITIALIZED
                  0005e608    00000002     F2837xS_GlobalVariableDefs.obj (RomPrefetchRegsFile)

DcsmZ1RegsFile 
*          1    0005f000    00000024     UNINITIALIZED
                  0005f000    00000024     F2837xS_GlobalVariableDefs.obj (DcsmZ1RegsFile)

DcsmZ2RegsFile 
*          1    0005f040    00000024     UNINITIALIZED
                  0005f040    00000024     F2837xS_GlobalVariableDefs.obj (DcsmZ2RegsFile)

DcsmCommonRegsFile 
*          1    0005f070    00000008     UNINITIALIZED
                  0005f070    00000008     F2837xS_GlobalVariableDefs.obj (DcsmCommonRegsFile)

MemCfgRegsFile 
*          1    0005f400    00000080     UNINITIALIZED
                  0005f400    00000080     F2837xS_GlobalVariableDefs.obj (MemCfgRegsFile)

Emif1ConfigRegsFile 
*          1    0005f480    00000020     UNINITIALIZED
                  0005f480    00000020     F2837xS_GlobalVariableDefs.obj (Emif1ConfigRegsFile)

Emif2ConfigRegsFile 
*          1    0005f4a0    00000020     UNINITIALIZED
                  0005f4a0    00000020     F2837xS_GlobalVariableDefs.obj (Emif2ConfigRegsFile)

AccessProtectionRegsFile 
*          1    0005f4c0    00000040     UNINITIALIZED
                  0005f4c0    00000040     F2837xS_GlobalVariableDefs.obj (AccessProtectionRegsFile)

MemoryErrorRegsFile 
*          1    0005f500    00000040     UNINITIALIZED
                  0005f500    00000040     F2837xS_GlobalVariableDefs.obj (MemoryErrorRegsFile)

RomWaitStateRegsFile 
*          1    0005f540    00000002     UNINITIALIZED
                  0005f540    00000002     F2837xS_GlobalVariableDefs.obj (RomWaitStateRegsFile)

Flash0CtrlRegsFile 
*          1    0005f800    00000182     UNINITIALIZED
                  0005f800    00000182     F2837xS_GlobalVariableDefs.obj (Flash0CtrlRegsFile)

Flash0EccRegsFile 
*          1    0005fb00    00000028     UNINITIALIZED
                  0005fb00    00000028     F2837xS_GlobalVariableDefs.obj (Flash0EccRegsFile)

Flash1CtrlRegsFile 
*          1    0005fc00    00000182     UNINITIALIZED
                  0005fc00    00000182     F2837xS_GlobalVariableDefs.obj (Flash1CtrlRegsFile)

Flash1EccRegsFile 
*          1    0005ff00    00000028     UNINITIALIZED
                  0005ff00    00000028     F2837xS_GlobalVariableDefs.obj (Flash1EccRegsFile)

MODULE SUMMARY

       Module                             code    ro data   rw data
       ------                             ----    -------   -------
    .\
       I2c_Eeprom_func.obj                6914    0         6584   
       F2837xS_GlobalVariableDefs.obj     0       0         8373   
       I2c_Eeprom.obj                     5672    0         204    
       Global_Def.obj                     2404    0         912    
       F2837xS_DefaultISR.obj             2826    0         0      
       F2837xS_SysCtrl.obj                2550    0         0      
       protect_sw.obj                     2282    0         172    
       easy2837xS_sci_v8.5.obj            2082    0         180    
       t.obj                              724     0         1426   
       adc.obj                            1382    0         488    
       SCIA_Uart.obj                      906     0         896    
       SCIC_Uart.obj                      0       0         1646   
       ti.obj                             928     0         276    
       F2837xS_Gpio.obj                   1152    0         0      
       ntc_cal.obj                        728     0         334    
       init_test_func.obj                 914     0         81     
       F2837xS_PieVect.obj                76      0         896    
       protect_hw.obj                     574     0         63     
       F2837xS_Adc.obj                    442     0         0      
       RingBuff.obj                       266     0         77     
       F2837xS_EPwm.obj                   276     0         9      
       F2837xS_CpuTimers.obj              248     0         24     
       F2837xS_PieCtrl.obj                80      0         0      
       DSP28xxx_SectionCopy_nonBIOS.obj   61      0         0      
       DSP28xxx_CodeStartBranch.obj       10      0         0      
       F2837xS_usDelay.obj                8       0         0      
    +--+----------------------------------+-------+---------+---------+
       Total:                             33505   0         22641  
                                                                   
    C:/ti/ccsv8/tools/compiler/ti-cgt-c2000_15.12.1.LTS/lib/rts2800_fpu32.lib
       fs_div.obj                         272     0         0      
       boot.obj                           172     0         0      
       cpy_tbl.obj                        140     0         0      
       exit.obj                           82      0         34     
       l_div.obj                          84      0         0      
       ll_cmp.obj                         60      0         0      
       memcpy.obj                         60      0         0      
       cpy_utils.obj                      52      0         0      
       args_main.obj                      50      0         0      
       ll_aox.obj                         48      0         0      
       _lock.obj                          18      0         24     
       pre_init.obj                       4       0         0      
       startup.obj                        2       0         0      
    +--+----------------------------------+-------+---------+---------+
       Total:                             1044    0         58     
                                                                   
    D:/TI_Workspace_V8/DSP28377S/libraries/flash_api/f2837xs/lib/F021_API_F2837xS_FPU32.lib
       FlashStateMachine.obj              1900    0         0      
       Program.obj                        828     0         0      
       Read.obj                           550     0         0      
       Utilities.obj                      276     0         0      
       Init.obj                           190     0         12     
       BlankCheck.obj                     122     0         0      
       Async.obj                          72      0         0      
       Verify.obj                         34      0         0      
       Fapi_UserDefinedFunctions.obj      4       0         0      
    +--+----------------------------------+-------+---------+---------+
       Total:                             3976    0         12     
                                                                   
       Stack:                             0       0         512    
    +--+----------------------------------+-------+---------+---------+
       Grand Total:                       38525   0         23223  

GLOBAL DATA SYMBOLS: SORTED BY DATA PAGE

address     data page           name
--------    ----------------    ----
00000122       4 (00000100)     __stack

00000b00      2c (00000b00)     _AdcaResultRegs
00000b20      2c (00000b00)     _AdcbResultRegs

00000b40      2d (00000b40)     _AdccResultRegs
00000b60      2d (00000b40)     _AdcdResultRegs

00000c00      30 (00000c00)     _CpuTimer0Regs
00000c08      30 (00000c00)     _CpuTimer1Regs
00000c10      30 (00000c00)     _CpuTimer2Regs

00000ce0      33 (00000cc0)     _Cla1SoftIntRegs
00000ce0      33 (00000cc0)     _PieCtrlRegs

00000d00      34 (00000d00)     _EmuBMode
00000d00      34 (00000d00)     _PieVectTable
00000d01      34 (00000d00)     _EmuBootPins

00001000      40 (00001000)     _DmaRegs

00001400      50 (00001400)     _Cla1Regs

00004000     100 (00004000)     _EPwm1Regs

00004100     104 (00004100)     _EPwm2Regs

00004200     108 (00004200)     _EPwm3Regs

00004300     10c (00004300)     _EPwm4Regs

00004400     110 (00004400)     _EPwm5Regs

00004500     114 (00004500)     _EPwm6Regs

00004600     118 (00004600)     _EPwm7Regs

00004700     11c (00004700)     _EPwm8Regs

00004800     120 (00004800)     _EPwm9Regs

00004900     124 (00004900)     _EPwm10Regs

00004a00     128 (00004a00)     _EPwm11Regs

00004b00     12c (00004b00)     _EPwm12Regs

00005000     140 (00005000)     _ECap1Regs
00005020     140 (00005000)     _ECap2Regs

00005040     141 (00005040)     _ECap3Regs
00005060     141 (00005040)     _ECap4Regs

00005080     142 (00005080)     _ECap5Regs
000050a0     142 (00005080)     _ECap6Regs

00005100     144 (00005100)     _EQep1Regs

00005140     145 (00005140)     _EQep2Regs

00005180     146 (00005180)     _EQep3Regs

00005c00     170 (00005c00)     _DacaRegs
00005c10     170 (00005c00)     _DacbRegs
00005c20     170 (00005c00)     _DaccRegs

00005c80     172 (00005c80)     _Cmpss1Regs
00005ca0     172 (00005c80)     _Cmpss2Regs

00005cc0     173 (00005cc0)     _Cmpss3Regs
00005ce0     173 (00005cc0)     _Cmpss4Regs

00005d00     174 (00005d00)     _Cmpss5Regs
00005d20     174 (00005d00)     _Cmpss6Regs

00005d40     175 (00005d40)     _Cmpss7Regs
00005d60     175 (00005d40)     _Cmpss8Regs

00005e00     178 (00005e00)     _Sdfm1Regs

00005e80     17a (00005e80)     _Sdfm2Regs

00006000     180 (00006000)     _McbspaRegs

00006040     181 (00006040)     _McbspbRegs

00006100     184 (00006100)     _SpiaRegs
00006110     184 (00006100)     _SpibRegs
00006120     184 (00006100)     _SpicRegs

00006200     188 (00006200)     _UppRegs

00007000     1c0 (00007000)     _WdRegs

00007060     1c1 (00007040)     _NmiIntruptRegs
00007070     1c1 (00007040)     _XintRegs

00007200     1c8 (00007200)     _SciaRegs
00007210     1c8 (00007200)     _ScibRegs
00007220     1c8 (00007200)     _ScicRegs
00007230     1c8 (00007200)     _ScidRegs

00007300     1cc (00007300)     _I2caRegs

00007340     1cd (00007340)     _I2cbRegs

00007400     1d0 (00007400)     _AdcaRegs

00007480     1d2 (00007480)     _AdcbRegs

00007500     1d4 (00007500)     _AdccRegs

00007580     1d6 (00007580)     _AdcdRegs

00007900     1e4 (00007900)     _InputXbarRegs
00007920     1e4 (00007900)     _XbarRegs

00007940     1e5 (00007940)     _SyncSocRegs

00007980     1e6 (00007980)     _DmaClaSrcSelRegs

00007a00     1e8 (00007a00)     _EPwmXbarRegs

00007a80     1ea (00007a80)     _OutputXbarRegs

00007c00     1f0 (00007c00)     _GpioCtrlRegs

00007f00     1fc (00007f00)     _GpioDataRegs

0000ca1e     328 (0000ca00)     _use_ECO
0000ca1f     328 (0000ca00)     _i2c_step
0000ca20     328 (0000ca00)     _use_ECO_new
0000ca21     328 (0000ca00)     _i2c_check_ok
0000ca22     328 (0000ca00)     _wr_gain_check_sum_new
0000ca24     328 (0000ca00)     _rd_ad_check_sum
0000ca26     328 (0000ca00)     _wr_sys_check_sum_new
0000ca28     328 (0000ca00)     _wr_gain_check_sum
0000ca2a     328 (0000ca00)     _wr_sys_chk_sum
0000ca2c     328 (0000ca00)     _wr_gain_chk_sum
0000ca2e     328 (0000ca00)     _wr_ad_chk_sum
0000ca30     328 (0000ca00)     _rd_sys_check_sum
0000ca32     328 (0000ca00)     _rd_gain_check_sum
0000ca34     328 (0000ca00)     _wr_sys_check_sum
0000ca36     328 (0000ca00)     _tmp_rd_check_sum
0000ca38     328 (0000ca00)     _tmp_wr_check_sum
0000ca3a     328 (0000ca00)     _wr_ad_check_sum_new
0000ca3c     328 (0000ca00)     _wr_ad_check_sum
0000ca3e     328 (0000ca00)     __lock

0000ca40     329 (0000ca40)     _rw_event_array_cnt
0000ca41     329 (0000ca40)     _tmp_short
0000ca42     329 (0000ca40)     _system_fault_mode
0000ca43     329 (0000ca40)     _tmp_short_max
0000ca44     329 (0000ca40)     _store_array_event_p
0000ca45     329 (0000ca40)     _i2c_pri_pt
0000ca46     329 (0000ca40)     _i2c_array_SEQ
0000ca47     329 (0000ca40)     _i2c_sec_pt
0000ca48     329 (0000ca40)     _wr_pos
0000ca49     329 (0000ca40)     _array_pos
0000ca4a     329 (0000ca40)     _rw_EventCode_max
0000ca4b     329 (0000ca40)     _event_old
0000ca4c     329 (0000ca40)     _overlade_array_check
0000ca4d     329 (0000ca40)     _i2c_array_test
0000ca4e     329 (0000ca40)     _store_array_event
0000ca50     329 (0000ca40)     _sys_event

0000ca80     32a (0000ca80)     _sys_data_rd12

0000cb00     32c (0000cb00)     _sys_data_rd11

0000cb80     32e (0000cb80)     _sys_data_rd14

0000cc00     330 (0000cc00)     _sys_data_rd13

0000cc80     332 (0000cc80)     _sys_data_wr2

0000cd00     334 (0000cd00)     _sys_data_rd2

0000cd80     336 (0000cd80)     _sys_data_wr3

0000ce00     338 (0000ce00)     _sys_data_rd3

0000ce80     33a (0000ce80)     _sys_data_rd4

0000cf00     33c (0000cf00)     _sys_data_rd0

0000cf80     33e (0000cf80)     _sys_data_rd1

0000d000     340 (0000d000)     _sys_data_wr0

0000d080     342 (0000d080)     _sys_data_wr1

0000d100     344 (0000d100)     _sys_data_rd8

0000d180     346 (0000d180)     _sys_data_rd7

0000d200     348 (0000d200)     _sys_data_rd10

0000d280     34a (0000d280)     _sys_data_rd9

0000d300     34c (0000d300)     _sys_data_rd15

0000d380     34e (0000d380)     _sys_data_rd6

0000d400     350 (0000d400)     _sys_data_rd5

0000d480     352 (0000d480)     _Event_buff

0000d5c0     357 (0000d5c0)     _Event

0000d880     362 (0000d880)     _Event_new

0000db40     36d (0000db40)     _sys_data_wr

0000e340     38d (0000e340)     _Code_Date
0000e341     38d (0000e340)     _i2c_chk_end
0000e342     38d (0000e340)     _Code_Year
0000e343     38d (0000e340)     _Code_Month
0000e344     38d (0000e340)     _Firmware
0000e345     38d (0000e340)     _i2c_enable
0000e346     38d (0000e340)     _rtc_tm
0000e351     38d (0000e340)     _oht_dt

0000e380     38e (0000e380)     _sys_time

0000e3c0     38f (0000e3c0)     _sys_ref

0000e400     390 (0000e400)     _pi

0000e480     392 (0000e480)     _i2c

0000e500     394 (0000e500)     _adc

0000e640     399 (0000e640)     _protect

0000e8a2     3a2 (0000e880)     _Servo_Warn_Vol
0000e8a3     3a2 (0000e880)     _Ecap_NTC_PT_ref
0000e8a4     3a2 (0000e880)     _Ecap_NTC_OT_ref
0000e8a6     3a2 (0000e880)     _Edc_Eout_gap
0000e8a8     3a2 (0000e880)     _Eout_Fuse_Gap_Voltage
0000e8aa     3a2 (0000e880)     _out_Power
0000e8ac     3a2 (0000e880)     _Power_OV_check_value
0000e8ae     3a2 (0000e880)     _Ecap_Fuse_Gap_Voltage
0000e8b0     3a2 (0000e880)     _Edc_Ecap_gap
0000e8b2     3a2 (0000e880)     _out_power_value
0000e8b4     3a2 (0000e880)     _out_power_set_value
0000e8b6     3a2 (0000e880)     _OV_check_value
0000e8b8     3a2 (0000e880)     _Iout_OC_check_value
0000e8ba     3a2 (0000e880)     _UV_check_value
0000e8bc     3a2 (0000e880)     _Iac_OC_check_value
0000e8be     3a2 (0000e880)     __unlock

0000e8c0     3a3 (0000e8c0)     _scic_rxd_chk_sum
0000e8c1     3a3 (0000e8c0)     _scic_rxd_checksum
0000e8c2     3a3 (0000e8c0)     _init_scic_port
0000e8c3     3a3 (0000e8c0)     _scic_txd_chk_sum
0000e8c4     3a3 (0000e8c0)     _scic_rxd
0000e8c5     3a3 (0000e8c0)     _comm_hour1
0000e8c6     3a3 (0000e8c0)     _comm_min1
0000e8c7     3a3 (0000e8c0)     _comm_mon1
0000e8c8     3a3 (0000e8c0)     _comm_day1
0000e8c9     3a3 (0000e8c0)     _rtc_tm_check
0000e8ca     3a3 (0000e8c0)     _txd_end
0000e8cb     3a3 (0000e8c0)     _scic_Flag
0000e8cc     3a3 (0000e8c0)     _scic_Flag_cnt
0000e8cd     3a3 (0000e8c0)     _scic_rxd_SEQ
0000e8ce     3a3 (0000e8c0)     _scic_txd
0000e8cf     3a3 (0000e8c0)     _comm_year1
0000e8d0     3a3 (0000e8c0)     _rxd_end
0000e8d1     3a3 (0000e8c0)     _rxd_pos
0000e8d2     3a3 (0000e8c0)     _txd_pos
0000e8d3     3a3 (0000e8c0)     _error_array_send_cnt
0000e8d4     3a3 (0000e8c0)     _error_array_send_cnt2
0000e8d5     3a3 (0000e8c0)     _err_num
0000e8d6     3a3 (0000e8c0)     _event_array_send_cnt
0000e8d7     3a3 (0000e8c0)     _rtc_tm_check_cnt
0000e8d8     3a3 (0000e8c0)     _EV_Send_SEQ_cnt
0000e8d9     3a3 (0000e8c0)     _scic_txd_delay_cnt_ref
0000e8da     3a3 (0000e8c0)     _EV_Send_SEQ
0000e8db     3a3 (0000e8c0)     _scic_txd_errorlog_send
0000e8dc     3a3 (0000e8c0)     _comm_day
0000e8dd     3a3 (0000e8c0)     _comm_hour
0000e8de     3a3 (0000e8c0)     _comm_year
0000e8df     3a3 (0000e8c0)     _comm_mon
0000e8e0     3a3 (0000e8c0)     _comm_sec1
0000e8e1     3a3 (0000e8c0)     _RS232_Warning
0000e8e2     3a3 (0000e8c0)     _send_errorlog_pt
0000e8e3     3a3 (0000e8c0)     _comm_sec
0000e8e4     3a3 (0000e8c0)     _scic_txd_enable
0000e8e5     3a3 (0000e8c0)     _OHT_Position
0000e8e6     3a3 (0000e8c0)     _OHT_state
0000e8e7     3a3 (0000e8c0)     _hex_dec_ena
0000e8e8     3a3 (0000e8c0)     _comm_min
0000e8ea     3a3 (0000e8c0)     _tmp_data_Iout
0000e8ec     3a3 (0000e8c0)     _init_scic_cnt
0000e8ee     3a3 (0000e8c0)     _init_scic_cnt_ref
0000e8f0     3a3 (0000e8c0)     _scic_txd_delay_cnt

0000e900     3a4 (0000e900)     _sys_event2

0000e940     3a5 (0000e940)     _tmp_data

0000e980     3a6 (0000e980)     _txd_buf

0000eb80     3ae (0000eb80)     _rxd_buf

0000ed80     3b6 (0000ed80)     _uart_rx_cnt
0000ed81     3b6 (0000ed80)     _uart_rx_start_flag
0000ed82     3b6 (0000ed80)     _uart_rx_frame_flag
0000ed83     3b6 (0000ed80)     _uart_tx_pos
0000ed84     3b6 (0000ed80)     _uart_tx_cnt

0000edc0     3b7 (0000edc0)     _uart_rx_buf

0000ee80     3ba (0000ee80)     _uart_tx_buf

0000f0d8     3c3 (0000f0c0)     _Iac_sag_level
0000f0d9     3c3 (0000f0c0)     _UV_Check
0000f0da     3c3 (0000f0c0)     _sag_gen
0000f0db     3c3 (0000f0c0)     _t1_prd_val
0000f0dc     3c3 (0000f0c0)     _GATE_TEST
0000f0dd     3c3 (0000f0c0)     _Iac_recover_level
0000f0de     3c3 (0000f0c0)     _test_array_store
0000f0df     3c3 (0000f0c0)     _uv_test
0000f0e0     3c3 (0000f0c0)     _Edc_sw_gap
0000f0e1     3c3 (0000f0c0)     _RLY_SEQ
0000f0e2     3c3 (0000f0c0)     _Edc_sw_ref_max
0000f0e3     3c3 (0000f0c0)     _sw_onoff_time
0000f0e4     3c3 (0000f0c0)     _RLY_TEST
0000f0e5     3c3 (0000f0c0)     _gate_sw_cnt
0000f0e6     3c3 (0000f0c0)     _cpu_timer0_msec
0000f0e7     3c3 (0000f0c0)     _sys_mode
0000f0e8     3c3 (0000f0c0)     _uv_enable_cnt
0000f0ea     3c3 (0000f0c0)     _uv_enable_time
0000f0ec     3c3 (0000f0c0)     _Processing_Time_max
0000f0ee     3c3 (0000f0c0)     _Processing_Time_min
0000f0f0     3c3 (0000f0c0)     _Vchop_gap
0000f0f2     3c3 (0000f0c0)     _Processing_Time
0000f0f4     3c3 (0000f0c0)     _Vchop_ref
0000f0f6     3c3 (0000f0c0)     _Iac_outage_cnt
0000f0f8     3c3 (0000f0c0)     _Iac_sag_cnt
0000f0fa     3c3 (0000f0c0)     _Iac_rever_cnt
0000f0fc     3c3 (0000f0c0)     _uv_check_cnt
0000f0fe     3c3 (0000f0c0)     _t1_prd

0000f101     3c4 (0000f100)     _RunTime_FlashUpdate_flag
0000f103     3c4 (0000f100)     _CSM_Password_Data
0000f10b     3c4 (0000f100)     _FD_Buffer

0000f398     3ce (0000f380)     _CpuTimer1
0000f3a0     3ce (0000f380)     _CpuTimer2
0000f3a8     3ce (0000f380)     _CpuTimer0
0000f3b0     3ce (0000f380)     _Fapi_GlobalInit

0000f3c0     3cf (0000f3c0)     _ad_read_mux_cnt
0000f3c1     3cf (0000f3c0)     _ad_read_chk_cnt
0000f3c2     3cf (0000f3c0)     _ad_read_mux
0000f3c3     3cf (0000f3c0)     _ad_read_mux_seq
0000f3c4     3cf (0000f3c0)     _ad_read_mux_time
0000f3c6     3cf (0000f3c0)     _ad_result
0000f3d8     3cf (0000f3c0)     _ad_offset
0000f3ea     3cf (0000f3c0)     _ad_offset_new

0000f400     3d0 (0000f400)     _ad_scale_new

0000f440     3d1 (0000f440)     _ad_scale
0000f464     3d1 (0000f440)     _ezDSP_uWrongISRCount
0000f465     3d1 (0000f440)     _ezDSP_ucRx
0000f466     3d1 (0000f440)     _ezDSP_uPECount
0000f467     3d1 (0000f440)     _ezDSP_uBRKDTCount
0000f468     3d1 (0000f440)     _ezDSP_uOECount
0000f469     3d1 (0000f440)     _ezDSP_uAddrRdCnt
0000f46a     3d1 (0000f440)     _ezDSP_uDataRdCnt
0000f46b     3d1 (0000f440)     _ezDSP_uChksum
0000f46c     3d1 (0000f440)     _ezDSP_uState
0000f46d     3d1 (0000f440)     _ezDSP_uData
0000f46e     3d1 (0000f440)     _ezDSP_uFECount
0000f46f     3d1 (0000f440)     _ezDSP_Version_SCI
0000f470     3d1 (0000f440)     _ezDSP_uRead8BPossible
0000f471     3d1 (0000f440)     _ezDSP_uRead16BPossible
0000f472     3d1 (0000f440)     _ezDSP_ulData
0000f474     3d1 (0000f440)     _ezDSP_ulAddr
0000f476     3d1 (0000f440)     _ezDSP_fFloat
0000f478     3d1 (0000f440)     _ezDSP_ullData

0000f480     3d2 (0000f480)     _Temp_Low
0000f481     3d2 (0000f480)     _Temp_High
0000f482     3d2 (0000f480)     _temp_cnt2
0000f483     3d2 (0000f480)     _temp_cnt
0000f484     3d2 (0000f480)     _NTC_Seq
0000f486     3d2 (0000f480)     _CHOP_Temp
0000f488     3d2 (0000f480)     _Ecap2_Temp
0000f48a     3d2 (0000f480)     _RES_Cap_Temp
0000f48c     3d2 (0000f480)     _Ecap1_Temp
0000f48e     3d2 (0000f480)     _Filter_Cap_Temp
0000f490     3d2 (0000f480)     _TB_Temp
0000f492     3d2 (0000f480)     _Filter_L_Temp
0000f494     3d2 (0000f480)     _CHOP_R2_Temp
0000f496     3d2 (0000f480)     _CHOP_R1_Temp
0000f498     3d2 (0000f480)     _temp_value2
0000f49a     3d2 (0000f480)     _Temp_ad_fil
0000f49c     3d2 (0000f480)     _temp_value
0000f49e     3d2 (0000f480)     _NTC_Temp2
0000f4a0     3d2 (0000f480)     _PickUp_Temp
0000f4a2     3d2 (0000f480)     _Ecap_AMB_Temp
0000f4a4     3d2 (0000f480)     _Temp_ad_fil2
0000f4a6     3d2 (0000f480)     _IGBT_Temp
0000f4a8     3d2 (0000f480)     _NTC_Temp
0000f4aa     3d2 (0000f480)     _NTC_Temp_Buff

0000f4c0     3d3 (0000f4c0)     _ezDSP_nEndPos
0000f4c1     3d3 (0000f4c0)     _ezDSP_nMaxBuffSize
0000f4c2     3d3 (0000f4c0)     _ezDSP_nStartPos
0000f4c3     3d3 (0000f4c0)     _ezDSP_ringBuffer
0000f4f5     3d3 (0000f4c0)     _LED_SEQ
0000f4f6     3d3 (0000f4c0)     _led_cnt
0000f4f7     3d3 (0000f4c0)     _led_time
0000f4f8     3d3 (0000f4c0)     _dis_LED
0000f4f9     3d3 (0000f4c0)     _dis_LED_SEQ
0000f4fa     3d3 (0000f4c0)     _LED_TEST
0000f4fb     3d3 (0000f4c0)     _led_val
0000f4fc     3d3 (0000f4c0)     _i2c_rtc_read_cnt
0000f4fd     3d3 (0000f4c0)     _power_on_chk

0000f500     3d4 (0000f500)     _out_Protect_Relay_ON
0000f501     3d4 (0000f500)     _out_SMPS_reset
0000f502     3d4 (0000f500)     _out_SAG_GEN_ON
0000f503     3d4 (0000f500)     _out_SYS_Fault_ON
0000f504     3d4 (0000f500)     _HW_Output_SIG_Check
0000f505     3d4 (0000f500)     _out_nGate_Reset_ON
0000f506     3d4 (0000f500)     _out_do_spare_ON
0000f508     3d4 (0000f500)     ___TI_enable_exit_profile_output
0000f50a     3d4 (0000f500)     ___TI_cleanup_ptr
0000f50c     3d4 (0000f500)     ___TI_dtors_ptr

0000f954     3e5 (0000f940)     _PieVectTableInit

0000fb14     3ec (0000fb00)     _FlashBankInfo

00047000    11c0 (00047000)     _Emif1Regs

00047800    11e0 (00047800)     _Emif2Regs

00050024    1400 (00050000)     _FlashPumpSemaphoreRegs

0005d000    1740 (0005d000)     _DevCfgRegs

0005d180    1746 (0005d180)     _AnalogSubsysRegs

0005d200    1748 (0005d200)     _ClkCfgRegs

0005d300    174c (0005d300)     _CpuSysRegs

0005e608    1798 (0005e600)     _RomPrefetchRegs

0005f000    17c0 (0005f000)     _DcsmZ1Regs

0005f040    17c1 (0005f040)     _DcsmZ2Regs
0005f070    17c1 (0005f040)     _DcsmCommonRegs

0005f400    17d0 (0005f400)     _MemCfgRegs

0005f480    17d2 (0005f480)     _Emif1ConfigRegs
0005f4a0    17d2 (0005f480)     _Emif2ConfigRegs

0005f4c0    17d3 (0005f4c0)     _AccessProtectionRegs

0005f500    17d4 (0005f500)     _MemoryErrorRegs

0005f540    17d5 (0005f540)     _RomWaitStateRegs

0005f800    17e0 (0005f800)     _Flash0CtrlRegs

0005fb00    17ec (0005fb00)     _Flash0EccRegs

0005fc00    17f0 (0005fc00)     _Flash1CtrlRegs

0005ff00    17fc (0005ff00)     _Flash1EccRegs

GLOBAL SYMBOLS: SORTED ALPHABETICALLY BY Name 

page  address   name                                     
----  -------   ----                                     
0     00008000  .text                                    
0     0000c826  C$$EXIT                                  
0     0000c28d  FS$$DIV                                  
0     0000c7d3  L$$DIV                                   
0     0000c7e2  L$$MOD                                   
0     0000c9bb  LL$$AND                                  
0     0000c932  LL$$CMP                                  
0     0000c9c3  LL$$OR                                   
0     0000c9cb  LL$$XOR                                  
0     0000c7f0  UL$$DIV                                  
0     0000c7f7  UL$$MOD                                  
0     0000c944  ULL$$CMP                                 
0     00009953  _ADCA1_ISR                               
0     00009bd3  _ADCA2_ISR                               
0     00009bdd  _ADCA3_ISR                               
0     00009be7  _ADCA4_ISR                               
0     00009bc9  _ADCA_EVT_ISR                            
0     0000995d  _ADCB1_ISR                               
0     00009bfb  _ADCB2_ISR                               
0     00009c05  _ADCB3_ISR                               
0     00009c0f  _ADCB4_ISR                               
0     00009bf1  _ADCB_EVT_ISR                            
0     00009967  _ADCC1_ISR                               
0     00009d63  _ADCC2_ISR                               
0     00009d6d  _ADCC3_ISR                               
0     00009d77  _ADCC4_ISR                               
0     00009d59  _ADCC_EVT_ISR                            
0     00009985  _ADCD1_ISR                               
0     00009d8b  _ADCD2_ISR                               
0     00009d95  _ADCD3_ISR                               
0     00009d9f  _ADCD4_ISR                               
0     00009d81  _ADCD_EVT_ISR                            
0     00009ddb  _AUX_PLL_SLIP_ISR                        
1     0005f4c0  _AccessProtectionRegs                    
0     0000c099  _AdcSetMode                              
1     00007400  _AdcaRegs                                
1     00000b00  _AdcaResultRegs                          
1     00007480  _AdcbRegs                                
1     00000b20  _AdcbResultRegs                          
1     00007500  _AdccRegs                                
1     00000b40  _AdccResultRegs                          
1     00007580  _AdcdRegs                                
1     00000b60  _AdcdResultRegs                          
0     0000c32c  _AddRing                                 
1     0005d180  _AnalogSubsysRegs                        
0     0000a716  _AuxAuxClkSel                            
0     0000a700  _AuxIntOsc2Sel                           
0     0000a70a  _AuxXtalOscSel                           
0     00009ba1  _CANA0_ISR                               
0     00009bab  _CANA1_ISR                               
0     00009bb5  _CANB0_ISR                               
0     00009bbf  _CANB1_ISR                               
0     0000f496  _CHOP_R1_Temp                            
0     0000f494  _CHOP_R2_Temp                            
0     0000f486  _CHOP_Temp                               
0     00009c19  _CLA1_1_ISR                              
0     00009c23  _CLA1_2_ISR                              
0     00009c2d  _CLA1_3_ISR                              
0     00009c37  _CLA1_4_ISR                              
0     00009c41  _CLA1_5_ISR                              
0     00009c4b  _CLA1_6_ISR                              
0     00009c55  _CLA1_7_ISR                              
0     00009c5f  _CLA1_8_ISR                              
0     00009de5  _CLA_OVERFLOW_ISR                        
0     00009def  _CLA_UNDERFLOW_ISR                       
0     0000f103  _CSM_Password_Data                       
0     0000c13c  _CalAdcINL                               
0     000085d9  _Check_Event                             
0     00009610  _Check_I2C_Data                          
1     00001400  _Cla1Regs                                
0     00000ce0  _Cla1SoftIntRegs                         
1     0005d200  _ClkCfgRegs                              
1     00005c80  _Cmpss1Regs                              
1     00005ca0  _Cmpss2Regs                              
1     00005cc0  _Cmpss3Regs                              
1     00005ce0  _Cmpss4Regs                              
1     00005d00  _Cmpss5Regs                              
1     00005d20  _Cmpss6Regs                              
1     00005d40  _Cmpss7Regs                              
1     00005d60  _Cmpss8Regs                              
0     0000e340  _Code_Date                               
0     0000e343  _Code_Month                              
0     0000e342  _Code_Year                               
0     0000c45d  _ConfigCpuTimer                          
1     0005d300  _CpuSysRegs                              
0     0000f3a8  _CpuTimer0                               
1     00000c00  _CpuTimer0Regs                           
0     0000f398  _CpuTimer1                               
1     00000c08  _CpuTimer1Regs                           
0     0000f3a0  _CpuTimer2                               
1     00000c10  _CpuTimer2Regs                           
0     0000a6bb  _CsmUnlock                               
0     000098a9  _DATALOG_ISR                             
0     00009aed  _DMA_CH1_ISR                             
0     00009af7  _DMA_CH2_ISR                             
0     00009b01  _DMA_CH3_ISR                             
0     00009b0b  _DMA_CH4_ISR                             
0     00009b15  _DMA_CH5_ISR                             
0     00009b1f  _DMA_CH6_ISR                             
1     00005c00  _DacaRegs                                
1     00005c10  _DacbRegs                                
1     00005c20  _DaccRegs                                
1     0005f070  _DcsmCommonRegs                          
1     0005f000  _DcsmZ1Regs                              
1     0005f040  _DcsmZ2Regs                              
1     0005d000  _DevCfgRegs                              
0     0000a3cf  _DisableDog                              
0     0000a381  _DisablePeripheralClocks                 
1     00007980  _DmaClaSrcSelRegs                        
1     00001000  _DmaRegs                                 
0     0000a157  _Do_DSP28377S_FlashBank_Change           
0     0000a1d7  _Do_DSP28377S_Runtime_Flash_Update_Check 
0     0000a283  _Do_DSP28377S_Runtime_Flash_Update_Finish
0     0000a224  _Do_Flash_CSM_Unlock                     
0     00009f56  _Do_Flash_Erase                          
0     0000a0b1  _Do_Flash_Verify                         
0     00009fd2  _Do_Flash_Write                          
0     0000a2c3  _Do_Regulator_Error_Data_Request         
0     0000a2ba  _Do_Regulator_Normal_Info_Reqeust        
0     00009a43  _ECAP1_ISR                               
0     00009a4d  _ECAP2_ISR                               
0     00009a57  _ECAP3_ISR                               
0     00009a61  _ECAP4_ISR                               
0     00009a6b  _ECAP5_ISR                               
0     00009a75  _ECAP6_ISR                               
1     00005000  _ECap1Regs                               
1     00005020  _ECap2Regs                               
1     00005040  _ECap3Regs                               
1     00005060  _ECap4Regs                               
1     00005080  _ECap5Regs                               
1     000050a0  _ECap6Regs                               
0     00009da9  _EMIF_ERROR_ISR                          
0     00009e03  _EMPTY_ISR                               
0     000098bd  _EMU_ISR                                 
0     00009cff  _EPWM10_ISR                              
0     00009cd7  _EPWM10_TZ_ISR                           
0     00009d09  _EPWM11_ISR                              
0     00009ce1  _EPWM11_TZ_ISR                           
0     00009d13  _EPWM12_ISR                              
0     00009ceb  _EPWM12_TZ_ISR                           
0     000099f3  _EPWM1_ISR                               
0     000099a3  _EPWM1_TZ_ISR                            
0     0000c27a  _EPWM2_GATE_BLOCK                        
0     0000c26c  _EPWM2_GATE_OPEN                         
0     000099fd  _EPWM2_ISR                               
0     000099ad  _EPWM2_TZ_ISR                            
0     00009a07  _EPWM3_ISR                               
0     000099b7  _EPWM3_TZ_ISR                            
0     00009a11  _EPWM4_ISR                               
0     000099c1  _EPWM4_TZ_ISR                            
0     00009a1b  _EPWM5_ISR                               
0     000099cb  _EPWM5_TZ_ISR                            
0     00009a25  _EPWM6_ISR                               
0     000099d5  _EPWM6_TZ_ISR                            
0     00009a2f  _EPWM7_ISR                               
0     000099df  _EPWM7_TZ_ISR                            
0     00009a39  _EPWM8_ISR                               
0     000099e9  _EPWM8_TZ_ISR                            
0     00009cf5  _EPWM9_ISR                               
0     00009ccd  _EPWM9_TZ_ISR                            
0     0000c285  _EPWM_GATE_ALL_BLOCK                     
0     0000c277  _EPWM_GATE_ALL_OPEN                      
0     0000c288  _EPWM_GATE_Set_All_Zero                  
1     00004900  _EPwm10Regs                              
1     00004a00  _EPwm11Regs                              
1     00004b00  _EPwm12Regs                              
1     00004000  _EPwm1Regs                               
1     00004100  _EPwm2Regs                               
1     00004200  _EPwm3Regs                               
1     00004300  _EPwm4Regs                               
1     00004400  _EPwm5Regs                               
1     00004500  _EPwm6Regs                               
1     00004600  _EPwm7Regs                               
1     00004700  _EPwm8Regs                               
1     00004800  _EPwm9Regs                               
1     00007a00  _EPwmXbarRegs                            
0     00009a7f  _EQEP1_ISR                               
0     00009a89  _EQEP2_ISR                               
0     00009a93  _EQEP3_ISR                               
1     00005100  _EQep1Regs                               
1     00005140  _EQep2Regs                               
1     00005180  _EQep3Regs                               
0     0000e8da  _EV_Send_SEQ                             
0     0000e8d8  _EV_Send_SEQ_cnt                         
0     0000f48c  _Ecap1_Temp                              
0     0000f488  _Ecap2_Temp                              
0     0000f4a2  _Ecap_AMB_Temp                           
0     0000e8ae  _Ecap_Fuse_Gap_Voltage                   
0     0000e8a4  _Ecap_NTC_OT_ref                         
0     0000e8a3  _Ecap_NTC_PT_ref                         
0     0000e8b0  _Edc_Ecap_gap                            
0     0000e8a6  _Edc_Eout_gap                            
0     0000f0e0  _Edc_sw_gap                              
0     0000f0e2  _Edc_sw_ref_max                          
1     0005f480  _Emif1ConfigRegs                         
1     00047000  _Emif1Regs                               
1     0005f4a0  _Emif2ConfigRegs                         
1     00047800  _Emif2Regs                               
1     00000d00  _EmuBMode                                
1     00000d01  _EmuBootPins                             
0     0000a3dd  _EnableDog                               
0     0000c86e  _EnableInterrupts                        
0     0000e8a8  _Eout_Fuse_Gap_Voltage                   
0     0000d5c0  _Event                                   
0     0000d480  _Event_buff                              
0     0000d880  _Event_new                               
0     0000c358  _ExtractRing                             
0     0000fc7d  _F28x_usDelay                            
0     0000f10b  _FD_Buffer                               
0     00009dbd  _FLASH_CORRECTABLE_ERROR_ISR             
0     00009c91  _FPU_OVERFLOW_ISR                        
0     00009c9b  _FPU_UNDERFLOW_ISR                       
0     0000f3b0  _Fapi_GlobalInit                         
0     0000c77d  _Fapi_calculateFletcherChecksum          
0     0000c9f3  _Fapi_checkFsmForReady                   
0     0000c638  _Fapi_doBlankCheck                       
0     0000c9d3  _Fapi_doVerifyBy16bits                   
0     0000c89d  _Fapi_flushPipeline                      
0     0000ca12  _Fapi_getFsmStatus                       
0     0000c498  _Fapi_initializeAPI                      
0     0000c6e6  _Fapi_isAddressEcc                       
0     0000c90e  _Fapi_issueAsyncCommandWithAddress       
0     0000b889  _Fapi_issueProgrammingCommand            
0     0000ca19  _Fapi_serviceWatchdogTimer               
0     0000c8c3  _Fapi_setActiveFlashBank                 
0     0000c8e9  _Fapi_setupBankSectorEnable              
0     0000c54d  _Fapi_setupEepromSectorEnable            
0     0000c96e  _Fapi_waitDelay                          
0     0000f48e  _Filter_Cap_Temp                         
0     0000f492  _Filter_L_Temp                           
0     0000e344  _Firmware                                
1     0005f800  _Flash0CtrlRegs                          
1     0005fb00  _Flash0EccRegs                           
1     0005fc00  _Flash1CtrlRegs                          
1     0005ff00  _Flash1EccRegs                           
0     0000fb14  _FlashBankInfo                           
0     0000fc61  _FlashOff_Bank0                          
0     0000fc6f  _FlashOff_Bank1                          
1     00050024  _FlashPumpSemaphoreRegs                  
0     0000bcfd  _GATE_FAULT_RESET                        
0     0000bd33  _GATE_LOGIC_TEST                         
0     0000f0dc  _GATE_TEST                               
0     0000b675  _GPIO_EnableUnbondedIOPullups            
0     0000b650  _GPIO_EnableUnbondedIOPullupsFor100Pin   
0     0000b637  _GPIO_EnableUnbondedIOPullupsFor176Pin   
0     0000b68b  _GPIO_ReadPin                            
0     0000b5dc  _GPIO_SetupLock                          
0     0000b4c0  _GPIO_SetupPinMux                        
0     0000b548  _GPIO_SetupPinOptions                    
0     0000b605  _GPIO_SetupXINT1Gpio                     
0     0000b60f  _GPIO_SetupXINT2Gpio                     
0     0000b619  _GPIO_SetupXINT3Gpio                     
0     0000b623  _GPIO_SetupXINT4Gpio                     
0     0000b62d  _GPIO_SetupXINT5Gpio                     
0     0000b6a2  _GPIO_WritePin                           
0     0000c386  _GetSizeRing                             
0     00009e43  _Get_Uart_Frame_CheckSum                 
1     00007c00  _GpioCtrlRegs                            
1     00007f00  _GpioDataRegs                            
0     0000a734  _HALT                                    
0     0000a745  _HIB                                     
0     0000f504  _HW_Output_SIG_Check                     
0     0000bff7  _HardWare_Input_Signal_Check             
0     0000bf7a  _HardWare_Output_Signal_Check            
0     0000bd01  _Hardware_Check                          
0     00009b33  _I2CA_FIFO_ISR                           
0     00009b29  _I2CA_ISR                                
0     00009b47  _I2CB_FIFO_ISR                           
0     00009b3d  _I2CB_ISR                                
0     0000805f  _I2C_ADRY_check                          
0     0000803a  _I2C_BB_check                            
0     000097d2  _I2C_Read_Write                          
0     0000804c  _I2C_SCD_check                           
0     00008028  _I2C_STP_check                           
1     00007300  _I2caRegs                                
1     00007340  _I2cbRegs                                
0     0000a720  _IDLE                                    
0     0000f4a6  _IGBT_Temp                               
0     000098d1  _ILLEGAL_ISR                             
0     00009ca5  _IPC0_ISR                                
0     00009caf  _IPC1_ISR                                
0     00009cb9  _IPC2_ISR                                
0     00009cc3  _IPC3_ISR                                
0     0000e8bc  _Iac_OC_check_value                      
0     0000f0f6  _Iac_outage_cnt                          
0     0000f0dd  _Iac_recover_level                       
0     0000f0fa  _Iac_rever_cnt                           
0     0000f0f8  _Iac_sag_cnt                             
0     0000f0d8  _Iac_sag_level                           
0     0000b0a6  _InitAdc                                 
0     0000a5d4  _InitAuxPll                              
0     0000c41c  _InitCpuTimers                           
0     0000c203  _InitEPwm                                
0     0000c25a  _InitEPwm2Gpio                           
0     0000c257  _InitEPwmGpio                            
0     0000fc0f  _InitFlash_Bank0                         
0     0000fc38  _InitFlash_Bank1                         
0     0000b480  _InitGpio                                
0     00008000  _InitI2C                                 
0     0000a2fd  _InitPeripheralClocks                    
0     0000c84f  _InitPieCtrl                             
0     0000c877  _InitPieVectTable                        
0     0000a2cc  _InitSysCtrl                             
0     0000a3e5  _InitSysPll                              
0     0000bf37  _Init_SCIA                               
1     00007900  _InputXbarRegs                           
0     0000e8b8  _Iout_OC_check_value                     
0     0000c392  _IsRingEmpty                             
0     0000f4f5  _LED_SEQ                                 
0     0000b6db  _LED_SET                                 
0     0000f4fa  _LED_TEST                                
0     0000b6f1  _LED_control                             
0     00009ac5  _MCBSPA_RX_ISR                           
0     00009acf  _MCBSPA_TX_ISR                           
0     00009ad9  _MCBSPB_RX_ISR                           
0     00009ae3  _MCBSPB_TX_ISR                           
1     00006000  _McbspaRegs                              
1     00006040  _McbspbRegs                              
1     0005f400  _MemCfgRegs                              
1     0005f500  _MemoryErrorRegs                         
0     000098c7  _NMI_ISR                                 
0     00009e10  _NOTUSED_ISR                             
0     0000ba27  _NTC_Cal                                 
0     0000f484  _NTC_Seq                                 
0     0000f4a8  _NTC_Temp                                
0     0000f49e  _NTC_Temp2                               
0     0000f4aa  _NTC_Temp_Buff                           
1     00007060  _NmiIntruptRegs                          
0     0000e8e5  _OHT_Position                            
0     0000e8e6  _OHT_state                               
0     0000e8b6  _OV_check_value                          
1     00007a80  _OutputXbarRegs                          
0     00009df9  _PIE_RESERVED_ISR                        
0     0000f4a0  _PickUp_Temp                             
1     00000ce0  _PieCtrlRegs                             
1     00000d00  _PieVectTable                            
0     0000f954  _PieVectTableInit                        
0     0000e8ac  _Power_OV_check_value                    
0     0000f0f2  _Processing_Time                         
0     0000f0ec  _Processing_Time_max                     
0     0000f0ee  _Processing_Time_min                     
0     00009dc7  _RAM_ACCESS_VIOLATION_ISR                
0     00009db3  _RAM_CORRECTABLE_ERROR_ISR               
0     0000f48a  _RES_Cap_Temp                            
0     0000f0e1  _RLY_SEQ                                 
0     0000f0e4  _RLY_TEST                                
0     0000e8e1  _RS232_Warning                           
0     000098b3  _RTOS_ISR                                
0     0000c36c  _ReadRing                                
0     000080a3  _Read_8bit_I2C_Data                      
0     0000828b  _Read_BQ32000                            
0     000082be  _Read_BQ32000_data_all                   
0     0000845a  _Read_EventCode                          
0     000089db  _Read_Event_Array_Data                   
0     0000869d  _Read_Event_pt                           
0     00008185  _Read_I2C_Data                           
0     000081cc  _Read_I2C_float_Data                     
0     000081f2  _Read_I2C_long_Data                      
0     0000a3b7  _ReleaseFlashPump                        
0     0000c315  _ResetRing                               
1     0005e608  _RomPrefetchRegs                         
1     0005f540  _RomWaitStateRegs                        
0     0000f101  _RunTime_FlashUpdate_flag                
0     00009b79  _SCIA_RX_ISR                             
0     00009b83  _SCIA_TX_ISR                             
0     00009b8d  _SCIB_RX_ISR                             
0     00009b97  _SCIB_TX_ISR                             
0     00009b51  _SCIC_RX_ISR                             
0     00009b5b  _SCIC_TX_ISR                             
0     00009b65  _SCID_RX_ISR                             
0     00009b6f  _SCID_TX_ISR                             
0     00009d1d  _SD1_ISR                                 
0     00009d27  _SD2_ISR                                 
0     00009a9d  _SPIA_RX_ISR                             
0     00009aa7  _SPIA_TX_ISR                             
0     00009ab1  _SPIB_RX_ISR                             
0     00009abb  _SPIB_TX_ISR                             
0     00009d31  _SPIC_RX_ISR                             
0     00009d3b  _SPIC_TX_ISR                             
0     0000a729  _STANDBY                                 
0     0000bd3d  _SYSTEM_FAULT                            
0     00009dd1  _SYS_PLL_SLIP_ISR                        
0     0000bd3e  _Sag_Outage_Check                        
1     00007200  _SciaRegs                                
1     00007210  _ScibRegs                                
1     00007220  _ScicRegs                                
1     00007230  _ScidRegs                                
1     00005e00  _Sdfm1Regs                               
1     00005e80  _Sdfm2Regs                               
0     0000a399  _SeizeFlashPump_Bank0                    
0     0000a3a8  _SeizeFlashPump_Bank1                    
0     0000be48  _Send_Uart_Frame                         
0     0000a3c1  _ServiceDog                              
0     0000e8a2  _Servo_Warn_Vol                          
0     00008501  _Set_Event                               
0     0000bd20  _Software_Check                          
1     00006100  _SpiaRegs                                
1     00006110  _SpibRegs                                
1     00006120  _SpicRegs                                
0     00008b53  _Store_Event_Array_Data                  
0     0000bcfc  _Sub_Main_loop                           
1     00007940  _SyncSocRegs                             
0     0000a6dc  _SysIntOsc1Sel                           
0     0000a6e8  _SysIntOsc2Sel                           
0     0000a6f4  _SysXtalOscSel                           
0     0000b6c0  _System_Check_after_Power_ON             
0     0000f490  _TB_Temp                                 
0     0000998f  _TIMER0_ISR                              
0     00009895  _TIMER1_ISR                              
0     0000989f  _TIMER2_ISR                              
0     0000f481  _Temp_High                               
0     0000f480  _Temp_Low                                
0     0000f49a  _Temp_ad_fil                             
0     0000f4a4  _Temp_ad_fil2                            
0     0000be75  _UART_RX_Process                         
0     00009d45  _UPPA_ISR                                
0     00009d4f  _USBA_ISR                                
0     00009935  _USER10_ISR                              
0     0000993f  _USER11_ISR                              
0     00009949  _USER12_ISR                              
0     000098db  _USER1_ISR                               
0     000098e5  _USER2_ISR                               
0     000098ef  _USER3_ISR                               
0     000098f9  _USER4_ISR                               
0     00009903  _USER5_ISR                               
0     0000990d  _USER6_ISR                               
0     00009917  _USER7_ISR                               
0     00009921  _USER8_ISR                               
0     0000992b  _USER9_ISR                               
0     0000f0d9  _UV_Check                                
0     0000e8ba  _UV_check_value                          
1     00006200  _UppRegs                                 
0     00009c87  _VCU_ISR                                 
0     0000f0f0  _Vchop_gap                               
0     0000f0f4  _Vchop_ref                               
0     00009999  _WAKE_ISR                                
1     00007000  _WdRegs                                  
0     0000806e  _Write_8bit_I2C_Data                     
0     00008218  _Write_BQ32000                           
0     0000825d  _Write_BQ32000_all                       
0     000083a9  _Write_EventCode                         
0     000086ad  _Write_Event_Array_Data                  
0     00008691  _Write_Event_pt                          
0     000080d7  _Write_I2C_float_Data                    
0     0000812b  _Write_I2C_long_Data                     
0     00008630  _Write_I2C_longlong_Data                 
0     00009971  _XINT1_ISR                               
0     0000997b  _XINT2_ISR                               
0     00009c69  _XINT3_ISR                               
0     00009c73  _XINT4_ISR                               
0     00009c7d  _XINT5_ISR                               
1     00007920  _XbarRegs                                
1     00007070  _XintRegs                                
0     0000c9fe  __Fapi_calculateOtpChecksum              
0     0000c71c  __Fapi_checkRegionForValueBy16bits       
0     0000c7a9  __Fapi_divideUnsignedLong                
0     0000c74e  __Fapi_issueFsmCommand                   
0     0000c39a  __Fapi_loopRegionForValue                
0     0000c675  __Fapi_loopRegionForValueBy16bits        
0     0000c9e4  __Fapi_scaleCycleValues                  
0     0000c7fd  __Fapi_setupSectorsForWrite              
0     00000322  __STACK_END                              
abs   00000200  __STACK_SIZE                             
0     0000f50a  ___TI_cleanup_ptr                        
0     0000f50c  ___TI_dtors_ptr                          
0     0000f508  ___TI_enable_exit_profile_output         
abs   ffffffff  ___TI_pprof_out_hndl                     
abs   ffffffff  ___TI_prof_data_size                     
abs   ffffffff  ___TI_prof_data_start                    
abs   ffffffff  ___binit__                               
abs   ffffffff  ___c_args__                              
0     0000f510  ___cinit__                               
0     0000ca1e  ___etext__                               
abs   ffffffff  ___pinit__                               
0     00008000  ___text__                                
0     0000c9a2  __args_main                              
0     0000ca3e  __lock                                   
0     0000ca11  __nop                                    
0     0000ca0d  __register_lock                          
0     0000ca09  __register_unlock                        
0     00000122  __stack                                  
0     0000ca1d  __system_post_cinit                      
0     0000ca1b  __system_pre_init                        
0     0000e8be  __unlock                                 
0     0000c826  _abort                                   
0     0000f3d8  _ad_offset                               
0     0000f3ea  _ad_offset_new                           
0     0000f3c1  _ad_read_chk_cnt                         
0     0000f3c2  _ad_read_mux                             
0     0000f3c0  _ad_read_mux_cnt                         
0     0000f3c3  _ad_read_mux_seq                         
0     0000f3c4  _ad_read_mux_time                        
0     0000f3c6  _ad_result                               
0     0000f440  _ad_scale                                
0     0000f400  _ad_scale_new                            
0     0000e500  _adc                                     
0     0000c6ae  _adca1_isr                               
0     0000ca49  _array_pos                               
0     00009e1f  _asc2hex                                 
0     0000c4f7  _c_int00                                 
0     00084a24  _cinit_loadstart                         
0     0000f510  _cinit_runstart                          
abs   00000441  _cinit_size                              
0     0000e8dc  _comm_day                                
0     0000e8c8  _comm_day1                               
0     0000e8dd  _comm_hour                               
0     0000e8c5  _comm_hour1                              
0     0000e8e8  _comm_min                                
0     0000e8c6  _comm_min1                               
0     0000e8df  _comm_mon                                
0     0000e8c7  _comm_mon1                               
0     0000e8e3  _comm_sec                                
0     0000e8e0  _comm_sec1                               
0     0000e8de  _comm_year                               
0     0000e8cf  _comm_year1                              
0     000082b1  _conv_rtc_data                           
0     0000c5f2  _copy_in                                 
0     0000c176  _cpu_timer0_isr                          
0     0000f0e6  _cpu_timer0_msec                         
0     0000c988  _ddcopy                                  
0     0000bba4  _delay_ms                                
0     0000bb93  _delay_us                                
0     0000f4f8  _dis_LED                                 
0     0000f4f9  _dis_LED_SEQ                             
0     0000c988  _dpcopy                                  
0     0000c20c  _ePWM2_SetUp                             
0     0000c5a2  _easyDSP_SCI_Init                        
0     0000abce  _easy_RXINT_ISR                          
0     0000af4b  _easy_TXINT_ISR                          
0     00084e68  _econst_loadstart                        
0     0000f954  _econst_runstart                         
abs   00000230  _econst_size                             
0     0000c1ac  _epwm2_isr                               
0     0000e8d5  _err_num                                 
0     0000e8d3  _error_array_send_cnt                    
0     0000e8d4  _error_array_send_cnt2                   
0     0000e8d6  _event_array_send_cnt                    
0     0000ca4b  _event_old                               
0     0000c828  _exit                                    
0     0000f46f  _ezDSP_Version_SCI                       
0     0000f476  _ezDSP_fFloat                            
0     0000f4c0  _ezDSP_nEndPos                           
0     0000f4c1  _ezDSP_nMaxBuffSize                      
0     0000f4c2  _ezDSP_nStartPos                         
0     0000f4c3  _ezDSP_ringBuffer                        
0     0000f469  _ezDSP_uAddrRdCnt                        
0     0000f467  _ezDSP_uBRKDTCount                       
0     0000f46b  _ezDSP_uChksum                           
0     0000f46d  _ezDSP_uData                             
0     0000f46a  _ezDSP_uDataRdCnt                        
0     0000f46e  _ezDSP_uFECount                          
0     0000f468  _ezDSP_uOECount                          
0     0000f466  _ezDSP_uPECount                          
0     0000f471  _ezDSP_uRead16BPossible                  
0     0000f470  _ezDSP_uRead8BPossible                   
0     0000f46c  _ezDSP_uState                            
0     0000f464  _ezDSP_uWrongISRCount                    
0     0000f465  _ezDSP_ucRx                              
0     0000f474  _ezDSP_ulAddr                            
0     0000f472  _ezDSP_ulData                            
0     0000f478  _ezDSP_ullData                           
0     0000f0e5  _gate_sw_cnt                             
0     00009e56  _get_byte_from_string                    
0     00009e38  _hex2asc                                 
0     0000e8e7  _hex_dec_ena                             
0     0000c07d  _hw_Gate_Fault_check                     
0     0000c061  _hw_HeatSink_OT_85_check                 
0     0000c045  _hw_Protection_Board_check               
0     0000c027  _hw_SMPS_Fault_check                     
0     0000e480  _i2c                                     
0     00008ff4  _i2c_ad_data_read                        
0     00008e2c  _i2c_ad_data_write                       
0     0000ca46  _i2c_array_SEQ                           
0     0000ca4d  _i2c_array_test                          
0     0000ca21  _i2c_check_ok                            
0     0000e341  _i2c_chk_end                             
0     00008d81  _i2c_data_init                           
0     0000e345  _i2c_enable                              
0     000094ff  _i2c_gain_data_read                      
0     0000943b  _i2c_gain_data_write                     
0     0000ca45  _i2c_pri_pt                              
0     0000f4fc  _i2c_rtc_read_cnt                        
0     0000ca47  _i2c_sec_pt                              
0     0000ca1f  _i2c_step                                
0     00009350  _i2c_system_data_read                    
0     000092cb  _i2c_system_data_write                   
0     0000b755  _init_adc_data_struct                    
0     00009e1a  _init_global_variables                   
0     0000b757  _init_protect_data_struct                
0     0000b756  _init_ref_data_struct                    
0     0000e8ec  _init_scic_cnt                           
0     0000e8ee  _init_scic_cnt_ref                       
0     0000e8c2  _init_scic_port                          
0     0000b847  _init_struct_data_all                    
0     0000bd94  _interrupt_routine                       
0     0000f4f6  _led_cnt                                 
0     0000f4f7  _led_time                                
0     0000f4fb  _led_val                                 
0     0000bbb5  _main                                    
0     0000c950  _memcpy                                  
0     0000e351  _oht_dt                                  
0     0000e8aa  _out_Power                               
0     0000f500  _out_Protect_Relay_ON                    
0     0000f502  _out_SAG_GEN_ON                          
0     0000f501  _out_SMPS_reset                          
0     0000f503  _out_SYS_Fault_ON                        
0     0000f506  _out_do_spare_ON                         
0     0000f505  _out_nGate_Reset_ON                      
0     0000e8b4  _out_power_set_value                     
0     0000e8b2  _out_power_value                         
0     0000ca4c  _overlade_array_check                    
0     0000c988  _pdcopy                                  
0     0000e400  _pi                                      
0     00008000  _pinit_loadstart                         
0     00008000  _pinit_runstart                          
abs   00000000  _pinit_size                              
0     0000f4fd  _power_on_chk                            
0     0000c988  _ppcopy                                  
0     0000e640  _protect                                 
0     00085098  _ramfuncs_loadstart                      
0     0000fb84  _ramfuncs_runstart                       
abs   000000fd  _ramfuncs_size                           
0     0000ca24  _rd_ad_check_sum                         
0     0000ca32  _rd_gain_check_sum                       
0     0000ca30  _rd_sys_check_sum                        
0     0000af8f  _read_ad_value                           
0     0000831e  _rtc_time_check                          
0     0000e346  _rtc_tm                                  
0     0000e8c9  _rtc_tm_check                            
0     0000e8d7  _rtc_tm_check_cnt                        
0     0000ca4a  _rw_EventCode_max                        
0     0000ca40  _rw_event_array_cnt                      
0     0000eb80  _rxd_buf                                 
0     0000e8d0  _rxd_end                                 
0     0000e8d1  _rxd_pos                                 
0     0000f0da  _sag_gen                                 
0     0000fbb2  _scia_rx_isr                             
0     0000fb84  _scia_tx_isr                             
0     0000e8cb  _scic_Flag                               
0     0000e8cc  _scic_Flag_cnt                           
0     0000e8c4  _scic_rxd                                
0     0000e8cd  _scic_rxd_SEQ                            
0     0000e8c1  _scic_rxd_checksum                       
0     0000e8c0  _scic_rxd_chk_sum                        
0     0000e8ce  _scic_txd                                
0     0000e8c3  _scic_txd_chk_sum                        
0     0000e8f0  _scic_txd_delay_cnt                      
0     0000e8d9  _scic_txd_delay_cnt_ref                  
0     0000e8e4  _scic_txd_enable                         
0     0000e8db  _scic_txd_errorlog_send                  
0     0000e8e2  _send_errorlog_pt                        
0     0000ca4e  _store_array_event                       
0     0000ca44  _store_array_event_p                     
0     0000aadf  _sw_ECAP_NTC_Check                       
0     0000a887  _sw_Ecap_Check                           
0     0000a9fb  _sw_Ecap_Fuse_Open_Check                 
0     0000a759  _sw_Edc_Check                            
0     0000a7f0  _sw_Eout_Check                           
0     0000aa2b  _sw_IGBT_NTC_Check                       
0     0000a97f  _sw_Iac_Check                            
0     0000a920  _sw_Iout_Check                           
0     0000a9cd  _sw_Output_Fuse_Open_Check               
0     0000aa73  _sw_PickUp_NTC_Check                     
0     0000ab6f  _sw_Power_Check                          
0     0000f0e3  _sw_onoff_time                           
0     00085198  _switch_loadstart                        
0     0000fc84  _switch_runstart                         
abs   00000020  _switch_size                             
0     0000cf00  _sys_data_rd0                            
0     0000cf80  _sys_data_rd1                            
0     0000d200  _sys_data_rd10                           
0     0000cb00  _sys_data_rd11                           
0     0000ca80  _sys_data_rd12                           
0     0000cc00  _sys_data_rd13                           
0     0000cb80  _sys_data_rd14                           
0     0000d300  _sys_data_rd15                           
0     0000cd00  _sys_data_rd2                            
0     0000ce00  _sys_data_rd3                            
0     0000ce80  _sys_data_rd4                            
0     0000d400  _sys_data_rd5                            
0     0000d380  _sys_data_rd6                            
0     0000d180  _sys_data_rd7                            
0     0000d100  _sys_data_rd8                            
0     0000d280  _sys_data_rd9                            
0     0000db40  _sys_data_wr                             
0     0000d000  _sys_data_wr0                            
0     0000d080  _sys_data_wr1                            
0     0000cc80  _sys_data_wr2                            
0     0000cd80  _sys_data_wr3                            
0     0000ca50  _sys_event                               
0     0000e900  _sys_event2                              
0     0000f0e7  _sys_mode                                
0     0000e3c0  _sys_ref                                 
0     0000e380  _sys_time                                
0     0000ca42  _system_fault_mode                       
0     0000f0fe  _t1_prd                                  
0     0000f0db  _t1_prd_val                              
0     0000f483  _temp_cnt                                
0     0000f482  _temp_cnt2                               
0     0000f49c  _temp_value                              
0     0000f498  _temp_value2                             
0     0000f0de  _test_array_store                        
0     00080004  _text_loadstart                          
0     00008000  _text_runstart                           
abs   00004a1e  _text_size                               
0     0000e940  _tmp_data                                
0     0000e8ea  _tmp_data_Iout                           
0     0000ca36  _tmp_rd_check_sum                        
0     0000ca41  _tmp_short                               
0     0000ca43  _tmp_short_max                           
0     0000ca38  _tmp_wr_check_sum                        
0     0000e980  _txd_buf                                 
0     0000e8ca  _txd_end                                 
0     0000e8d2  _txd_pos                                 
0     0000edc0  _uart_rx_buf                             
0     0000ed80  _uart_rx_cnt                             
0     0000ed82  _uart_rx_frame_flag                      
0     0000ed81  _uart_rx_start_flag                      
0     0000ee80  _uart_tx_buf                             
0     0000ed84  _uart_tx_cnt                             
0     0000ed83  _uart_tx_pos                             
0     0000ca1e  _use_ECO                                 
0     0000ca20  _use_ECO_new                             
0     0000f0fc  _uv_check_cnt                            
0     0000f0e8  _uv_enable_cnt                           
0     0000f0ea  _uv_enable_time                          
0     0000f0df  _uv_test                                 
0     0000ca3c  _wr_ad_check_sum                         
0     0000ca3a  _wr_ad_check_sum_new                     
0     0000ca2e  _wr_ad_chk_sum                           
0     0000ca28  _wr_gain_check_sum                       
0     0000ca22  _wr_gain_check_sum_new                   
0     0000ca2c  _wr_gain_chk_sum                         
0     0000ca48  _wr_pos                                  
0     0000ca34  _wr_sys_check_sum                        
0     0000ca26  _wr_sys_check_sum_new                    
0     0000ca2a  _wr_sys_chk_sum                          
abs   ffffffff  binit                                    
0     0000f510  cinit                                    
0     00080000  code_start                               
0     000851b8  copy_sections                            
0     0000ca1e  etext                                    
abs   ffffffff  pinit                                    

GLOBAL SYMBOLS: SORTED BY Symbol Address 

page  address   name                                     
----  -------   ----                                     
0     00000122  __stack                                  
0     00000322  __STACK_END                              
0     00000ce0  _Cla1SoftIntRegs                         
0     00008000  .text                                    
0     00008000  _InitI2C                                 
0     00008000  ___text__                                
0     00008000  _pinit_loadstart                         
0     00008000  _pinit_runstart                          
0     00008000  _text_runstart                           
0     00008028  _I2C_STP_check                           
0     0000803a  _I2C_BB_check                            
0     0000804c  _I2C_SCD_check                           
0     0000805f  _I2C_ADRY_check                          
0     0000806e  _Write_8bit_I2C_Data                     
0     000080a3  _Read_8bit_I2C_Data                      
0     000080d7  _Write_I2C_float_Data                    
0     0000812b  _Write_I2C_long_Data                     
0     00008185  _Read_I2C_Data                           
0     000081cc  _Read_I2C_float_Data                     
0     000081f2  _Read_I2C_long_Data                      
0     00008218  _Write_BQ32000                           
0     0000825d  _Write_BQ32000_all                       
0     0000828b  _Read_BQ32000                            
0     000082b1  _conv_rtc_data                           
0     000082be  _Read_BQ32000_data_all                   
0     0000831e  _rtc_time_check                          
0     000083a9  _Write_EventCode                         
0     0000845a  _Read_EventCode                          
0     00008501  _Set_Event                               
0     000085d9  _Check_Event                             
0     00008630  _Write_I2C_longlong_Data                 
0     00008691  _Write_Event_pt                          
0     0000869d  _Read_Event_pt                           
0     000086ad  _Write_Event_Array_Data                  
0     000089db  _Read_Event_Array_Data                   
0     00008b53  _Store_Event_Array_Data                  
0     00008d81  _i2c_data_init                           
0     00008e2c  _i2c_ad_data_write                       
0     00008ff4  _i2c_ad_data_read                        
0     000092cb  _i2c_system_data_write                   
0     00009350  _i2c_system_data_read                    
0     0000943b  _i2c_gain_data_write                     
0     000094ff  _i2c_gain_data_read                      
0     00009610  _Check_I2C_Data                          
0     000097d2  _I2C_Read_Write                          
0     00009895  _TIMER1_ISR                              
0     0000989f  _TIMER2_ISR                              
0     000098a9  _DATALOG_ISR                             
0     000098b3  _RTOS_ISR                                
0     000098bd  _EMU_ISR                                 
0     000098c7  _NMI_ISR                                 
0     000098d1  _ILLEGAL_ISR                             
0     000098db  _USER1_ISR                               
0     000098e5  _USER2_ISR                               
0     000098ef  _USER3_ISR                               
0     000098f9  _USER4_ISR                               
0     00009903  _USER5_ISR                               
0     0000990d  _USER6_ISR                               
0     00009917  _USER7_ISR                               
0     00009921  _USER8_ISR                               
0     0000992b  _USER9_ISR                               
0     00009935  _USER10_ISR                              
0     0000993f  _USER11_ISR                              
0     00009949  _USER12_ISR                              
0     00009953  _ADCA1_ISR                               
0     0000995d  _ADCB1_ISR                               
0     00009967  _ADCC1_ISR                               
0     00009971  _XINT1_ISR                               
0     0000997b  _XINT2_ISR                               
0     00009985  _ADCD1_ISR                               
0     0000998f  _TIMER0_ISR                              
0     00009999  _WAKE_ISR                                
0     000099a3  _EPWM1_TZ_ISR                            
0     000099ad  _EPWM2_TZ_ISR                            
0     000099b7  _EPWM3_TZ_ISR                            
0     000099c1  _EPWM4_TZ_ISR                            
0     000099cb  _EPWM5_TZ_ISR                            
0     000099d5  _EPWM6_TZ_ISR                            
0     000099df  _EPWM7_TZ_ISR                            
0     000099e9  _EPWM8_TZ_ISR                            
0     000099f3  _EPWM1_ISR                               
0     000099fd  _EPWM2_ISR                               
0     00009a07  _EPWM3_ISR                               
0     00009a11  _EPWM4_ISR                               
0     00009a1b  _EPWM5_ISR                               
0     00009a25  _EPWM6_ISR                               
0     00009a2f  _EPWM7_ISR                               
0     00009a39  _EPWM8_ISR                               
0     00009a43  _ECAP1_ISR                               
0     00009a4d  _ECAP2_ISR                               
0     00009a57  _ECAP3_ISR                               
0     00009a61  _ECAP4_ISR                               
0     00009a6b  _ECAP5_ISR                               
0     00009a75  _ECAP6_ISR                               
0     00009a7f  _EQEP1_ISR                               
0     00009a89  _EQEP2_ISR                               
0     00009a93  _EQEP3_ISR                               
0     00009a9d  _SPIA_RX_ISR                             
0     00009aa7  _SPIA_TX_ISR                             
0     00009ab1  _SPIB_RX_ISR                             
0     00009abb  _SPIB_TX_ISR                             
0     00009ac5  _MCBSPA_RX_ISR                           
0     00009acf  _MCBSPA_TX_ISR                           
0     00009ad9  _MCBSPB_RX_ISR                           
0     00009ae3  _MCBSPB_TX_ISR                           
0     00009aed  _DMA_CH1_ISR                             
0     00009af7  _DMA_CH2_ISR                             
0     00009b01  _DMA_CH3_ISR                             
0     00009b0b  _DMA_CH4_ISR                             
0     00009b15  _DMA_CH5_ISR                             
0     00009b1f  _DMA_CH6_ISR                             
0     00009b29  _I2CA_ISR                                
0     00009b33  _I2CA_FIFO_ISR                           
0     00009b3d  _I2CB_ISR                                
0     00009b47  _I2CB_FIFO_ISR                           
0     00009b51  _SCIC_RX_ISR                             
0     00009b5b  _SCIC_TX_ISR                             
0     00009b65  _SCID_RX_ISR                             
0     00009b6f  _SCID_TX_ISR                             
0     00009b79  _SCIA_RX_ISR                             
0     00009b83  _SCIA_TX_ISR                             
0     00009b8d  _SCIB_RX_ISR                             
0     00009b97  _SCIB_TX_ISR                             
0     00009ba1  _CANA0_ISR                               
0     00009bab  _CANA1_ISR                               
0     00009bb5  _CANB0_ISR                               
0     00009bbf  _CANB1_ISR                               
0     00009bc9  _ADCA_EVT_ISR                            
0     00009bd3  _ADCA2_ISR                               
0     00009bdd  _ADCA3_ISR                               
0     00009be7  _ADCA4_ISR                               
0     00009bf1  _ADCB_EVT_ISR                            
0     00009bfb  _ADCB2_ISR                               
0     00009c05  _ADCB3_ISR                               
0     00009c0f  _ADCB4_ISR                               
0     00009c19  _CLA1_1_ISR                              
0     00009c23  _CLA1_2_ISR                              
0     00009c2d  _CLA1_3_ISR                              
0     00009c37  _CLA1_4_ISR                              
0     00009c41  _CLA1_5_ISR                              
0     00009c4b  _CLA1_6_ISR                              
0     00009c55  _CLA1_7_ISR                              
0     00009c5f  _CLA1_8_ISR                              
0     00009c69  _XINT3_ISR                               
0     00009c73  _XINT4_ISR                               
0     00009c7d  _XINT5_ISR                               
0     00009c87  _VCU_ISR                                 
0     00009c91  _FPU_OVERFLOW_ISR                        
0     00009c9b  _FPU_UNDERFLOW_ISR                       
0     00009ca5  _IPC0_ISR                                
0     00009caf  _IPC1_ISR                                
0     00009cb9  _IPC2_ISR                                
0     00009cc3  _IPC3_ISR                                
0     00009ccd  _EPWM9_TZ_ISR                            
0     00009cd7  _EPWM10_TZ_ISR                           
0     00009ce1  _EPWM11_TZ_ISR                           
0     00009ceb  _EPWM12_TZ_ISR                           
0     00009cf5  _EPWM9_ISR                               
0     00009cff  _EPWM10_ISR                              
0     00009d09  _EPWM11_ISR                              
0     00009d13  _EPWM12_ISR                              
0     00009d1d  _SD1_ISR                                 
0     00009d27  _SD2_ISR                                 
0     00009d31  _SPIC_RX_ISR                             
0     00009d3b  _SPIC_TX_ISR                             
0     00009d45  _UPPA_ISR                                
0     00009d4f  _USBA_ISR                                
0     00009d59  _ADCC_EVT_ISR                            
0     00009d63  _ADCC2_ISR                               
0     00009d6d  _ADCC3_ISR                               
0     00009d77  _ADCC4_ISR                               
0     00009d81  _ADCD_EVT_ISR                            
0     00009d8b  _ADCD2_ISR                               
0     00009d95  _ADCD3_ISR                               
0     00009d9f  _ADCD4_ISR                               
0     00009da9  _EMIF_ERROR_ISR                          
0     00009db3  _RAM_CORRECTABLE_ERROR_ISR               
0     00009dbd  _FLASH_CORRECTABLE_ERROR_ISR             
0     00009dc7  _RAM_ACCESS_VIOLATION_ISR                
0     00009dd1  _SYS_PLL_SLIP_ISR                        
0     00009ddb  _AUX_PLL_SLIP_ISR                        
0     00009de5  _CLA_OVERFLOW_ISR                        
0     00009def  _CLA_UNDERFLOW_ISR                       
0     00009df9  _PIE_RESERVED_ISR                        
0     00009e03  _EMPTY_ISR                               
0     00009e10  _NOTUSED_ISR                             
0     00009e1a  _init_global_variables                   
0     00009e1f  _asc2hex                                 
0     00009e38  _hex2asc                                 
0     00009e43  _Get_Uart_Frame_CheckSum                 
0     00009e56  _get_byte_from_string                    
0     00009f56  _Do_Flash_Erase                          
0     00009fd2  _Do_Flash_Write                          
0     0000a0b1  _Do_Flash_Verify                         
0     0000a157  _Do_DSP28377S_FlashBank_Change           
0     0000a1d7  _Do_DSP28377S_Runtime_Flash_Update_Check 
0     0000a224  _Do_Flash_CSM_Unlock                     
0     0000a283  _Do_DSP28377S_Runtime_Flash_Update_Finish
0     0000a2ba  _Do_Regulator_Normal_Info_Reqeust        
0     0000a2c3  _Do_Regulator_Error_Data_Request         
0     0000a2cc  _InitSysCtrl                             
0     0000a2fd  _InitPeripheralClocks                    
0     0000a381  _DisablePeripheralClocks                 
0     0000a399  _SeizeFlashPump_Bank0                    
0     0000a3a8  _SeizeFlashPump_Bank1                    
0     0000a3b7  _ReleaseFlashPump                        
0     0000a3c1  _ServiceDog                              
0     0000a3cf  _DisableDog                              
0     0000a3dd  _EnableDog                               
0     0000a3e5  _InitSysPll                              
0     0000a5d4  _InitAuxPll                              
0     0000a6bb  _CsmUnlock                               
0     0000a6dc  _SysIntOsc1Sel                           
0     0000a6e8  _SysIntOsc2Sel                           
0     0000a6f4  _SysXtalOscSel                           
0     0000a700  _AuxIntOsc2Sel                           
0     0000a70a  _AuxXtalOscSel                           
0     0000a716  _AuxAuxClkSel                            
0     0000a720  _IDLE                                    
0     0000a729  _STANDBY                                 
0     0000a734  _HALT                                    
0     0000a745  _HIB                                     
0     0000a759  _sw_Edc_Check                            
0     0000a7f0  _sw_Eout_Check                           
0     0000a887  _sw_Ecap_Check                           
0     0000a920  _sw_Iout_Check                           
0     0000a97f  _sw_Iac_Check                            
0     0000a9cd  _sw_Output_Fuse_Open_Check               
0     0000a9fb  _sw_Ecap_Fuse_Open_Check                 
0     0000aa2b  _sw_IGBT_NTC_Check                       
0     0000aa73  _sw_PickUp_NTC_Check                     
0     0000aadf  _sw_ECAP_NTC_Check                       
0     0000ab6f  _sw_Power_Check                          
0     0000abce  _easy_RXINT_ISR                          
0     0000af4b  _easy_TXINT_ISR                          
0     0000af8f  _read_ad_value                           
0     0000b0a6  _InitAdc                                 
0     0000b480  _InitGpio                                
0     0000b4c0  _GPIO_SetupPinMux                        
0     0000b548  _GPIO_SetupPinOptions                    
0     0000b5dc  _GPIO_SetupLock                          
0     0000b605  _GPIO_SetupXINT1Gpio                     
0     0000b60f  _GPIO_SetupXINT2Gpio                     
0     0000b619  _GPIO_SetupXINT3Gpio                     
0     0000b623  _GPIO_SetupXINT4Gpio                     
0     0000b62d  _GPIO_SetupXINT5Gpio                     
0     0000b637  _GPIO_EnableUnbondedIOPullupsFor176Pin   
0     0000b650  _GPIO_EnableUnbondedIOPullupsFor100Pin   
0     0000b675  _GPIO_EnableUnbondedIOPullups            
0     0000b68b  _GPIO_ReadPin                            
0     0000b6a2  _GPIO_WritePin                           
0     0000b6c0  _System_Check_after_Power_ON             
0     0000b6db  _LED_SET                                 
0     0000b6f1  _LED_control                             
0     0000b755  _init_adc_data_struct                    
0     0000b756  _init_ref_data_struct                    
0     0000b757  _init_protect_data_struct                
0     0000b847  _init_struct_data_all                    
0     0000b889  _Fapi_issueProgrammingCommand            
0     0000ba27  _NTC_Cal                                 
0     0000bb93  _delay_us                                
0     0000bba4  _delay_ms                                
0     0000bbb5  _main                                    
0     0000bcfc  _Sub_Main_loop                           
0     0000bcfd  _GATE_FAULT_RESET                        
0     0000bd01  _Hardware_Check                          
0     0000bd20  _Software_Check                          
0     0000bd33  _GATE_LOGIC_TEST                         
0     0000bd3d  _SYSTEM_FAULT                            
0     0000bd3e  _Sag_Outage_Check                        
0     0000bd94  _interrupt_routine                       
0     0000be48  _Send_Uart_Frame                         
0     0000be75  _UART_RX_Process                         
0     0000bf37  _Init_SCIA                               
0     0000bf7a  _HardWare_Output_Signal_Check            
0     0000bff7  _HardWare_Input_Signal_Check             
0     0000c027  _hw_SMPS_Fault_check                     
0     0000c045  _hw_Protection_Board_check               
0     0000c061  _hw_HeatSink_OT_85_check                 
0     0000c07d  _hw_Gate_Fault_check                     
0     0000c099  _AdcSetMode                              
0     0000c13c  _CalAdcINL                               
0     0000c176  _cpu_timer0_isr                          
0     0000c1ac  _epwm2_isr                               
0     0000c203  _InitEPwm                                
0     0000c20c  _ePWM2_SetUp                             
0     0000c257  _InitEPwmGpio                            
0     0000c25a  _InitEPwm2Gpio                           
0     0000c26c  _EPWM2_GATE_OPEN                         
0     0000c277  _EPWM_GATE_ALL_OPEN                      
0     0000c27a  _EPWM2_GATE_BLOCK                        
0     0000c285  _EPWM_GATE_ALL_BLOCK                     
0     0000c288  _EPWM_GATE_Set_All_Zero                  
0     0000c28d  FS$$DIV                                  
0     0000c315  _ResetRing                               
0     0000c32c  _AddRing                                 
0     0000c358  _ExtractRing                             
0     0000c36c  _ReadRing                                
0     0000c386  _GetSizeRing                             
0     0000c392  _IsRingEmpty                             
0     0000c39a  __Fapi_loopRegionForValue                
0     0000c41c  _InitCpuTimers                           
0     0000c45d  _ConfigCpuTimer                          
0     0000c498  _Fapi_initializeAPI                      
0     0000c4f7  _c_int00                                 
0     0000c54d  _Fapi_setupEepromSectorEnable            
0     0000c5a2  _easyDSP_SCI_Init                        
0     0000c5f2  _copy_in                                 
0     0000c638  _Fapi_doBlankCheck                       
0     0000c675  __Fapi_loopRegionForValueBy16bits        
0     0000c6ae  _adca1_isr                               
0     0000c6e6  _Fapi_isAddressEcc                       
0     0000c71c  __Fapi_checkRegionForValueBy16bits       
0     0000c74e  __Fapi_issueFsmCommand                   
0     0000c77d  _Fapi_calculateFletcherChecksum          
0     0000c7a9  __Fapi_divideUnsignedLong                
0     0000c7d3  L$$DIV                                   
0     0000c7e2  L$$MOD                                   
0     0000c7f0  UL$$DIV                                  
0     0000c7f7  UL$$MOD                                  
0     0000c7fd  __Fapi_setupSectorsForWrite              
0     0000c826  C$$EXIT                                  
0     0000c826  _abort                                   
0     0000c828  _exit                                    
0     0000c84f  _InitPieCtrl                             
0     0000c86e  _EnableInterrupts                        
0     0000c877  _InitPieVectTable                        
0     0000c89d  _Fapi_flushPipeline                      
0     0000c8c3  _Fapi_setActiveFlashBank                 
0     0000c8e9  _Fapi_setupBankSectorEnable              
0     0000c90e  _Fapi_issueAsyncCommandWithAddress       
0     0000c932  LL$$CMP                                  
0     0000c944  ULL$$CMP                                 
0     0000c950  _memcpy                                  
0     0000c96e  _Fapi_waitDelay                          
0     0000c988  _ddcopy                                  
0     0000c988  _dpcopy                                  
0     0000c988  _pdcopy                                  
0     0000c988  _ppcopy                                  
0     0000c9a2  __args_main                              
0     0000c9bb  LL$$AND                                  
0     0000c9c3  LL$$OR                                   
0     0000c9cb  LL$$XOR                                  
0     0000c9d3  _Fapi_doVerifyBy16bits                   
0     0000c9e4  __Fapi_scaleCycleValues                  
0     0000c9f3  _Fapi_checkFsmForReady                   
0     0000c9fe  __Fapi_calculateOtpChecksum              
0     0000ca09  __register_unlock                        
0     0000ca0d  __register_lock                          
0     0000ca11  __nop                                    
0     0000ca12  _Fapi_getFsmStatus                       
0     0000ca19  _Fapi_serviceWatchdogTimer               
0     0000ca1b  __system_pre_init                        
0     0000ca1d  __system_post_cinit                      
0     0000ca1e  ___etext__                               
0     0000ca1e  _use_ECO                                 
0     0000ca1e  etext                                    
0     0000ca1f  _i2c_step                                
0     0000ca20  _use_ECO_new                             
0     0000ca21  _i2c_check_ok                            
0     0000ca22  _wr_gain_check_sum_new                   
0     0000ca24  _rd_ad_check_sum                         
0     0000ca26  _wr_sys_check_sum_new                    
0     0000ca28  _wr_gain_check_sum                       
0     0000ca2a  _wr_sys_chk_sum                          
0     0000ca2c  _wr_gain_chk_sum                         
0     0000ca2e  _wr_ad_chk_sum                           
0     0000ca30  _rd_sys_check_sum                        
0     0000ca32  _rd_gain_check_sum                       
0     0000ca34  _wr_sys_check_sum                        
0     0000ca36  _tmp_rd_check_sum                        
0     0000ca38  _tmp_wr_check_sum                        
0     0000ca3a  _wr_ad_check_sum_new                     
0     0000ca3c  _wr_ad_check_sum                         
0     0000ca3e  __lock                                   
0     0000ca40  _rw_event_array_cnt                      
0     0000ca41  _tmp_short                               
0     0000ca42  _system_fault_mode                       
0     0000ca43  _tmp_short_max                           
0     0000ca44  _store_array_event_p                     
0     0000ca45  _i2c_pri_pt                              
0     0000ca46  _i2c_array_SEQ                           
0     0000ca47  _i2c_sec_pt                              
0     0000ca48  _wr_pos                                  
0     0000ca49  _array_pos                               
0     0000ca4a  _rw_EventCode_max                        
0     0000ca4b  _event_old                               
0     0000ca4c  _overlade_array_check                    
0     0000ca4d  _i2c_array_test                          
0     0000ca4e  _store_array_event                       
0     0000ca50  _sys_event                               
0     0000ca80  _sys_data_rd12                           
0     0000cb00  _sys_data_rd11                           
0     0000cb80  _sys_data_rd14                           
0     0000cc00  _sys_data_rd13                           
0     0000cc80  _sys_data_wr2                            
0     0000cd00  _sys_data_rd2                            
0     0000cd80  _sys_data_wr3                            
0     0000ce00  _sys_data_rd3                            
0     0000ce80  _sys_data_rd4                            
0     0000cf00  _sys_data_rd0                            
0     0000cf80  _sys_data_rd1                            
0     0000d000  _sys_data_wr0                            
0     0000d080  _sys_data_wr1                            
0     0000d100  _sys_data_rd8                            
0     0000d180  _sys_data_rd7                            
0     0000d200  _sys_data_rd10                           
0     0000d280  _sys_data_rd9                            
0     0000d300  _sys_data_rd15                           
0     0000d380  _sys_data_rd6                            
0     0000d400  _sys_data_rd5                            
0     0000d480  _Event_buff                              
0     0000d5c0  _Event                                   
0     0000d880  _Event_new                               
0     0000db40  _sys_data_wr                             
0     0000e340  _Code_Date                               
0     0000e341  _i2c_chk_end                             
0     0000e342  _Code_Year                               
0     0000e343  _Code_Month                              
0     0000e344  _Firmware                                
0     0000e345  _i2c_enable                              
0     0000e346  _rtc_tm                                  
0     0000e351  _oht_dt                                  
0     0000e380  _sys_time                                
0     0000e3c0  _sys_ref                                 
0     0000e400  _pi                                      
0     0000e480  _i2c                                     
0     0000e500  _adc                                     
0     0000e640  _protect                                 
0     0000e8a2  _Servo_Warn_Vol                          
0     0000e8a3  _Ecap_NTC_PT_ref                         
0     0000e8a4  _Ecap_NTC_OT_ref                         
0     0000e8a6  _Edc_Eout_gap                            
0     0000e8a8  _Eout_Fuse_Gap_Voltage                   
0     0000e8aa  _out_Power                               
0     0000e8ac  _Power_OV_check_value                    
0     0000e8ae  _Ecap_Fuse_Gap_Voltage                   
0     0000e8b0  _Edc_Ecap_gap                            
0     0000e8b2  _out_power_value                         
0     0000e8b4  _out_power_set_value                     
0     0000e8b6  _OV_check_value                          
0     0000e8b8  _Iout_OC_check_value                     
0     0000e8ba  _UV_check_value                          
0     0000e8bc  _Iac_OC_check_value                      
0     0000e8be  __unlock                                 
0     0000e8c0  _scic_rxd_chk_sum                        
0     0000e8c1  _scic_rxd_checksum                       
0     0000e8c2  _init_scic_port                          
0     0000e8c3  _scic_txd_chk_sum                        
0     0000e8c4  _scic_rxd                                
0     0000e8c5  _comm_hour1                              
0     0000e8c6  _comm_min1                               
0     0000e8c7  _comm_mon1                               
0     0000e8c8  _comm_day1                               
0     0000e8c9  _rtc_tm_check                            
0     0000e8ca  _txd_end                                 
0     0000e8cb  _scic_Flag                               
0     0000e8cc  _scic_Flag_cnt                           
0     0000e8cd  _scic_rxd_SEQ                            
0     0000e8ce  _scic_txd                                
0     0000e8cf  _comm_year1                              
0     0000e8d0  _rxd_end                                 
0     0000e8d1  _rxd_pos                                 
0     0000e8d2  _txd_pos                                 
0     0000e8d3  _error_array_send_cnt                    
0     0000e8d4  _error_array_send_cnt2                   
0     0000e8d5  _err_num                                 
0     0000e8d6  _event_array_send_cnt                    
0     0000e8d7  _rtc_tm_check_cnt                        
0     0000e8d8  _EV_Send_SEQ_cnt                         
0     0000e8d9  _scic_txd_delay_cnt_ref                  
0     0000e8da  _EV_Send_SEQ                             
0     0000e8db  _scic_txd_errorlog_send                  
0     0000e8dc  _comm_day                                
0     0000e8dd  _comm_hour                               
0     0000e8de  _comm_year                               
0     0000e8df  _comm_mon                                
0     0000e8e0  _comm_sec1                               
0     0000e8e1  _RS232_Warning                           
0     0000e8e2  _send_errorlog_pt                        
0     0000e8e3  _comm_sec                                
0     0000e8e4  _scic_txd_enable                         
0     0000e8e5  _OHT_Position                            
0     0000e8e6  _OHT_state                               
0     0000e8e7  _hex_dec_ena                             
0     0000e8e8  _comm_min                                
0     0000e8ea  _tmp_data_Iout                           
0     0000e8ec  _init_scic_cnt                           
0     0000e8ee  _init_scic_cnt_ref                       
0     0000e8f0  _scic_txd_delay_cnt                      
0     0000e900  _sys_event2                              
0     0000e940  _tmp_data                                
0     0000e980  _txd_buf                                 
0     0000eb80  _rxd_buf                                 
0     0000ed80  _uart_rx_cnt                             
0     0000ed81  _uart_rx_start_flag                      
0     0000ed82  _uart_rx_frame_flag                      
0     0000ed83  _uart_tx_pos                             
0     0000ed84  _uart_tx_cnt                             
0     0000edc0  _uart_rx_buf                             
0     0000ee80  _uart_tx_buf                             
0     0000f0d8  _Iac_sag_level                           
0     0000f0d9  _UV_Check                                
0     0000f0da  _sag_gen                                 
0     0000f0db  _t1_prd_val                              
0     0000f0dc  _GATE_TEST                               
0     0000f0dd  _Iac_recover_level                       
0     0000f0de  _test_array_store                        
0     0000f0df  _uv_test                                 
0     0000f0e0  _Edc_sw_gap                              
0     0000f0e1  _RLY_SEQ                                 
0     0000f0e2  _Edc_sw_ref_max                          
0     0000f0e3  _sw_onoff_time                           
0     0000f0e4  _RLY_TEST                                
0     0000f0e5  _gate_sw_cnt                             
0     0000f0e6  _cpu_timer0_msec                         
0     0000f0e7  _sys_mode                                
0     0000f0e8  _uv_enable_cnt                           
0     0000f0ea  _uv_enable_time                          
0     0000f0ec  _Processing_Time_max                     
0     0000f0ee  _Processing_Time_min                     
0     0000f0f0  _Vchop_gap                               
0     0000f0f2  _Processing_Time                         
0     0000f0f4  _Vchop_ref                               
0     0000f0f6  _Iac_outage_cnt                          
0     0000f0f8  _Iac_sag_cnt                             
0     0000f0fa  _Iac_rever_cnt                           
0     0000f0fc  _uv_check_cnt                            
0     0000f0fe  _t1_prd                                  
0     0000f101  _RunTime_FlashUpdate_flag                
0     0000f103  _CSM_Password_Data                       
0     0000f10b  _FD_Buffer                               
0     0000f398  _CpuTimer1                               
0     0000f3a0  _CpuTimer2                               
0     0000f3a8  _CpuTimer0                               
0     0000f3b0  _Fapi_GlobalInit                         
0     0000f3c0  _ad_read_mux_cnt                         
0     0000f3c1  _ad_read_chk_cnt                         
0     0000f3c2  _ad_read_mux                             
0     0000f3c3  _ad_read_mux_seq                         
0     0000f3c4  _ad_read_mux_time                        
0     0000f3c6  _ad_result                               
0     0000f3d8  _ad_offset                               
0     0000f3ea  _ad_offset_new                           
0     0000f400  _ad_scale_new                            
0     0000f440  _ad_scale                                
0     0000f464  _ezDSP_uWrongISRCount                    
0     0000f465  _ezDSP_ucRx                              
0     0000f466  _ezDSP_uPECount                          
0     0000f467  _ezDSP_uBRKDTCount                       
0     0000f468  _ezDSP_uOECount                          
0     0000f469  _ezDSP_uAddrRdCnt                        
0     0000f46a  _ezDSP_uDataRdCnt                        
0     0000f46b  _ezDSP_uChksum                           
0     0000f46c  _ezDSP_uState                            
0     0000f46d  _ezDSP_uData                             
0     0000f46e  _ezDSP_uFECount                          
0     0000f46f  _ezDSP_Version_SCI                       
0     0000f470  _ezDSP_uRead8BPossible                   
0     0000f471  _ezDSP_uRead16BPossible                  
0     0000f472  _ezDSP_ulData                            
0     0000f474  _ezDSP_ulAddr                            
0     0000f476  _ezDSP_fFloat                            
0     0000f478  _ezDSP_ullData                           
0     0000f480  _Temp_Low                                
0     0000f481  _Temp_High                               
0     0000f482  _temp_cnt2                               
0     0000f483  _temp_cnt                                
0     0000f484  _NTC_Seq                                 
0     0000f486  _CHOP_Temp                               
0     0000f488  _Ecap2_Temp                              
0     0000f48a  _RES_Cap_Temp                            
0     0000f48c  _Ecap1_Temp                              
0     0000f48e  _Filter_Cap_Temp                         
0     0000f490  _TB_Temp                                 
0     0000f492  _Filter_L_Temp                           
0     0000f494  _CHOP_R2_Temp                            
0     0000f496  _CHOP_R1_Temp                            
0     0000f498  _temp_value2                             
0     0000f49a  _Temp_ad_fil                             
0     0000f49c  _temp_value                              
0     0000f49e  _NTC_Temp2                               
0     0000f4a0  _PickUp_Temp                             
0     0000f4a2  _Ecap_AMB_Temp                           
0     0000f4a4  _Temp_ad_fil2                            
0     0000f4a6  _IGBT_Temp                               
0     0000f4a8  _NTC_Temp                                
0     0000f4aa  _NTC_Temp_Buff                           
0     0000f4c0  _ezDSP_nEndPos                           
0     0000f4c1  _ezDSP_nMaxBuffSize                      
0     0000f4c2  _ezDSP_nStartPos                         
0     0000f4c3  _ezDSP_ringBuffer                        
0     0000f4f5  _LED_SEQ                                 
0     0000f4f6  _led_cnt                                 
0     0000f4f7  _led_time                                
0     0000f4f8  _dis_LED                                 
0     0000f4f9  _dis_LED_SEQ                             
0     0000f4fa  _LED_TEST                                
0     0000f4fb  _led_val                                 
0     0000f4fc  _i2c_rtc_read_cnt                        
0     0000f4fd  _power_on_chk                            
0     0000f500  _out_Protect_Relay_ON                    
0     0000f501  _out_SMPS_reset                          
0     0000f502  _out_SAG_GEN_ON                          
0     0000f503  _out_SYS_Fault_ON                        
0     0000f504  _HW_Output_SIG_Check                     
0     0000f505  _out_nGate_Reset_ON                      
0     0000f506  _out_do_spare_ON                         
0     0000f508  ___TI_enable_exit_profile_output         
0     0000f50a  ___TI_cleanup_ptr                        
0     0000f50c  ___TI_dtors_ptr                          
0     0000f510  ___cinit__                               
0     0000f510  _cinit_runstart                          
0     0000f510  cinit                                    
0     0000f954  _PieVectTableInit                        
0     0000f954  _econst_runstart                         
0     0000fb14  _FlashBankInfo                           
0     0000fb84  _ramfuncs_runstart                       
0     0000fb84  _scia_tx_isr                             
0     0000fbb2  _scia_rx_isr                             
0     0000fc0f  _InitFlash_Bank0                         
0     0000fc38  _InitFlash_Bank1                         
0     0000fc61  _FlashOff_Bank0                          
0     0000fc6f  _FlashOff_Bank1                          
0     0000fc7d  _F28x_usDelay                            
0     0000fc84  _switch_runstart                         
0     00080000  code_start                               
0     00080004  _text_loadstart                          
0     00084a24  _cinit_loadstart                         
0     00084e68  _econst_loadstart                        
0     00085098  _ramfuncs_loadstart                      
0     00085198  _switch_loadstart                        
0     000851b8  copy_sections                            
1     00000b00  _AdcaResultRegs                          
1     00000b20  _AdcbResultRegs                          
1     00000b40  _AdccResultRegs                          
1     00000b60  _AdcdResultRegs                          
1     00000c00  _CpuTimer0Regs                           
1     00000c08  _CpuTimer1Regs                           
1     00000c10  _CpuTimer2Regs                           
1     00000ce0  _PieCtrlRegs                             
1     00000d00  _EmuBMode                                
1     00000d00  _PieVectTable                            
1     00000d01  _EmuBootPins                             
1     00001000  _DmaRegs                                 
1     00001400  _Cla1Regs                                
1     00004000  _EPwm1Regs                               
1     00004100  _EPwm2Regs                               
1     00004200  _EPwm3Regs                               
1     00004300  _EPwm4Regs                               
1     00004400  _EPwm5Regs                               
1     00004500  _EPwm6Regs                               
1     00004600  _EPwm7Regs                               
1     00004700  _EPwm8Regs                               
1     00004800  _EPwm9Regs                               
1     00004900  _EPwm10Regs                              
1     00004a00  _EPwm11Regs                              
1     00004b00  _EPwm12Regs                              
1     00005000  _ECap1Regs                               
1     00005020  _ECap2Regs                               
1     00005040  _ECap3Regs                               
1     00005060  _ECap4Regs                               
1     00005080  _ECap5Regs                               
1     000050a0  _ECap6Regs                               
1     00005100  _EQep1Regs                               
1     00005140  _EQep2Regs                               
1     00005180  _EQep3Regs                               
1     00005c00  _DacaRegs                                
1     00005c10  _DacbRegs                                
1     00005c20  _DaccRegs                                
1     00005c80  _Cmpss1Regs                              
1     00005ca0  _Cmpss2Regs                              
1     00005cc0  _Cmpss3Regs                              
1     00005ce0  _Cmpss4Regs                              
1     00005d00  _Cmpss5Regs                              
1     00005d20  _Cmpss6Regs                              
1     00005d40  _Cmpss7Regs                              
1     00005d60  _Cmpss8Regs                              
1     00005e00  _Sdfm1Regs                               
1     00005e80  _Sdfm2Regs                               
1     00006000  _McbspaRegs                              
1     00006040  _McbspbRegs                              
1     00006100  _SpiaRegs                                
1     00006110  _SpibRegs                                
1     00006120  _SpicRegs                                
1     00006200  _UppRegs                                 
1     00007000  _WdRegs                                  
1     00007060  _NmiIntruptRegs                          
1     00007070  _XintRegs                                
1     00007200  _SciaRegs                                
1     00007210  _ScibRegs                                
1     00007220  _ScicRegs                                
1     00007230  _ScidRegs                                
1     00007300  _I2caRegs                                
1     00007340  _I2cbRegs                                
1     00007400  _AdcaRegs                                
1     00007480  _AdcbRegs                                
1     00007500  _AdccRegs                                
1     00007580  _AdcdRegs                                
1     00007900  _InputXbarRegs                           
1     00007920  _XbarRegs                                
1     00007940  _SyncSocRegs                             
1     00007980  _DmaClaSrcSelRegs                        
1     00007a00  _EPwmXbarRegs                            
1     00007a80  _OutputXbarRegs                          
1     00007c00  _GpioCtrlRegs                            
1     00007f00  _GpioDataRegs                            
1     00047000  _Emif1Regs                               
1     00047800  _Emif2Regs                               
1     00050024  _FlashPumpSemaphoreRegs                  
1     0005d000  _DevCfgRegs                              
1     0005d180  _AnalogSubsysRegs                        
1     0005d200  _ClkCfgRegs                              
1     0005d300  _CpuSysRegs                              
1     0005e608  _RomPrefetchRegs                         
1     0005f000  _DcsmZ1Regs                              
1     0005f040  _DcsmZ2Regs                              
1     0005f070  _DcsmCommonRegs                          
1     0005f400  _MemCfgRegs                              
1     0005f480  _Emif1ConfigRegs                         
1     0005f4a0  _Emif2ConfigRegs                         
1     0005f4c0  _AccessProtectionRegs                    
1     0005f500  _MemoryErrorRegs                         
1     0005f540  _RomWaitStateRegs                        
1     0005f800  _Flash0CtrlRegs                          
1     0005fb00  _Flash0EccRegs                           
1     0005fc00  _Flash1CtrlRegs                          
1     0005ff00  _Flash1EccRegs                           
abs   00000000  _pinit_size                              
abs   00000020  _switch_size                             
abs   000000fd  _ramfuncs_size                           
abs   00000200  __STACK_SIZE                             
abs   00000230  _econst_size                             
abs   00000441  _cinit_size                              
abs   00004a1e  _text_size                               
abs   ffffffff  ___TI_pprof_out_hndl                     
abs   ffffffff  ___TI_prof_data_size                     
abs   ffffffff  ___TI_prof_data_start                    
abs   ffffffff  ___binit__                               
abs   ffffffff  ___c_args__                              
abs   ffffffff  ___pinit__                               
abs   ffffffff  binit                                    
abs   ffffffff  pinit                                    

[743 symbols]