Site Index
Support Home
Emulators Home
C2000 Drivers
C3x/C4x Drivers
C5000 Drivers
C6000 Drivers
OMAP Drivers
Utilities
Ordering Info.
Emulator Site Support Site Main Site
### SDFlash Utility Description SDFlash is a Windows GUI based utility that allows the user to flash program a DSP Target using a Spectrum Digital JTAG Emulator. Each target requires Flash programming algorithms specific to that specific DSP and the Flash memory on that board. Installation Two parts are required in the SDFlash installation; (a)SDFlash GUI, (b)Device specific flashing algorithms. SDFlash is distributed as component of the standard Spectrum Digital Emulation drivers. This is the same emulation driver installation that is used to support Code Composer Studio. If a current release of Spectrum Digital emulation drivers is already installed, only the flashing algorithms are required to finish the installation. If an old version of SDFlash or our emulation drivers is currently installed, un-install the older version, then install the latest drivers. Use the table below to locate the flashing algortithms that best suit the target system that will be programmed. Download the algorithms and install (or unzip) thim to the SDFlash\myprojects directory shown below: -CCS v3.3 directory: C:\CCStudio_v3.3\specdig\SDFlash\myprojects -CCS v4.x directory: C:\Program Files\Texas Instruments\ccsv4\emulation\specdig\sdflash\myprojects * These are the default Code Composer Studio install directories, modify the path to match your instal Directory if it is different Once the driver installation has completed, there will be a blue, square icon on the desktop titled 'SDFlash'. The SDFlash Utility can be launched from this icon. If the icon is not present, then the SDFlash can be launched from the SDFlash.exe located in the install directory as follows: -CCS v3.3 directory: C:\CCStudio_v3.3\specdig\SDFlash\bin -CCS v4.x directory: C:\Program Files\Texas Instruments\ccsv4\emulation\specdig\sdflash\bin Documentation SDFlash FAQ
C2800 Family
Release Date | Description | Utility
Sept 20, 2011 | SDFlash and Prog28x v1.65 update to support device unlock after reset. Prog28x includes source code. Replace your current CCSv4 or CCSv5 SDFlash directory with the update. The F28xx algorithms will enable unlocking as by setting the PMSTAddress field to non-zero value. | Download Prog28x SRC
C2800 Family
Release Date | Description | Algorithms
August 5, 2009 | C2834x SDFlash Algos V1.0 for programming external Flash connected via XINTF | Download Readme
June 8, 2009 | C2834x SDFlash Algos V1.0 for programming external SPI Serial EEPROM or Flash connected via SPI-A. | Download Readme
March 17, 2009 | F2803x SDFlash JTAG algos. Uses TI F2803x Flash API 1.0. | Download Readme
March 10, 2009 | F2802x SDFlash JTAG algos. Uses TI F2802x Flash API 1.0. | Download Readme
September 5, 2008 | V3.3 SDFlash serial patch for flash programming via an RS232 serial link. Includes algos for F280x, F2804x, F281x, F2833x, and F2823x devices. Uses TI F281x Flash API V2.10, TI F280x Flash API V1.00, TI F280x Flash API V3.02, TI F2833x Flash API V2.10, and TI F2823x Flash API V2.10. Requires SDFlash v1.60 or later. All previous serial algos are obsolete and not recommended. | Download Readme
August 18, 2008 | F2833x SDFlash JTAG algos. Uses TI F2833x Flash API V2.1. | Download Readme
August 7, 2008 | F2823x SDFlash JTAG algos. Uses TI F2823x Flash API V2.1. | Download Readme
October 31, 2006 | F2801x SDFlash JTAG algos. Uses TI F28015/F28016 Flash API V1.00. | Download Readme
August 15, 2006 | F2804x SDFlash JTAG algos. Uses TI F28044 Flash API V1.00. | Download Readme
July 28, 2006 | F280x SDFlash JTAG algos. Uses TI F2809 Flash API V1.00 and F2808/F2806/F2802/F2801 Flash API V3.02. All previous JTAG algos are obsolete and not recommended. | Download Readme
August 5, 2005 | V4.1 F2812/F2811/F2810 JTAG Algos for Rev C silicon and later, (TMP/TMS). Uses TI F281x Flash API V2.10. All previous JTAG algos are obsolete and not recommended. | Download Readme
March 30, 2007 | V3.1 SDFlash serial patch for flash programming via an RS232 serial link. Includes algos for F280x, F2804x, and F281x devices. Uses TI F281x Flash API V2.10, TI F280x Flash API V1.00, and TI F280x Flash API V3.02. Requires SDFlash v1.60 or later. All previous serial algos are obsolete and not recommended. | Download Readme
21-Jun-2004 | F281x Algos for SPI Serial EEPROM connected to SPI-A> | Download Readme
08-Jun-2002 | F2812/F2811/F2810 Algos for Rev A silicon. | Download
C2400 Family
Release Date | Description | Algorithms
26-Oct-2005 | TMS320LF2401A: Requires SDFlash v1.62.03 or higher. See "Introduction to SDFlash (C24XX)" below for details. | Download
26-Oct-2005 | TMS320LF2407A: Requires SDFlash v1.62.03 or higher. See "Introduction to SDFlash (C24XX)" below for details. | Download
22-July-2004 | SDFlash v1.62.03. Replaces SDFlash.exe that is installed in C2000 Driver release v2.20.03. Unzip into \specdig\sdflash\bin. SDFlash version 1.63 is included in emulation driver install version 2.21 and higher. | Download
13-Oct-2003 | TMS32F241, TMS320F243 | Download
| ©Copyright 2002-2014 Spectrum Digital, Inc. All Rights Reserved. |