Issue description:
  The XRS PIN reversed twice within 1ms while customer doing the TMS320F280049PZQ power down test, and the VDDIO(3.3V) is keep falling down,  customer used RC filter in XRS pin.

[image: cid:image018.jpg@01D3D31E.434FF6F0]
Figure 1 XRS PIN test waveform
CH1: XRS pin   CH3: VDDIO（3.3V）

Support Need:
[bookmark: _GoBack]  Could you kindly help give comments on the reason the XRS reversed twice during power off within 1ms? And comments for external circuit design of XRS connection?

   [image: cid:image020.png@01D3D31E.434FF6F0]
Figure 2： external schematic of XRS pin
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