MotorWare f2806x Module API Documentation

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- c
- d
- e
- f
- g
- h
- i
- l
- m
- o
- p
- q
- r
- s
- t
- u
- v

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - u -

- usDelay() : usDelay.h
- use_all : svgen_current.h
- USER_calcPIgains() : 32b/user.c
- USER_checkForErrors() : 32b/user.c
- USER_computeFlux() : 32b/user.c
- USER_computeFlux_pu_to_VpHz_sf() : 32b/user.c
- USER_computeFlux_pu_to_Wb_sf() : 32b/user.c
- USER_computeTorque_Flux_Iq_pu_to_Nm_sf() : 32b/user.c
- USER_computeTorque_lbin() : 32b/user.c
- USER_computeTorque_Ls_Id_Iq_pu_to_Nm_sf() : 32b/user.c
- USER_computeTorque_Nm() : 32b/user.c
- USER_ErrorCode_ctrlFreq_Hz_High : fast/src/32b/userParams.h
- USER_ErrorCode_ctrlFreq_Hz_Low : fast/src/32b/userParams.h
- USER_ErrorCode_ctrlPeriod_sec_High : fast/src/32b/userParams.h
- USER_ErrorCode_ctrlPeriod_sec_Low : fast/src/32b/userParams.h
- USER_ErrorCode_current_sf_High : fast/src/32b/userParams.h
- USER_ErrorCode_current_sf_Low : fast/src/32b/userParams.h
- USER_ErrorCode_dcBusPole_rps_High : fast/src/32b/userParams.h
- USER_ErrorCode_dcBusPole_rps_Low : fast/src/32b/userParams.h
- USER_ErrorCode_directionPole_rps_High : fast/src/32b/userParams.h
- USER_ErrorCode_directionPole_rps_Low : fast/src/32b/userParams.h
- USER_ErrorCode_e : fast/src/32b/userParams.h
- USER_ErrorCode_estFreq_Hz_High : fast/src/32b/userParams.h
- USER_ErrorCode_estFreq_Hz_Low : fast/src/32b/userParams.h
- USER_ErrorCode_estKappa_High : fast/src/32b/userParams.h
- USER_ErrorCode_estKappa_Low : fast/src/32b/userParams.h
- USER_ErrorCode_fluxEstFreq_Hz_High : fast/src/32b/userParams.h
- USER_ErrorCode_fluxEstFreq_Hz_Low : fast/src/32b/userParams.h
- USER_ErrorCode_fluxFraction_High : fast/src/32b/userParams.h
- USER_ErrorCode_fluxFraction_Low : fast/src/32b/userParams.h
- USER_ErrorCode_fluxPole_rps_High : fast/src/32b/userParams.h
- USER_ErrorCode_fluxPole_rps_Low : fast/src/32b/userParams.h
- USER_ErrorCode_forceAngleFreq_Hz_High : fast/src/32b/userParams.h
- USER_ErrorCode_forceAngleFreq_Hz_Low : fast/src/32b/userParams.h
- USER_ErrorCode_IdRated_delta_High : fast/src/32b/userParams.h
- USER_ErrorCode_IdRated_delta_Low : fast/src/32b/userParams.h
- USER_ErrorCode_IdRated_High : fast/src/32b/userParams.h
- USER_ErrorCode_IdRated_Low : fast/src/32b/userParams.h
- USER_ErrorCode_IdRatedFraction_indEst_High : fast/src/32b/userParams.h
- USER_ErrorCode_IdRatedFraction_indEst_Low : fast/src/32b/userParams.h
- USER_ErrorCode_IdRatedFraction_ratedFlux_High : fast/src/32b/userParams.h
- USER_ErrorCode_IdRatedFraction_ratedFlux_Low : fast/src/32b/userParams.h
- USER_ErrorCode_indEst_speedMaxFraction_High : fast/src/32b/userParams.h
- USER_ErrorCode_indEst_speedMaxFraction_Low : fast/src/32b/userParams.h
- USER_ErrorCode_iqFullScaleCurrent_A_High : fast/src/32b/userParams.h
- USER_ErrorCode_iqFullScaleCurrent_A_Low : fast/src/32b/userParams.h
- USER_ErrorCode_iqFullScaleFreq_Hz_High : fast/src/32b/userParams.h
- USER_ErrorCode_iqFullScaleFreq_Hz_Low : fast/src/32b/userParams.h
- USER_ErrorCode_iqFullScaleVoltage_V_High : fast/src/32b/userParams.h
- USER_ErrorCode_iqFullScaleVoltage_V_Low : fast/src/32b/userParams.h
- USER_ErrorCode_maxAccel_est_Hzps_High : fast/src/32b/userParams.h
- USER_ErrorCode_maxAccel_est_Hzps_Low : fast/src/32b/userParams.h
- USER_ErrorCode_maxAccel_Hzps_High : fast/src/32b/userParams.h
- USER_ErrorCode_maxAccel_Hzps_Low : fast/src/32b/userParams.h
- USER_ErrorCode_maxCurrent_High : fast/src/32b/userParams.h
- USER_ErrorCode_maxCurrent_indEst_High : fast/src/32b/userParams.h
- USER_ErrorCode_maxCurrent_indEst_Low : fast/src/32b/userParams.h
- USER_ErrorCode_maxCurrent_Low : fast/src/32b/userParams.h
- USER_ErrorCode_maxCurrent_resEst_High : fast/src/32b/userParams.h
- USER_ErrorCode_maxCurrent_resEst_Low : fast/src/32b/userParams.h
- USER_ErrorCode_maxCurrentSlope_High : fast/src/32b/userParams.h
- USER_ErrorCode_maxCurrentSlope_Low : fast/src/32b/userParams.h
- USER_ErrorCode_maxCurrentSlope_powerWarp_High : fast/src/32b/userParams.h
- USER_ErrorCode_maxCurrentSlope_powerWarp_Low : fast/src/32b/userParams.h
- USER_ErrorCode_maxNegativeIdCurrent_a_High : fast/src/32b/userParams.h
- USER_ErrorCode_maxNegativeIdCurrent_a_Low : fast/src/32b/userParams.h
- USER_ErrorCode_maxVsMag_pu_High : fast/src/32b/userParams.h
- USER_ErrorCode_maxVsMag_pu_Low : fast/src/32b/userParams.h
- USER_ErrorCode_motor_Ls_d_High : fast/src/32b/userParams.h
- USER_ErrorCode_motor_Ls_d_Low : fast/src/32b/userParams.h
- USER_ErrorCode_motor_Ls_q_High : fast/src/32b/userParams.h
- USER_ErrorCode_motor_Ls_q_Low : fast/src/32b/userParams.h
- USER_ErrorCode_motor_numPolePairs_High : fast/src/32b/userParams.h
- USER_ErrorCode_motor_numPolePairs_Low : fast/src/32b/userParams.h
- USER_ErrorCode_motor_ratedFlux_High : fast/src/32b/userParams.h
- USER_ErrorCode_motor_ratedFlux_Low : fast/src/32b/userParams.h
- USER_ErrorCode_motor_Rr_High : fast/src/32b/userParams.h
- USER_ErrorCode_motor_Rr_Low : fast/src/32b/userParams.h
- USER_ErrorCode_motor_Rs_High : fast/src/32b/userParams.h
- USER_ErrorCode_motor_Rs_Low : fast/src/32b/userParams.h
- USER_ErrorCode_motor_type_Unknown : fast/src/32b/userParams.h
- USER_ErrorCode_NoError : fast/src/32b/userParams.h
- USER_ErrorCode_numCtrlTicksPerCurrentTick_High : fast/src/32b/userParams.h
- USER_ErrorCode_numCtrlTicksPerCurrentTick_Low : fast/src/32b/userParams.h
- USER_ErrorCode_numCtrlTicksPerEstTick_High : fast/src/32b/userParams.h
- USER_ErrorCode_numCtrlTicksPerEstTick_Low : fast/src/32b/userParams.h
- USER_ErrorCode_numCtrlTicksPerSpeedTick_High : fast/src/32b/userParams.h
- USER_ErrorCode_numCtrlTicksPerSpeedTick_Low : fast/src/32b/userParams.h
- USER_ErrorCode_numCtrlTicksPerTrajTick_High : fast/src/32b/userParams.h
- USER_ErrorCode_numCtrlTicksPerTrajTick_Low : fast/src/32b/userParams.h
- USER_ErrorCode_numCurrentSensors_High : fast/src/32b/userParams.h
- USER_ErrorCode_numCurrentSensors_Low : fast/src/32b/userParams.h
- USER_ErrorCode_numIsrTicksPerCtrlTick_High : fast/src/32b/userParams.h
- USER_ErrorCode_numIsrTicksPerCtrlTick_Low : fast/src/32b/userParams.h
- USER_ErrorCode_numPwmTicksPerIsrTick_High : fast/src/32b/userParams.h
- USER_ErrorCode_numPwmTicksPerIsrTick_Low : fast/src/32b/userParams.h
- USER_ErrorCode_numVoltageSensors_High : fast/src/32b/userParams.h
- USER_ErrorCode_numVoltageSensors_Low : fast/src/32b/userParams.h
- USER_ErrorCode_offsetPole_rps_High : fast/src/32b/userParams.h
- USER_ErrorCode_offsetPole_rps_Low : fast/src/32b/userParams.h
- USER_ErrorCode_powerWarpGain_High : fast/src/32b/userParams.h
- USER_ErrorCode_powerWarpGain_Low : fast/src/32b/userParams.h
- USER_ErrorCode_pwmFreq_kHz_High : fast/src/32b/userParams.h
- USER_ErrorCode_pwmFreq_kHz_Low : fast/src/32b/userParams.h
- USER_ErrorCode_RoverL_estFreq_Hz_High : fast/src/32b/userParams.h
- USER_ErrorCode_RoverL_estFreq_Hz_Low : fast/src/32b/userParams.h
- USER_ErrorCode_speedPole_rps_High : fast/src/32b/userParams.h
- USER_ErrorCode_speedPole_rps_Low : fast/src/32b/userParams.h
- USER_ErrorCode_systemFreq_MHz_High : fast/src/32b/userParams.h
- USER_ErrorCode_systemFreq_MHz_Low : fast/src/32b/userParams.h
- USER_ErrorCode_trajFreq_Hz_High : fast/src/32b/userParams.h
- USER_ErrorCode_trajFreq_Hz_Low : fast/src/32b/userParams.h
- USER_ErrorCode_voltage_sf_High : fast/src/32b/userParams.h
- USER_ErrorCode_voltage_sf_Low : fast/src/32b/userParams.h
- USER_ErrorCode_voltageFilterPole_Hz_High : fast/src/32b/userParams.h
- USER_ErrorCode_voltageFilterPole_Hz_Low : fast/src/32b/userParams.h
- USER_ErrorCode_zeroSpeedLimit_High : fast/src/32b/userParams.h
- USER_ErrorCode_zeroSpeedLimit_Low : fast/src/32b/userParams.h
- USER_getErrorCode() : 32b/user.c
- USER_numErrorCodes : fast/src/32b/userParams.h
- USER_Params : user/src/32b/userParams.h , user/src/float/userParams.h , fast/src/32b/userParams.h
- USER_setErrorCode() : 32b/user.c
- USER_setParams() : 32b/user.c , float/user.c
- USER_softwareUpdate1p6() : 32b/user.c