MotorWare f2806x Module API Documentation

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - s -

- s0 : ST_PosConv_t , ST_PosPlan_t , ST_VelId_t , ST_VelPlan_t
- s1 : ST_PosCtl_t , ST_VelCtl_t , ST_VelMove_t
- s4 : ST_PosMove_t
- sample_count : _ENC_Obj_
- sample_period : _ENC_Obj_
- sample_time : _SLIP_Obj_
- SampleTimeOverTimeConst : ST_PosConvCfg_t
- SecureROM : ST_Ver_t
- Sensorless : ST_VelIdCfg_t
- sinTh : _IPARK_Obj_ , _PARK_Obj_
- size : _DLOG_4CH_
- skip_cntr : _DLOG_4CH_
- SlipVel : ST_PosConv_t
- spd_max : _CTRL_Obj_
- spd_out : _CTRL_Obj_
- spd_ref : _CTRL_Obj_
- speed_cutoff : _ENC_Obj_
- speed_fb_Hz : _CTRL_Obj_
- speed_fb_pu : _CTRL_Obj_
- speed_gain : _ENC_Obj_
- speed_lpf_cx : _ENC_Obj_
- speed_lpf_cy : _ENC_Obj_
- speed_lpf_out : _ENC_Obj_
- speed_out_A : _CTRL_Obj_
- speed_outMax_A : _CTRL_Obj_
- speed_outMax_pu : _CTRL_Obj_
- speed_outMin_A : _CTRL_Obj_
- speed_ref_Hz : _CTRL_Obj_ , _EST_InputData_
- speed_ref_pu : _CTRL_Obj_
- speed_rps : _ANGLE_Obj_
- speedCtrlPeriod_sec : _CTRL_Obj_
- speedEst_rps : _ANGLE_Obj_
- speedPole_rps : _USER_Params_
- spiA : _HAL_Obj_
- spiAHandle : _HAL_Obj_
- spiB : _HAL_Obj_
- spiBHandle : _HAL_Obj_
- state : _CAL_Obj_ , _CTRL_Obj_
- STATUS : ST_PosConv_t , ST_PosCtl_t , ST_PosMove_t , ST_PosPlan_t , ST_VelCtl_t , ST_VelId_t , ST_VelMove_t , ST_VelPlan_t
- svgen : _CTRL_Obj_
- svgenHandle : _CTRL_Obj_
- systemFreq_MHz : _USER_Params_