MotorWare f2806x Driver API Documentation

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- c
- d
- e
- f
- g
- i
- l
- o
- p
- q
- s
- t
- u
- w

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - s -

- SCI_BaudRate_115_2_kBaud : sci.h
- SCI_BaudRate_19_2_kBaud : sci.h
- SCI_BaudRate_57_6_kBaud : sci.h
- SCI_BaudRate_9_6_kBaud : sci.h
- SCI_BaudRate_e : sci.h
- SCI_CharLength_1_Bit : sci.h
- SCI_CharLength_2_Bits : sci.h
- SCI_CharLength_3_Bits : sci.h
- SCI_CharLength_4_Bits : sci.h
- SCI_CharLength_5_Bits : sci.h
- SCI_CharLength_6_Bits : sci.h
- SCI_CharLength_7_Bits : sci.h
- SCI_CharLength_8_Bits : sci.h
- SCI_CharLength_e : sci.h
- SCI_clearAutoBaudDetect() : sci.h , sci.c
- SCI_clearRxFifoInt() : sci.c , sci.h
- SCI_clearRxFifoOvf() : sci.c , sci.h
- SCI_clearTxFifoInt() : sci.c , sci.h
- SCI_disable() : sci.c , sci.h
- SCI_disableAutoBaudAlign() : sci.c , sci.h
- SCI_disableLoopBack() : sci.c , sci.h
- SCI_disableParity() : sci.c , sci.h
- SCI_disableRx() : sci.h , sci.c
- SCI_disableRxErrorInt() : sci.c , sci.h
- SCI_disableRxFifoInt() : sci.c , sci.h
- SCI_disableRxInt() : sci.c , sci.h
- SCI_disableSleep() : sci.c , sci.h
- SCI_disableTx() : sci.c , sci.h
- SCI_disableTxFifoEnh() : sci.c , sci.h
- SCI_disableTxFifoInt() : sci.c , sci.h
- SCI_disableTxInt() : sci.c , sci.h
- SCI_disableTxWake() : sci.c , sci.h
- SCI_enable() : sci.c , sci.h
- SCI_enableAutoBaudAlign() : sci.c , sci.h
- SCI_enableChannels() : sci.c , sci.h
- SCI_enableLoopBack() : sci.c , sci.h
- SCI_enableParity() : sci.c , sci.h
- SCI_enableRx() : sci.c , sci.h
- SCI_enableRxErrorInt() : sci.h , sci.c
- SCI_enableRxFifo() : sci.c , sci.h
- SCI_enableRxFifoInt() : sci.c , sci.h
- SCI_enableRxInt() : sci.c , sci.h
- SCI_enableSleep() : sci.c , sci.h
- SCI_enableTx() : sci.c , sci.h
- SCI_enableTxFifo() : sci.c , sci.h
- SCI_enableTxFifoEnh() : sci.c , sci.h
- SCI_enableTxFifoInt() : sci.c , sci.h
- SCI_enableTxInt() : sci.c , sci.h
- SCI_enableTxWake() : sci.c , sci.h
- SCI_FifoLevel_1_Word : sci.h
- SCI_FifoLevel_2_Words : sci.h
- SCI_FifoLevel_3_Words : sci.h
- SCI_FifoLevel_4_Words : sci.h
- SCI_FifoLevel_e : sci.h
- SCI_FifoLevel_Empty : sci.h
- SCI_FifoStatus_1_Word : sci.h
- SCI_FifoStatus_2_Words : sci.h
- SCI_FifoStatus_3_Words : sci.h
- SCI_FifoStatus_4_Words : sci.h
- SCI_FifoStatus_e : sci.h
- SCI_FifoStatus_Empty : sci.h
- SCI_getDataBlocking() : sci.c , sci.h
- SCI_getDataNonBlocking() : sci.c , sci.h
- SCI_getRxFifoStatus() : sci.c , sci.h
- SCI_getTxFifoStatus() : sci.c , sci.h
- SCI_Handle : sci.h
- SCI_init() : sci.c , sci.h
- SCI_Mode_AddressBit : sci.h
- SCI_Mode_e : sci.h
- SCI_Mode_IdleLine : sci.h
- SCI_NumStopBits_e : sci.h
- SCI_NumStopBits_One : sci.h
- SCI_NumStopBits_Two : sci.h
- SCI_Obj : sci.h
- SCI_Parity_e : sci.h
- SCI_Parity_Even : sci.h
- SCI_Parity_Odd : sci.h
- SCI_Priority_AfterRxRxSeq : sci.h
- SCI_Priority_e : sci.h
- SCI_Priority_FreeRun : sci.h
- SCI_Priority_Immediate : sci.h
- SCI_putDataBlocking() : sci.c , sci.h
- SCI_putDataNonBlocking() : sci.c , sci.h
- SCI_read() : sci.h
- SCI_reset() : sci.h , sci.c
- SCI_resetChannels() : sci.c , sci.h
- SCI_resetRxFifo() : sci.c , sci.h
- SCI_resetTxFifo() : sci.c , sci.h
- SCI_rxDataReady() : sci.h
- SCI_SCICCR_CHAR_LENGTH_BITS : sci.h
- SCI_SCICCR_LB_ENA_BITS : sci.h
- SCI_SCICCR_MODE_BITS : sci.h
- SCI_SCICCR_PARITY_BITS : sci.h
- SCI_SCICCR_PARITY_ENA_BITS : sci.h
- SCI_SCICCR_STOP_BITS : sci.h
- SCI_SCICTL1_RESET_BITS : sci.h
- SCI_SCICTL1_RX_ERR_INT_ENA_BITS : sci.h
- SCI_SCICTL1_RXENA_BITS : sci.h
- SCI_SCICTL1_SLEEP_BITS : sci.h
- SCI_SCICTL1_TXENA_BITS : sci.h
- SCI_SCICTL1_TXWAKE_BITS : sci.h
- SCI_SCICTL2_RX_INT_ENA_BITS : sci.h
- SCI_SCICTL2_TX_INT_ENA_BITS : sci.h
- SCI_SCICTL2_TXEMPTY_BITS : sci.h
- SCI_SCICTL2_TXRDY_BITS : sci.h
- SCI_SCIFFCT_ABD_BITS : sci.h
- SCI_SCIFFCT_ABDCLR_BITS : sci.h
- SCI_SCIFFCT_CDC_BITS : sci.h
- SCI_SCIFFCT_DELAY_BITS : sci.h
- SCI_SCIFFRX_FIFO_OVF_BITS : sci.h
- SCI_SCIFFRX_FIFO_OVFCLR_BITS : sci.h
- SCI_SCIFFRX_FIFO_RESET_BITS : sci.h
- SCI_SCIFFRX_FIFO_ST_BITS : sci.h
- SCI_SCIFFRX_IENA_BITS : sci.h
- SCI_SCIFFRX_IL_BITS : sci.h
- SCI_SCIFFRX_INT_BITS : sci.h
- SCI_SCIFFRX_INTCLR_BITS : sci.h
- SCI_SCIFFTX_CHAN_RESET_BITS : sci.h
- SCI_SCIFFTX_FIFO_ENA_BITS : sci.h
- SCI_SCIFFTX_FIFO_RESET_BITS : sci.h
- SCI_SCIFFTX_FIFO_ST_BITS : sci.h
- SCI_SCIFFTX_IENA_BITS : sci.h
- SCI_SCIFFTX_IL_BITS : sci.h
- SCI_SCIFFTX_INT_BITS : sci.h
- SCI_SCIFFTX_INTCLR_BITS : sci.h
- SCI_SCIRXST_BRKDT_BITS : sci.h
- SCI_SCIRXST_FE_BITS : sci.h
- SCI_SCIRXST_OE_BITS : sci.h
- SCI_SCIRXST_PE_BITS : sci.h
- SCI_SCIRXST_RXERROR_BITS : sci.h
- SCI_SCIRXST_RXRDY_BITS : sci.h
- SCI_SCIRXST_RXWAKE_BITS : sci.h
- SCI_setBaudRate() : sci.c , sci.h
- SCI_setCharLength() : sci.c , sci.h
- SCI_setMode() : sci.c , sci.h
- SCI_setNumStopBits() : sci.c , sci.h
- SCI_setParity() : sci.c , sci.h
- SCI_setPriority() : sci.c , sci.h
- SCI_setRxFifoIntLevel() : sci.c , sci.h
- SCI_setTxDelay() : sci.c , sci.h
- SCI_setTxFifoIntLevel() : sci.c , sci.h
- SCI_txReady() : sci.h
- SCI_write() : sci.h
- SCIA_BASE_ADDR : sci.h
- SCIB_BASE_ADDR : sci.h
- SPI_BaudRate_1_MBaud : spi.h
- SPI_BaudRate_e : spi.h
- SPI_BaudRate_LSPCLK_Over_Four : spi.h
- SPI_CharLength_10_Bits : spi.h
- SPI_CharLength_11_Bits : spi.h
- SPI_CharLength_12_Bits : spi.h
- SPI_CharLength_13_Bits : spi.h
- SPI_CharLength_14_Bits : spi.h
- SPI_CharLength_15_Bits : spi.h
- SPI_CharLength_16_Bits : spi.h
- SPI_CharLength_1_Bit : spi.h
- SPI_CharLength_2_Bits : spi.h
- SPI_CharLength_3_Bits : spi.h
- SPI_CharLength_4_Bits : spi.h
- SPI_CharLength_5_Bits : spi.h
- SPI_CharLength_6_Bits : spi.h
- SPI_CharLength_7_Bits : spi.h
- SPI_CharLength_8_Bits : spi.h
- SPI_CharLength_9_Bits : spi.h
- SPI_CharLength_e : spi.h
- SPI_clearRxFifoInt() : spi.c , spi.h
- SPI_clearRxFifoOvf() : spi.c , spi.h
- SPI_clearTxFifoInt() : spi.c , spi.h
- SPI_ClkPhase_Delayed : spi.h
- SPI_ClkPhase_e : spi.h
- SPI_ClkPhase_Normal : spi.h
- SPI_ClkPolarity_e : spi.h
- SPI_ClkPolarity_OutputFallingEdge_InputRisingEdge : spi.h
- SPI_ClkPolarity_OutputRisingEdge_InputFallingEdge : spi.h
- SPI_disableInt() : spi.c , spi.h
- SPI_disableLoopBack() : spi.c , spi.h
- SPI_disableOverRunInt() : spi.c , spi.h
- SPI_disableRxFifoInt() : spi.c , spi.h
- SPI_disableTx() : spi.c , spi.h
- SPI_disableTxFifoEnh() : spi.c , spi.h
- SPI_disableTxFifoInt() : spi.c , spi.h
- SPI_EmulationSuspend_e : spi.h
- SPI_enable() : spi.c , spi.h
- SPI_enableChannels() : spi.h , spi.c
- SPI_enableInt() : spi.c , spi.h
- SPI_enableLoopBack() : spi.h , spi.c
- SPI_enableOverRunInt() : spi.c , spi.h
- SPI_enableRxFifo() : spi.c , spi.h
- SPI_enableRxFifoInt() : spi.c , spi.h
- SPI_enableTx() : spi.c , spi.h
- SPI_enableTxFifo() : spi.c , spi.h
- SPI_enableTxFifoEnh() : spi.h , spi.c
- SPI_enableTxFifoInt() : spi.c , spi.h
- SPI_FifoLevel_1_Word : spi.h
- SPI_FifoLevel_2_Words : spi.h
- SPI_FifoLevel_3_Words : spi.h
- SPI_FifoLevel_4_Words : spi.h
- SPI_FifoLevel_e : spi.h
- SPI_FifoLevel_Empty : spi.h
- SPI_FifoStatus_1_Word : spi.h
- SPI_FifoStatus_2_Words : spi.h
- SPI_FifoStatus_3_Words : spi.h
- SPI_FifoStatus_4_Words : spi.h
- SPI_FifoStatus_e : spi.h
- SPI_FifoStatus_Empty : spi.h
- SPI_getIntFlagStatus() : spi.c , spi.h
- SPI_getRxFifoStatus() : spi.c , spi.h
- SPI_getTxBufferStatus() : spi.c , spi.h
- SPI_getTxFifoStatus() : spi.c , spi.h
- SPI_Handle : spi.h
- SPI_init() : spi.h , spi.c
- SPI_IntFlagStatus_Completed : spi.h
- SPI_IntFlagStatus_e : spi.h
- SPI_IntFlagStatus_InProgress : spi.h
- SPI_Mode_e : spi.h
- SPI_Mode_Master : spi.h
- SPI_Mode_Slave : spi.h
- SPI_Obj : spi.h
- SPI_Priority_AfterRxRxSeq : spi.h
- SPI_Priority_e : spi.h
- SPI_Priority_FreeRun : spi.h
- SPI_Priority_Immediate : spi.h
- SPI_read() : spi.h
- SPI_readEmu() : spi.h
- SPI_reset() : spi.c , spi.h
- SPI_resetChannels() : spi.c , spi.h
- SPI_resetRxFifo() : spi.c , spi.h
- SPI_resetTxFifo() : spi.c , spi.h
- SPI_setBaudRate() : spi.h , spi.c
- SPI_setCharLength() : spi.h , spi.c
- SPI_setClkPhase() : spi.h , spi.c
- SPI_setClkPolarity() : spi.c , spi.h
- SPI_setMode() : spi.h , spi.c
- SPI_setPriority() : spi.h , spi.c
- SPI_setRxFifoIntLevel() : spi.c , spi.h
- SPI_setSteInv() : spi.c , spi.h
- SPI_setSuspend() : spi.h , spi.c
- SPI_setTriWire() : spi.c , spi.h
- SPI_setTxDelay() : spi.h , spi.c
- SPI_setTxFifoIntLevel() : spi.c , spi.h
- SPI_SPICCR_CHAR_LENGTH_BITS : spi.h
- SPI_SPICCR_CLKPOL_BITS : spi.h
- SPI_SPICCR_RESET_BITS : spi.h
- SPI_SPICCR_SPILBK_BITS : spi.h
- SPI_SPICTL_CLK_PHASE_BITS : spi.h
- SPI_SPICTL_INT_ENA_BITS : spi.h
- SPI_SPICTL_MODE_BITS : spi.h
- SPI_SPICTL_OVRRUN_INT_ENA_BITS : spi.h
- SPI_SPICTL_TALK_BITS : spi.h
- SPI_SPIFFRX_FIFO_OVF_BITS : spi.h
- SPI_SPIFFRX_FIFO_OVFCLR_BITS : spi.h
- SPI_SPIFFRX_FIFO_RESET_BITS : spi.h
- SPI_SPIFFRX_FIFO_ST_BITS : spi.h
- SPI_SPIFFRX_IENA_BITS : spi.h
- SPI_SPIFFRX_IL_BITS : spi.h
- SPI_SPIFFRX_INT_BITS : spi.h
- SPI_SPIFFRX_INTCLR_BITS : spi.h
- SPI_SPIFFTX_CHAN_RESET_BITS : spi.h
- SPI_SPIFFTX_FIFO_ENA_BITS : spi.h
- SPI_SPIFFTX_FIFO_RESET_BITS : spi.h
- SPI_SPIFFTX_FIFO_ST_BITS : spi.h
- SPI_SPIFFTX_IENA_BITS : spi.h
- SPI_SPIFFTX_IL_BITS : spi.h
- SPI_SPIFFTX_INT_BITS : spi.h
- SPI_SPIFFTX_INTCLR_BITS : spi.h
- SPI_SPIPRI_STE_INV_BITS : spi.h
- SPI_SPIPRI_SUSP_BITS : spi.h
- SPI_SPIPRI_TRIWIRE : spi.h
- SPI_SPIST_INTFLAG_BITS : spi.h
- SPI_SPIST_TXBUF_BITS : spi.h
- SPI_SteInv_ActiveHigh : spi.h
- SPI_SteInv_ActiveLow : spi.h
- SPI_SteInv_e : spi.h
- SPI_TriWire_e : spi.h
- SPI_TriWire_NormalFourWire : spi.h
- SPI_TriWire_ThreeWire : spi.h
- SPI_TxBufferStatus_e : spi.h
- SPI_TxBufferStatus_Empty : spi.h
- SPI_TxBufferStatus_Full : spi.h
- SPI_TxSuspend_00 : spi.h
- SPI_TxSuspend_10 : spi.h
- SPI_TxSuspend_free : spi.h
- SPI_write() : spi.h
- SPI_write8() : spi.h
- SPIA_BASE_ADDR : spi.h
- SPIB_BASE_ADDR : spi.h