MotorWare f2806x Driver API Documentation

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- c
- d
- e
- f
- g
- i
- l
- o
- p
- q
- s
- t
- u
- w

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - g -

- GPIO_0_Mode_EPWM1A : gpio.h
- GPIO_0_Mode_GeneralPurpose : gpio.h
- GPIO_0_Mode_Rsvd_2 : gpio.h
- GPIO_0_Mode_Rsvd_3 : gpio.h
- GPIO_10_Mode_ADCSOCBO_NOT : gpio.h
- GPIO_10_Mode_EPWM6A : gpio.h
- GPIO_10_Mode_GeneralPurpose : gpio.h
- GPIO_10_Mode_Rsvd_2 : gpio.h
- GPIO_11_Mode_ECAP1 : gpio.h
- GPIO_11_Mode_EPWM6B : gpio.h
- GPIO_11_Mode_GeneralPurpose : gpio.h
- GPIO_11_Mode_SCIRXDB : gpio.h
- GPIO_12_Mode_GeneralPurpose : gpio.h
- GPIO_12_Mode_SCITXDA : gpio.h
- GPIO_12_Mode_SPISIMOB : gpio.h
- GPIO_12_Mode_TZ1_NOT : gpio.h
- GPIO_13_Mode_GeneralPurpose : gpio.h
- GPIO_13_Mode_Rsvd_2 : gpio.h
- GPIO_13_Mode_SPISOMIB : gpio.h
- GPIO_13_Mode_TZ2_NOT : gpio.h
- GPIO_14_Mode_GeneralPurpose : gpio.h
- GPIO_14_Mode_SCITXDB : gpio.h
- GPIO_14_Mode_SPICLKB : gpio.h
- GPIO_14_Mode_TZ3_NOT : gpio.h
- GPIO_15_Mode_ECAP2 : gpio.h
- GPIO_15_Mode_GeneralPurpose : gpio.h
- GPIO_15_Mode_SCIRXDB : gpio.h
- GPIO_15_Mode_SPISTEB_NOT : gpio.h
- GPIO_16_Mode_GeneralPurpose : gpio.h
- GPIO_16_Mode_Rsvd_2 : gpio.h
- GPIO_16_Mode_SPISIMOA : gpio.h
- GPIO_16_Mode_TZ2_NOT : gpio.h
- GPIO_17_Mode_GeneralPurpose : gpio.h
- GPIO_17_Mode_Rsvd_2 : gpio.h
- GPIO_17_Mode_SPISOMIA : gpio.h
- GPIO_17_Mode_TZ3_NOT : gpio.h
- GPIO_18_Mode_GeneralPurpose : gpio.h
- GPIO_18_Mode_SCITXDB : gpio.h
- GPIO_18_Mode_SPICLKA : gpio.h
- GPIO_18_Mode_XCLKOUT : gpio.h
- GPIO_19_Mode_ECAP1 : gpio.h
- GPIO_19_Mode_GeneralPurpose : gpio.h
- GPIO_19_Mode_SCIRXDB : gpio.h
- GPIO_19_Mode_SPISTEA_NOT : gpio.h
- GPIO_1_Mode_COMP1OUT : gpio.h
- GPIO_1_Mode_EPWM1B : gpio.h
- GPIO_1_Mode_GeneralPurpose : gpio.h
- GPIO_1_Mode_Rsvd_2 : gpio.h
- GPIO_20_Mode_COMP1OUT : gpio.h
- GPIO_20_Mode_EQEP1A : gpio.h
- GPIO_20_Mode_GeneralPurpose : gpio.h
- GPIO_20_Mode_MDXA : gpio.h
- GPIO_21_Mode_COMP2OUT : gpio.h
- GPIO_21_Mode_EQEP1B : gpio.h
- GPIO_21_Mode_GeneralPurpose : gpio.h
- GPIO_21_Mode_MDRA : gpio.h
- GPIO_22_Mode_EQEP1S : gpio.h
- GPIO_22_Mode_GeneralPurpose : gpio.h
- GPIO_22_Mode_MCLKXA : gpio.h
- GPIO_22_Mode_SCITXDB : gpio.h
- GPIO_23_Mode_EQEP1I : gpio.h
- GPIO_23_Mode_GeneralPurpose : gpio.h
- GPIO_23_Mode_MFSXA : gpio.h
- GPIO_23_Mode_SCIRXDB : gpio.h
- GPIO_24_Mode_ECAP1 : gpio.h
- GPIO_24_Mode_EQEP2A : gpio.h
- GPIO_24_Mode_GeneralPurpose : gpio.h
- GPIO_24_Mode_SPISIMOB : gpio.h
- GPIO_25_Mode_ECAP2 : gpio.h
- GPIO_25_Mode_EQEP2B : gpio.h
- GPIO_25_Mode_GeneralPurpose : gpio.h
- GPIO_25_Mode_SPISOMIB : gpio.h
- GPIO_26_Mode_ECAP3 : gpio.h
- GPIO_26_Mode_EQEP2I : gpio.h
- GPIO_26_Mode_GeneralPurpose : gpio.h
- GPIO_26_Mode_SPICLKB : gpio.h
- GPIO_27_Mode_EQEP2S : gpio.h
- GPIO_27_Mode_GeneralPurpose : gpio.h
- GPIO_27_Mode_HRCAP2 : gpio.h
- GPIO_27_Mode_SPISTEB_NOT : gpio.h
- GPIO_28_Mode_GeneralPurpose : gpio.h
- GPIO_28_Mode_SCIRXDA : gpio.h
- GPIO_28_Mode_SDDA : gpio.h
- GPIO_28_Mode_TZ2_NOT : gpio.h
- GPIO_29_Mode_GeneralPurpose : gpio.h
- GPIO_29_Mode_SCITXDA : gpio.h
- GPIO_29_Mode_SCLA : gpio.h
- GPIO_29_Mode_TZ3_NOT : gpio.h
- GPIO_2_Mode_EPWM2A : gpio.h
- GPIO_2_Mode_GeneralPurpose : gpio.h
- GPIO_2_Mode_Rsvd_2 : gpio.h
- GPIO_2_Mode_Rsvd_3 : gpio.h
- GPIO_30_Mode_CANRXA : gpio.h
- GPIO_30_Mode_EPWM7A : gpio.h
- GPIO_30_Mode_EQEP2I : gpio.h
- GPIO_30_Mode_GeneralPurpose : gpio.h
- GPIO_31_Mode_CANTXA : gpio.h
- GPIO_31_Mode_EPWM8A : gpio.h
- GPIO_31_Mode_EQEP2S : gpio.h
- GPIO_31_Mode_GeneralPurpose : gpio.h
- GPIO_32_Mode_ADCSOCAO_NOT : gpio.h
- GPIO_32_Mode_EPWMSYNCI : gpio.h
- GPIO_32_Mode_GeneralPurpose : gpio.h
- GPIO_32_Mode_SDAA : gpio.h
- GPIO_33_Mode_ADCSOCBO_NOT : gpio.h
- GPIO_33_Mode_EPWMSYNCO : gpio.h
- GPIO_33_Mode_GeneralPurpose : gpio.h
- GPIO_33_Mode_SCLA : gpio.h
- GPIO_34_Mode_COMP2OUT : gpio.h
- GPIO_34_Mode_COMP3OUT : gpio.h
- GPIO_34_Mode_GeneralPurpose : gpio.h
- GPIO_34_Mode_Rsvd_2 : gpio.h
- GPIO_35_Mode_JTAG_TDI : gpio.h
- GPIO_35_Mode_Rsvd_1 : gpio.h
- GPIO_35_Mode_Rsvd_2 : gpio.h
- GPIO_35_Mode_Rsvd_3 : gpio.h
- GPIO_36_Mode_JTAG_TMS : gpio.h
- GPIO_36_Mode_Rsvd_1 : gpio.h
- GPIO_36_Mode_Rsvd_2 : gpio.h
- GPIO_36_Mode_Rsvd_3 : gpio.h
- GPIO_37_Mode_JTAG_TDO : gpio.h
- GPIO_37_Mode_Rsvd_1 : gpio.h
- GPIO_37_Mode_Rsvd_2 : gpio.h
- GPIO_37_Mode_Rsvd_3 : gpio.h
- GPIO_38_Mode_JTAG_TCK : gpio.h
- GPIO_38_Mode_Rsvd_1 : gpio.h
- GPIO_38_Mode_Rsvd_2 : gpio.h
- GPIO_38_Mode_Rsvd_3 : gpio.h
- GPIO_39_Mode_GeneralPurpose : gpio.h
- GPIO_39_Mode_Rsvd_1 : gpio.h
- GPIO_39_Mode_Rsvd_2 : gpio.h
- GPIO_39_Mode_Rsvd_3 : gpio.h
- GPIO_3_Mode_COMP2OUT : gpio.h
- GPIO_3_Mode_EPWM2B : gpio.h
- GPIO_3_Mode_GeneralPurpose : gpio.h
- GPIO_3_Mode_SPISOMIA : gpio.h
- GPIO_40_Mode_EPWM7A : gpio.h
- GPIO_40_Mode_GeneralPurpose : gpio.h
- GPIO_40_Mode_Rsvd_3 : gpio.h
- GPIO_40_Mode_SCITXDB : gpio.h
- GPIO_41_Mode_EPWM7B : gpio.h
- GPIO_41_Mode_GeneralPurpose : gpio.h
- GPIO_41_Mode_Rsvd_3 : gpio.h
- GPIO_41_Mode_SCIRXDB : gpio.h
- GPIO_42_Mode_COMP1OUT : gpio.h
- GPIO_42_Mode_EPWM8A : gpio.h
- GPIO_42_Mode_GeneralPurpose : gpio.h
- GPIO_42_Mode_TZ1_NOT : gpio.h
- GPIO_43_Mode_COMP2OUT : gpio.h
- GPIO_43_Mode_EPWM8B : gpio.h
- GPIO_43_Mode_GeneralPurpose : gpio.h
- GPIO_43_Mode_TZ2_NOT : gpio.h
- GPIO_44_Mode_EPWM7B : gpio.h
- GPIO_44_Mode_GeneralPurpose : gpio.h
- GPIO_44_Mode_MFSRA : gpio.h
- GPIO_44_Mode_SCIRXDB : gpio.h
- GPIO_4_Mode_EPWM3A : gpio.h
- GPIO_4_Mode_GeneralPurpose : gpio.h
- GPIO_4_Mode_Rsvd_2 : gpio.h
- GPIO_4_Mode_Rsvd_3 : gpio.h
- GPIO_50_Mode_EQEP1A : gpio.h
- GPIO_50_Mode_GeneralPurpose : gpio.h
- GPIO_50_Mode_MDXA : gpio.h
- GPIO_50_Mode_TZ1_NOT : gpio.h
- GPIO_51_Mode_EQEP1B : gpio.h
- GPIO_51_Mode_GeneralPurpose : gpio.h
- GPIO_51_Mode_MDRA : gpio.h
- GPIO_51_Mode_TZ2_NOT : gpio.h
- GPIO_52_Mode_EQEP1S : gpio.h
- GPIO_52_Mode_GeneralPurpose : gpio.h
- GPIO_52_Mode_MCLKXA : gpio.h
- GPIO_52_Mode_TZ3_NOT : gpio.h
- GPIO_53_Mode_EQEP1I : gpio.h
- GPIO_53_Mode_GeneralPurpose : gpio.h
- GPIO_53_Mode_MFSXA : gpio.h
- GPIO_53_Mode_Rsvd_1 : gpio.h
- GPIO_54_Mode_EQEP2A : gpio.h
- GPIO_54_Mode_GeneralPurpose : gpio.h
- GPIO_54_Mode_HRCAP1 : gpio.h
- GPIO_54_Mode_SPISIMOA : gpio.h
- GPIO_55_Mode_EQEP2B : gpio.h
- GPIO_55_Mode_GeneralPurpose : gpio.h
- GPIO_55_Mode_HRCAP2 : gpio.h
- GPIO_55_Mode_SPISOMIA : gpio.h
- GPIO_56_Mode_EQEP2I : gpio.h
- GPIO_56_Mode_GeneralPurpose : gpio.h
- GPIO_56_Mode_HRCAP3 : gpio.h
- GPIO_56_Mode_SPICLKA : gpio.h
- GPIO_57_Mode_EQEP2S : gpio.h
- GPIO_57_Mode_GeneralPurpose : gpio.h
- GPIO_57_Mode_HRCAP4 : gpio.h
- GPIO_57_Mode_SPISTEA_NOT : gpio.h
- GPIO_58_Mode_EPWM7A : gpio.h
- GPIO_58_Mode_GeneralPurpose : gpio.h
- GPIO_58_Mode_MCLKRA : gpio.h
- GPIO_58_Mode_SCITXDB : gpio.h
- GPIO_5_Mode_ECAP1 : gpio.h
- GPIO_5_Mode_EPWM3B : gpio.h
- GPIO_5_Mode_GeneralPurpose : gpio.h
- GPIO_5_Mode_SPISIMOA : gpio.h
- GPIO_6_Mode_EPWM4A : gpio.h
- GPIO_6_Mode_EPWMSYNCI : gpio.h
- GPIO_6_Mode_EPWMSYNCO : gpio.h
- GPIO_6_Mode_GeneralPurpose : gpio.h
- GPIO_7_Mode_ECAP2 : gpio.h
- GPIO_7_Mode_EPWM4B : gpio.h
- GPIO_7_Mode_GeneralPurpose : gpio.h
- GPIO_7_Mode_SCIRXDA : gpio.h
- GPIO_8_Mode_ADCSOCAO_NOT : gpio.h
- GPIO_8_Mode_EPWM5A : gpio.h
- GPIO_8_Mode_GeneralPurpose : gpio.h
- GPIO_8_Mode_Rsvd_2 : gpio.h
- GPIO_9_Mode_ECAP3 : gpio.h
- GPIO_9_Mode_EPWM5B : gpio.h
- GPIO_9_Mode_GeneralPurpose : gpio.h
- GPIO_9_Mode_SCITXDB : gpio.h
- GPIO_BASE_ADDR : gpio.h
- GPIO_Direction_e : gpio.h
- GPIO_Direction_Input : gpio.h
- GPIO_Direction_Output : gpio.h
- GPIO_getData() : gpio.c , gpio.h
- GPIO_getPortData() : gpio.c , gpio.h
- GPIO_GPMUX_CONFIG_BITS : gpio.h
- GPIO_GPMUX_NUMGPIOS_PER_REG : gpio.h
- GPIO_GPxCTRL_QUALPRDx_BITS : gpio.h
- GPIO_GPxCTRL_QUALPRDx_NUMBITS_PER_REG : gpio.h
- GPIO_GPxQSELx_NUMGPIOS_PER_REG : gpio.h
- GPIO_GPxQSELy_GPIOx_BITS : gpio.h
- GPIO_Handle : gpio.h
- GPIO_init() : gpio.h , gpio.c
- GPIO_lpmSelect() : gpio.h , gpio.c
- GPIO_Mode_e : gpio.h
- GPIO_Number_0 : gpio.h
- GPIO_Number_1 : gpio.h
- GPIO_Number_10 : gpio.h
- GPIO_Number_11 : gpio.h
- GPIO_Number_12 : gpio.h
- GPIO_Number_13 : gpio.h
- GPIO_Number_14 : gpio.h
- GPIO_Number_15 : gpio.h
- GPIO_Number_16 : gpio.h
- GPIO_Number_17 : gpio.h
- GPIO_Number_18 : gpio.h
- GPIO_Number_19 : gpio.h
- GPIO_Number_2 : gpio.h
- GPIO_Number_20 : gpio.h
- GPIO_Number_21 : gpio.h
- GPIO_Number_22 : gpio.h
- GPIO_Number_23 : gpio.h
- GPIO_Number_24 : gpio.h
- GPIO_Number_25 : gpio.h
- GPIO_Number_26 : gpio.h
- GPIO_Number_27 : gpio.h
- GPIO_Number_28 : gpio.h
- GPIO_Number_29 : gpio.h
- GPIO_Number_3 : gpio.h
- GPIO_Number_30 : gpio.h
- GPIO_Number_31 : gpio.h
- GPIO_Number_32 : gpio.h
- GPIO_Number_33 : gpio.h
- GPIO_Number_34 : gpio.h
- GPIO_Number_35 : gpio.h
- GPIO_Number_36 : gpio.h
- GPIO_Number_37 : gpio.h
- GPIO_Number_38 : gpio.h
- GPIO_Number_39 : gpio.h
- GPIO_Number_4 : gpio.h
- GPIO_Number_40 : gpio.h
- GPIO_Number_41 : gpio.h
- GPIO_Number_42 : gpio.h
- GPIO_Number_43 : gpio.h
- GPIO_Number_44 : gpio.h
- GPIO_Number_5 : gpio.h
- GPIO_Number_50 : gpio.h
- GPIO_Number_51 : gpio.h
- GPIO_Number_52 : gpio.h
- GPIO_Number_53 : gpio.h
- GPIO_Number_54 : gpio.h
- GPIO_Number_55 : gpio.h
- GPIO_Number_56 : gpio.h
- GPIO_Number_57 : gpio.h
- GPIO_Number_58 : gpio.h
- GPIO_Number_6 : gpio.h
- GPIO_Number_7 : gpio.h
- GPIO_Number_8 : gpio.h
- GPIO_Number_9 : gpio.h
- GPIO_Number_e : gpio.h
- GPIO_numGpios : gpio.h
- GPIO_Obj : gpio.h
- GPIO_Port_A : gpio.h
- GPIO_Port_B : gpio.h
- GPIO_Port_e : gpio.h
- GPIO_Pullup_Disable : gpio.h
- GPIO_Pullup_e : gpio.h
- GPIO_Pullup_Enable : gpio.h
- GPIO_Qual_ASync : gpio.h
- GPIO_Qual_e : gpio.h
- GPIO_Qual_Sample_3 : gpio.h
- GPIO_Qual_Sample_6 : gpio.h
- GPIO_Qual_Sync : gpio.h
- GPIO_read() : gpio.c , gpio.h
- GPIO_setDirection() : gpio.c , gpio.h
- GPIO_setExtInt() : gpio.h , gpio.c
- GPIO_setHigh() : gpio.h , gpio.c
- GPIO_setLow() : gpio.h , gpio.c
- GPIO_setMode() : gpio.c , gpio.h
- GPIO_setPortData() : gpio.c , gpio.h
- GPIO_setPullup() : gpio.h , gpio.c
- GPIO_setQualification() : gpio.h , gpio.c
- GPIO_setQualificationPeriod() : gpio.h , gpio.c
- GPIO_toggle() : gpio.h , gpio.c