MotorWare f2806x Driver API Documentation

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- c
- d
- e
- f
- g
- i
- l
- o
- p
- q
- s
- t
- u
- w

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - d -

- DevEmuRegs : emu.h
- DINT : cpu.h
- DISABLE_INTERRUPTS : cpu.h
- DISABLE_PROTECTED_REGISTER_WRITE_MODE : cpu.h
- DRTM : cpu.h
- DRV8301_ADDR_MASK : drv8301.h
- DRV8301_buildCtrlWord() : drv8301.h
- DRV8301_CTRL1_GATE_CURRENT_BITS : drv8301.h
- DRV8301_CTRL1_GATE_RESET_BITS : drv8301.h
- DRV8301_CTRL1_OC_ADJ_SET_BITS : drv8301.h
- DRV8301_CTRL1_OC_MODE_BITS : drv8301.h
- DRV8301_CTRL1_PWM_MODE_BITS : drv8301.h
- DRV8301_CTRL2_DC_CAL_1_BITS : drv8301.h
- DRV8301_CTRL2_DC_CAL_2_BITS : drv8301.h
- DRV8301_CTRL2_GAIN_BITS : drv8301.h
- DRV8301_CTRL2_OC_TOFF_BITS : drv8301.h
- DRV8301_CTRL2_OCTW_SET_BITS : drv8301.h
- DRV8301_CtrlMode_e : drv8301.h
- DRV8301_CtrlMode_Read : drv8301.h
- DRV8301_CtrlMode_Write : drv8301.h
- DRV8301_DATA_MASK : drv8301.h
- DRV8301_DcCalMode_Ch1_Load : drv8301.h
- DRV8301_DcCalMode_Ch1_NoLoad : drv8301.h
- DRV8301_DcCalMode_Ch2_Load : drv8301.h
- DRV8301_DcCalMode_Ch2_NoLoad : drv8301.h
- DRV8301_DcCalMode_e : drv8301.h
- DRV8301_enable() : drv8301.c , drv8301.h
- DRV8301_FAULT_TYPE_MASK : drv8301.h
- DRV8301_FaultType_e : drv8301.h
- DRV8301_FaultType_FETHA_OC : drv8301.h
- DRV8301_FaultType_FETHB_OC : drv8301.h
- DRV8301_FaultType_FETHC_OC : drv8301.h
- DRV8301_FaultType_FETLA_OC : drv8301.h
- DRV8301_FaultType_FETLB_OC : drv8301.h
- DRV8301_FaultType_FETLC_OC : drv8301.h
- DRV8301_FaultType_GVDD_OV : drv8301.h
- DRV8301_FaultType_GVDD_UV : drv8301.h
- DRV8301_FaultType_NoFault : drv8301.h
- DRV8301_FaultType_OTSD : drv8301.h
- DRV8301_FaultType_OTW : drv8301.h
- DRV8301_FaultType_PVDD_UV : drv8301.h
- DRV8301_getDcCalMode() : drv8301.c , drv8301.h
- DRV8301_getFaultType() : drv8301.c , drv8301.h
- DRV8301_getId() : drv8301.c , drv8301.h
- DRV8301_GETID : drv8301.h
- DRV8301_getOcLevel() : drv8301.c , drv8301.h
- DRV8301_getOcMode() : drv8301.c , drv8301.h
- DRV8301_getOcOffTimeMode() : drv8301.c , drv8301.h
- DRV8301_getOcTwMode() : drv8301.c , drv8301.h
- DRV8301_getPeakCurrent() : drv8301.c , drv8301.h
- DRV8301_getPwmMode() : drv8301.c , drv8301.h
- DRV8301_getShuntAmpGain() : drv8301.c , drv8301.h
- DRV8301_getStatusRegister1() : drv8301.h
- DRV8301_getStatusRegister2() : drv8301.h
- DRV8301_Handle : drv8301.h
- DRV8301_init() : drv8301.c , drv8301.h
- DRV8301_isFault() : drv8301.c , drv8301.h
- DRV8301_isReset() : drv8301.c , drv8301.h
- DRV8301_Obj : drv8301.h
- DRV8301_OcMode_CurrentLimit : drv8301.h
- DRV8301_OcMode_Disabled : drv8301.h
- DRV8301_OcMode_e : drv8301.h
- DRV8301_OcMode_LatchShutDown : drv8301.h
- DRV8301_OcMode_ReportOnly : drv8301.h
- DRV8301_OcOffTimeMode_Ctrl : drv8301.h
- DRV8301_OcOffTimeMode_e : drv8301.h
- DRV8301_OcOffTimeMode_Normal : drv8301.h
- DRV8301_OcTwMode_Both : drv8301.h
- DRV8301_OcTwMode_e : drv8301.h
- DRV8301_OcTwMode_OC_Only : drv8301.h
- DRV8301_OcTwMode_OT_Only : drv8301.h
- DRV8301_PeakCurrent_0p25_A : drv8301.h
- DRV8301_PeakCurrent_0p70_A : drv8301.h
- DRV8301_PeakCurrent_1p70_A : drv8301.h
- DRV8301_PeakCurrent_e : drv8301.h
- DRV8301_PwmMode_e : drv8301.h
- DRV8301_PwmMode_Six_Inputs : drv8301.h
- DRV8301_PwmMode_Three_Inputs : drv8301.h
- DRV8301_readData() : drv8301.c , drv8301.h
- DRV8301_readSpi() : drv8301.c , drv8301.h
- DRV8301_RegName_Control_1 : drv8301.h
- DRV8301_RegName_Control_2 : drv8301.h
- DRV8301_RegName_e : drv8301.h
- DRV8301_RegName_Status_1 : drv8301.h
- DRV8301_RegName_Status_2 : drv8301.h
- DRV8301_reset() : drv8301.h , drv8301.c
- DRV8301_Reset_All : drv8301.h
- DRV8301_Reset_e : drv8301.h
- DRV8301_Reset_Normal : drv8301.h
- DRV8301_resetEnableTimeout() : drv8301.h
- DRV8301_resetRxTimeout() : drv8301.h
- DRV8301_RW_MASK : drv8301.h
- DRV8301_setDcCalMode() : drv8301.h , drv8301.c
- DRV8301_setGpioHandle() : drv8301.c , drv8301.h
- DRV8301_setGpioNumber() : drv8301.c , drv8301.h
- DRV8301_setOcLevel() : drv8301.c , drv8301.h
- DRV8301_setOcMode() : drv8301.h , drv8301.c
- DRV8301_setOcOffTimeMode() : drv8301.c , drv8301.h
- DRV8301_setOcTwMode() : drv8301.h , drv8301.c
- DRV8301_setPeakCurrent() : drv8301.c , drv8301.h
- DRV8301_setPwmMode() : drv8301.h , drv8301.c
- DRV8301_setShuntAmpGain() : drv8301.c , drv8301.h
- DRV8301_setSpiHandle() : drv8301.h , drv8301.c
- DRV8301_setupSpi() : drv8301.c , drv8301.h
- DRV8301_ShuntAmpGain_10VpV : drv8301.h
- DRV8301_ShuntAmpGain_20VpV : drv8301.h
- DRV8301_ShuntAmpGain_40VpV : drv8301.h
- DRV8301_ShuntAmpGain_80VpV : drv8301.h
- DRV8301_ShuntAmpGain_e : drv8301.h
- DRV8301_ShuntAmpNumber_1 : drv8301.h
- DRV8301_ShuntAmpNumber_2 : drv8301.h
- DRV8301_ShuntAmpNumber_e : drv8301.h
- DRV8301_STATUS1_FAULT_BITS : drv8301.h
- DRV8301_STATUS1_FETHA_OC_BITS : drv8301.h
- DRV8301_STATUS1_FETHB_OC_BITS : drv8301.h
- DRV8301_STATUS1_FETHC_OC_BITS : drv8301.h
- DRV8301_STATUS1_FETLA_OC_BITS : drv8301.h
- DRV8301_STATUS1_FETLB_OC_BITS : drv8301.h
- DRV8301_STATUS1_FETLC_OC_BITS : drv8301.h
- DRV8301_STATUS1_GVDD_UV_BITS : drv8301.h
- DRV8301_STATUS1_OTSD_BITS : drv8301.h
- DRV8301_STATUS1_OTW_BITS : drv8301.h
- DRV8301_STATUS1_PVDD_UV_BITS : drv8301.h
- DRV8301_STATUS2_GVDD_OV_BITS : drv8301.h
- DRV8301_STATUS2_ID_BITS : drv8301.h
- DRV8301_VdsLevel_0p060_V : drv8301.h
- DRV8301_VdsLevel_0p068_V : drv8301.h
- DRV8301_VdsLevel_0p076_V : drv8301.h
- DRV8301_VdsLevel_0p086_V : drv8301.h
- DRV8301_VdsLevel_0p097_V : drv8301.h
- DRV8301_VdsLevel_0p109_V : drv8301.h
- DRV8301_VdsLevel_0p123_V : drv8301.h
- DRV8301_VdsLevel_0p138_V : drv8301.h
- DRV8301_VdsLevel_0p155_V : drv8301.h
- DRV8301_VdsLevel_0p175_V : drv8301.h
- DRV8301_VdsLevel_0p197_V : drv8301.h
- DRV8301_VdsLevel_0p222_V : drv8301.h
- DRV8301_VdsLevel_0p250_V : drv8301.h
- DRV8301_VdsLevel_0p282_V : drv8301.h
- DRV8301_VdsLevel_0p317_V : drv8301.h
- DRV8301_VdsLevel_0p358_V : drv8301.h
- DRV8301_VdsLevel_0p403_V : drv8301.h
- DRV8301_VdsLevel_0p454_V : drv8301.h
- DRV8301_VdsLevel_0p511_V : drv8301.h
- DRV8301_VdsLevel_0p576_V : drv8301.h
- DRV8301_VdsLevel_0p648_V : drv8301.h
- DRV8301_VdsLevel_0p730_V : drv8301.h
- DRV8301_VdsLevel_0p822_V : drv8301.h
- DRV8301_VdsLevel_0p926_V : drv8301.h
- DRV8301_VdsLevel_1p043_V : drv8301.h
- DRV8301_VdsLevel_1p175_V : drv8301.h
- DRV8301_VdsLevel_1p324_V : drv8301.h
- DRV8301_VdsLevel_1p491_V : drv8301.h
- DRV8301_VdsLevel_1p679_V : drv8301.h
- DRV8301_VdsLevel_1p892_V : drv8301.h
- DRV8301_VdsLevel_2p131_V : drv8301.h
- DRV8301_VdsLevel_2p400_V : drv8301.h
- DRV8301_VdsLevel_e : drv8301.h
- DRV8301_Word_t : drv8301.h
- DRV8301_writeData() : drv8301.h , drv8301.c
- DRV8301_writeSpi() : drv8301.c , drv8301.h
- Drv8301SpiOutputDataSelect_e : drv8301.h
- DRV_SPI_8301_CTRL1_t_ : drv8301.h
- DRV_SPI_8301_CTRL2_t_ : drv8301.h
- DRV_SPI_8301_Stat1_t_ : drv8301.h
- DRV_SPI_8301_Stat2_t_ : drv8301.h
- DRV_SPI_8301_Vars_t : drv8301.h