<?xml version="1.0" encoding="UTF-8" standalone="no"?>
<configurations XML_version="1.2" id="configurations_0">
        
    <configuration XML_version="1.2" id="configuration_0">
                
        <instance XML_version="1.2" desc="Texas Instruments XDS100v2 USB Debug Probe" href="connections/TIXDS100v2_Connection.xml" id="Texas Instruments XDS100v2 USB Debug Probe" xml="TIXDS100v2_Connection.xml" xmlpath="connections"/>
                
        <connection XML_version="1.2" id="Texas Instruments XDS100v2 USB Debug Probe">
                        
            <instance XML_version="1.2" href="drivers/tixds100v2icepick_c.xml" id="drivers" xml="tixds100v2icepick_c.xml" xmlpath="drivers"/>
                        
            <instance XML_version="1.2" href="drivers/tixds100v2c28x.xml" id="drivers" xml="tixds100v2c28x.xml" xmlpath="drivers"/>
                        
            <instance XML_version="1.2" href="drivers/tixds100v2cla2.xml" id="drivers" xml="tixds100v2cla2.xml" xmlpath="drivers"/>
                        
            <instance XML_version="1.2" href="drivers/tixds100v2cs_child.xml" id="drivers" xml="tixds100v2cs_child.xml" xmlpath="drivers"/>
                        
            <instance XML_version="1.2" href="drivers/tixds100v2cs_dap.xml" id="drivers" xml="tixds100v2cs_dap.xml" xmlpath="drivers"/>
                        
            <instance XML_version="1.2" href="drivers/tixds100v2cortexM.xml" id="drivers" xml="tixds100v2cortexM.xml" xmlpath="drivers"/>
                        
            <instance XML_version="1.2" href="drivers/tixds510ajsm.xml" id="drivers" xml="tixds510ajsm.xml" xmlpath="drivers"/>
                        
            <platform XML_version="1.2" id="platform_0">
                                
                <instance XML_version="1.2" desc="TMS320F28388D" href="devices/f28388d.xml" id="TMS320F28388D" xml="f28388d.xml" xmlpath="devices"/>
                                
                <device HW_revision="1" XML_version="1.2" description="" id="TMS320F28388D" partnum="TMS320F28388D" simulation="no">
                                        
                    <router HW_revision="1.0" XML_version="1.2" description="ICEPick_C router" id="IcePick_C_0" isa="ICEPICK_C">
                                                
                        <subpath id="Subpath_1">
                                                        
                            <property Type="numericfield" Value="0x11" desc="Port Number_0" id="Port Number"/>
                                                    
                        </subpath>
                                                
                        <subpath id="CM">
                                                        
                            <property Type="numericfield" Value="0x12" desc="Port Number_1" id="Port Number"/>
                                                    
                        </subpath>
                                            
                    </router>
                                    
                </device>
                            
            </platform>
                    
        </connection>
            
    </configuration>
    
</configurations>
