################################################################################
# Automatically-generated file. Do not edit!
################################################################################

SHELL = cmd.exe

# Add inputs and outputs from these tool invocations to the build variables 
CMD_SRCS += \
../28069_RAM_lnk.cmd \
F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/headers/cmd/F2806x_Headers_nonBIOS.cmd 

LIB_SRCS += \
F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/MWare/driverlib/Debug/driverlib.lib \
F:/ti/c2000/C2000Ware_1_00_03_00/libraries/communications/usb/f2806x/lib/usblib.lib 

ASM_SRCS += \
../F2806x_CodeStartBranch_ebss_init.asm \
F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/common/source/F2806x_usDelay.asm 

C_SRCS += \
F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/common/source/F2806x_DefaultIsr.c \
F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/headers/source/F2806x_GlobalVariableDefs.c \
F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/common/source/F2806x_PieCtrl.c \
F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/common/source/F2806x_PieVect.c \
F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/MWare/driverlib/sysctl.c \
../uartstdio.c \
F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/MWare/driverlib/usb.c \
../usb_dev_serial.c \
F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/MWare/driverlib/usb_hal.c \
../usb_serial_structs.c 

C_DEPS += \
./F2806x_DefaultIsr.d \
./F2806x_GlobalVariableDefs.d \
./F2806x_PieCtrl.d \
./F2806x_PieVect.d \
./sysctl.d \
./uartstdio.d \
./usb.d \
./usb_dev_serial.d \
./usb_hal.d \
./usb_serial_structs.d 

OBJS += \
./F2806x_CodeStartBranch_ebss_init.obj \
./F2806x_DefaultIsr.obj \
./F2806x_GlobalVariableDefs.obj \
./F2806x_PieCtrl.obj \
./F2806x_PieVect.obj \
./F2806x_usDelay.obj \
./sysctl.obj \
./uartstdio.obj \
./usb.obj \
./usb_dev_serial.obj \
./usb_hal.obj \
./usb_serial_structs.obj 

ASM_DEPS += \
./F2806x_CodeStartBranch_ebss_init.d \
./F2806x_usDelay.d 

OBJS__QUOTED += \
"F2806x_CodeStartBranch_ebss_init.obj" \
"F2806x_DefaultIsr.obj" \
"F2806x_GlobalVariableDefs.obj" \
"F2806x_PieCtrl.obj" \
"F2806x_PieVect.obj" \
"F2806x_usDelay.obj" \
"sysctl.obj" \
"uartstdio.obj" \
"usb.obj" \
"usb_dev_serial.obj" \
"usb_hal.obj" \
"usb_serial_structs.obj" 

C_DEPS__QUOTED += \
"F2806x_DefaultIsr.d" \
"F2806x_GlobalVariableDefs.d" \
"F2806x_PieCtrl.d" \
"F2806x_PieVect.d" \
"sysctl.d" \
"uartstdio.d" \
"usb.d" \
"usb_dev_serial.d" \
"usb_hal.d" \
"usb_serial_structs.d" 

ASM_DEPS__QUOTED += \
"F2806x_CodeStartBranch_ebss_init.d" \
"F2806x_usDelay.d" 

ASM_SRCS__QUOTED += \
"../F2806x_CodeStartBranch_ebss_init.asm" \
"F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/common/source/F2806x_usDelay.asm" 

C_SRCS__QUOTED += \
"F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/common/source/F2806x_DefaultIsr.c" \
"F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/headers/source/F2806x_GlobalVariableDefs.c" \
"F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/common/source/F2806x_PieCtrl.c" \
"F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/common/source/F2806x_PieVect.c" \
"F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/MWare/driverlib/sysctl.c" \
"../uartstdio.c" \
"F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/MWare/driverlib/usb.c" \
"../usb_dev_serial.c" \
"F:/ti/c2000/C2000Ware_1_00_03_00/device_support/f2806x/MWare/driverlib/usb_hal.c" \
"../usb_serial_structs.c" 


