[Header]
bq EVSW Version = 0.9.59	
DeviceName = bq20z95 v1.50
Time = 09/01/2018 10:29:58	


[Voltage(1st Level Safety)]
COV Threshold = 4250
COV Time = 2
COV Recovery = 4100
COV Delta = 20
COV Temp. Hys = 10.0
POV Threshold = 8500
POV Time = 2
POV Recovery = 8200
CUV Threshold = 2900
CUV Time = 2
CUV Recovery = 3000
PUV Threshold = 5800
PUV Time = 2
PUV Recovery = 6000
[Current(1st Level Safety)]
OC (1st Tier) Chg = 3200
OC (1st Tier) Chg Time = 2
OC Chg Recovery = 200
OC (1st Tier) Dsg = 6000
OC (1st Tier) Dsg Time = 2
OC Dsg Recovery = 200
OC (2nd Tier) Chg = 3500
OC (2nd Tier) Chg Time = 3
OC (2nd Tier) Dsg = 7000
OC (2nd Tier) Dsg Time = 2
Current Recovery Time = 8
AFE OC Dsg = 05
AFE OC Dsg Time = 0F
AFE OC Dsg Recovery = 5
AFE SC Chg Cfg = 64
AFE SC Dsg Cfg = 64
AFE SC Recovery = 1
[Temperature(1st Level Safety)]
Over Temp Chg = 45.0
OT Chg Time = 2
OT Chg Recovery = 40.0
Over Temp Dsg = 60.0
OT Dsg Time = 2
OT Dsg Recovery = 55.0
[Host Comm(1st Level Safety)]
Host Watchdog Timeout = 0

[Voltage(2nd Level Safety)]
SOV Threshold = 8800
SOV Time = 10
Cell Imbalance Current = 5
Cell Imbalance Fail Voltage = 1000
Cell Imbalance Time = 0
Battery Rest Time = 1800
Min CIM-check voltage = 3000
PFIN Detect Time = 0
[Current(2nd Level Safety)]
SOC Chg = 5000
SOC Chg Time = 5
SOC Dsg = 8000
SOC Dsg Time = 3
[Temperature(2nd Level Safety)]
SOT Chg = 65.0
SOT Chg Time = 5
SOT Dsg = 75.0
SOT Dsg Time = 5
Open Thermistor = -33.3
Open Time = 10
[FET Verification(2nd Level Safety)]
FET Fail Limit = 20
FET Fail Time = 0
[AFE Verification(2nd Level Safety)]
AFE Check Time = 0
AFE Fail Limit = 10
AFE Fail Recovery Time = 20
AFE Init Retry Limit = 6
AFE Init Limit = 20
[Fuse Verification(2nd Level Safety)]
Fuse Fail Limit = 2
Fuse Fail Time = 0

[Charge Inhibit Cfg(Charge Control)]
Chg Inhibit Temp Low = 0.0
Chg Inhibit Temp High = 48.0
Temp Hys = 1.0
[Pre-Charge Cfg(Charge Control)]
Pre-chg Current = 256
Pre-chg Temp = 12.0
Pre-chg Voltage = 2200
Recovery Voltage = 3000
[Fast Charge Cfg(Charge Control)]
Fast Charge Current = 2000
Charging Voltage = 8400
Delta Temp = 5.0
Suspend Low Temp = -5.0
Suspend High Temp = 55.0
[Pulse Charge Cfg(Charge Control)]
Turn ON Voltage = 4150
Turn OFF Voltage = 4250
Max ON Pulse Time = 0.00
Min OFF Pulse Time = 0.00
Max OFF Voltage = 4270
[Termination Cfg.(Charge Control)]
Maintenance Current = 0
Taper Current = 200
Taper Voltage = 300
Current Taper Window = 40
TCA Set % = -1
TCA Clear % = 95
FC Set % = -1
FC Clear % = 98
[Cell Balancing Cfg(Charge Control)]
Min Cell Deviation = 1750
[Charging Faults(Charge Control)]
Over Charging Voltage = 500
Over Charging Volt Time = 2
Over Charging Current = 500
Over Charging Curr Time = 2
Over Charging Curr Recov = 100
Depleted Voltage = 4000
Depleted Voltage Time = 2
Depleted Recovery = 4250
Over Charge Capacity = 300
Over Charge Recovery = 2
FC-MTO = 10800
PC-MTO = 3600
Charge Fault Cfg = 00

[Data(SBS Configuration)]
Rem Cap Alarm = 300
Rem Energy Alarm = 4320
Rem Time Alarm = 10
Init Battery Mode = 0081
Design Voltage = 7400
Spec Info = 0031
Manuf Date = 04-2017
Ser. Num. = 0001
Cycle Count = 3
CC Threshold = 3600
CC % = 90
CF MaxError Limit = 100
Design Capacity = 4000
Design Energy = 29600
Manuf Name =  ###
Device Name = ###
Device Chemistry = ###
[Configuration(SBS Configuration)]
TDA Set % = 6
TDA Clear % = 8
FD Set % = 2
FD Clear % = 5
TDA Set Volt Threshold = 5000
TDA Set Volt Time = 5
TDA Clear Volt = 5600
FD Set Volt Threshold = 6000
FD Volt Time = 5
FD Clear Volt = 6100

[Manufacturer Data(System Data)]
Pack Lot Code = 0000
PCB Lot Code = 0000
Firmware Version = ###
Hardware Revision = 0000
Cell Revision = 0000
[Manufacturer Info(System Data)]
Manuf. Info = 0123456789ABCDEF0123456789ABCDE
[Lifetime Data(System Data)]
Lifetime Max Temp = 53.8
Lifetime Min Temp = 12.9
Lifetime Max Cell Voltage = 6464
Lifetime Min Cell Voltage = 784
Lifetime Max Pack Voltage = 8400
Lifetime Min Pack Voltage = 6000
Lifetime Max Chg Current = 2004
Lifetime Max Dsg Current = -2413
Lifetime Max Chg Power = 16500
Lifetime Max Dsg Power = -16750
Life Max AvgDsg Cur = -1997
Life Max AvgDsg Pow = -1478
Lifetime Avg Temp = 21.5
[Lifetime Temp Samples(System Data)]
LT Temp Samples = 15014

[Registers(Configuration)]
Operation Cfg A = 0129
Operation Cfg B = 2D58
Operation Cfg C = 0005
Permanent Fail Cfg = 0000
Non-Removable Cfg = 0000
[AFE(Configuration)]
AFE.State_CTL = 00

[LED Cfg(LED Support)]
LED Flash Rate = 2.000
LED Blink Rate = 1.000
LED Delay = 48.8
LED Hold Time = 4
CHG Flash Alarm = 10
CHG Thresh 1 = 0
CHG Thresh 2 = 20
CHG Thresh 3 = 40
CHG Thresh 4 = 60
CHG Thresh 5 = 80
DSG Flash Alarm = 10
DSG Thresh 1 = 0
DSG Thresh 2 = 20
DSG Thresh 3 = 40
DSG Thresh 4 = 60
DSG Thresh 5 = 80
Sink Current = 3

[Power(Power)]
Flash Update OK Voltage = 6000
Shutdown Voltage = 5500
Shutdown Time = 10
Cell Shutdown Voltage = 2750
Cell Shutdown Time = 10
Charger Present = 3000
Sleep Current = 10
Bus Low Time = 5
Cal Inhibit Temp Low = 5.0
Cal Inhibit Temp High = 45.0
Sleep Voltage Time = 5
Sleep Current Time = 20
Wake Current Reg = 03

[IT Cfg(Gas Gauging)]
Load Select = 3
Load Mode = 0
Term Voltage = 6700
User Rate-mA = 0
User Rate-mW = 0
Reserve Cap-mAh = 0
Reserve Cap-mWh = 0
[Current Thresholds(Gas Gauging)]
Dsg Current Threshold = 100
Chg Current Threshold = 50
Quit Current = 10
Dsg Relax Time = 1
Chg Relax Time = 60
[State(Gas Gauging)]
Qmax Cell 0 = 4355
Qmax Cell 1 = 4347
Qmax Cell 2 = 4000
Qmax Cell 3 = 4000
Qmax Pack = 4347
Update Status = 06
Avg I Last Run = -801
Avg P Last Run = -607
Delta Voltage = 6

[R_a0(Ra Table)]
Cell0 R_a flag = 0055
Cell0 R_a 0 = 150
Cell0 R_a 1 = 179
Cell0 R_a 2 = 203
Cell0 R_a 3 = 193
Cell0 R_a 4 = 188
Cell0 R_a 5 = 184
Cell0 R_a 6 = 202
Cell0 R_a 7 = 207
Cell0 R_a 8 = 215
Cell0 R_a 9 = 202
Cell0 R_a 10 = 214
Cell0 R_a 11 = 257
Cell0 R_a 12 = 315
Cell0 R_a 13 = 164
Cell0 R_a 14 = 960
[R_a1(Ra Table)]
Cell1 R_a flag = 0000
Cell1 R_a 0 = 162
Cell1 R_a 1 = 192
Cell1 R_a 2 = 218
Cell1 R_a 3 = 209
Cell1 R_a 4 = 206
Cell1 R_a 5 = 197
Cell1 R_a 6 = 222
Cell1 R_a 7 = 229
Cell1 R_a 8 = 232
Cell1 R_a 9 = 218
Cell1 R_a 10 = 234
Cell1 R_a 11 = 286
Cell1 R_a 12 = 337
Cell1 R_a 13 = 179
Cell1 R_a 14 = 1058
[R_a2(Ra Table)]
Cell2 R_a flag = FF55
Cell2 R_a 0 = 142
Cell2 R_a 1 = 169
Cell2 R_a 2 = 194
Cell2 R_a 3 = 209
Cell2 R_a 4 = 163
Cell2 R_a 5 = 172
Cell2 R_a 6 = 198
Cell2 R_a 7 = 202
Cell2 R_a 8 = 190
Cell2 R_a 9 = 180
Cell2 R_a 10 = 200
Cell2 R_a 11 = 235
Cell2 R_a 12 = 284
Cell2 R_a 13 = 328
Cell2 R_a 14 = 1932
[R_a3(Ra Table)]
Cell3 R_a flag = FF55
Cell3 R_a 0 = 142
Cell3 R_a 1 = 169
Cell3 R_a 2 = 194
Cell3 R_a 3 = 209
Cell3 R_a 4 = 163
Cell3 R_a 5 = 172
Cell3 R_a 6 = 198
Cell3 R_a 7 = 202
Cell3 R_a 8 = 190
Cell3 R_a 9 = 180
Cell3 R_a 10 = 200
Cell3 R_a 11 = 235
Cell3 R_a 12 = 284
Cell3 R_a 13 = 328
Cell3 R_a 14 = 1932
[R_a0x(Ra Table)]
xCell0 R_a flag = 0000
xCell0 R_a 0 = 150
xCell0 R_a 1 = 179
xCell0 R_a 2 = 203
xCell0 R_a 3 = 193
xCell0 R_a 4 = 188
xCell0 R_a 5 = 184
xCell0 R_a 6 = 202
xCell0 R_a 7 = 207
xCell0 R_a 8 = 215
xCell0 R_a 9 = 202
xCell0 R_a 10 = 214
xCell0 R_a 11 = 257
xCell0 R_a 12 = 260
xCell0 R_a 13 = 135
xCell0 R_a 14 = 792
[R_a1x(Ra Table)]
xCell1 R_a flag = 0055
xCell1 R_a 0 = 162
xCell1 R_a 1 = 192
xCell1 R_a 2 = 218
xCell1 R_a 3 = 209
xCell1 R_a 4 = 206
xCell1 R_a 5 = 197
xCell1 R_a 6 = 222
xCell1 R_a 7 = 229
xCell1 R_a 8 = 232
xCell1 R_a 9 = 218
xCell1 R_a 10 = 234
xCell1 R_a 11 = 286
xCell1 R_a 12 = 337
xCell1 R_a 13 = 442
xCell1 R_a 14 = 2612
[R_a2x(Ra Table)]
xCell2 R_a flag = FFFF
xCell2 R_a 0 = 142
xCell2 R_a 1 = 169
xCell2 R_a 2 = 194
xCell2 R_a 3 = 209
xCell2 R_a 4 = 163
xCell2 R_a 5 = 172
xCell2 R_a 6 = 198
xCell2 R_a 7 = 202
xCell2 R_a 8 = 190
xCell2 R_a 9 = 180
xCell2 R_a 10 = 200
xCell2 R_a 11 = 235
xCell2 R_a 12 = 284
xCell2 R_a 13 = 328
xCell2 R_a 14 = 1932
[R_a3x(Ra Table)]
xCell3 R_a flag = FFFF
xCell3 R_a 0 = 142
xCell3 R_a 1 = 169
xCell3 R_a 2 = 194
xCell3 R_a 3 = 209
xCell3 R_a 4 = 163
xCell3 R_a 5 = 172
xCell3 R_a 6 = 198
xCell3 R_a 7 = 202
xCell3 R_a 8 = 190
xCell3 R_a 9 = 180
xCell3 R_a 10 = 200
xCell3 R_a 11 = 235
xCell3 R_a 12 = 284
xCell3 R_a 13 = 328
xCell3 R_a 14 = 1932

[Device Status Data(PF Status)]
PF Flags 1 = 0000
Fuse Flag = 00
PF Voltage = 0
PF C4 Voltage = 0
PF C3 Voltage = 0
PF C2 Voltage = 0
PF C1 Voltage = 0
PF Current = 0
PF Temperature = 0.0
PF Batt Stat = 00
PF RC-mAh = 0
PF RC-10mWh = 0
PF Chg Status = 0000
PF Safety Status = 0000
PF Flags 2 = 0000
[AFE Regs(PF Status)]
AFE Status = 00
AFE Output = 00
AFE State = 00
AFE Function = 00
AFE Cell Select = 00
AFE OLV = 00
AFE OLT = 00
AFE SCC = 00
AFE SCD = 00

[Data(Calibration)]
CC Gain = 10.328
CC Delta = 10.328
Ref Voltage = 1222.40
AFE Pack Gain = 740.26
CC Offset = -0.268
Board Offset = -46.1
Int Temp Offset = 0.0
Ext1 Temp Offset = -1.4
Ext2 Temp Offset = 0.0
[Config(Calibration)]
CC Current = 3000
Voltage Signal = 8400
Temp Signal = 298.0
CC Offset Time = 250
ADC Offset Time = 32
CC Gain Time = 250
Voltage Time = 1984
Temperature Time = 32
Cal Mode Timeout = 300
[Temp Model(Calibration)]
Ext Coef 1 = -28285
Ext Coef 2 = 20848
Ext Coef 3 = -7537
Ext Coef 4 = 401.2
Ext Min AD = 0
Ext Max Temp = 401.2
Int Coef 1 = 0
Int Coef 2 = 0
Int Coef 3 = -11136
Int Coef 4 = 575.4
Int Min AD = 0
Int Max Temp = 575.4
[Current(Calibration)]
Filter = 239
Deadband = 6
CC Deadband = 10.0
