|  |
| --- |
|  |
| CH1=VIN(37V), CH2=VSW | CH1=VOUT(48V), CH2=VSW |
| Audible sound is present but minimal. Tested till 240mA load.Sound is proportional to the amount of load. Max load requireemnt is 400mA.  |
| Schematic for the above waveforms |