|  |  |
| --- | --- |
|  | |
| CH1=VIN(37V), CH2=VSW | CH1=VOUT(48V), CH2=VSW |
| Audible sound is present but minimal. Tested till 240mA load.  Sound is proportional to the amount of load. Max load requireemnt is 400mA. | |
| Schematic for the above waveforms | |