{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["LM(2)5118 Calculator","Bill of Materials","Bode Plots","Worksheet","Graph"],"not_rendered":{"charts":12,"images":1,"macros":0,"external_links":0,"defined_names":95,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"LM(2)5118 Calculator","index":0,"n_rows":113,"n_cols":7,"rows_kept":113,"cut":false,"hidden":false,"merged":[]}
["LM(2)5118 Quick Start Component Calculator",null,null,null,"Version 2.01"]
["Revision date:  April 2014"]
[]
[]
[]
[" Step 1 - Application Requirements"]
[null,null,"Vout (V)",null,48]
[" Enter design requirements in the shaded cells",null,"Vin(min) (V)",null,42]
[null,null,"Vin(max) (V)",null,53]
[null,null,"Maximum Average Load Current Iout (A)",null,4.2]
[null,null,"Ripple Current as % of Maximum Load Current (%)",null,0.4]
[null,null,"Effciency of Converter (%)",null,0.9]
[null,null,"VCCX Voltage (V)",null,0]
[null,null,"Vin at start of  Transition to Buck-Boost Mode (V)",null,{"$f":"1.33*Vout","v":63.84}]
[null,null,"Buck-Boost Mode Operation",null,{"$f":"IF(Vinmin<1.4*Vout,\"YES\",\"NO\")","v":"YES"}]
[]
[null,null,"Recommended Controller IC",null,{"$f":"IF(E15 = \"NO\", \"LM5116\", \"LM5118\")","v":"LM5118"}]
[]
["Step 2 - Switching Frequency"]
[null,null,"Maximum Possible Switching Frequency (kHz)",null,{"$f":"IF(Fmax<610,Fmax,500)","v":500}]
[{"$f":"IF(E21>=E20,\"Violation of Minimum On-Time or Max Frequency\",\"\")","v":""},null,"Switching Frequency (kHz)",null,132]
[{"$f":"IF(E21>=E20,\"Reduce Switching Frequency\",\"\")","v":""},null,"Timing Resistor, Rt (kW)",null,{"$f":"6.4*10^3/Fsw-3.02","v":45.464848484848481}]
[{"$f":"IF(Dviolate<DMaximumAll,\"Check Switching Frequency or Decrease Vin\",\"\")","v":""}]
["Step 3 - Inductor Value"]
[null,null,"Calculated Buck Mode Inductor Value, Lb (µH)",null,{"$f":"IF(Vinmax>E14,((Vout*(Vinmax-Vout))/(Vinmax*Fsw*(Ripple*Iout)))*1000,\"NA\")","v":"NA"}]
[null,null,"Calculated Buck-Boost Mode Inductor Value, Lb-b (µH)",null,{"$f":"IF(BuckBoostMode=\"YES\",(((Vinmin)*Vout)/((Vinmin+Vout)*Fsw*Ripple*Iout))*1000,\"NA\")","v":101.01010101010101}]
[null,null,"Actual Chosen Inductor Value, L (µH)",null,100]
[null,null,"Inductor Tolerance (%)",null,0.2]
[]
["Step 4 - Calculate Output and Inductor Currents Based on Chosen Inductor"]
[null,null,"Buck mode Ripple Current at Vin(max), ΔI (A)",null,{"$f":"IF(Vinmax>E14,((Vout*(Vinmax-Vout))/(Vinmax*L*Fsw))*1000,\"NA\")","v":"NA"}]
[null,null,"Buck-Boost Ripple Current at Vin(min), ΔI (A)",null,{"$f":"(Vout*Vinmin)/(Fsw*L*(Vout+Vinmin))*1000","v":1.696969696969697}]
[null,null,"Buck-Boost Ripple Current at Vin=Vout, ΔI (A) ",null,{"$f":"IF(Vinmax>=Vout,(Vout*Vout)/((Vout+Vout)*Fsw*L)*1000,\"NA\")","v":1.8181818181818181}]
[null,null,"Buck mode Ripple Current at Vin(max), Including inductor tolerance, ΔI (A)",null,{"$f":"IrippleBuck/(1-L_tol)","v":{"$error":"#VALUE!"}}]
[null,null,"Buck-Boost Ripple Current at Vin(min), Including inductor tolerance, ΔI (A)",null,{"$f":"IrippleBB/(1-L_tol)","v":2.1212121212121211}]
[null,null,"Buck Average Inductor Current at Vin(max), Including Effciency (A)",null,{"$f":"Iout/Eff","v":4.666666666666667}]
[null,null,"Buck-Boost Average Inductor Current at Vin(min), Including Effciency (A)",null,{"$f":"((Vout+Vinmin)/Vinmin)*(Iout/Eff)","v":10}]
[null,null,"Buck-Mode Peak Inductor Current, Ip(b) (A)",null,{"$f":"IF(Vinmax>E14,ILavgBuck+E34/2,\"NA\")","v":"NA"}]
[null,null,"Buck-Boost Mode Peak Inductor Current, Ip(b-b) (A)",null,{"$f":"IF(BuckBoostMode=\"YES\",ILavgBB+E35/2,\"NA\")","v":11.060606060606061}," "]
[]
["Step 5 - Sense Resistor"]
[null,null,"Current Limit Margin (% beyond Max Load) (%)",null,0.2]
[null,null,"Buck Mode K Factor (K)",null,{"$f":"1+(10/(Vinmax-Vout))","v":3}]
[null,null,"Selected Buck Mode K Factor (K)",null,4]
[null,null,"Buck-Boost Mode K Factor (K)",null,{"$f":"1+(10/Vinmin)","v":1.2380952380952381}]
[null,null,"Selected Buck-Boost Mode K Factor (K)",null,2.5]
[null,null,"Current Sense Resistor, Rs (mW)",null,{"$f":"IF((2.5*(1-E42))/(10*(ILavgBB+(IrippleBB*KBB)/2))*1000<(1.25*(1-E42))/(10*(ILavgBuck+(IrippleBuck*KBuck)/2))*1000,(2.5*(1-E42))/(10*(ILavgBB+(IrippleBB*KBB)/2))*1000,(1.25*(1-E42))/(10*(ILavgBuck+(IrippleBuck*KBuck)/2))*1000)","v":{"$error":"#VALUE!"}}," "]
[null,null,"Closest Standard Value, Rs (mW)",null,20]
[]
["Step 6 - Ramp Capacitor"]
[null,null,"Cramp (pF)",null,{"$f":"(L*5*10^-6)/(10*Rs)*10^9","v":2500}]
[null,null,"Closest Smaller Standard Value, Cramp (pF)",null,2500]
[null,null,"Rramp (kW)",null,{"$f":"IF(Vout>20,7/(Vout*5*10^-6-50*10^-6)*10^-3,\"NA\")","v":36.842105263157904}]
[]
["Step 7 - Current Limits"]
[null,null,"Buck Mode Peak Inductor Current Limit (A)",null,{"$f":"IF(ILPeakLimitBuck<IpeakBuck,\"Error\",ILPeakLimitBuck)","v":"Error"}]
[null,null,"Buck-Boost Mode Peak Inductor Current Limit (A)",null,{"$f":"IF(ILPeakLimitBB<IpeakBB,\"Error\",ILPeakLimitBB)","v":12.095959595959595}]
[]
["Step 9 - Output Capacitors (Based on Worst Case Conditions for Each Mode)"]
[null,null,"Target output ripple (mV)",null,500]
[null,null,"Buck-Boost Duty cycle at Vin(min) (%)",null,{"$f":"Vout/(Vinmin+Vout)","v":0.53333333333333333}]
[null,null,"Buck-Boost RMS Ripple Current in Output Cap (A)",null,{"$f":"SQRT(-(DBB*Iout^2)/(DBB-1))","v":4.4899888641287298}]
[null,null,"Minimum COUT output Capacitor Value (µF)",null,{"$f":"Iout*Vout/(Vinmin+Vout)/(Fsw*DeltaVout)*1000000","v":33.939393939393945}]
[null,null,"Required COUT ESR (mW)",null,{"$f":"DeltaVout/(Iout/(1-E61)+IrippleBB/2)","v":50.769230769230774}]
[null,null,"Chosen COUT output capacitor value (µF)",null,200]
[null,null,"Actual COUT ESR (mW)",null,50]
[null,null,"Buck Mode Output Ripple Voltage (mV)",null,{"$f":"IF(Vinmax<BuckMode,\"NA\",Coutesr*((Iout/(1-E61)+(IrippleBB/2))))","v":"NA"}]
[]
["Step 10 - Input Capacitors (Based on Worst Case Conditions for Each Mode)"]
[null,null,"Buck-Boost RMS Input Ripple Current (A)",null,{"$f":"(Iout/(1-DBB))*SQRT(DBB*(1-DBB))","v":4.4899888641287298}]
[null,null,"Buck-Boost Mode Peak to Peak Current Ripple in Input Cap (A)",null,{"$f":"IpeakBB","v":11.060606060606061}]
[null,null,"Buck Mode RMS input Ripple Current (A)",null,{"$f":"IF(Vinmax<BuckMode,\"NA\",Iout*0.5)","v":"NA"}]
[null,null,"Buck Mode Peak to Peak Current Ripple in Input Cap (A)",null,{"$f":"IpeakBuck","v":"NA"}]
[null,null,"Initial Input Capacitor Value(μF)",null,{"$f":"E39/2/Fsw*1000","v":41.896235078053259}]
[null,null,"Chosen CIN Input Capacitor Value (µF)",null,820]
[]
["Step 11 - Feedback Resistors"]
[null,null,"Rfb2 (W)",null,38300]
[null,null,"Rfb1 (W)",null,{"$f":"_Rfb2/((Vout/1.23)-1)","v":1007.2482360487493}]
[]
["Step 12 - Chb & Cvcc Capacitor"]
[null,null,"High-side MOSFET Qg at VGS=10V (nC)",null,30]
[null,null,"Minimum Bootstrap Capacitor Chb (µF)",null,{"$f":"E82*10^-3/(0.05*7)","v":8.5714285714285701E-2}]
[null,null,"Chosen Value for Chb (µF)",null,0.1]
[null,null,"Minimum VCC Bypass Capacitor Cvcc (µF)",null,{"$f":"10*E84","v":1}]
[]
["Step 13 - Error Amplifier Compensation"]
[null,null,"Right Half Plane Zero Frequency (kHz)",null,{"$f":"((Rout*(1-DBB)^2)/(2*PI()*L*DBB*10^-6))/1000","v":7.4272306776217825}]
[null,null,"Capacitor ESR Zero Frequency (kHz)",null,{"$f":"1/(Cout*Coutesr*2*PI()*10^-6)","v":15.915494309189533}]
[null,null,"Capacitor Pole Frequency (kHz)",null,{"$f":"(1+DBB)/(2*PI()*Cout*Rout*10^-3)","v":0.1067664409908131}]
[null,null,"Bandwidth (kHz)",null,{"$f":"fmodRzero/4","v":1.8568076694054456}]
[null,null,"Selected Bandwith (kHz)",null,1.8]
[null,null,"Target Compensation Zero (kHz)",null,{"$f":"fcutoff/10","v":0.18}]
[null,null,"Target Compensation Pole (kHz)",null,{"$f":"fmodRzero","v":7.4272306776217825}]
[null,null,"Cpole (nF)",null,{"$f":"fcompZero/(fcompPole*_Rfb2*CompGain)*10^9","v":0.58299798986188311}]
[null,null,"Select Nearest Standard Cpole Value (nF)",null,0.47]
[null,null,"Czero (nF)",null,{"$f":"((1/(CompGain*_Rfb2))-E95*10^-9)*10^9","v":23.472893983993739},null," "]
[null,null,"Select Nearest Standard Czero Value (nF)",null,22]
[null,null,"Rcomp (W)",null,{"$f":"1/(fcompZero*2*3.14*E97*10^-9)","v":37687.837085238338}]
[null,null,"Select nearest Standard Rcomp Value (W)",null,37688]
[]
["Step 14 - Soft Start capacitor"]
[null,null,"Choose soft-start time (ms)",null,3]
[null,null,"Soft Start Capacitor Value (nF)",null,{"$f":"(E103*10^(-5))/1.23*10^6","v":24.390243902439028}]
[]
["Step 15 - UVLO Threshold and Hiccup Mode Restart"]
[null,null,"Minimum Value of Resistor Ruv1  (kW)",null,{"$f":"Vinmax","v":53}]
[null,null,"Chosen Value of  Ruv1 (kW)",null,75]
[null,null,"Desired Undervoltage Threshold (V)",null,4]
[null,null,"Ruv2 Value (kW)",null,{"$f":"1.23*E108/(E109+5*E108*10^(-3)-1.23)","v":29.332273449920507}]
[null,null,"Choose off-time of hiccup duty cycle (µs)",null,723]
[null,null,"Vin voltage for desired hiccup mode off-time  (V)  ",null,12]
[null,null,"Hiccup Mode Off-time Capacitor Value Cr (nF)",null,{"$f":"-(E111*(E110+E108))/(E110*E108*LN(1-((0.98*(E110+E108))/(E110*E112))))","v":99.917863427169848}]

{"sheet":"Bill of Materials","index":1,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[null,"LM5118 List of Components"]
[]
[null,"Component","Description","Value","Minimum Rating"]
[null,"L","Inductor",{"$f":"L","v":100},{"$f":"ILPeakLimitBB","v":12.095959595959595}]
[null,"Cin ","Input capacitor",{"$f":"Cin","v":820},{"$f":"Vinmax","v":53}]
[null,"Cramp","Ramp capacitor",{"$f":"Cramp","v":2500},16]
[null,"Css","Soft start capacitor",{"$f":"Css","v":24.390243902439028},6]
[null,"Cout","Output capacitor",{"$f":"Cout","v":200},{"$f":"Vout","v":48}]
[null,"Cr","UVLO filter capacitor",{"$f":"Cr","v":99.917863427169848},16]
[null,"Cpole","Compensation capacitor",{"$f":"Cpole","v":0.47},6]
[null,"Czero","Compensation capacitor",{"$f":"Czero","v":22},6]
[null,"Cvcc","VCC bypass capacitor",{"$f":"Cvcc","v":1},12]
[null,"Chb","HB-SW bypass capacitor",{"$f":"Chb","v":0.1},{"$f":"MAX(Vccx,VCC)","v":7}]
[null,"Rfb1","Feedback resistor",{"$f":"_Rfb1","v":1007.2482360487493},"1/16 W"]
[null,"Rfb2","Feedback resistor",{"$f":"_Rfb2","v":38300},"1/16 W"]
[null,"Ruv1","UVLO divider resistor",{"$f":"_Ruv1","v":75},{"$f":"IF(AND(Vinmax^2/(_Ruv2*1000)<0.05,Vinmax<=50),\"1/16W\",\"1/8W\")","v":"1/8W"}]
[null,"Ruv2","UVLO divider resistor",{"$f":"_Ruv2","v":29.332273449920507},"1/16 W"]
[null,"Rs","Sense resistor",{"$f":"Rs","v":20},{"$f":"IF(PRS_BB>PRS_B,PRS_BB,PRS_B)","v":2}]
[null,"Rt","Oscillator timing resistor",{"$f":"Rt","v":45.464848484848481},"1/16 W"]
[null,"Rramp","Optional ramp resistor",{"$f":"Rramp","v":36.842105263157904},{"$f":"IF(D20=\"NA\",\"-\",\"1/16 W\")","v":"1/16 W"}]
[null,"Rcomp","Compensation resistor",{"$f":"Rcomp/1000","v":37.688000000000002},"1/16 W"]

{"sheet":"Bode Plots","index":2,"n_rows":24,"n_cols":24,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
["Buck-Boost Mode",null,null,null,null,null,null,null,null,null,null,null,"Buck Mode "]
[null,"Frequency (Hz)","Frequency (rad/sec)","Modulator\nGain\n(dB)","Modulator\nPhase\n(deg)","Error Amplifier Gain\n(dB)","Error Amplifier Phase (deg)","Overall Loop\nGain\n(dB)","Loop\nPhase\n(deg)",null,null,null,null,"Frequency (Hz)","Frequency (rad/sec)","Modulator\nGain\n(dB)","Modulator\nPhase\n(deg)","Error Amplifier Gain\n(dB)","Error Amplifier Phase (deg)","Overall Loop\nGain\n(dB)","Loop\nPhase\n(deg)"]
[null,0.1,{"$f":"2*PI()*B3","v":0.62831853071795862},{"$f":"20*LOG(AmBB*IMABS(IMDIV(IMPRODUCT(COMPLEX(1,-C3/wrBB),COMPLEX(1,C3/wzBB)),COMPLEX(1,C3/wpBB))))","v":24.806639297257284},{"$f":"IMARGUMENT(IMDIV(IMPRODUCT(COMPLEX(1,-C3/wrBB),COMPLEX(1,C3/wzBB)),COMPLEX(1,C3/wpBB)))*(180/PI())","v":-5.4076009152008296E-2},{"$f":"20*LOG(Afb*IMABS(IMDIV(IMDIV(COMPLEX(1,C3/wzea),COMPLEX(1,C3/wpea)),COMPLEX(0,C3))))","v":65.340366883245935},{"$f":"IMARGUMENT(IMDIV(IMDIV(COMPLEX(-1,-C3/wzea),COMPLEX(1,C3/wpea)),COMPLEX(0,C3)))*(180/PI())","v":90.029224550570717},{"$f":"D3+F3","v":90.147006180503212},{"$f":"E3+G3","v":89.975148541418704},null,"Modulator - Buck-Boost",null,null,0.1,{"$f":"2*PI()*N3","v":0.62831853071795862},{"$f":"20*LOG(Amb*IMABS(IMDIV(COMPLEX(1,O3/wzb),COMPLEX(1,O3/wpb))))","v":35.139230068931766},{"$f":"IMARGUMENT(IMDIV(COMPLEX(1,O3/wzb),COMPLEX(1,O3/wpb)))*(180/PI())","v":-8.1925657713101674E-2},{"$f":"20*LOG(Afb*IMABS(IMDIV(IMDIV(COMPLEX(1,O3/wzea),COMPLEX(1,O3/wpea)),COMPLEX(0,O3))))","v":65.340366883245935},{"$f":"IMARGUMENT(IMDIV(IMDIV(COMPLEX(-1,-O3/wzea),COMPLEX(1,O3/wpea)),COMPLEX(0,O3)))*(180/PI())","v":90.029224550570717},{"$f":"P3+R3","v":100.4795969521777},{"$f":"Q3+S3","v":89.947298892857617},null,"Modulator - Buck"]
[null,0.2,{"$f":"2*PI()*B4","v":1.2566370614359172},24.806627870426894,-0.10815192414794166,59.319770504454262,90.058449084939539,84.126398374881148,89.950297160791592,null,"rad/sec","Hz",null,0.2,{"$f":"2*PI()*N4","v":1.2566370614359172},35.139203197015611,-0.16385097599220691,59.319770504454262,90.058449084939539,{"$f":"P4+R4","v":94.458973701469873},{"$f":"Q4+S4","v":89.894598108947335},null,"rad/sec","Hz"]
[null,0.5,{"$f":"2*PI()*B5","v":3.1415926535897931},24.806547883456492,-0.27037816265935644,51.360995072348288,90.146122428817222,76.167542955804777,89.875744266157866,"wp",{"$f":"(1+DBB)/(Cout*10^-6*Rout)","v":670.83333333333337},{"$f":"K5/(2*PI())","v":106.76644099081314},null,0.5,{"$f":"2*PI()*N5","v":3.1415926535897931},35.139015098258064,-0.40962150006199716,51.360995072348288,90.146122428817222,86.500010170606345,89.73650092875522,"wz",{"$f":"1/(Cout*10^-6*Coutesr*10^-3)","v":100000.00000000001},{"$f":"W5/(2*PI())","v":15915.494309189537}]
[null,1,{"$f":"2*PI()*B6","v":6.2831853071795862},24.80626222773634,-0.54074455655268427,45.340483519827146,90.292242832439896,70.146745747563486,89.751498275887215,"wr",{"$f":"(Rout*(1-DBB)^2)/(L*10^-6*DBB)","v":46666.666666666672},{"$f":"K6/(2*PI())","v":7427.2306776217838},null,1,{"$f":"2*PI()*N6","v":6.2831853071795862},35.138343383480432,-0.81920057717435235,45.340483519827146,90.292242832439896,80.478826903307578,89.47304225526554,"wp",{"$f":"1/(Cout*10^-6*Rout)","v":437.50000000000006},{"$f":"W6/(2*PI())","v":69.630287602704215}]
[null,2,{"$f":"2*PI()*B7","v":12.566370614359172},24.805119792802465,-1.0813949815559807,39.320237031589144,90.584469464312761,64.125356824391616,89.503074482756787,"wz",{"$f":"1/(Cout*10^-6*Coutesr*10^-3)","v":100000.00000000001},{"$f":"K7/(2*PI())","v":15915.494309189537},null,2,{"$f":"2*PI()*N7","v":12.566370614359172},35.135657562855911,-1.6380619281528794,39.320237031589144,90.584469464312761,74.455894594445056,88.946407536159882,null,"Gain","dB"]
[null,5,31.415926535897931,24.797131156104946,-2.7018422293835713,31.36391002774257,91.460890261604902,56.161041183847516,88.75904803222133,null,"Gain","dB",null,5,31.415926535897931,35.116903184951553,-4.0892359268850074,31.36391002774257,91.460890261604902,66.48081321269413,87.371654334719892,"Am",{"$f":"Rout/Ri","v":57.142857142857139},{"$f":"20*LOG(Amb)","v":35.139239026274112}]
[null,10,62.831853071795862,24.768719732000338,-5.3919918496902053,25.352131373632908,92.919759401491916,50.12085110563325,87.527767551801716,"Am",{"$f":"(Rout/Ri)*((1-DBB)/(1+DBB))","v":17.391304347826086},{"$f":"20*LOG(K9)","v":24.806643106207389},null,10,62.831853071795862,35.050576766892796,-8.1366886968484717,25.352131373632908,92.919759401491916,60.402708140525704,84.78307070464345]
[null,20,125.66370614359172,24.656897922634311,-10.69224190454648,19.366638250974699,95.823447769298198,44.02353617360901,85.13120586475172,null,null,null,null,20,125.66370614359172,34.794959468276673,-15.953723825138557,19.366638250974699,95.823447769298198,54.161597719251375,79.869723944159645]
[null,50,314.15926535897933,23.945719769840291,-25.299963312379219,11.645940132126636,104.28784606788331,35.591659901966928,78.987882755504089,null,"Error Amp",null,null,50,314.15926535897933,33.333331405973695,-35.501308507109187,11.645940132126636,104.28784606788331,44.979271538100335,68.786537560774121,null,"Error Amp"]
[null,100,628.31853071795865,22.072347498675015,-43.537048665872938,6.3826751894168883,116.89346134763038,28.455022688091901,73.356412681757433,null,"rad/sec","Hz",null,100,628.31853071795865,30.278584412198114,-54.790399123172364,6.3826751894168883,116.89346134763038,36.661259601615001,62.103062224458014,null,"rad/sec","Hz"]
[null,200,1256.6370614359173,18.269619312117065,-62.727786572719751,2.5100212024517461,134.92769513813761,20.779640514568811,72.199908565417857,"wpea",{"$f":"(Czero*10^-9+Cpole*10^-9)/(Cpole*10^-9*Czero*10^-9*Rcomp)","v":57660.637866764766},{"$f":"wpea/(2*PI())","v":9176.9755383273314},null,200,1256.6370614359173,25.478421255625353,-70.084402177541605,2.5100212024517461,134.92769513813761,27.988442458077099,64.843292960596003,"wpea",{"$f":"(Czero*10^-9+Cpole*10^-9)/(Cpole*10^-9*Czero*10^-9*Rcomp)","v":57660.637866764766},{"$f":"wpea/(2*PI())","v":9176.9755383273314}]
[null,500,3141.5926535897929,11.226219789142561,-79.998413367353749,0.26069126871704917,155.87929826738446,11.486911057859611,75.880884900030708,"wzea",{"$f":"1/(Czero*10^-9*Rcomp)","v":1206.0747573377587},{"$f":"wzea/(2*PI())","v":191.95275936866247},null,500,3141.5926535897929,17.936668286688359,-80.272537153756261,0.26069126871704917,155.87929826738446,18.197359555405409,75.606761113628195,"wzea",{"$f":"1/(Czero*10^-9*Rcomp)","v":1206.0747573377587},{"$f":"wzea/(2*PI())","v":191.95275936866247}]
[null,1000,6283.1853071795858,5.4212475691505517,-87.978717582953863,-0.21764431556048741,162.91519497369026,5.2036032535900647,74.9364773907364,null,"Gain","dB",null,1000,6283.1853071795858,11.991308956948634,-82.42163349098179,-0.21764431556048741,162.91519497369026,11.773664641388146,80.493561482708472,null,"Gain","dB"]
[null,2000,12566.370614359172,-0.28555600987990726,-94.852896030865992,-0.48522518723808999,162.22314007363846,-0.7707811971179972,67.37024404277247,"Afb",{"$f":"1/(_Rfb2*(Czero*10^-9+Cpole*10^-9))","v":1161.9786637477762},{"$f":"20*LOG(K16)","v":61.303963072244969},null,2000,12566.370614359172,6.0373871977743949,-80.843588750718183,-0.48522518723808999,162.22314007363846,5.5521620105363052,81.379551322920278,"Afb",{"$f":"1/(_Rfb2*(Czero*10^-9+Cpole*10^-9))","v":1161.9786637477762},{"$f":"20*LOG(W16)","v":61.303963072244969}]
[null,5000,31415.926535897932,-6.574023526128272,-105.28451594348795,-1.4460315957191279,149.21806730391236,-8.020055121847399,43.933551360424417,null,null,null,null,5000,31415.926535897932,-1.5762638402406257,-71.761552762849206,-1.4460315957191279,149.21806730391236,-3.0222954359597534,77.456514541063157]
[null,10000,62831.853071795864,-8.6887219116560797,-110.64426468813478,-3.7212243310267001,131.44285331319384,-12.40994624268278,20.798588625059054,null,null,null,null,10000,62831.853071795864,-6.5599376347476337,-57.459146651446893,-3.7212243310267001,131.44285331319384,-10.281161965774334,73.983706661746936]
[null,20000,125663.70614359173,-7.3655031605400918,-107.83296700937805,-7.9195292256322691,114.09807857972797,-15.285032386172361,6.2651115703499158,null,null,null,null,20000,125663.70614359173,-9.9107061269913359,-38.312411979610836,-7.9195292256322691,114.09807857972797,-17.830235352623603,75.785666600117139]
[null,50000,314159.26535897929,-1.5842949484328119,-99.085246326805617,-15.192755587449817,100.1803257752522,-16.77705053588263,1.0950794484465831,null,null,null,null,50000,314159.26535897929,-11.622068320528211,-17.576996770875052,-15.192755587449817,100.1803257752522,-26.814823907978028,82.603329004377144]
[null,100000,628318.53071795858,4.054921966562917,-94.734197886850524,-21.105935777560823,95.133352647733943,-17.051013810997908,0.39915476088341961,null,null,null,null,100000,628318.53071795858,-11.932564033538892,-9.0031658694260948,-21.105935777560823,95.133352647733943,-33.038499811099712,86.130186778307845]
[null,200000,1256637.0614359172,9.9763967247200735,-92.392511434646195,-27.099260037394824,92.572176706094936,-17.122863312674752,0.17966527144874078,null,null,null,null,200000,1256637.0614359172,-12.013785047016903,-4.5299177018974346,-27.099260037394824,92.572176706094936,-39.113045084411723,88.042259004197504]
[null,500000,3141592.653589793,17.907153711546535,-90.959895836871638,-35.050392202579765,91.029489709332026,-17.14323849103323,6.9593872460387729E-2,null,null,null,null,500000,3141592.653589793,-12.036801815413691,-1.8151866776538936,-35.050392202579765,91.029489709332026,-47.087194017993454,89.214303031678128]
[null,1000000,6283185.307179586,23.923736999106712,-90.480155256577675,-41.069895579092076,90.514789124477062,-17.146158579985364,3.4633867899387383E-2,null,null,null,null,1000000,6283185.307179586,-12.040099906144938,-0.90782414801436107,-41.069895579092076,90.514789124477062,-53.109995485237015,89.606964976462706]

{"sheet":"Worksheet","index":3,"n_rows":89,"n_cols":6,"rows_kept":89,"cut":false,"hidden":true,"merged":[]}
[]
[null,null,null,null,"10 is buck","10 is buck-boost"]
[]
[null,{"$f":"IF(Vout>0.7*Vin_nominal,\"Buck-Boost Mode\",\"Buck Mode\")","v":{"$error":"#NAME?"}},null,"Vin","Vout"]
[null,null,null,null,12]
[null,null,null,20,{"$f":"IF(E5<0.7*D6,10,0)","v":10},{"$f":"IF(E5>0.7*D6,10,0)","v":0}]
[null,null,null,19,{"$f":"IF(E5<0.7*D7,10,0)","v":10},{"$f":"IF(E5>0.7*D7,10,0)","v":0}]
[null,null,null,18,{"$f":"IF(E5<0.7*D8,10,0)","v":10},{"$f":"IF(E5>0.7*D8,10,0)","v":0}]
[null,null,null,17,{"$f":"IF(E5<0.7*D9,10,0)","v":0},{"$f":"IF(E5>0.7*D9,10,0)","v":10}]
[null,null,null,16,{"$f":"IF(E5<0.7*D10,10,0)","v":0},{"$f":"IF(E5>0.7*D10,10,0)","v":10}]
[null,null,null,14,{"$f":"IF(E7<0.7*D11,10,0)","v":0},{"$f":"IF(E5>0.7*D11,10,0)","v":10}]
[null,null,null,13,{"$f":"IF(E8<0.7*D12,10,0)","v":0},{"$f":"IF(E5>0.7*D12,10,0)","v":10}]
[null,null,null,12,{"$f":"IF(E5<0.7*D13,10,0)","v":0},{"$f":"IF(E5>0.7*D13,10,0)","v":10}]
[null,null,null,11,{"$f":"IF(E5<0.7*D14,10,0)","v":0},{"$f":"IF(E5>0.7*D14,10,0)","v":10}]
[null,null,null,10,{"$f":"IF(E5<0.7*D15,10,0)","v":0},{"$f":"IF(E5>0.7*D15,10,0)","v":10}]
[]
[null,null,null,null,12]
[null,null,13,75,{"$f":"E17/0.7","v":17.142857142857142},{"$f":"E18","v":17.142857142857142}]
[null,null,13,74,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,73,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,72,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,71,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,70,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,{"$f":"D23-1","v":69},{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,68,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,67,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,66,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,65,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,64,17.142857142857142]
[null,null,13,63,17.142857142857142]
[null,null,13,62,17.142857142857142]
[null,null,13,61,17.142857142857142]
[null,null,13,60,17.142857142857142]
[null,null,13,{"$f":"D33-1","v":59},17.142857142857142]
[null,null,13,58,17.142857142857142]
[null,null,13,57,17.142857142857142]
[null,null,13,56,17.142857142857142]
[null,null,13,55,17.142857142857142]
[null,null,13,54,17.142857142857142]
[null,null,13,53,17.142857142857142]
[null,null,13,52,17.142857142857142]
[null,null,13,51,17.142857142857142]
[null,null,13,50,17.142857142857142]
[null,null,13,49,17.142857142857142]
[null,null,13,48,17.142857142857142]
[null,null,13,47,17.142857142857142]
[null,null,13,46,17.142857142857142]
[null,null,13,45,17.142857142857142]
[null,null,13,44,17.142857142857142]
[null,null,13,43,17.142857142857142]
[null,null,13,42,17.142857142857142]
[null,null,13,41,17.142857142857142]
[null,null,13,40,17.142857142857142]
[null,null,13,39,17.142857142857142]
[null,null,13,38,17.142857142857142]
[null,null,13,37,17.142857142857142]
[null,null,13,36,17.142857142857142]
[null,null,13,35,17.142857142857142]
[null,null,13,34,17.142857142857142]
[null,null,13,33,17.142857142857142]
[null,null,13,32,17.142857142857142]
[null,null,13,31,17.142857142857142]
[null,null,13,30,17.142857142857142]
[null,null,13,29,17.142857142857142]
[null,null,13,28,17.142857142857142]
[null,null,13,27,17.142857142857142]
[null,null,13,26,17.142857142857142]
[null,null,13,25,17.142857142857142]
[null,null,13,24,17.142857142857142]
[null,null,13,23,17.142857142857142]
[null,null,13,22,17.142857142857142]
[null,null,13,21,17.142857142857142]
[null,null,13,20,17.142857142857142]
[null,null,13,19,17.142857142857142]
[null,null,13,18,17.142857142857142]
[null,null,13,17,17.142857142857142]
[null,null,13,16,17.142857142857142]
[null,null,13,15,17.142857142857142]
[null,null,13,14,17.142857142857142]
[null,null,13,13,17.142857142857142]
[null,null,13,12,17.142857142857142]
[null,null,13,11,17.142857142857142]
[null,null,13,10,17.142857142857142]
[null,null,13,9,17.142857142857142]
[null,null,13,8,17.142857142857142]
[null,null,13,7,17.142857142857142]
[null,null,13,6,17.142857142857142]
[null,null,13,5,17.142857142857142]
[null,null,13,4,17.142857142857142]

{"sheet":"Graph","index":4,"n_rows":13,"n_cols":13,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[null,null,"Vinmin","Vinmax","Lower ts limit","Upper ts limit","Lo B-B Voltage","Hi B-B voltage","Lower Buck","Upper Buck"]
[]
[]
[null,null,{"$f":"Vinmin","v":42},{"$f":"Vinmax","v":53},{"$f":"1.15*Vout","v":55.199999999999996},{"$f":"Vout/0.75","v":64},{"$f":"Vinmin","v":42},{"$f":"E7","v":55.199999999999996},{"$f":"Vout/0.75","v":64},{"$f":"Vinmax","v":53},null,{"$f":"Vout","v":48},{"$f":"Vin_nominal","v":{"$error":"#NAME?"}}]
[null,null,"Buck-Boost",null,null,null,5,{"$f":"IF(Vinmax<H7,Vinmax,H7)","v":53}]
[null,null,"Graph-Trans",null,null,{"$f":"IF(Vinmax>F7,F7,IF(Vinmax>E7,Vinmax,0))","v":0}]
[null,null,"Offset-Trans",null,null,{"$f":"F9-H8","v":-53}]
[]
[null,"NEW ","Buck",null,null,null,null,{"$f":"IF(Vinmax>F7,Vinmax,0)","v":0}]
[null,"Offset","Offset-Buck",null,null,null,null,{"$f":"H12-F7","v":-64}]