Just USB-C Cable Attached – showing CC lines add Rd fixed resistor

TI TPS25751EVM

Vbus=0V , CC-yellow = open Vbus=5V, CC- Yellow = 3V **State -Attached.SRC**

A screen with a colorful graph

AI-generated content may be incorrect. A screen with colorful lines

AI-generated content may be incorrect.

Custom design

A screen with a graph on it

AI-generated content may be incorrect. A screen with colorful lines on it

AI-generated content may be incorrect.

Vbus=9V , CC-yellow = open Vbus=9V, CC- Yellow = open **STATE Attach.Wait.Src**