{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["Revision History","Converter填寫範例","Converter","定義","Part owner list","常見問題 Q&A","Member"],"not_rendered":{"charts":0,"images":24,"macros":1,"external_links":2,"defined_names":23,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Revision History","index":0,"n_rows":65,"n_cols":4,"rows_kept":65,"cut":false,"hidden":false,"merged":[[3,3,6,3],[3,0,6,0],[3,1,6,1],[54,1,64,1],[54,0,64,0],[54,3,64,3],[7,3,53,3],[7,0,53,0],[7,1,53,1]]}
["Date","Rev.","Revision Description","Approved By"]
["2023-10-12","A00","Initial release to A-rev.","Maddux_Li"]
["2024-06-11","A01","Remove a spece between tape and width from \"TAPE WIDTH\" and \"TAPE WIDTH Tolerance\"","Maddux_Li"]
["2024-09-23","A02","Remove the \":\" from ","Maddux_Li"]
[null,null,"Remove the \"*Package Dimension (D nom X E nom X A max) (mm)\""]
[null,null,"Remove the \"*Lead pin Dimension (b nom X L nom) (mm)\""]
[null,null,"Adjust the naming of lead pins"]
["2024-11-29","A03","Separate the converter into an independent cover page","Maddux_Li"]
[null,null,"Added the sheet of revision history"]
[null,null,"Changed PSL/ECSL Catelog to converter"]
[null,null,"Changed category to Buck/Step-down Converter,Boost/Step-up Converter,SVID Step-down Converter,Switched Cap Converter/3-level"]
[null,null,"Changed package size to package type"]
[null,null,"Added IC manufacture process (monolithic or multi-chip)"]
[null,null,"If the footprint is non-standard the PITCH (Pin-to-Pin) and lead pin dimensionis will display NA."]
[null,null,"If feedback and setting architecture is digital the VREF and Output Voltage Accuracy will display NA"]
[null,null,"Separate input operating voltage range to VIN/VCC/driver VCC supply operation voltage range"]
[null,null,"Separate shutdown current to VIN/VCC shutdown current"]
[null,null,"Added the quiescent current of VIN/VCC/Driver VCC"]
[null,null,"Added power rail 1,power rail 2,power rail3 parameter for multi-rail converter"]
[null,null,"Added the switching frequency type and settings"]
[null,null,"Changed the unit of switching frequency from MHz to kHz"]
[null,null,"Separate the UVLO to VIN/VCC/Driver VCC UVLO"]
[null,null,"Add the VREF type and settings with fixed and VID"]
[null,null,"Added the max/min for output voltage accuracy"]
[null,null,"Added the Tj into the condition for output voltage accuracy"]
[null,null,"Changed enable pin definition to drop-down menu"]
[null,null,"Added the operation mode of converter"]
[null,null,"Segregate the enable pin impedance to \"Pull high/Low\" and \"Impedance value\""]
[null,null,"Segregate the enable slew rate or hysteresis to two columns."]
[null,null,"Separate high side driver resistor to Rsource and Rsink."]
[null,null,"Separate low side driver resistor to Rsource and Rsink."]
[null,null,"Added the OVP and OCP settings with different type"]
[null,null,"Add Ics for Itrip source current and Itrip Temperature Slope."]
[null,null,"Added note \"The current source for current limit\" for Itrip"]
[null,null,"Added the unit for \"Itrip Source Current\", \"Itrip Temperature Slope\" and \"Powergood Delay Time\""]
[null,null,"Added the softstart settings with different type"]
[null,null,"Segregate the powergood delay time to \"Low To High\" and \"High To Low\""]
[null,null,"Added the rated current for POL judgment whether the UIS need to be test(drop-down menu)"]
[null,null,"Added the COMPAL CE exempt from UIS(drop-down menu)"]
[null,null,"Added the UIS test condition of MOSFET"]
[null,null,"Remove the \"Controller W/Driver or W/O Driver\" and \"Charger Architecture\""]
[null,null,"Changed operation temperature range to recommended operating junction temperature range"]
[null,null,"Added the example for ESD HBM and CDM"]
[null,null,"Added the colume for datasheet version release date"]
[null,null,"Added the defined of Package dimension for IC 圖示/定義"]
[null,null,"Changed the image of lead pin dimension for IC 圖示/定義"]
[null,null,"Added the defined of converter power rail 1,power rail 2,power rail 3定義"]
[null,null,"Added the defined of Paper, Embossed 示意圖"]
[null,null,"Added the defined of pin count 圖示/定義"]
[null,null,"Added the defined of enable voltage 填寫定義"]
[null,null,"Added absolute VIN supply voltage and LX/SW switching absolute parameters"]
[null,null,"Added the Output Voltage Architecture and parameters"]
[null,null,"Added the Rated Current、OVP protection mode、OCP protection mode"]
[null,null,"Change PIN1 definition to follow EIA"]
["2025-09-01","A04","Added the sheet-常見問題 Q&A and sheet-Part owner list","Maddux_Li"]
[null,null,"Added the notice at the sheet of Converter"]
[null,null,"Added the package dimension definition at 定義(三) for SOT and SC70… package."]
[null,null,"Modify the note for the following parameters.\n1. What Output Voltage That Switching Frequency Will Lower Than 450kHz (V)\n2. Enable Minimum Slew Rate"]
[null,null,"Added the note for the folloeing parameters.\n1. Enable Pin Definition-Pull High/Low\n2. Output Voltage Accuracy (%) -- Min\n3. OVP Delay Time\n4. Powergood Delay Time"]
[null,null,"Modify the spalling of PITCH (Pin-to-Pin) (mm) to Pitch (Pin-to-Pin) (mm)"]
[null,null,"Added CCM mode and DCM mode for Operation mode-1/Operation mode-2"]
[null,null,"Added NA for the following parameters\n1. OCP Type\n2. VREF - Reference Voltage Type"]
[null,null,"Added the feature of prohibiting the modification of data brought in by macros"]
[null,null,"Changed the print cover page to the PDF function to be output via export"]
[null,null,"Added the initial PDF file naming."]

{"sheet":"Converter填寫範例","index":1,"n_rows":361,"n_cols":3,"rows_kept":361,"cut":false,"hidden":false,"merged":[[350,2,355,2],[43,2,46,2],[32,2,34,2],[339,2,347,2],[8,2,16,2],[102,2,106,2],[199,2,203,2],[296,2,300,2],[140,2,143,2],[237,2,240,2]]}
["Converter REV A04"]
["Item","Example","Note"]
["*PSL/ECSL Catelog","Converter"]
["*Category","Buck/Step-down","▼下拉式選單"]
["*Function","POL"]
["*Manufacturer","SILERGY"]
["*Manufacturer PN","SYV138ARHC","填寫完整Manufacturer PN"]
["*Package Type","QFN","填寫封裝類型即可，e.g. QFN,DFN,WLCSP…"]
["*Length(D) Nominal (mm)",2.5,"請參考定義(三)"]
["*Length(D) Upper Tolerance (+)",0.1]
["*Length(D) Lower Tolerance (-)",0.1]
["*Width(E) Nominal (mm)",2.5]
["*Width(E) Upper Tolerance (+)",0.1]
["*Width(E) Lower Tolerance (-)",0.1]
["*Height(A) Nominal (mm)",0.55000000000000004]
["*Height(A) Upper Tolerance (+)",0.1]
["*Height(A) Lower Tolerance (-)",0.1]
["*Footprint Type","Standard","▼下拉式選單\n請參考定義(四)"]
["*DXF Document for Non-Standard Footprint","X","▼下拉式選單\n如為Non-Standard footprint必需要提供"]
["*Pitch (Pin-to-Pin) (mm)",0.45]
["*Pin Count",16,"請參考定義八"]
["IC Manufacture Process (Monolithic or Multi-chip)","monolithic","▼下拉式選單"]
["*Feedback and Setting Architecture","Analog","▼下拉式選單"]
["VIN/VCC/Driver VCC supply type","Combine","▼下拉式選單\nVCC:The power of logic/control circuits,  Driver VCC:The power of high/Low side gate dirve"]
["Recommended VIN Supply Operation Voltage Range (V)","4~24","Input Voltage for High side MOS drain\nRange的部分請用波浪號「 ~ 」表示"]
["Absolute VIN Supply Voltage Range (V)","-0.3~28","Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Recommended VCC Supply Operation Voltage Range (V)","3.15~3.45","Logic/Control circuits input voltage\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Recommended Driver VCC Supply Operation Voltage Range (V)","NA","High/Low side gate dirve input voltage\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["LX/SW Switching Node Peak/AC Absolute Voltage Range (V)","-5~29","Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["VIN Shutdown Current, EN=0V (uA) -- Max",9]
["VCC Shutdown Current, EN=0V (uA) -- Max","NA","Logic/Control circuits off-mode current"]
["Driver VCC Shutdown Current, EN=0V (uA) -- Max","NA","High/Low side gate dirve off-mode current"]
["Vin Quiescent Current (uA) -- Max",170,"Enable=High, IOUT=0A, device not switching"]
["VCC Quiescent Current (uA) -- Max","NA"]
["Driver VCC Quiescent Current (uA) -- Max","NA"]
["VCC UVLO Threshold Voltage (V)-Rising -- Max","NA"]
["VCC UVLO Threshold Voltage (V)-Falling -- Max","NA"]
["Driver VCC UVLO Threshold Voltage (V)-Rising -- Max","NA"]
["Driver VCC UVLO Threshold Voltage (V)-Falling -- Max","NA"]
["Power railⅠ","Yes","▼下拉式選單\nPower railⅠ/Power railⅡ/power railⅢ請參考定義六"]
["Ⅰ- Output Voltage Architecture","Adjustable","▼下拉式選單"]
["Ⅰ- Output Voltage-Fixed (V) -- Typ","NA"]
["Ⅰ- Output Voltage-Adjustable (V)","0.6~2.5","Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅰ- Output Voltage-Selectable 1 (V) -- Typ","NA","Selectable 1~4 請依電壓由小到大填寫"]
["Ⅰ- Output Voltage-Selectable 2 (V) -- Typ","NA"]
["Ⅰ- Output Voltage-Selectable 3 (V) -- Typ","NA"]
["Ⅰ- Output Voltage-Selectable 4 (V) -- Typ","NA"]
["Ⅰ- Rated Current (A) -- Typ",8]
["Ⅰ- Switching Frequency Type","Fixed","▼下拉式選單"]
["Ⅰ- Switching Frequency-Fixed (kHz) -- Typ",600]
["Ⅰ- Switching Frequency-Adjust by Resistor (kHz) -- Max","NA"]
["Ⅰ- Switching Frequency-Adjust by Resistor (kHz) -- Min","NA"]
["Ⅰ- Switching Frequency-Programmable (kHz) -- Max","NA"]
["Ⅰ- Switching Frequency-Programmable (kHz) -- Min","NA"]
["Ⅰ- Switching Frequency-Other","NA","當Switching Frequency Type 為Other 時，需描述為何種type"]
["Ⅰ- Switching Frequency-Other (kHz)","NA","Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格\n當Switching Frequency Type 為Other 時需填寫此欄位"]
["Ⅰ- What Output Voltage That Switching Frequency Will Lower Than 450kHz (V)",null,"1. COT 架構及High level input voltage converter需填寫此欄位\n2. 使用Vin=20V測試\n3. Low level input voltage converter及output voltage 為Fixed的converter，此欄位請填寫NA\n4. 應用在此電壓以下，需考慮輸出電容增加或使用bulk cap."]
["Ⅰ- VIN UVLO Threshold Voltage (V)-Rising -- Max",3.9]
["Ⅰ- VIN UVLO Threshold Voltage (V)-Falling -- Max",3.4]
["Ⅰ- VREF - Reference Voltage Type","Fixed","▼下拉式選單"]
["Ⅰ- VREF -Fixed (V) -- Min",0.59399999999999997]
["Ⅰ- VREF -Fixed (V) -- Typ",0.6]
["Ⅰ- VREF -Fixed (V) -- Max",0.60599999999999998]
["Ⅰ- VREF -VID0 (V) -- Min","NA"]
["Ⅰ- VREF -VID0 (V) -- Typ","NA"]
["Ⅰ- VREF -VID0 (V) -- Max","NA"]
["Ⅰ- VREF -VID1 (V) -- Min","NA"]
["Ⅰ- VREF -VID1 (V) -- Typ","NA"]
["Ⅰ- VREF -VID1 (V) -- Max","NA"]
["Ⅰ- Output Voltage Accuracy (%) -- Max",1]
["Ⅰ- Output Voltage Accuracy (%) -- Min",-1,"數值前請加「-」號。e.g. -1、-0.5"]
["Ⅰ- Condition for Output Voltage Accuracy (℃) -- Tj ",25,"Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅰ- Enable Pin Definition","Tri-State","▼下拉式選單"]
["Ⅰ- Enable Pin Type","Enable Voltage","▼下拉式選單"]
["Ⅰ- Enable/Disable Voltage SPEC (V)-Enable -- Min",1,"100% guaranteed to high voltage\n請參考定義(九)"]
["Ⅰ- Enable/Disable Voltage SPEC (V)-Disable -- Max",0.4,"100% guaranteed to low voltage\n請參考定義(九)"]
["Ⅰ- Enable/Disable Voltage Threshold (V)-Enable -- Max","NA","100% guaranteed to high voltage\n請參考定義(九)"]
["Ⅰ- Enable/Disable Voltage Threshold (V)-Disable -- Min","NA","100% guaranteed to low voltage\n請參考定義(九)"]
["Ⅰ- Enable Have Hysteresis","No","▼下拉式選單"]
["Ⅰ- Enable Hysteresis (mV)","NA","VHigh – Vlow"]
["Ⅰ- Enable Minimum Slew Rate (mV/uS)","NA","如果沒有hysteresis, 需填寫IC 允許的enable最小slew rate。\n確認當enable voltage 爬升速度過慢或是在eanble/diasble voltage threshold 中震盪是否會誤動作"]
["Ⅰ- Operation mode-1","PFM Mode","▼下拉式選單"]
["Ⅰ- Enable Voltage for Operation Mode-1 (V) -- Min",0.4]
["Ⅰ- Enable Voltage for Operation Mode-1 (V) -- Max",0]
["Ⅰ- Operation Mode-2","Force CCM Mode","▼下拉式選單"]
["Ⅰ- Enable Voltage for Operation Mode-2 (V) -- Min",4]
["Ⅰ- Enable Voltage for Operation Mode-2 (V) -- Max",1]
["Ⅰ- Enable Pin Definition-Other","NA","Enable Pin Definition為other 時，需填寫此欄位描述Enable Pin Definition"]
["Ⅰ- Enable Voltage for Operation Mode-Other(V) -- Min","NA","Enable Pin Definition為other 時，需填寫此欄位"]
["Ⅰ- Enable Voltage for Operation Mode-Other(V) -- Max","NA","Enable Pin Definition為other 時，需填寫此欄位"]
["Ⅰ- Enable Pin Definition-Pull High/Low","Pull Low","▼下拉式選單\n此欄位是確認IC enable pin內部是否有pull high/pull low 電阻。如無此設計請選擇NO。\n當選擇NO，Enable Pin Internal Pull High/Pull Low Resistor欄位會自動帶入NA。"]
["Ⅰ- Enable Pin Internal Pull High/Pull Low Resistor(k ohm)","NA"]
["Ⅰ- High Side On Resistance (mΩ) -- Typ",20]
["Ⅰ- Low Side On Resistance (mΩ) -- Typ",10]
["Ⅰ- High Side Driver Resistor Rsource (ohm) -- Typ","NA"]
["Ⅰ- High Side Driver Resistor Rsink (ohm) -- Typ","NA"]
["Ⅰ- Low side Driver Resistor Rsource (ohm) -- Typ","NA"]
["Ⅰ- Low Side Driver Resistor Rsink (ohm) -- Typ","NA"]
["Ⅰ- Dead Time High Side Off to Low Side On (ns) -- Typ",10]
["Ⅰ- Dead Time Low Side Off to High Side On (ns) -- Typ",10]
["Ⅰ- OVP Type","Fixed","▼下拉式選單\nThis OVP is for output voltage"]
["Ⅰ- OVP protection mode","Hiccup","▼下拉式選單"]
["Ⅰ- OVP Threshold-Percentage (%) -- Min",115,"This OVP is for output voltage"]
["Ⅰ- OVP Threshold-Fixed (V) -- Min","NA"]
["Ⅰ- OVP Threshold-Programmable (V) -- Min","NA"]
["Ⅰ- OVP Threshold-Programmable (V) -- Max","NA"]
["Ⅰ- OVP Threshold-Programmable Step (mV)","NA"]
["Ⅰ- OVP Threshold-Relative to VID/DAC (mV)","NA","If OVP Threshold=VID/Vo/DAC+\"Voltage(fixed value)\", please fill in voltage with fixed value."]
["Ⅰ- OVP Threshold-Other","NA","OVP type為Other 時，需填寫此欄位描述OVP架構"]
["Ⅰ- OVP Threshold-Other (V)","NA","OVP type為Other 時，需填寫此欄位"]
["Ⅰ- Absolute OVP Threshold (V) -- Max","NA"]
["Ⅰ- Absolute OVP Threshold (V) -- Min","NA"]
["Ⅰ- OVP Delay Time Type","No","▼下拉式選單\n如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅰ- OVP Delay Time-Fixed Value (uS) -- Min","NA","如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅰ- OVP Delay Time-Programable (uS) -- Max","NA","如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅰ- OVP Delay Time-Programable (uS) -- Min","NA","如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅰ- OCP Type","Selectable","▼下拉式選單"]
["Ⅰ- OCP protection mode","Hiccup","▼下拉式選單"]
["Ⅰ- OCP Threshold -Fixed (A) -- Min","NA"]
["Ⅰ- OCP Threshold-Low  (A) -- Min",8,"Current limit pin is pull low"]
["Ⅰ- OCP Threshold-Floating  (A) -- Min",12,"Current limit pin is floating"]
["Ⅰ- OCP Threshold-High (A) -- Min",16,"Current limit pin is pull high"]
["Ⅰ- OCP Threshold-Adjust by Resistor (A)","NA","請填寫OCP可調整範圍\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅰ- OCP Threshold-Other","NA","OCP type為Other 時，需填寫此欄位描述OCP架構"]
["Ⅰ- OCP Threshold-Other (A) -- Min","NA","OCP type為Other 時，需填寫此欄位\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅰ- Itrip/Ics Source Current (uA)","NA","The current source for current limit\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅰ- Itrip/Ics Temperature Coefficient (ppm/℃)","NA"]
["Ⅰ- Softstart Type","Fixed","▼下拉式選單"]
["Ⅰ- Softstart (mS)-Fixed -- Max",1.2,"From EN=High to Vout=95%"]
["Ⅰ- Softstart (mS)-Fixed -- Min",1.98,"From EN=High to Vout=95%"]
["Ⅰ- Softstart-Relative to VID/DAC(mS) -- Max","NA","1. If Softstart=\"Fixed value\" (mS) + VID slow rate, please fill in the fixed value.\n2. From EN=High to Vout=95%"]
["Ⅰ- Softstart-Relative to VID/DAC(mS) -- Min","NA"]
["Ⅰ- Softstart-Other","NA","Softstart type為Other 時，需填寫此欄位描述Softstart架構"]
["Ⅰ- Softstart-Other (mS)","NA","Softstart type為Other 時，需填寫此欄位"]
["Ⅰ- Powergood Delay Time-Low to High (uS)",200,"如datasheet 僅標示power good deglitch time，請填寫power good deglitch time在此欄位。"]
["Ⅰ- Powergood Delay Time-High to Low (uS)",30,"如datasheet 僅標示power good deglitch time，請填寫power good deglitch time在此欄位。"]
["Power rail Ⅱ","No","▼下拉式選單\nPower railⅠ/Power railⅡ/power railⅢ請參考定義(六)"]
["Ⅱ- Output Voltage Architecture","NA","下拉式選單"]
["Ⅱ- Output Voltage-Fixed (V) -- Typ","NA"]
["Ⅱ- Output Voltage-Adjustable (V)","NA","Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅱ- Output Voltage-Selectable 1 (V) -- Typ","NA","Selectable 1~4 請依電壓由小到大填寫"]
["Ⅱ- Output Voltage-Selectable 2 (V) -- Typ","NA"]
["Ⅱ- Output Voltage-Selectable 3 (V) -- Typ","NA"]
["Ⅱ- Output Voltage-Selectable 4 (V) -- Typ","NA"]
["Ⅱ- Rated Current (A) -- Typ","NA"]
["Ⅱ- Switching Frequency Type","NA","▼下拉式選單"]
["Ⅱ- Switching Frequency-Fixed (kHz) -- Typ","NA"]
["Ⅱ- Switching Frequency-Adjust by Resistor (kHz) -- Max","NA"]
["Ⅱ- Switching Frequency-Adjust by Resistor (kHz) -- Min","NA"]
["Ⅱ- Switching Frequency-Programmable (kHz) -- Max","NA"]
["Ⅱ- Switching Frequency-Programmable (kHz) -- Min","NA"]
["Ⅱ- Switching Frequency-Other","NA","當Switching Frequency Type 為Other 時，需描述為何種type"]
["Ⅱ- Switching Frequency-Other (kHz)","NA","Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格\n當Switching Frequency Type 為Other 時需填寫此欄位"]
["Ⅱ- What Output Voltage That Switching Frequency Will Lower Than 450kHz (V)","NA","1. COT 架構及High level input voltage converter需填寫此欄位\n2. 使用Vin=20V測試\n3. Low level input voltage converter及output voltage 為Fixed的converter，此欄位請填寫NA\n4. 應用在此電壓以下，需考慮輸出電容增加或使用bulk cap."]
["Ⅱ- VIN UVLO Threshold Voltage (V)-Rising -- Max","NA"]
["Ⅱ- VIN UVLO Threshold Voltage (V)-Falling -- Max","NA"]
["Ⅱ- VREF - Reference Voltage Type","NA","▼下拉式選單"]
["Ⅱ- VREF -Fixed (V) -- Min","NA"]
["Ⅱ- VREF -Fixed (V) -- Typ","NA"]
["Ⅱ- VREF -Fixed (V) -- Max","NA"]
["Ⅱ- VREF -VID0 (V) -- Min","NA"]
["Ⅱ- VREF -VID0 (V) -- Typ","NA"]
["Ⅱ- VREF -VID0 (V) -- Max","NA"]
["Ⅱ- VREF -VID1 (V) -- Min","NA"]
["Ⅱ- VREF -VID1 (V) -- Typ","NA"]
["Ⅱ- VREF -VID1 (V) -- Max","NA"]
["Ⅱ- Output Voltage Accuracy (%) -- Max","NA"]
["Ⅱ- Output Voltage Accuracy (%) -- Min","NA","數值前請加「-」號。e.g. -1、-0.5"]
["Ⅱ- Condition for Output Voltage Accuracy (℃) -- Tj ","NA","Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅱ- Enable Pin Definition","NA","▼下拉式選單"]
["Ⅱ- Enable Pin Type","NA","▼下拉式選單"]
["Ⅱ- Enable/Disable Voltage SPEC (V)-Enable -- Min","NA","100% guaranteed to high voltage\n請參考定義(九)"]
["Ⅱ- Enable/Disable Voltage SPEC (V)-Disable -- Max","NA","100% guaranteed to low voltage\n請參考定義(九)"]
["Ⅱ- Enable/Disable Voltage Threshold (V)-Enable -- Max","NA","100% guaranteed to high voltage\n請參考定義(九)"]
["Ⅱ- Enable/Disable Voltage Threshold (V)-Disable -- Min","NA","100% guaranteed to low voltage\n請參考定義(九)"]
["Ⅱ- Enable Have Hysteresis","NA","▼下拉式選單"]
["Ⅱ- Enable Hysteresis (mV)","NA","VHigh – Vlow"]
["Ⅱ- Enable Minimum Slew Rate (mV/uS)","NA","如果沒有hysteresis, 需填寫IC 允許的enable最小slew rate。\n確認當enable voltage 爬升速度過慢或是在eanble/diasble voltage threshold 中震盪是否會誤動作"]
["Ⅱ- Operation mode-1","NA","▼下拉式選單"]
["Ⅱ- Enable Voltage for Operation Mode-1 (V) -- Min","NA"]
["Ⅱ- Enable Voltage for Operation Mode-1 (V) -- Max","NA"]
["Ⅱ- Operation Mode-2","NA","▼下拉式選單"]
["Ⅱ- Enable Voltage for Operation Mode-2 (V) -- Min","NA"]
["Ⅱ- Enable Voltage for Operation Mode-2 (V) -- Max","NA"]
["Ⅱ- Enable Pin Definition-Other","NA","Enable Pin Definition為other 時，需填寫此欄位描述Enable Pin Definition"]
["Ⅱ- Enable Voltage for Operation Mode-Other(V) -- Min","NA","Enable Pin Definition為other 時，需填寫此欄位"]
["Ⅱ- Enable Voltage for Operation Mode-Other(V) -- Max","NA","Enable Pin Definition為other 時，需填寫此欄位"]
["Ⅱ- Enable Pin Definition-Pull High/Low","NA","▼下拉式選單\n此欄位是確認IC enable pin內部是否有pull high/pull low 電阻。如無此設計請選擇NO。\n當選擇NO，Enable Pin Internal Pull High/Pull Low Resistor欄位會自動帶入NA。"]
["Ⅱ- Enable Pin Internal Pull High/Pull Low Resistor(k ohm)","NA"]
["Ⅱ- High Side On Resistance (mΩ) -- Typ","NA"]
["Ⅱ- Low Side On Resistance (mΩ) -- Typ","NA"]
["Ⅱ- High Side Driver Resistor Rsource (ohm) -- Typ","NA"]
["Ⅱ- High Side Driver Resistor Rsink (ohm) -- Typ","NA"]
["Ⅱ- Low side Driver Resistor Rsource (ohm) -- Typ","NA"]
["Ⅱ- Low Side Driver Resistor Rsink (ohm) -- Typ","NA"]
["Ⅱ- Dead Time High Side Off to Low Side On (ns) -- Typ","NA"]
["Ⅱ- Dead Time Low Side Off to High Side On (ns) -- Typ","NA"]
["Ⅱ- OVP Type","NA","▼下拉式選單\nThis OVP is for output voltage"]
["Ⅱ- OVP protection mode","NA","▼下拉式選單"]
["Ⅱ- OVP Threshold-Percentage (%) -- Min","NA","This OVP is for output voltage"]
["Ⅱ- OVP Threshold-Fixed (V) -- Min","NA"]
["Ⅱ- OVP Threshold-Programmable (V) -- Min","NA"]
["Ⅱ- OVP Threshold-Programmable (V) -- Max","NA"]
["Ⅱ- OVP Threshold-Programmable Step (mV)","NA"]
["Ⅱ- OVP Threshold-Relative to VID/DAC (mV)","NA","If OVP Threshold=VID/Vo/DAC+\"Voltage(fixed value)\",  please fill in voltage with fixed value."]
["Ⅱ- OVP Threshold-Other","NA","OVP type為Other 時，需填寫此欄位描述OVP架構"]
["Ⅱ- OVP Threshold-Other (V)","NA","OVP type為Other 時，需填寫此欄位"]
["Ⅱ- Absolute OVP Threshold (V) -- Max","NA"]
["Ⅱ- Absolute OVP Threshold (V) -- Min","NA"]
["Ⅱ- OVP Delay Time Type","NA","▼下拉式選單\n如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅱ- OVP Delay Time-Fixed Value (uS) -- Min","NA","如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅱ- OVP Delay Time-Programable (uS) -- Max","NA","如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅱ- OVP Delay Time-Programable (uS) -- Min","NA","如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅱ- OCP Type","NA","▼下拉式選單"]
["Ⅱ- OCP protection mode","NA","▼下拉式選單"]
["Ⅱ- OCP Threshold -Fixed (A) -- Min","NA"]
["Ⅱ- OCP Threshold-Low (A) -- Min","NA","Current limit pin is pull low"]
["Ⅱ- OCP Threshold-Floating (A) -- Min","NA","Current limit pin is floating"]
["Ⅱ- OCP Threshold-High (A) -- Min","NA","Current limit pin is pull high"]
["Ⅱ- OCP Threshold-Adjust by Resistor (A)","NA","請填寫OCP可調整範圍\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅱ- OCP Threshold-Other","NA","OCP type為Other 時，需填寫此欄位描述OCP架構"]
["Ⅱ- OCP Threshold-Other (A) -- Min","NA","OCP type為Other 時，需填寫此欄位"]
["Ⅱ- Itrip/Ics Source Current (uA)","NA","The current source for current limit\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅱ- Itrip/Ics Temperature Coefficient (ppm/℃)","NA"]
["Ⅱ- Softstart Type","NA","▼下拉式選單"]
["Ⅱ- Softstart (mS)-Fixed -- Max","NA","From EN=High to Vout=95%"]
["Ⅱ- Softstart (mS)-Fixed -- Min","NA","From EN=High to Vout=95%"]
["Ⅱ- Softstart-Relative to VID/DAC(mS) -- Max","NA","1. If Softstart=\"Fixed value\" (mS) + VID slow rate, please fill in the fixed value.\n2. From EN=High to Vout=95%"]
["Ⅱ- Softstart-Relative to VID/DAC(mS) -- Min","NA"]
["Ⅱ- Softstart-Other","NA","Softstart type為Other 時，需填寫此欄位描述Softstart架構"]
["Ⅱ- Softstart-Other (mS)","NA","Softstart type為Other 時，需填寫此欄位"]
["Ⅱ- Powergood Delay Time-Low to High (uS)","NA","如datasheet 僅標示power good deglitch time，請填寫power good deglitch time在此欄位。"]
["Ⅱ- Powergood Delay Time-High to Low (uS)","NA","如datasheet 僅標示power good deglitch time，請填寫power good deglitch time在此欄位。"]
["Power rail Ⅲ","No","▼下拉式選單\nPower railⅠ/Power railⅡ/power railⅢ請參考定義(六)"]
["Ⅲ- Output Voltage Architecture","NA","▼下拉式選單"]
["Ⅲ- Output Voltage-Fixed (V) -- Typ","NA"]
["Ⅲ- Output Voltage-Adjustable (V)","NA","Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅲ- Output Voltage-Selectable 1 (V) -- Typ","NA","Selectable 1~4 請依電壓由小到大填寫"]
["Ⅲ- Output Voltage-Selectable 2 (V) -- Typ","NA"]
["Ⅲ- Output Voltage-Selectable 3 (V) -- Typ","NA"]
["Ⅲ- Output Voltage-Selectable 4 (V) -- Typ","NA"]
["Ⅲ- Rated Current (A) -- Typ","NA"]
["Ⅲ- Switching Frequency Type","NA","▼下拉式選單"]
["Ⅲ- Switching Frequency-Fixed (kHz) -- Typ","NA"]
["Ⅲ- Switching Frequency-Adjust by Resistor (kHz) -- Max","NA"]
["Ⅲ- Switching Frequency-Adjust by Resistor (kHz) -- Min","NA"]
["Ⅲ- Switching Frequency-Programmable (kHz) -- Max","NA"]
["Ⅲ- Switching Frequency-Programmable (kHz) -- Min","NA"]
["Ⅲ- Switching Frequency-Other","NA","當Switching Frequency Type 為Other 時，需描述為何種type"]
["Ⅲ- Switching Frequency-Other (kHz)","NA","Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格\n當Switching Frequency Type 為Other 時需填寫此欄位"]
["Ⅲ- What Output Voltage That Switching Frequency Will Lower Than 450kHz (V)","NA","1. COT 架構及High level input voltage converter需填寫此欄位\n2. 使用Vin=20V測試\n3. Low level input voltage converter及output voltage 為Fixed的converter，此欄位請填寫NA\n4. 應用在此電壓以下，需考慮輸出電容增加或使用bulk cap."]
["Ⅲ- VIN UVLO Threshold Voltage (V)-Rising -- Max","NA"]
["Ⅲ- VIN UVLO Threshold Voltage (V)-Falling -- Max","NA"]
["Ⅲ- VREF - Reference Voltage Type","NA","▼下拉式選單"]
["Ⅲ- VREF -Fixed (V) -- Min","NA"]
["Ⅲ- VREF -Fixed (V) -- Typ","NA"]
["Ⅲ- VREF -Fixed (V) -- Max","NA"]
["Ⅲ- VREF -VID0 (V) -- Min","NA"]
["Ⅲ- VREF -VID0 (V) -- Typ","NA"]
["Ⅲ- VREF -VID0 (V) -- Max","NA"]
["Ⅲ- VREF -VID1 (V) -- Min","NA"]
["Ⅲ- VREF -VID1 (V) -- Typ","NA"]
["Ⅲ- VREF -VID1 (V) -- Max","NA"]
["Ⅲ- Output Voltage Accuracy (%) -- Max","NA"]
["Ⅲ- Output Voltage Accuracy (%) -- Min","NA","數值前請加「-」號。e.g. -1、-0.5"]
["Ⅲ- Condition for Output Voltage Accuracy (℃) -- Tj ","NA","Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅲ- Enable Pin Definition","NA","▼下拉式選單"]
["Ⅲ- Enable Pin Type","NA","▼下拉式選單"]
["Ⅲ- Enable/Disable Voltage SPEC (V)-Enable -- Min","NA","100% guaranteed to high voltage\n請參考定義(九)"]
["Ⅲ- Enable/Disable Voltage SPEC (V)-Disable -- Max","NA","100% guaranteed to low voltage\n請參考定義(九)"]
["Ⅲ- Enable/Disable Voltage Threshold (V)-Enable -- Max","NA","100% guaranteed to high voltage\n請參考定義(九)"]
["Ⅲ- Enable/Disable Voltage Threshold (V)-Disable -- Min","NA","100% guaranteed to low voltage\n請參考定義(九)"]
["Ⅲ- Enable Have Hysteresis","NA","▼下拉式選單"]
["Ⅲ- Enable Hysteresis (mV)","NA","VHigh – Vlow"]
["Ⅲ- Enable Minimum Slew Rate (mV/uS)","NA","如果沒有hysteresis, 需填寫IC 允許的enable最小slew rate。\n確認當enable voltage 爬升速度過慢或是在eanble/diasble voltage threshold 中震盪是否會誤動作"]
["Ⅲ- Operation mode-1","NA","▼下拉式選單"]
["Ⅲ- Enable Voltage for Operation Mode-1 (V) -- Min","NA"]
["Ⅲ- Enable Voltage for Operation Mode-1 (V) -- Max","NA"]
["Ⅲ- Operation Mode-2","NA","▼下拉式選單"]
["Ⅲ- Enable Voltage for Operation Mode-2 (V) -- Min","NA"]
["Ⅲ- Enable Voltage for Operation Mode-2 (V) -- Max","NA"]
["Ⅲ- Enable Pin Definition-Other","NA","Enable Pin Definition為other 時，需填寫此欄位描述Enable Pin Definition"]
["Ⅲ- Enable Voltage for Operation Mode-Other(V) -- Min","NA","Enable Pin Definition為other 時，需填寫此欄位"]
["Ⅲ- Enable Voltage for Operation Mode-Other(V) -- Max","NA","Enable Pin Definition為other 時，需填寫此欄位"]
["Ⅲ- Enable Pin Definition-Pull High/Low","NA","▼下拉式選單\n此欄位是確認IC enable pin內部是否有pull high/pull low 電阻。如無此設計請選擇NO。\n當選擇NO，Enable Pin Internal Pull High/Pull Low Resistor欄位會自動帶入NA。"]
["Ⅲ- Enable Pin Internal Pull High/Pull Low Resistor(k ohm)","NA"]
["Ⅲ- High Side On Resistance (mΩ) -- Typ","NA"]
["Ⅲ- Low Side On Resistance (mΩ) -- Typ","NA"]
["Ⅲ- High Side Driver Resistor Rsource (ohm) -- Typ","NA"]
["Ⅲ- High Side Driver Resistor Rsink (ohm) -- Typ","NA"]
["Ⅲ- Low side Driver Resistor Rsource (ohm) -- Typ","NA"]
["Ⅲ- Low Side Driver Resistor Rsink (ohm) -- Typ","NA"]
["Ⅲ- Dead Time High Side Off to Low Side On (ns) -- Typ","NA"]
["Ⅲ- Dead Time Low Side Off to High Side On (ns) -- Typ","NA"]
["Ⅲ- OVP Type","NA","▼下拉式選單\nThis OVP is for output voltage"]
["Ⅲ- OVP protection mode","NA","▼下拉式選單"]
["Ⅲ- OVP Threshold-Percentage (%) -- Min","NA","This OVP is for output voltage"]
["Ⅲ- OVP Threshold-Fixed (V) -- Min","NA"]
["Ⅲ- OVP Threshold-Programmable (V) -- Min","NA"]
["Ⅲ- OVP Threshold-Programmable (V) -- Max","NA"]
["Ⅲ- OVP Threshold-Programmable Step (mV)","NA"]
["Ⅲ- OVP Threshold-Relative to VID/DAC (mV)","NA","If OVP Threshold=VID/Vo/DAC+\"Voltage(fixed value)\",  please fill in voltage with fixed value."]
["Ⅲ- OVP Threshold-Other","NA","OVP type為Other 時，需填寫此欄位描述OVP架構。"]
["Ⅲ- OVP Threshold-Other (V)","NA"]
["Ⅲ- Absolute OVP Threshold (V) -- Max","NA"]
["Ⅲ- Absolute OVP Threshold (V) -- Min","NA"]
["Ⅲ- OVP Delay Time Type","NA","▼下拉式選單\n如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅲ- OVP Delay Time-Fixed Value (uS) -- Min","NA","如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅲ- OVP Delay Time-Programable (uS) -- Max","NA","如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅲ- OVP Delay Time-Programable (uS) -- Min","NA","如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅲ- OCP Type","NA","▼下拉式選單"]
["Ⅲ- OCP protection mode","NA","▼下拉式選單"]
["Ⅲ- OCP Threshold -Fixed (A) -- Min","NA"]
["Ⅲ- OCP Threshold-Low (A) -- Min","NA","Current limit pin is pull low"]
["Ⅲ- OCP Threshold-Floating (A) -- Min","NA","Current limit pin is floating"]
["Ⅲ- OCP Threshold-High (A) -- Min","NA","Current limit pin is pull high"]
["Ⅲ- OCP Threshold-Adjust by Resistor (A)","NA","請填寫OCP可調整範圍\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅲ- OCP Threshold-Other","NA","OCP type為Other 時，需填寫此欄位描述OCP架構"]
["Ⅲ- OCP Threshold-Other (A) -- Min","NA","OCP type為Other 時，需填寫此欄位"]
["Ⅲ- Itrip/Ics Source Current (uA)","NA","The current source for current limit\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅲ- Itrip/Ics Temperature Coefficient (ppm/℃)","NA"]
["Ⅲ- Softstart Type","NA","▼下拉式選單"]
["Ⅲ- Softstart (mS)-Fixed -- Max","NA","From EN=High to Vout=95%"]
["Ⅲ- Softstart (mS)-Fixed -- Min","NA","From EN=High to Vout=95%"]
["Ⅲ- Softstart-Relative to VID/DAC(mS) -- Max","NA","1. If Softstart=\"Fixed value\" (mS) + VID slow rate, please fill in the fixed value.\n2. From EN=High to Vout=95%"]
["Ⅲ- Softstart-Relative to VID/DAC(mS) -- Min","NA"]
["Ⅲ- Softstart-Other","NA","Softstart type為Other 時，需填寫此欄位描述Softstart架構"]
["Ⅲ- Softstart-Other (mS)","NA","Softstart type為Other 時，需填寫此欄位"]
["Ⅲ- Powergood Delay Time-Low to High (uS)","NA","如datasheet 僅標示power good deglitch time，請填寫power good deglitch time在此欄位。"]
["Ⅲ- Powergood Delay Time-High to Low (uS)","NA","如datasheet 僅標示power good deglitch time，請填寫power good deglitch time在此欄位。"]
["Which Rated Current of The Power Rail Is Over 10A That Needs to Testing UIS ","NA"]
["COMPAL CE Exempt from UIS","NA","▼下拉式選單"]
["High Side UIS Test for MOSFET (Production line) at Package Level","NA","▼下拉式選單"]
["Low Side UIS Test for MOSFET (Production line) at Package Level","NA","▼下拉式選單"]
["Recommended Operating Junction Temperature Range (℃)","-40~125","Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["*ESD (CDM)","C4(500~<1000)","▼下拉式選單\ne.g. If CDM is passed 1000V, please select the C5"]
["*ESD (HBM)","2(2000~<4000)","▼下拉式選單\ne.g. If HBM is passed 2000V, please select the 2"]
["*Lead Free","MY (Manuf_LF)","▼下拉式選單"]
["*Ecology (MSD Declaration)","Green Part(RoHS)","▼下拉式選單\nSPEC當中需宣告"]
["*Tape Width (mm)",8,"請參考定義二"]
["*Tape Width Upper Tolerance (+)",0.3]
["*Tape Width Lower Tolerance (-)",0.3]
["*Component Pitch (mm)",4]
["*Component Pitch Upper Tolerance (+)",0.1]
["*Component Pitch Lower Tolerance (-)",0.1]
["*Tape Depth (mm)",0.85]
["*Tape Depth Upper Tolerance (+)",0.2]
["*Tape Depth Lower Tolerance (-)",0.2]
["*PIN1","第二象限","▼下拉式選單\n請參考定義(一)，Follow EIA 481象限定義填寫"]
["*Lead Pin Type","No Lead","▼下拉式選單\n請參考定義(十)"]
["*Lead Pin b Nominal (mm)",0.2,"請參考定義(五)\nNon-Standard footprint及 WLCSP、BGA…等 package type 不需填寫"]
["*Lead Pin b Upper Tolerance (+)",0.8]
["*Lead Pin b Lower Tolerance (-)",0.8]
["*Lead Pin L Nominal (mm)",0.4]
["*Lead Pin L Upper Tolerance (+)",0.1]
["*Lead Pin L Lower Tolerance (-)",0.1]
["*Multiple Thermal Pin","NO","▼下拉式選單"]
["*Packing: (T&R or Tray)","T&R","▼下拉式選單"]
["*Packaging Material: (Paper or Embossed)","Embossed","▼下拉式選單\n此欄位為料帶材質，請參考定義(七)"]
["*Datasheet Version","0.9B","請依照版本填寫"]
["*Datasheet Version Release Date",2021,"日期請依照 \"西元年/月/日\" 填寫，ex. 2018/10/10 \n若僅有年、月，請填寫當月份1日，ex. 2018/10/1"]

{"sheet":"Converter","index":2,"n_rows":362,"n_cols":7,"rows_kept":362,"cut":false,"hidden":false,"merged":[[351,2,356,2],[44,2,47,2],[340,2,348,2],[33,2,35,2],[9,2,17,2],[103,2,107,2],[200,2,204,2],[297,2,301,2],[141,2,144,2],[238,2,241,2]]}
[]
["Converter REV A04"]
["Item","Application","Note"]
["*PSL/ECSL Catelog","Converter"]
["*Category",null,"▼下拉式選單"]
["*Function","POL"]
["*Manufacturer"]
["*Manufacturer PN",null,"填寫完整Manufacturer PN"]
["*Package Type",null,"填寫封裝類型即可，e.g. QFN,DFN,WLCSP…"]
["*Length(D) Nominal (mm)",null,"請參考定義(三)"]
["*Length(D) Upper Tolerance (+)"]
["*Length(D) Lower Tolerance (-)"]
["*Width(E) Nominal (mm)"]
["*Width(E) Upper Tolerance (+)"]
["*Width(E) Lower Tolerance (-)"]
["*Height(A) Nominal (mm)"]
["*Height(A) Upper Tolerance (+)"]
["*Height(A) Lower Tolerance (-)"]
["*Footprint Type",null,"▼下拉式選單\n請參考定義(四)"]
["*DXF Document for Non-Standard Footprint",null,"▼下拉式選單\n如為Non-Standard footprint必需要提供"]
["*Pitch (Pin-to-Pin) (mm)"]
["*Pin Count",null,"請參考定義八"]
["IC Manufacture Process (Monolithic or Multi-chip)",null,"▼下拉式選單"]
["*Feedback and Setting Architecture",null,"▼下拉式選單"]
["VIN/VCC/Driver VCC supply type",null,"▼下拉式選單\nVCC:The power of logic/control circuits,  Driver VCC:The power of high/Low side gate dirve"]
["Recommended VIN Supply Operation Voltage Range (V)",null,"Input Voltage for High side MOS drain\nRange的部分請用波浪號「 ~ 」表示"]
["Absolute VIN Supply Voltage Range (V)",null,"Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Recommended VCC Supply Operation Voltage Range (V)",null,"Logic/Control circuits input voltage\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Recommended Driver VCC Supply Operation Voltage Range (V)",null,"High/Low side gate dirve input voltage\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["LX/SW Switching Node Peak/AC Absolute Voltage Range (V)",null,"Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["VIN Shutdown Current, EN=0V (uA) -- Max"]
["VCC Shutdown Current, EN=0V (uA) -- Max",null,"Logic/Control circuits off-mode current"]
["Driver VCC Shutdown Current, EN=0V (uA) -- Max",null,"High/Low side gate dirve off-mode current"]
["Vin Quiescent Current (uA) -- Max",null,"Enable=High, IOUT=0A, device not switching"]
["VCC Quiescent Current (uA) -- Max"]
["Driver VCC Quiescent Current (uA) -- Max"]
["VCC UVLO Threshold Voltage (V)-Rising -- Max"]
["VCC UVLO Threshold Voltage (V)-Falling -- Max"]
["Driver VCC UVLO Threshold Voltage (V)-Rising -- Max"]
["Driver VCC UVLO Threshold Voltage (V)-Falling -- Max"]
["Power railⅠ",null,"▼下拉式選單\nPower railⅠ/Power railⅡ/power railⅢ請參考定義六"]
["Ⅰ- Output Voltage Architecture",null,"▼下拉式選單"]
["Ⅰ- Output Voltage-Fixed (V) -- Typ"]
["Ⅰ- Output Voltage-Adjustable (V)",null,"Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅰ- Output Voltage-Selectable 1 (V) -- Typ",null,"Selectable 1~4 請依電壓由小到大填寫"]
["Ⅰ- Output Voltage-Selectable 2 (V) -- Typ"]
["Ⅰ- Output Voltage-Selectable 3 (V) -- Typ"]
["Ⅰ- Output Voltage-Selectable 4 (V) -- Typ"]
["Ⅰ- Rated Current (A) -- Typ"]
["Ⅰ- Switching Frequency Type",null,"▼下拉式選單"]
["Ⅰ- Switching Frequency-Fixed (kHz) -- Typ"]
["Ⅰ- Switching Frequency-Adjust by Resistor (kHz) -- Max"]
["Ⅰ- Switching Frequency-Adjust by Resistor (kHz) -- Min"]
["Ⅰ- Switching Frequency-Programmable (kHz) -- Max"]
["Ⅰ- Switching Frequency-Programmable (kHz) -- Min"]
["Ⅰ- Switching Frequency-Other",null,"當Switching Frequency Type 為Other 時，需描述為何種type"]
["Ⅰ- Switching Frequency-Other (kHz)",null,"Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格\n當Switching Frequency Type 為Other 時需填寫此欄位"]
["Ⅰ- What Output Voltage That Switching Frequency Will Lower Than 450kHz (V)",null,"1. COT 架構及High level input voltage converter需填寫此欄位\n2. 使用Vin=20V測試\n3. Low level input voltage converter及output voltage 為Fixed的converter，此欄位請填寫NA\n4. 應用在此電壓以下，需考慮輸出電容增加或使用bulk cap."]
["Ⅰ- VIN UVLO Threshold Voltage (V)-Rising -- Max"]
["Ⅰ- VIN UVLO Threshold Voltage (V)-Falling -- Max"]
["Ⅰ- VREF - Reference Voltage Type",null,"▼下拉式選單"]
["Ⅰ- VREF -Fixed (V) -- Min"]
["Ⅰ- VREF -Fixed (V) -- Typ"]
["Ⅰ- VREF -Fixed (V) -- Max"]
["Ⅰ- VREF -VID0 (V) -- Min"]
["Ⅰ- VREF -VID0 (V) -- Typ"]
["Ⅰ- VREF -VID0 (V) -- Max"]
["Ⅰ- VREF -VID1 (V) -- Min"]
["Ⅰ- VREF -VID1 (V) -- Typ"]
["Ⅰ- VREF -VID1 (V) -- Max"]
["Ⅰ- Output Voltage Accuracy (%) -- Max"]
["Ⅰ- Output Voltage Accuracy (%) -- Min",null,"數值前請加「-」號。e.g. -1、-0.5"]
["Ⅰ- Condition for Output Voltage Accuracy (℃) -- Tj ",null,"Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅰ- Enable Pin Definition",null,"▼下拉式選單"]
["Ⅰ- Enable Pin Type",null,"▼下拉式選單"]
["Ⅰ- Enable/Disable Voltage SPEC (V)-Enable -- Min",null,"100% guaranteed to high voltage\n請參考定義(九)"]
["Ⅰ- Enable/Disable Voltage SPEC (V)-Disable -- Max",null,"100% guaranteed to low voltage\n請參考定義(九)"]
["Ⅰ- Enable/Disable Voltage Threshold (V)-Enable -- Max",null,"100% guaranteed to high voltage\n請參考定義(九)"]
["Ⅰ- Enable/Disable Voltage Threshold (V)-Disable -- Min",null,"100% guaranteed to low voltage\n請參考定義(九)"]
["Ⅰ- Enable Have Hysteresis",null,"▼下拉式選單"]
["Ⅰ- Enable Hysteresis (mV)",null,"VHigh – Vlow"]
["Ⅰ- Enable Minimum Slew Rate (mV/uS)",null,"如果沒有hysteresis, 需填寫IC 允許的enable最小slew rate。\n確認當enable voltage 爬升速度過慢或是在eanble/diasble voltage threshold 中震盪是否會誤動作"]
["Ⅰ- Operation mode-1",null,"▼下拉式選單"]
["Ⅰ- Enable Voltage for Operation Mode-1 (V) -- Min"]
["Ⅰ- Enable Voltage for Operation Mode-1 (V) -- Max"]
["Ⅰ- Operation Mode-2",null,"▼下拉式選單"]
["Ⅰ- Enable Voltage for Operation Mode-2 (V) -- Min"]
["Ⅰ- Enable Voltage for Operation Mode-2 (V) -- Max"]
["Ⅰ- Enable Pin Definition-Other",null,"Enable Pin Definition為other 時，需填寫此欄位描述Enable Pin Definition"]
["Ⅰ- Enable Voltage for Operation Mode-Other(V) -- Min",null,"Enable Pin Definition為other 時，需填寫此欄位"]
["Ⅰ- Enable Voltage for Operation Mode-Other(V) -- Max",null,"Enable Pin Definition為other 時，需填寫此欄位"]
["Ⅰ- Enable Pin Definition-Pull High/Low",null,"▼下拉式選單\n此欄位是確認IC enable pin內部是否有pull high/pull low 電阻。如無此設計請選擇NO。\n當選擇NO，Enable Pin Internal Pull High/Pull Low Resistor欄位會自動帶入NA。"]
["Ⅰ- Enable Pin Internal Pull High/Pull Low Resistor(k ohm)"]
["Ⅰ- High Side On Resistance (mΩ) -- Typ"]
["Ⅰ- Low Side On Resistance (mΩ) -- Typ"]
["Ⅰ- High Side Driver Resistor Rsource (ohm) -- Typ"]
["Ⅰ- High Side Driver Resistor Rsink (ohm) -- Typ"]
["Ⅰ- Low side Driver Resistor Rsource (ohm) -- Typ"]
["Ⅰ- Low Side Driver Resistor Rsink (ohm) -- Typ"]
["Ⅰ- Dead Time High Side Off to Low Side On (ns) -- Typ"]
["Ⅰ- Dead Time Low Side Off to High Side On (ns) -- Typ"]
["Ⅰ- OVP Type",null,"▼下拉式選單\nThis OVP is for output voltage"]
["Ⅰ- OVP protection mode",null,"▼下拉式選單"]
["Ⅰ- OVP Threshold-Percentage (%) -- Min",null,"This OVP is for output voltage"]
["Ⅰ- OVP Threshold-Fixed (V) -- Min"]
["Ⅰ- OVP Threshold-Programmable (V) -- Min"]
["Ⅰ- OVP Threshold-Programmable (V) -- Max"]
["Ⅰ- OVP Threshold-Programmable Step (mV)"]
["Ⅰ- OVP Threshold-Relative to VID/DAC (mV)",null,"If OVP Threshold=VID/Vo/DAC+\"Voltage(fixed value)\", please fill in voltage with fixed value."]
["Ⅰ- OVP Threshold-Other",null,"OVP type為Other 時，需填寫此欄位描述OVP架構"]
["Ⅰ- OVP Threshold-Other (V)",null,"OVP type為Other 時，需填寫此欄位"]
["Ⅰ- Absolute OVP Threshold (V) -- Max"]
["Ⅰ- Absolute OVP Threshold (V) -- Min"]
["Ⅰ- OVP Delay Time Type",null,"▼下拉式選單\n如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅰ- OVP Delay Time-Fixed Value (uS) -- Min",null,"如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅰ- OVP Delay Time-Programable (uS) -- Max",null,"如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅰ- OVP Delay Time-Programable (uS) -- Min",null,"如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅰ- OCP Type",null,"▼下拉式選單"]
["Ⅰ- OCP protection mode",null,"▼下拉式選單"]
["Ⅰ- OCP Threshold -Fixed (A) -- Min"]
["Ⅰ- OCP Threshold-Low  (A) -- Min",null,"Current limit pin is pull low"]
["Ⅰ- OCP Threshold-Floating  (A) -- Min",null,"Current limit pin is floating"]
["Ⅰ- OCP Threshold-High (A) -- Min",null,"Current limit pin is pull high"]
["Ⅰ- OCP Threshold-Adjust by Resistor (A)",null,"請填寫OCP可調整範圍\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅰ- OCP Threshold-Other",null,"OCP type為Other 時，需填寫此欄位描述OCP架構"]
["Ⅰ- OCP Threshold-Other (A) -- Min",null,"OCP type為Other 時，需填寫此欄位\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅰ- Itrip/Ics Source Current (uA)",null,"The current source for current limit\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅰ- Itrip/Ics Temperature Coefficient (ppm/℃)"]
["Ⅰ- Softstart Type",null,"▼下拉式選單"]
["Ⅰ- Softstart (mS)-Fixed -- Max",null,"From EN=High to Vout=95%"]
["Ⅰ- Softstart (mS)-Fixed -- Min",null,"From EN=High to Vout=95%"]
["Ⅰ- Softstart-Relative to VID/DAC(mS) -- Max",null,"1. If Softstart=\"Fixed value\" (mS) + VID slow rate, please fill in the fixed value.\n2. From EN=High to Vout=95%"]
["Ⅰ- Softstart-Relative to VID/DAC(mS) -- Min"]
["Ⅰ- Softstart-Other",null,"Softstart type為Other 時，需填寫此欄位描述Softstart架構"]
["Ⅰ- Softstart-Other (mS)",null,"Softstart type為Other 時，需填寫此欄位"]
["Ⅰ- Powergood Delay Time-Low to High (uS)",null,"如datasheet 僅標示power good deglitch time，請填寫power good deglitch time在此欄位。"]
["Ⅰ- Powergood Delay Time-High to Low (uS)",null,"如datasheet 僅標示power good deglitch time，請填寫power good deglitch time在此欄位。"]
["Power rail Ⅱ",null,"▼下拉式選單\nPower railⅠ/Power railⅡ/power railⅢ請參考定義(六)"]
["Ⅱ- Output Voltage Architecture",null,"下拉式選單"]
["Ⅱ- Output Voltage-Fixed (V) -- Typ"]
["Ⅱ- Output Voltage-Adjustable (V)",null,"Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅱ- Output Voltage-Selectable 1 (V) -- Typ",null,"Selectable 1~4 請依電壓由小到大填寫"]
["Ⅱ- Output Voltage-Selectable 2 (V) -- Typ"]
["Ⅱ- Output Voltage-Selectable 3 (V) -- Typ"]
["Ⅱ- Output Voltage-Selectable 4 (V) -- Typ"]
["Ⅱ- Rated Current (A) -- Typ"]
["Ⅱ- Switching Frequency Type",null,"▼下拉式選單"]
["Ⅱ- Switching Frequency-Fixed (kHz) -- Typ"]
["Ⅱ- Switching Frequency-Adjust by Resistor (kHz) -- Max"]
["Ⅱ- Switching Frequency-Adjust by Resistor (kHz) -- Min"]
["Ⅱ- Switching Frequency-Programmable (kHz) -- Max"]
["Ⅱ- Switching Frequency-Programmable (kHz) -- Min"]
["Ⅱ- Switching Frequency-Other",null,"當Switching Frequency Type 為Other 時，需描述為何種type"]
["Ⅱ- Switching Frequency-Other (kHz)",null,"Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格\n當Switching Frequency Type 為Other 時需填寫此欄位"]
["Ⅱ- What Output Voltage That Switching Frequency Will Lower Than 450kHz (V)",null,"1. COT 架構及High level input voltage converter需填寫此欄位\n2. 使用Vin=20V測試\n3. Low level input voltage converter及output voltage 為Fixed的converter，此欄位請填寫NA\n4. 應用在此電壓以下，需考慮輸出電容增加或使用bulk cap."]
["Ⅱ- VIN UVLO Threshold Voltage (V)-Rising -- Max"]
["Ⅱ- VIN UVLO Threshold Voltage (V)-Falling -- Max"]
["Ⅱ- VREF - Reference Voltage Type",null,"▼下拉式選單"]
["Ⅱ- VREF -Fixed (V) -- Min"]
["Ⅱ- VREF -Fixed (V) -- Typ"]
["Ⅱ- VREF -Fixed (V) -- Max"]
["Ⅱ- VREF -VID0 (V) -- Min"]
["Ⅱ- VREF -VID0 (V) -- Typ"]
["Ⅱ- VREF -VID0 (V) -- Max"]
["Ⅱ- VREF -VID1 (V) -- Min"]
["Ⅱ- VREF -VID1 (V) -- Typ"]
["Ⅱ- VREF -VID1 (V) -- Max"]
["Ⅱ- Output Voltage Accuracy (%) -- Max"]
["Ⅱ- Output Voltage Accuracy (%) -- Min",null,"數值前請加「-」號。e.g. -1、-0.5"]
["Ⅱ- Condition for Output Voltage Accuracy (℃) -- Tj ",null,"Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅱ- Enable Pin Definition",null,"▼下拉式選單"]
["Ⅱ- Enable Pin Type",null,"▼下拉式選單"]
["Ⅱ- Enable/Disable Voltage SPEC (V)-Enable -- Min",null,"100% guaranteed to high voltage\n請參考定義(九)"]
["Ⅱ- Enable/Disable Voltage SPEC (V)-Disable -- Max",null,"100% guaranteed to low voltage\n請參考定義(九)"]
["Ⅱ- Enable/Disable Voltage Threshold (V)-Enable -- Max",null,"100% guaranteed to high voltage\n請參考定義(九)"]
["Ⅱ- Enable/Disable Voltage Threshold (V)-Disable -- Min",null,"100% guaranteed to low voltage\n請參考定義(九)"]
["Ⅱ- Enable Have Hysteresis",null,"▼下拉式選單"]
["Ⅱ- Enable Hysteresis (mV)",null,"VHigh – Vlow"]
["Ⅱ- Enable Minimum Slew Rate (mV/uS)",null,"如果沒有hysteresis, 需填寫IC 允許的enable最小slew rate。\n確認當enable voltage 爬升速度過慢或是在eanble/diasble voltage threshold 中震盪是否會誤動作"]
["Ⅱ- Operation mode-1",null,"▼下拉式選單"]
["Ⅱ- Enable Voltage for Operation Mode-1 (V) -- Min"]
["Ⅱ- Enable Voltage for Operation Mode-1 (V) -- Max"]
["Ⅱ- Operation Mode-2",null,"▼下拉式選單"]
["Ⅱ- Enable Voltage for Operation Mode-2 (V) -- Min"]
["Ⅱ- Enable Voltage for Operation Mode-2 (V) -- Max"]
["Ⅱ- Enable Pin Definition-Other",null,"Enable Pin Definition為other 時，需填寫此欄位描述Enable Pin Definition"]
["Ⅱ- Enable Voltage for Operation Mode-Other(V) -- Min",null,"Enable Pin Definition為other 時，需填寫此欄位"]
["Ⅱ- Enable Voltage for Operation Mode-Other(V) -- Max",null,"Enable Pin Definition為other 時，需填寫此欄位"]
["Ⅱ- Enable Pin Definition-Pull High/Low",null,"▼下拉式選單\n此欄位是確認IC enable pin內部是否有pull high/pull low 電阻。如無此設計請選擇NO。\n當選擇NO，Enable Pin Internal Pull High/Pull Low Resistor欄位會自動帶入NA。"]
["Ⅱ- Enable Pin Internal Pull High/Pull Low Resistor(k ohm)"]
["Ⅱ- High Side On Resistance (mΩ) -- Typ"]
["Ⅱ- Low Side On Resistance (mΩ) -- Typ"]
["Ⅱ- High Side Driver Resistor Rsource (ohm) -- Typ"]
["Ⅱ- High Side Driver Resistor Rsink (ohm) -- Typ"]
["Ⅱ- Low side Driver Resistor Rsource (ohm) -- Typ"]
["Ⅱ- Low Side Driver Resistor Rsink (ohm) -- Typ"]
["Ⅱ- Dead Time High Side Off to Low Side On (ns) -- Typ"]
["Ⅱ- Dead Time Low Side Off to High Side On (ns) -- Typ"]
["Ⅱ- OVP Type",null,"▼下拉式選單\nThis OVP is for output voltage"]
["Ⅱ- OVP protection mode",null,"▼下拉式選單"]
["Ⅱ- OVP Threshold-Percentage (%) -- Min",null,"This OVP is for output voltage"]
["Ⅱ- OVP Threshold-Fixed (V) -- Min"]
["Ⅱ- OVP Threshold-Programmable (V) -- Min"]
["Ⅱ- OVP Threshold-Programmable (V) -- Max"]
["Ⅱ- OVP Threshold-Programmable Step (mV)"]
["Ⅱ- OVP Threshold-Relative to VID/DAC (mV)",null,"If OVP Threshold=VID/Vo/DAC+\"Voltage(fixed value)\",  please fill in voltage with fixed value."]
["Ⅱ- OVP Threshold-Other",null,"OVP type為Other 時，需填寫此欄位描述OVP架構"]
["Ⅱ- OVP Threshold-Other (V)",null,"OVP type為Other 時，需填寫此欄位"]
["Ⅱ- Absolute OVP Threshold (V) -- Max"]
["Ⅱ- Absolute OVP Threshold (V) -- Min"]
["Ⅱ- OVP Delay Time Type",null,"▼下拉式選單\n如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅱ- OVP Delay Time-Fixed Value (uS) -- Min",null,"如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅱ- OVP Delay Time-Programable (uS) -- Max",null,"如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅱ- OVP Delay Time-Programable (uS) -- Min",null,"如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅱ- OCP Type",null,"▼下拉式選單"]
["Ⅱ- OCP protection mode",null,"▼下拉式選單"]
["Ⅱ- OCP Threshold -Fixed (A) -- Min"]
["Ⅱ- OCP Threshold-Low (A) -- Min",null,"Current limit pin is pull low"]
["Ⅱ- OCP Threshold-Floating (A) -- Min",null,"Current limit pin is floating"]
["Ⅱ- OCP Threshold-High (A) -- Min",null,"Current limit pin is pull high"]
["Ⅱ- OCP Threshold-Adjust by Resistor (A)",null,"請填寫OCP可調整範圍\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅱ- OCP Threshold-Other",null,"OCP type為Other 時，需填寫此欄位描述OCP架構"]
["Ⅱ- OCP Threshold-Other (A) -- Min",null,"OCP type為Other 時，需填寫此欄位"]
["Ⅱ- Itrip/Ics Source Current (uA)",null,"The current source for current limit\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅱ- Itrip/Ics Temperature Coefficient (ppm/℃)"]
["Ⅱ- Softstart Type",null,"▼下拉式選單"]
["Ⅱ- Softstart (mS)-Fixed -- Max",null,"From EN=High to Vout=95%"]
["Ⅱ- Softstart (mS)-Fixed -- Min",null,"From EN=High to Vout=95%"]
["Ⅱ- Softstart-Relative to VID/DAC(mS) -- Max",null,"1. If Softstart=\"Fixed value\" (mS) + VID slow rate, please fill in the fixed value.\n2. From EN=High to Vout=95%"]
["Ⅱ- Softstart-Relative to VID/DAC(mS) -- Min"]
["Ⅱ- Softstart-Other",null,"Softstart type為Other 時，需填寫此欄位描述Softstart架構"]
["Ⅱ- Softstart-Other (mS)",null,"Softstart type為Other 時，需填寫此欄位"]
["Ⅱ- Powergood Delay Time-Low to High (uS)",null,"如datasheet 僅標示power good deglitch time，請填寫power good deglitch time在此欄位。"]
["Ⅱ- Powergood Delay Time-High to Low (uS)",null,"如datasheet 僅標示power good deglitch time，請填寫power good deglitch time在此欄位。"]
["Power rail Ⅲ",null,"▼下拉式選單\nPower railⅠ/Power railⅡ/power railⅢ請參考定義(六)"]
["Ⅲ- Output Voltage Architecture",null,"▼下拉式選單"]
["Ⅲ- Output Voltage-Fixed (V) -- Typ"]
["Ⅲ- Output Voltage-Adjustable (V)",null,"Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅲ- Output Voltage-Selectable 1 (V) -- Typ",null,"Selectable 1~4 請依電壓由小到大填寫"]
["Ⅲ- Output Voltage-Selectable 2 (V) -- Typ"]
["Ⅲ- Output Voltage-Selectable 3 (V) -- Typ"]
["Ⅲ- Output Voltage-Selectable 4 (V) -- Typ"]
["Ⅲ- Rated Current (A) -- Typ"]
["Ⅲ- Switching Frequency Type",null,"▼下拉式選單"]
["Ⅲ- Switching Frequency-Fixed (kHz) -- Typ"]
["Ⅲ- Switching Frequency-Adjust by Resistor (kHz) -- Max"]
["Ⅲ- Switching Frequency-Adjust by Resistor (kHz) -- Min"]
["Ⅲ- Switching Frequency-Programmable (kHz) -- Max"]
["Ⅲ- Switching Frequency-Programmable (kHz) -- Min"]
["Ⅲ- Switching Frequency-Other",null,"當Switching Frequency Type 為Other 時，需描述為何種type"]
["Ⅲ- Switching Frequency-Other (kHz)",null,"Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格\n當Switching Frequency Type 為Other 時需填寫此欄位"]
["Ⅲ- What Output Voltage That Switching Frequency Will Lower Than 450kHz (V)",null,"1. COT 架構及High level input voltage converter需填寫此欄位\n2. 使用Vin=20V測試\n3. Low level input voltage converter及output voltage 為Fixed的converter，此欄位請填寫NA\n4. 應用在此電壓以下，需考慮輸出電容增加或使用bulk cap."]
["Ⅲ- VIN UVLO Threshold Voltage (V)-Rising -- Max"]
["Ⅲ- VIN UVLO Threshold Voltage (V)-Falling -- Max"]
["Ⅲ- VREF - Reference Voltage Type",null,"▼下拉式選單"]
["Ⅲ- VREF -Fixed (V) -- Min"]
["Ⅲ- VREF -Fixed (V) -- Typ"]
["Ⅲ- VREF -Fixed (V) -- Max"]
["Ⅲ- VREF -VID0 (V) -- Min"]
["Ⅲ- VREF -VID0 (V) -- Typ"]
["Ⅲ- VREF -VID0 (V) -- Max"]
["Ⅲ- VREF -VID1 (V) -- Min"]
["Ⅲ- VREF -VID1 (V) -- Typ"]
["Ⅲ- VREF -VID1 (V) -- Max"]
["Ⅲ- Output Voltage Accuracy (%) -- Max"]
["Ⅲ- Output Voltage Accuracy (%) -- Min",null,"數值前請加「-」號。e.g. -1、-0.5"]
["Ⅲ- Condition for Output Voltage Accuracy (℃) -- Tj ",null,"Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅲ- Enable Pin Definition",null,"▼下拉式選單"]
["Ⅲ- Enable Pin Type",null,"▼下拉式選單"]
["Ⅲ- Enable/Disable Voltage SPEC (V)-Enable -- Min",null,"100% guaranteed to high voltage\n請參考定義(九)"]
["Ⅲ- Enable/Disable Voltage SPEC (V)-Disable -- Max",null,"100% guaranteed to low voltage\n請參考定義(九)"]
["Ⅲ- Enable/Disable Voltage Threshold (V)-Enable -- Max",null,"100% guaranteed to high voltage\n請參考定義(九)"]
["Ⅲ- Enable/Disable Voltage Threshold (V)-Disable -- Min",null,"100% guaranteed to low voltage\n請參考定義(九)"]
["Ⅲ- Enable Have Hysteresis",null,"▼下拉式選單"]
["Ⅲ- Enable Hysteresis (mV)",null,"VHigh – Vlow"]
["Ⅲ- Enable Minimum Slew Rate (mV/uS)",null,"如果沒有hysteresis, 需填寫IC 允許的enable最小slew rate。\n確認當enable voltage 爬升速度過慢或是在eanble/diasble voltage threshold 中震盪是否會誤動作"]
["Ⅲ- Operation mode-1",null,"▼下拉式選單"]
["Ⅲ- Enable Voltage for Operation Mode-1 (V) -- Min"]
["Ⅲ- Enable Voltage for Operation Mode-1 (V) -- Max"]
["Ⅲ- Operation Mode-2",null,"▼下拉式選單"]
["Ⅲ- Enable Voltage for Operation Mode-2 (V) -- Min"]
["Ⅲ- Enable Voltage for Operation Mode-2 (V) -- Max"]
["Ⅲ- Enable Pin Definition-Other",null,"Enable Pin Definition為other 時，需填寫此欄位描述Enable Pin Definition"]
["Ⅲ- Enable Voltage for Operation Mode-Other(V) -- Min",null,"Enable Pin Definition為other 時，需填寫此欄位"]
["Ⅲ- Enable Voltage for Operation Mode-Other(V) -- Max",null,"Enable Pin Definition為other 時，需填寫此欄位"]
["Ⅲ- Enable Pin Definition-Pull High/Low",null,"▼下拉式選單\n此欄位是確認IC enable pin內部是否有pull high/pull low 電阻。如無此設計請選擇NO。\n當選擇NO，Enable Pin Internal Pull High/Pull Low Resistor欄位會自動帶入NA。"]
["Ⅲ- Enable Pin Internal Pull High/Pull Low Resistor(k ohm)"]
["Ⅲ- High Side On Resistance (mΩ) -- Typ"]
["Ⅲ- Low Side On Resistance (mΩ) -- Typ"]
["Ⅲ- High Side Driver Resistor Rsource (ohm) -- Typ"]
["Ⅲ- High Side Driver Resistor Rsink (ohm) -- Typ"]
["Ⅲ- Low side Driver Resistor Rsource (ohm) -- Typ"]
["Ⅲ- Low Side Driver Resistor Rsink (ohm) -- Typ"]
["Ⅲ- Dead Time High Side Off to Low Side On (ns) -- Typ"]
["Ⅲ- Dead Time Low Side Off to High Side On (ns) -- Typ"]
["Ⅲ- OVP Type",null,"▼下拉式選單\nThis OVP is for output voltage"]
["Ⅲ- OVP protection mode",null,"▼下拉式選單"]
["Ⅲ- OVP Threshold-Percentage (%) -- Min",null,"This OVP is for output voltage"]
["Ⅲ- OVP Threshold-Fixed (V) -- Min"]
["Ⅲ- OVP Threshold-Programmable (V) -- Min"]
["Ⅲ- OVP Threshold-Programmable (V) -- Max"]
["Ⅲ- OVP Threshold-Programmable Step (mV)"]
["Ⅲ- OVP Threshold-Relative to VID/DAC (mV)",null,"If OVP Threshold=VID/Vo/DAC+\"Voltage(fixed value)\",  please fill in voltage with fixed value."]
["Ⅲ- OVP Threshold-Other",null,"OVP type為Other 時，需填寫此欄位描述OVP架構。"]
["Ⅲ- OVP Threshold-Other (V)"]
["Ⅲ- Absolute OVP Threshold (V) -- Max"]
["Ⅲ- Absolute OVP Threshold (V) -- Min"]
["Ⅲ- OVP Delay Time Type",null,"▼下拉式選單\n如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅲ- OVP Delay Time-Fixed Value (uS) -- Min",null,"如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅲ- OVP Delay Time-Programable (uS) -- Max",null,"如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅲ- OVP Delay Time-Programable (uS) -- Min",null,"如datasheet 僅標示OVP deglitch time ，請填寫OVP deglitch time在此欄位。"]
["Ⅲ- OCP Type",null,"▼下拉式選單"]
["Ⅲ- OCP protection mode",null,"▼下拉式選單"]
["Ⅲ- OCP Threshold -Fixed (A) -- Min"]
["Ⅲ- OCP Threshold-Low (A) -- Min",null,"Current limit pin is pull low"]
["Ⅲ- OCP Threshold-Floating (A) -- Min",null,"Current limit pin is floating"]
["Ⅲ- OCP Threshold-High (A) -- Min",null,"Current limit pin is pull high"]
["Ⅲ- OCP Threshold-Adjust by Resistor (A)",null,"請填寫OCP可調整範圍\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅲ- OCP Threshold-Other",null,"OCP type為Other 時，需填寫此欄位描述OCP架構"]
["Ⅲ- OCP Threshold-Other (A) -- Min",null,"OCP type為Other 時，需填寫此欄位"]
["Ⅲ- Itrip/Ics Source Current (uA)",null,"The current source for current limit\nRange的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["Ⅲ- Itrip/Ics Temperature Coefficient (ppm/℃)"]
["Ⅲ- Softstart Type",null,"▼下拉式選單"]
["Ⅲ- Softstart (mS)-Fixed -- Max",null,"From EN=High to Vout=95%"]
["Ⅲ- Softstart (mS)-Fixed -- Min",null,"From EN=High to Vout=95%"]
["Ⅲ- Softstart-Relative to VID/DAC(mS) -- Max",null,"1. If Softstart=\"Fixed value\" (mS) + VID slow rate, please fill in the fixed value.\n2. From EN=High to Vout=95%"]
["Ⅲ- Softstart-Relative to VID/DAC(mS) -- Min"]
["Ⅲ- Softstart-Other",null,"Softstart type為Other 時，需填寫此欄位描述Softstart架構"]
["Ⅲ- Softstart-Other (mS)",null,"Softstart type為Other 時，需填寫此欄位"]
["Ⅲ- Powergood Delay Time-Low to High (uS)",null,"如datasheet 僅標示power good deglitch time，請填寫power good deglitch time在此欄位。"]
["Ⅲ- Powergood Delay Time-High to Low (uS)",null,"如datasheet 僅標示power good deglitch time，請填寫power good deglitch time在此欄位。"]
["Which Rated Current of The Power Rail Is Over 10A That Needs to Testing UIS "]
["COMPAL CE Exempt from UIS",null,"▼下拉式選單"]
["High Side UIS Test for MOSFET (Production line) at Package Level",null,"▼下拉式選單"]
["Low Side UIS Test for MOSFET (Production line) at Package Level",null,"▼下拉式選單"]
["Recommended Operating Junction Temperature Range (℃)",null,"Range的部分請用波浪號「 ~ 」表示，並且~符號前後不要有空格"]
["*ESD (CDM)",null,"▼下拉式選單\ne.g. If CDM is passed 1000V, please select the C5"]
["*ESD (HBM)",null,"▼下拉式選單\ne.g. If HBM is passed 2000V, please select the 2"]
["*Lead Free",null,"▼下拉式選單"]
["*Ecology (MSD Declaration)",null,"▼下拉式選單\nSPEC當中需宣告"]
["*Tape Width (mm)",null,"請參考定義二"]
["*Tape Width Upper Tolerance (+)"]
["*Tape Width Lower Tolerance (-)"]
["*Component Pitch (mm)"]
["*Component Pitch Upper Tolerance (+)"]
["*Component Pitch Lower Tolerance (-)"]
["*Tape Depth (mm)"]
["*Tape Depth Upper Tolerance (+)"]
["*Tape Depth Lower Tolerance (-)"]
["*PIN1",null,"▼下拉式選單\n請參考定義(一)，Follow EIA 481象限定義填寫"]
["*Lead Pin Type",null,"▼下拉式選單\n請參考定義(十)"]
["*Lead Pin b Nominal (mm)",null,"請參考定義(五)\nNon-Standard footprint及 WLCSP、BGA…等 package type 不需填寫",null,null,null," "]
["*Lead Pin b Upper Tolerance (+)"]
["*Lead Pin b Lower Tolerance (-)"]
["*Lead Pin L Nominal (mm)"]
["*Lead Pin L Upper Tolerance (+)"]
["*Lead Pin L Lower Tolerance (-)"]
["*Multiple Thermal Pin",null,"▼下拉式選單"]
["*Packing: (T&R or Tray)",null,"▼下拉式選單"]
["*Packaging Material: (Paper or Embossed)",null,"▼下拉式選單\n此欄位為料帶材質，請參考定義(七)"]
["*Datasheet Version",null,"請依照版本填寫"]
["*Datasheet Version Release Date",null,"日期請依照 \"西元年/月/日\" 填寫，ex. 2018/10/10 \n若僅有年、月，請填寫當月份1日，ex. 2018/10/1"]

{"sheet":"定義","index":3,"n_rows":209,"n_cols":1,"rows_kept":209,"cut":false,"hidden":false,"merged":[]}
["定義(一) IC和MOS PIN1腳位象限(TAP孔朝上)-Follow EIA 定義"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["定義(二) "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["W=TAPE  WIDTH"]
["P=COMPONENT PITCH"]
["K0=TAPE DEPTH"]
[]
["定義(三) Package dimension for IC 圖示/定義"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["定義(四) Standard footprint 定義"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["定義(五) Lead pin Dimension for IC 圖示/定義"]
[]
[]
[]
[]
["定義(六) Converter Power rail 1/Power rail 2/Power rail 3定義"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["定義(七) Paper, Embossed 示意圖"]
["Paper"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Embossed"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["定義(八) Pin Count 圖示/定義"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["定義(九) Enable voltage and enable threshold 填寫定義"]
["Enable voltage: fill in the minimum for enable high/rising\n                            fill in the maximum for enable low/falling           "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Enable threshold : fill in the maximum for enable high/rising\n                                 fill in the minimum for enable low/falling           "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["定義(十) Lead pin type定義"]

{"sheet":"Part owner list","index":4,"n_rows":26,"n_cols":3,"rows_kept":26,"cut":false,"hidden":false,"merged":[[18,2,25,2],[19,0,20,0],[1,0,4,0],[1,2,10,2],[11,2,17,2]]}
["Cover Page","Category","Part Owner (Ext.)"]
["IC","Power PWM IC","Francis_Huang\n#17556"]
[null,"CPU/GPU/VPU Core IC"]
[null,"VR Driver"]
[null,"Others"]
["LED Driver IC","LED Driver IC"]
["PMIC","PMIC"]
["Logic Gate","Logic Gate"]
["OP","OP"]
["Charger IC","Charger IC"]
["Converter","Converter"]
["DR.MOS","DR.MOS","Lemon_Lee\n#17498"]
["Load Switch","Load Switch"]
["LDO","LDO"]
["MOSFET","MOSFET"]
["Transistor ","Transistor "]
["Diode","Diode"]
["Diode Zener","Diode Zener"]
["Choke","Choke","NickM_Chen\n#15110"]
["BulkCapacitor","Poly-Capacitor"]
[null,"E-Cap/OSCON"]
["Fuse","Fuse"]
["MLCC","MLCC"]
["Resistor","Resistor"]
["Thermistor","Thermistor"]
["Bead","Bead"]

{"sheet":"常見問題 Q&A","index":5,"n_rows":33,"n_cols":24,"rows_kept":33,"cut":false,"hidden":false,"merged":[[16,0,16,11],[17,0,31,11],[0,0,0,11],[1,0,15,11],[33,12,47,22],[33,23,47,33],[32,12,32,22],[32,23,32,33],[33,0,47,11],[32,0,32,11]]}
["Case1. 點擊“Print Cover Page to PDF”，無反應 ->需先啟用巨集"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Case2. 出現以下訊息，請確認Microsoft Office安裝的版本，若為32位元，請安裝64位元版本"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Case3. 若已經啟用巨集，點擊“Print Cover Page to PDF”，仍然無反應 -> 需解除檔案封鎖",null,null,null,null,null,null,null,null,null,null,null,"右鍵點擊檔案->內容",null,null,null,null,null,null,null,null,null,null,"一般->勾選解除封鎖->確定，再重新執行cover page檔案"]

{"sheet":"Member","index":6,"n_rows":400,"n_cols":1,"rows_kept":400,"cut":false,"hidden":true,"merged":[]}
["Pi. Uni (LKE)"]
[" Hsieh. Yosna (TPE)"]
[" Wang. Great (TPE)"]
[" Yu. Tina (PCP)"]
[" Lin. Yihsun (TPE)"]
[" Tsao. Denso (LKE)"]
[" Jeng. Jack (TPE)"]
[" Huang. Jack (TPE)"]
[" Hsu. Eric (TPE)"]
[" Wang. Jazz (TPE)"]
[" Juan. Kris (TPE)"]
[" Lee. Gavin (TPE)"]
[" Chai. Derek (TPE)"]
[" Wu. Jackson (TPE)"]
[" Zheng. Tony (TPE)"]
[" Lin. Ashley (TPE)"]
[" Yang. JohnBB (TPE)"]
[" Chang. PeterPC (TPE)"]
[" Wang. AndyF (TPE)"]
[" Wu. AlvinCJ (TPE)"]
[" Liu. Zeke (TPE)"]
[" Chang. Denny (TPE)"]
[" Tsai. Alvis (TPE)"]
[" Hsu. Jorden (TPE)"]
[" Peng. Jerry (TPE)"]
[" Wu. Vito (TPE)"]
[" Shih. Kane (TPE)"]
[" Chang. KevinYH (TPE)"]
[" Chang. DinoKT (TPE)"]
[" Chang. Iverson (TPE)"]
[" Huang. CharlieCC (TPE)"]
[" Chen. BenjaminC (TPE)"]
[" Tsai. Stanly (TPE)"]
[" Hsu. Kirk (TPE)"]
[" Chang. CharliePW (TPE)"]
[" Lin. TimWF (TPE)"]
[" Huang. Henry (TPE)"]
[" Chen. Charlene (TPE)"]
[" Chen. Roky (TPE)"]
[" Yang. Sammi (TPE)"]
[" Tung. Benson (TPE)"]
[" Shen. Gary (TPE)"]
[" Hsu. Steve (TPE)"]
[" Chuang. Chris (TPE)"]
[" Chu. Vincent (TPE)"]
[" Liao. Alicia (TPE)"]
[" Cheng. Marc (TPE)"]
[" Jiang. Ray (TPE)"]
[" Lin. Nielsen (TPE)"]
[" Li. Andrew (TPE)"]
[" Li. Edmond (TPE)"]
[" Lee. Scott (TPE)"]
[" Hsu. Garry (TPE)"]
[" Huang. River (TPE)"]
[" Chen. JohnSH (TPE)"]
[" Huang. Thomas (TPE)"]
[" Hu. Charlie (TPE)"]
[" Lin. JohnnyYC (TPE)"]
[" Chang. JohnJJ (TPE)"]
[" Tsai. JasonCC (TPE)"]
[" Hsu. Arthur (TPE)"]
[" Hsu. Steven (TPE)"]
[" Wu. Super (TPE)"]
[" Tang. Harry (TPE)"]
[" Chen. WayneWA (TPE)"]
[" Fang. Wes (TPE)"]
[" Wang. Steve (TPE)"]
[" Luo. Paul (TPE)"]
[" Huang. Xerxes (TPE)"]
[" Tsai. Bin (TPE)"]
[" Chang. Sosa (TPE)"]
[" Yuan. AndyAC (TPE)"]
[" Lin. CindyHC (TPE)"]
[" Chen. Jason (TPE)"]
[" Song. Ejko (TPE)"]
[" Huang. KevinHC (TPE)"]
[" Chiu. Willy (TPE)"]
[" Lin. LynnCY (PCP)"]
[" Hu. Andyw (PCP)"]
[" Jin. LeoJZ (TPE)"]
[" Chen. JohnsonYP (TPE)"]
[" Peng. Louis (PCP)"]
[" Chang. Melody (PCP)"]
[" Yeh. Benson (TPE)"]
[" Lee. DannyHT (TPE)"]
[" Lai. Mok (TPE)"]
[" Lin. Jonas (TPE)"]
[" Fu. Minus (TPE)"]
[" Huang. MarkHA (TPE)"]
[" Du. JerryJW (TPE)"]
[" Chen. Paul (TPE)"]
[" Yang. Allen (TPE)"]
[" Hung. Brandon (TPE)"]
[" Chang. JamesCY (TPE)"]
[" Wu. TomCF (TPE)"]
[" Lu. Stan (TPE)"]
[" Pan. Leo (PCP)"]
[" Tsai. EricYJ (PCP)"]
[" Cao. Jeremy (PCP)"]
[" Chien. Ryan (TPE)"]
[" Hsiang. Gary (PCP)"]
[" Lin. Crown (TPE)"]
[" Peng. Carter (PCP)"]
[" Cheng. Jacky (TPE)"]
[" Chung. MengYun (TPE)"]
[" Wang. KarenYQ (TPE)"]
[" Liu. Stanley (PCP)"]
[" Huang. Bill (PCP)"]
[" Chen. Eric (TPE)"]
[" Lin. Wendy (PCP)"]
[" Lee. Linda (TPE)"]
[" Lin. IvanC (PCP)"]
[" Ting. Terry (PCP)"]
[" Chiu. David (TPE)"]
[" Kang. Kang (TPE)"]
[" Chang. Jason (PCP)"]
[" Hsieh. Klins (TPE)"]
[" Tsai. PattyJJ (TPE)"]
[" Chen. AlexCL (TPE)"]
[" Chen. Layla (TPE)"]
[" Lin. StevenCH (PCP)"]
[" Wu. Boki (TPE)"]
[" Chen. JohnsonJJ (TPE)"]
[" Wu. Rod (PCP)"]
[" Ou. Darren (TPE)"]
[" Wang. KevinKW (PCP)"]
[" Wang. Benson (LKE)"]
[" Lee. Rainie (LKE)"]
[" Chang. Duncan (LKE)"]
[" Cheng. Alve (LKE)"]
[" Wu. Tom (LKE)"]
[" Lin. JerryJY (LKE)"]
[" Yen. PeterKJ (LKE)"]
[" Huang. ChrisJL (LKE)"]
[" Chen. JayYC (LKE)"]
[" Lin. Bonnie (LKE)"]
[" Kao. Ed (LKE)"]
[" Tsai. WillCH (LKE)"]
[" Chung. Vicky (LKE)"]
[" Hu. Johnny (LKE)"]
[" Chang. Joseph (LKE)"]
[" Hsieh. Ethan (LKE)"]
[" Lai. JasonYC (LKE)"]
[" Hsieh. Travis (LKE)"]
[" Huang. Jin (LKE)"]
[" Sun. Garbi (LKE)"]
[" Chen. DarrenCT (LKE)"]
[" Chang. AdamCW (TPE)"]
[" Ye. Sherry (LKE)"]
[" Chang. Alpha (LKE)"]
[" Liou. Jerry (LKE)"]
[" Chang. Lloyd (LKE)"]
[" Lee. Marcus (LKE)"]
[" Fan. Michael (LKE)"]
[" Liu. Kunter (LKE)"]
[" Feng. Tommy (LKE)"]
[" Wei. James (LKE)"]
[" Lin. Tommy (LKE)"]
[" Chiang. Benjamin (LKE)"]
[" Hsieh. JasonCH (LKE)"]
[" Chen. DorisYJ (LKE)"]
[" Chan. Riker (LKE)"]
[" Lin. Hubert (LKE)"]
[" Chou. Eric (LKE)"]
[" Li. PaulWX (LKE)"]
[" Hung. Chris (LKE)"]
[" Wu. Chen (LKE)"]
[" Hung. Kettie (LKE)"]
[" Yi. Steg (LKE)"]
[" Chao. Jay (LKE)"]
[" Chang. Jony (LKE)"]
[" Hung. Aaron (LKE)"]
[" Chen. FredHY (LKE)"]
[" Wang. Michael (TPE)"]
[" Hsu. Albert (TPE)"]
[" Chien. Vincent (TPE)"]
[" Lin. NeilWC (LKE)"]
[" Chen. ChrisCP (TPE)"]
[" Ke. Yang (TPE)"]
[" Huang. JeffC (TPE)"]
[" Huang. Jordan (TPE)"]
[" Wang. AaronWG (TPE)"]
[" Chang. KevinH (TPE)"]
[" Chen. AntonyWJ (TPE)"]
[" Kang. Vincent (TPE)"]
[" Liou. JackSJ (TPE)"]
[" Hsu. KaiL (TPE)"]
[" Xie. Bill (TPE)"]
[" Chen. Bryant (TPE)"]
[" Lu. Corn (TPE)"]
[" Lin. Jenny (TPE)"]
[" Xiao. Gary (TPE)"]
[" Hong. Anthony (TPE)"]
[" Chen. Yuren (TPE)"]
[" Hsieh. Allen (TPE)"]
[" Lee. LeoPT (KH)"]
[" Lee. AndyKC (TPE)"]
[" Chen. Ark (KH)"]
[" Lin. BobTY (KH)"]
[" Su. Hunter (TPE)"]
[" Lin. Toby (TPE)"]
[" Chen. JonathanJ (TPE)"]
[" Wu. MikeMY (TPE)"]
[" Wu. Morris (TPE)"]
[" Chen. KyleSK (TPE)"]
[" Hung. Joven (TPE)"]
[" Lee. JasonC (TPE)"]
[" Wen. AndyS (TPE)"]
[" Wu. Shane (TPE)"]
[" Chen. MichaelCC (TPE)"]
[" Li. VincentKL (LKE)"]
[" Huang. Kane (TPE)"]
[" Pan. JerryCY (LKE)"]
[" Shih. BenBJ (LKE)"]
[" Hsiao. Kevin (TPE)"]
[" Wu. MarsSS (LKE)"]
[" Huang. HarryYY (LKE)"]
[" Liao. Veronica (LKE)"]
[" Li. FrankH (TPE)"]
[" Tsai. SherrySH (LKE)"]
[" Fan. Hank (TPE)"]
[" Li. VicHY (LKE)"]
[" Pan. Sam (TPE)"]
[" Chang. TonyJ (TPE)"]
[" Wu. Hanter (LKE)"]
[" Wu. GeneJL (LKE)"]
[" Chang. EddyJY (TPE)"]
[" Huang. HankC (TPE)"]
[" Lee. LG (TPE)"]
[" Chiu. Leo (LKE)"]
[" Cheng. EricGT (TPE)"]
[" Wu. Kon (LKE)"]
[" Cheng. Gene (LKE)"]
[" Miu. ChiaHsiang (TPE)"]
[" Chung. Mike (TPE)"]
[" Lee. TedJM (TPE)"]
[" Liu. JuXi (LKE)"]
[" Tsai. Jeff (LKE)"]
[" You. Jerry (LKE)"]
[" He. Jeremy (LKE)"]
[" Chiu. Tom (TPE)"]
[" Lo. Bob (TPE)"]
[" Wang. Carlos (TPE)"]
[" Liu. Chain (TPE)"]
[" Wu. ChrisK (LKE)"]
[" Tsai. Eric (LKE)"]
[" Tsai. Lala (LKE)"]
[" Fang. Chad (LKE)"]
[" Wu. Judy (LKE)"]
[" Hsieh. Alex (TPE)"]
[" Cho. Vince (LKE)"]
[" Shih. Jim (LKE)"]
[" Chang. Yi (LKE)"]
[" Lai. Tom (TPE)"]
[" Lee. LeoY (TPE)"]
[" Huang. JaneHC (LKE)"]
[" Tseng. Grant (PCP)"]
[" Wang. DanielHW (LKE)"]
[" Kuo. KarenYH (LKE)"]
[" Tseng. TonyC (TPE)"]
[" Wang. JimmyCM (LKE)"]
[" Kuo. Yuanyu (TPE)"]
[" Le. VietQV (LKE)"]
[" Phan. Hasun (LKE)"]
[" Chien. Grace (TPE)"]
[" Li. Maddux (TPE)"]
[" Chen. Anson (TPE)"]
[" Guo. AndyBW (TPE)"]
[" Chen. ElsaYA (TPE)"]
[" Tseng. Tim (TPE)"]
[" Yu. TinaHT (LKE)"]
[" Chang. Kari (LKE)"]
[" Kao. Jessie (LKE)"]
[" Chen. Jocelyn (LKE)"]
[" Weng. Eric (TPE)"]
[" Chang. SamJY (TPE)"]
[" Cheng. LeoSL (TPE)"]
[" Wu. BensonYB (TPE)"]
[" Chen. MarkY (TPE)"]
[" Lin. TonyW (TPE)"]
[" Huang. TinaYu (TPE)"]
[" Tsao. Peterson (TPE)"]
[" Wu. KevinYC (TPE)"]
[" Zhuang. Kuonan (TPE)"]
[" Huang. Nic (TPE)"]
[" Chou. Elvis (TPE)"]
[" Tsai. Lawrance (TPE)"]
[" Lian. Alex (TPE)"]
[" Huang. Sheon (TPE)"]
[" Liao. Marcos (TPE)"]
[" Liao. LeoLW (TPE)"]
[" Liu. Ente (TPE)"]
[" Chang. JimmyC (TPE)"]
[" Hung. JohnS (TPE)"]
[" Ho. Vincent (TPE)"]
[" Wu. JackC (TPE)"]
[" Wang. Duncan (TPE)"]
[" Lin. JackyMK (TPE)"]
[" Chang. Dennis (TPE)"]
[" Lo. KevinHK (TPE)"]
[" Lai. Neil (TPE)"]
[" Wu. WilliamCH (TPE)"]
[" Chu. Miles (TPE)"]
[" Chen. Eddie (TPE)"]
[" Lin. Lanny (TPE)"]
[" Wang. Mason (TPE)"]
[" Lin. KevinHY (TPE)"]
[" Hou. Ansel (TPE)"]
[" Lin. BenYP (TPE)"]
[" Liu. Milly (TPE)"]
[" Chang. EasonWY (TPE)"]
[" Huang. Johnson (TPE)"]
[" Sun. Trista (TPE)"]
[" Lee. Mario (TPE)"]
[" Chang. Charlie (TPE)"]
[" Pan. Ken (TPE)"]
[" Wang. WendyJH (TPE)"]
[" Ku. Nick (TPE)"]
[" Liao. HankY (TPE)"]
[" Lin. JimW (TPE)"]
[" Wu. JasonM (TPE)"]
[" Chen. EasonY (TPE)"]
[" Ou. Bob (TPE)"]
[" Zeng. Sean (TPE)"]
[" Chang. Javen (TPE)"]
[" Ho. MenglinH (TPE)"]
[" Wu. VincentC (TPE)"]
[" Chen. Slean (TPE)"]
[" Wu. Jackie (TPE)"]
[" Lee. AllenST (TPE)"]
[" Lin. Funk (TPE)"]
[" Lin. Leif (TPE)"]
[" Liao. Rick (TPE)"]
[" Lo. Raymond (TPE)"]
[" Lo. Lucas (TPE)"]
[" Lee. DanielS (TPE)"]
[" Jiang. RyanS (TPE)"]
[" Su. Youcheng (TPE)"]
[" Hong. Andre (TPE)"]
[" Chen. JimW (TPE)"]
[" Wang. Yiwei (TPE)"]
[" Wu. Leon (TPE)"]
[" Huang. Eric (TPE)"]
[" Lin. Antony (CQ)"]
[" Chiang. Ray (TPE)"]
[" Chen. Francis (TPE)"]
[" Lin. William (TPE)"]
[" Yang. MarkL (TPE)"]
[" Chen. NeilWH (TPE)"]
[" Lin. Carol (TPE)"]
[" Lai. Ron (TPE)"]
[" Chen. GasolJ (TPE)"]
[" Yin. Jimmy (TPE)"]
[" Huang. Strike (TPE)"]
[" Shi. AllenH (TPE)"]
[" Chen. SeanY (TPE)"]
[" Yu. JayY (TPE)"]
[" Huang. JimJ (TPE)"]
[" Chang. AndyL (TPE)"]
[" Chen. JeffGH (TPE)"]
[" Chang. SimonS (TPE)"]
[" Wu. Zachary (TPE)"]
[" Lin. LeoH (TPE)"]
[" Cheng. KevinKL (TPE)"]
[" Lin. Creed (TPE)"]
[" Chen. JustinL (TPE)"]
[" Chen. Robert (TPE)"]
[" Wang. Liszt (TPE)"]
[" Chen. TimCT (TPE)"]
[" Chang. Eren (TPE)"]
[" Zhang. Atif (TPE)"]
[" Chen. LucasW (TPE)"]
[" Xie. JasonS (TPE)"]
[" Lin. JacksonCJ (TPE)"]
[" Huang. Kant (TPE)"]
[" Chen. AllenHC (TPE)"]
[" Chang. Junwei (TPE)"]
[" Chen. HawkHJ (TPE)"]
[" Shih. Willy (TPE)"]
[" Lin. Leoric (TPE)"]
[" Chen. Dick (TPE)"]
[" Kao. Jason (TPE)"]
[" Lee. Cloud (TPE)"]
[" Lee. Jeff (TPE)"]
[" Ueng. Josie (TPE)"]
[" Chuang. Neo (TPE)"]
[" Cheng. Clare (TPE)"]
[" Wu. Brian (TPE)"]
[" Liu. AaronKC (TPE)"]
[" Wu. PeterCC (TPE)"]
[" Huang. JesseKC (TPE)"]
[" Hung. Ryan (TPE)"]
[" Chien. Alex (TPE)"]
[" Ou. Ben (TPE)"]
[" Wu. Shi (TPE)"]
[" Liao. George (TPE)"]
[" Liao. Marks (TPE)"]
[" Huang. VincentY (TPE)"]
[" Chen. JasonJ (TPE)"]
[" Lai. Andy (TPE)"]