{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Alt A MDI","Alt A MDI-X","Alt B MDI","Alt B MDI-X","Note!","raw_data"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":10,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Alt A MDI","index":0,"n_rows":103,"n_cols":10,"rows_kept":103,"cut":false,"hidden":false,"merged":[[5,6,5,7],[8,0,8,1],[47,0,47,1],[93,0,93,3],[3,0,3,1],[34,0,34,1],[34,2,34,3],[57,0,57,1],[67,0,67,1],[8,2,8,3],[47,2,47,3],[57,2,57,3],[67,2,67,3],[5,3,5,4]]}
["PDA-600 AT TEST REPORT",null,null,"Coverage:","ALT A","MDI","Type-1","Software Version:","2.4.0.6"]
[null," 4/23/2025","17:31:21",null,"ALT B","MDI-X","Type-2 PHY","PDA Firmware:",2.08]
["Product Tested:",null,"Cycles:","Color Key:",null,null,"Type-2 LLDP","Report Ver:",{"$f":"ReportVersion","v":2.11}]
["EW7489ZI7_ES1",null,1,"PASS","FAIL","WARN","INFO","Serial Number","604A0196"]
[]
[]
[]
[]
["Detection & Classification",null,"PSE Emulation:",null,"Pairs:","A","Polarity:","MDI","Det_Cycles:",3]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"Rdet",25.33,"kohm",25.33,25.33,25.33,23.7,26.3,"P"]
[null,"Rdet_final",25.28,"kohm",25.28,25.28,25.28,23.7,26.3,"P"]
[null,"Rdet_unpwr",">99.00","kohm",99,99,99,"<12.00",">45.00","P"]
[null,"Rdet_at_Vmin",24.5,"kohm",24.5,24.5,24.5,23.7,26.3,"P"]
[null,"Rdet_at_Vmax",25.58,"kohm",25.58,25.58,25.58,23.7,26.3,"P"]
[null,"Rdet_Voffset",0.7,"VDC",0.7,0.7,0.7,0,1.9,"P"]
[null,"Cdet",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
[null,"Cdet_final",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
[null,"1 Event Classification"]
[null,"Iclass",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
[null,"ClassNum",4,null,4,4,"-",0,4,"P"]
[null,"Tclass",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
[null,"ClassStability",1,null,null,null,null,1,1,"P"]
[null,"Iclass_at_Vmin",39.6,"mA",39.6,39.6,39.6,36,44,"P"]
[null,"Iclass_at_Vmax",39.4,"mA",39.4,39.4,39.4,36,44,"P"]
[null,"2 Event Classification"]
[null,"Iclass_event1",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
[null,"Iclass_event2",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
[null,"MarkI",1.31,"mA",1.31,1.31,1.31,0.25,4,"P"]
[null,"ClassNum2",4,null,4,4,"-",0,4,"P"]
[null,"Tclass_event1",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
[null,"Tclass_event2",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
[null,"ClassStability_event1",1,null,null,null,null,1,1,"P"]
[null,"ClassStability_event2",1,null,null,null,null,1,1,"P"]
["Power-Up / Down"]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"InrushI_1",176.8,"mA",176.8,176.8,176.8,0,400,"P"]
[null,"InrushI_2",145,"mA",145,145,145,0,400,"P"]
[null,"IlimMinViolation",0,null,0,0,"-",0,0,"P"]
[null,"Pmax_Tdelay",0.6,"W",0.6,0.6,0.6,0,14.4,"P"]
[null,"Inrush_delayed",0,null,0,0,"-",0,0,"P"]
[null,"Von",37.799999999999997,"VDC",37.799999999999997,37.799999999999997,37.799999999999997,30,42,"P"]
[null,"Voff",35.6,"VDC",35.6,35.6,35.6,30,42,"P"]
[null,"Vhyst",2.2999999999999998,"VDC",2.2999999999999998,2.2999999999999998,2.2999999999999998,2.8,12,"WARN"]
[null,"BackfeedV",0,"VDC",0,0,0,0,2.8,"P"]
[null,"ClassRecover",0,null,0,0,"-",0,0,"P"]
[null,"SigRecoverTime",0,"sec",0,0,0,0,30,"P"]
["MDI Powered Type-1",null,"PSE Emulation:",null,"On Time:","10 sec","Off Time:","10 sec","Vport:",42]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"MinI_1",9.3000000000000007,"mA",9.3000000000000007,9.3000000000000007,9.3000000000000007,0,343.7,"P"]
[null,"MaxI_1",92.3,"mA",92.3,92.3,92.3,10,343.7,"P"]
[null,"Vport_1",42,"VDC",42,42,42,37,57,"INFO"]
[null,"Ppeak_1",3.87,"W",3.87,3.87,3.87,0,14.4,"P"]
[null,"Pavg_1",2.4700000000000002,"W",2.4700000000000002,2.4700000000000002,2.4700000000000002,0,13,"P"]
[null,"MPSViolation_1",0,null,0,0,"-",0,0,"P"]
[null,"TcutWindowViolation_1",0,null,0,0,"-",0,0,"P"]
[null,"DutyCycleViolation_1",0,null,0,0,"-",0,0,"P"]
["MDI Powered Type-2 PHY",null,"PSE Emulation:",null,"On Time:","10 sec","Off Time:","10 sec","Vport:",43.5]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"MinI_2",9.6,"mA",9.6,9.6,9.6,0,652.20000000000005,"P"]
[null,"MaxI_2",61.5,"mA",61.5,61.5,61.5,10,652.20000000000005,"P"]
[null,"Vport_2",43.4,"VDC",43.4,43.4,43.4,42.5,57,"INFO"]
[null,"Ppeak_2",2.67,"W",2.67,2.67,2.67,0,28.31,"P"]
[null,"Pavg_2",2.4900000000000002,"W",2.4900000000000002,2.4900000000000002,2.4900000000000002,0,25.5,"P"]
[null,"MPSViolation_2",0,null,0,0,"-",0,0,"P"]
[null,"TcutWindowViolation_2",0,null,0,0,"-",0,0,"P"]
[null,"DutyCycleViolation_2",0,null,0,0,"-",0,0,"P"]
["MDI Powered Type-2 LLDP",null,"PSE Emulation:",null,"On Time:","60 sec","Off Time:","10 sec","Vport:",43.5]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"MinI_PreAlloc",9.4,"mA",9.4,9.4,9.4,0,331.8,"P"]
[null,"MaxI_PreAlloc",89.9,"mA",89.9,89.9,89.9,10,331.8,"P"]
[null,"Vport_PreAlloc",43.5,"VDC",43.5,43.5,43.5,42.5,57,"INFO"]
[null,"Ppeak_PreAlloc",3.91,"W",3.91,3.91,3.91,0,14.4,"P"]
[null,"Pavg_PreAlloc",2.72,"W",2.72,2.72,2.72,0,13,"P"]
[null,"MPSViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
[null,"TcutWindowViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
[null,"DutyCycleViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
[null,"MinI_PostAlloc",-1,"mA",-1,-1,-1,0,0,"NA"]
[null,"MaxI_PostAlloc",-1,"mA",-1,-1,-1,10,0,"NA"]
[null,"Vport_PostAlloc",-1,"VDC",-1,-1,-1,0,57,"INFO"]
[null,"Ppeak_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"Pavg_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"MPSViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
[null,"TcutWindowViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
[null,"DutyCycleViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
[null,"MinI_AfterThrottle",-1,"mA",-1,-1,-1,0,0,"NA"]
[null,"MaxI_AfterThrottle",-1,"mA",-1,-1,-1,10,0,"NA"]
[null,"Vport_AfterThrottle",-1,"VDC",-1,-1,-1,0,57,"INFO"]
[null,"Ppeak_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"Pavg_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"MPSViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
[null,"TcutWindowViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
[null,"DutyCycleViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["PD LLDP Protocol Characteristics"]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"TimeToLink",-1,"sec",-1,-1,-1,null,null,"N/A"]
[null,"LinkSpeed",-1,"rate","-","-","-",null,null,"N/A"]
[null,"FirstReqTime",-1,"sec",-1,-1,-1,null,null,"N/A"]
[null,"PowerRequest",-1,"W",-1,-1,-1,0.1,25.5,"F"]
[null,"PDAckTime",-1,"sec",-1,-1,-1,0,10,"NA"]
[null,"AllocPowerEchoed",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"ThrottleAckTime",-1,"sec",-1,-1,-1,0,0,"F"]
[null,"ThrottlePowerReq",-1,"W",-1,-1,-1,0,0,"INFO"]

{"sheet":"Alt A MDI-X","index":1,"n_rows":103,"n_cols":10,"rows_kept":103,"cut":false,"hidden":false,"merged":[[93,0,93,3],[47,0,47,1],[47,2,47,3],[57,0,57,1],[57,2,57,3],[67,0,67,1],[67,2,67,3],[34,0,34,1],[34,2,34,3],[3,0,3,1],[5,3,5,4],[5,6,5,7],[8,0,8,1],[8,2,8,3]]}
["PDA-600 AT TEST REPORT",null,null,"Coverage:","ALT A","MDI","Type-1","Software Version:","2.4.0.6"]
[null," 4/23/2025","17:31:21",null,"ALT B","MDI-X","Type-2 PHY","PDA Firmware:",2.08]
["Product Tested:",null,"Cycles:","Color Key:",null,null,"Type-2 LLDP","Report Ver:",{"$f":"ReportVersion","v":2.11}]
["EW7489ZI7_ES1",null,1,"PASS","FAIL","WARN","INFO","Serial Number","604A0196"]
[]
[]
[]
[]
["Detection & Classification",null,"PSE Emulation:",null,"Pairs:","A","Polarity:","MDI-X","Det_Cycles:",3]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"Rdet",25.3,"kohm",25.3,25.3,25.3,23.7,26.3,"P"]
[null,"Rdet_final",25.33,"kohm",25.33,25.33,25.33,23.7,26.3,"P"]
[null,"Rdet_unpwr",">99.00","kohm",99,99,99,"<12.00",">45.00","P"]
[null,"Rdet_at_Vmin",24.74,"kohm",24.74,24.74,24.74,23.7,26.3,"P"]
[null,"Rdet_at_Vmax",25.66,"kohm",25.66,25.66,25.66,23.7,26.3,"P"]
[null,"Rdet_Voffset",0.7,"VDC",0.7,0.7,0.7,0,1.9,"P"]
[null,"Cdet",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
[null,"Cdet_final",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
[null,"1 Event Classification"]
[null,"Iclass",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
[null,"ClassNum",4,null,4,4,"-",0,4,"P"]
[null,"Tclass",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
[null,"ClassStability",1,null,null,null,null,1,1,"P"]
[null,"Iclass_at_Vmin",39.9,"mA",39.9,39.9,39.9,36,44,"P"]
[null,"Iclass_at_Vmax",39.5,"mA",39.5,39.5,39.5,36,44,"P"]
[null,"2 Event Classification"]
[null,"Iclass_event1",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
[null,"Iclass_event2",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
[null,"MarkI",1.31,"mA",1.31,1.31,1.31,0.25,4,"P"]
[null,"ClassNum2",4,null,4,4,"-",0,4,"P"]
[null,"Tclass_event1",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
[null,"Tclass_event2",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
[null,"ClassStability_event1",1,null,null,null,null,1,1,"P"]
[null,"ClassStability_event2",1,null,null,null,null,1,1,"P"]
["Power-Up / Down"]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"InrushI_1",144.6,"mA",144.6,144.6,144.6,0,400,"P"]
[null,"InrushI_2",147.19999999999999,"mA",147.19999999999999,147.19999999999999,147.19999999999999,0,400,"P"]
[null,"IlimMinViolation",0,null,0,0,"-",0,0,"P"]
[null,"Pmax_Tdelay",0.6,"W",0.6,0.6,0.6,0,14.4,"P"]
[null,"Inrush_delayed",0,null,0,0,"-",0,0,"P"]
[null,"Von",37.9,"VDC",37.9,37.9,37.9,30,42,"P"]
[null,"Voff",35.700000000000003,"VDC",35.700000000000003,35.700000000000003,35.700000000000003,30,42,"P"]
[null,"Vhyst",2.1,"VDC",2.1,2.1,2.1,2.8,12,"WARN"]
[null,"BackfeedV",0.1,"VDC",0.1,0.1,0.1,0,2.8,"P"]
[null,"ClassRecover",0,null,0,0,"-",0,0,"P"]
[null,"SigRecoverTime",0,"sec",0,0,0,0,30,"P"]
["MDI Powered Type-1",null,"PSE Emulation:",null,"On Time:","10 sec","Off Time:","10 sec","Vport:",42]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"MinI_1",9.6,"mA",9.6,9.6,9.6,0,341.9,"P"]
[null,"MaxI_1",90.7,"mA",90.7,90.7,90.7,10,341.9,"P"]
[null,"Vport_1",42.3,"VDC",42.3,42.3,42.3,37,57,"INFO"]
[null,"Ppeak_1",3.83,"W",3.83,3.83,3.83,0,14.4,"P"]
[null,"Pavg_1",2.5,"W",2.5,2.5,2.5,0,13,"P"]
[null,"MPSViolation_1",0,null,0,0,"-",0,0,"P"]
[null,"TcutWindowViolation_1",0,null,0,0,"-",0,0,"P"]
[null,"DutyCycleViolation_1",0,null,0,0,"-",0,0,"P"]
["MDI Powered Type-2 PHY",null,"PSE Emulation:",null,"On Time:","10 sec","Off Time:","10 sec","Vport:",43.5]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"MinI_2",9.6,"mA",9.6,9.6,9.6,0,649,"P"]
[null,"MaxI_2",61.4,"mA",61.4,61.4,61.4,10,649,"P"]
[null,"Vport_2",43.6,"VDC",43.6,43.6,43.6,42.5,57,"INFO"]
[null,"Ppeak_2",2.68,"W",2.68,2.68,2.68,0,28.31,"P"]
[null,"Pavg_2",2.5099999999999998,"W",2.5099999999999998,2.5099999999999998,2.5099999999999998,0,25.5,"P"]
[null,"MPSViolation_2",0,null,0,0,"-",0,0,"P"]
[null,"TcutWindowViolation_2",0,null,0,0,"-",0,0,"P"]
[null,"DutyCycleViolation_2",0,null,0,0,"-",0,0,"P"]
["MDI Powered Type-2 LLDP",null,"PSE Emulation:",null,"On Time:","60 sec","Off Time:","10 sec","Vport:",43.5]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"MinI_PreAlloc",9.5,"mA",9.5,9.5,9.5,0,330.2,"P"]
[null,"MaxI_PreAlloc",88.3,"mA",88.3,88.3,88.3,10,330.2,"P"]
[null,"Vport_PreAlloc",43.7,"VDC",43.7,43.7,43.7,42.5,57,"INFO"]
[null,"Ppeak_PreAlloc",3.86,"W",3.86,3.86,3.86,0,14.4,"P"]
[null,"Pavg_PreAlloc",2.74,"W",2.74,2.74,2.74,0,13,"P"]
[null,"MPSViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
[null,"TcutWindowViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
[null,"DutyCycleViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
[null,"MinI_PostAlloc",-1,"mA",-1,-1,-1,0,0,"NA"]
[null,"MaxI_PostAlloc",-1,"mA",-1,-1,-1,10,0,"NA"]
[null,"Vport_PostAlloc",-1,"VDC",-1,-1,-1,0,57,"INFO"]
[null,"Ppeak_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"Pavg_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"MPSViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
[null,"TcutWindowViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
[null,"DutyCycleViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
[null,"MinI_AfterThrottle",-1,"mA",-1,-1,-1,0,0,"NA"]
[null,"MaxI_AfterThrottle",-1,"mA",-1,-1,-1,10,0,"NA"]
[null,"Vport_AfterThrottle",-1,"VDC",-1,-1,-1,0,57,"INFO"]
[null,"Ppeak_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"Pavg_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"MPSViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
[null,"TcutWindowViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
[null,"DutyCycleViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["PD LLDP Protocol Characteristics"]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"TimeToLink",-1,"sec",-1,-1,-1,null,null,"N/A"]
[null,"LinkSpeed",-1,"rate","-","-","-",null,null,"N/A"]
[null,"FirstReqTime",-1,"sec",-1,-1,-1,null,null,"N/A"]
[null,"PowerRequest",-1,"W",-1,-1,-1,0.1,25.5,"F"]
[null,"PDAckTime",-1,"sec",-1,-1,-1,0,10,"NA"]
[null,"AllocPowerEchoed",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"ThrottleAckTime",-1,"sec",-1,-1,-1,0,0,"F"]
[null,"ThrottlePowerReq",-1,"W",-1,-1,-1,0,0,"INFO"]

{"sheet":"Alt B MDI","index":2,"n_rows":103,"n_cols":10,"rows_kept":103,"cut":false,"hidden":false,"merged":[[93,0,93,3],[47,0,47,1],[47,2,47,3],[57,0,57,1],[57,2,57,3],[67,0,67,1],[67,2,67,3],[34,0,34,1],[34,2,34,3],[3,0,3,1],[5,3,5,4],[5,6,5,7],[8,0,8,1],[8,2,8,3]]}
["PDA-600 AT TEST REPORT",null,null,"Coverage:","ALT A","MDI","Type-1","Software Version:","2.4.0.6"]
[null," 4/23/2025","17:31:21",null,"ALT B","MDI-X","Type-2 PHY","PDA Firmware:",2.08]
["Product Tested:",null,"Cycles:","Color Key:",null,null,"Type-2 LLDP","Report Ver:",{"$f":"ReportVersion","v":2.11}]
["EW7489ZI7_ES1",null,1,"PASS","FAIL","WARN","INFO","Serial Number","604A0196"]
[]
[]
[]
[]
["Detection & Classification",null,"PSE Emulation:",null,"Pairs:","B","Polarity:","MDI","Det_Cycles:",3]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"Rdet",25.28,"kohm",25.28,25.28,25.28,23.7,26.3,"P"]
[null,"Rdet_final",25.26,"kohm",25.26,25.26,25.26,23.7,26.3,"P"]
[null,"Rdet_unpwr",">99.00","kohm",99,99,99,"<12.00",">45.00","P"]
[null,"Rdet_at_Vmin",24.9,"kohm",24.9,24.9,24.9,23.7,26.3,"P"]
[null,"Rdet_at_Vmax",25.76,"kohm",25.76,25.76,25.76,23.7,26.3,"P"]
[null,"Rdet_Voffset",0.7,"VDC",0.7,0.7,0.7,0,1.9,"P"]
[null,"Cdet",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
[null,"Cdet_final",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
[null,"1 Event Classification"]
[null,"Iclass",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
[null,"ClassNum",4,null,4,4,"-",0,4,"P"]
[null,"Tclass",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
[null,"ClassStability",1,null,null,null,null,1,1,"P"]
[null,"Iclass_at_Vmin",39.4,"mA",39.4,39.4,39.4,36,44,"P"]
[null,"Iclass_at_Vmax",39.700000000000003,"mA",39.700000000000003,39.700000000000003,39.700000000000003,36,44,"P"]
[null,"2 Event Classification"]
[null,"Iclass_event1",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
[null,"Iclass_event2",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
[null,"MarkI",1.38,"mA",1.38,1.38,1.38,0.25,4,"P"]
[null,"ClassNum2",4,null,4,4,"-",0,4,"P"]
[null,"Tclass_event1",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
[null,"Tclass_event2",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
[null,"ClassStability_event1",1,null,null,null,null,1,1,"P"]
[null,"ClassStability_event2",1,null,null,null,null,1,1,"P"]
["Power-Up / Down"]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"InrushI_1",157.19999999999999,"mA",157.19999999999999,157.19999999999999,157.19999999999999,0,400,"P"]
[null,"InrushI_2",164.5,"mA",164.5,164.5,164.5,0,400,"P"]
[null,"IlimMinViolation",0,null,0,0,"-",0,0,"P"]
[null,"Pmax_Tdelay",0.6,"W",0.6,0.6,0.6,0,14.4,"P"]
[null,"Inrush_delayed",0,null,0,0,"-",0,0,"P"]
[null,"Von",37.799999999999997,"VDC",37.799999999999997,37.799999999999997,37.799999999999997,30,42,"P"]
[null,"Voff",35.5,"VDC",35.5,35.5,35.5,30,42,"P"]
[null,"Vhyst",2.2999999999999998,"VDC",2.2999999999999998,2.2999999999999998,2.2999999999999998,2.8,12,"WARN"]
[null,"BackfeedV",0,"VDC",0,0,0,0,2.8,"P"]
[null,"ClassRecover",0,null,0,0,"-",0,0,"P"]
[null,"SigRecoverTime",0,"sec",0,0,0,0,30,"P"]
["MDI Powered Type-1",null,"PSE Emulation:",null,"On Time:","10 sec","Off Time:","10 sec","Vport:",42]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"MinI_1",9,"mA",9,9,9,0,344.2,"P"]
[null,"MaxI_1",98.4,"mA",98.4,98.4,98.4,10,344.2,"P"]
[null,"Vport_1",42,"VDC",42,42,42,37,57,"INFO"]
[null,"Ppeak_1",4.13,"W",4.13,4.13,4.13,0,14.4,"P"]
[null,"Pavg_1",2.4700000000000002,"W",2.4700000000000002,2.4700000000000002,2.4700000000000002,0,13,"P"]
[null,"MPSViolation_1",0,null,0,0,"-",0,0,"P"]
[null,"TcutWindowViolation_1",0,null,0,0,"-",0,0,"P"]
[null,"DutyCycleViolation_1",0,null,0,0,"-",0,0,"P"]
["MDI Powered Type-2 PHY",null,"PSE Emulation:",null,"On Time:","10 sec","Off Time:","10 sec","Vport:",43.5]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"MinI_2",9.1,"mA",9.1,9.1,9.1,0,653.20000000000005,"P"]
[null,"MaxI_2",62.4,"mA",62.4,62.4,62.4,10,653.20000000000005,"P"]
[null,"Vport_2",43.3,"VDC",43.3,43.3,43.3,42.5,57,"INFO"]
[null,"Ppeak_2",2.7,"W",2.7,2.7,2.7,0,28.31,"P"]
[null,"Pavg_2",2.4900000000000002,"W",2.4900000000000002,2.4900000000000002,2.4900000000000002,0,25.5,"P"]
[null,"MPSViolation_2",0,null,0,0,"-",0,0,"P"]
[null,"TcutWindowViolation_2",0,null,0,0,"-",0,0,"P"]
[null,"DutyCycleViolation_2",0,null,0,0,"-",0,0,"P"]
["MDI Powered Type-2 LLDP",null,"PSE Emulation:",null,"On Time:","60 sec","Off Time:","10 sec","Vport:",43.5]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"MinI_PreAlloc",9.3000000000000007,"mA",9.3000000000000007,9.3000000000000007,9.3000000000000007,0,332.4,"P"]
[null,"MaxI_PreAlloc",115.6,"mA",115.6,115.6,115.6,10,332.4,"P"]
[null,"Vport_PreAlloc",43.5,"VDC",43.5,43.5,43.5,42.5,57,"INFO"]
[null,"Ppeak_PreAlloc",5.0199999999999996,"W",5.0199999999999996,5.0199999999999996,5.0199999999999996,0,14.4,"P"]
[null,"Pavg_PreAlloc",2.72,"W",2.72,2.72,2.72,0,13,"P"]
[null,"MPSViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
[null,"TcutWindowViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
[null,"DutyCycleViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
[null,"MinI_PostAlloc",-1,"mA",-1,-1,-1,0,0,"NA"]
[null,"MaxI_PostAlloc",-1,"mA",-1,-1,-1,10,0,"NA"]
[null,"Vport_PostAlloc",-1,"VDC",-1,-1,-1,0,57,"INFO"]
[null,"Ppeak_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"Pavg_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"MPSViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
[null,"TcutWindowViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
[null,"DutyCycleViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
[null,"MinI_AfterThrottle",-1,"mA",-1,-1,-1,0,0,"NA"]
[null,"MaxI_AfterThrottle",-1,"mA",-1,-1,-1,10,0,"NA"]
[null,"Vport_AfterThrottle",-1,"VDC",-1,-1,-1,0,57,"INFO"]
[null,"Ppeak_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"Pavg_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"MPSViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
[null,"TcutWindowViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
[null,"DutyCycleViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["PD LLDP Protocol Characteristics"]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"TimeToLink",-1,"sec",-1,-1,-1,null,null,"N/A"]
[null,"LinkSpeed",-1,"rate","-","-","-",null,null,"N/A"]
[null,"FirstReqTime",-1,"sec",-1,-1,-1,null,null,"N/A"]
[null,"PowerRequest",-1,"W",-1,-1,-1,0.1,25.5,"F"]
[null,"PDAckTime",-1,"sec",-1,-1,-1,0,10,"NA"]
[null,"AllocPowerEchoed",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"ThrottleAckTime",-1,"sec",-1,-1,-1,0,0,"F"]
[null,"ThrottlePowerReq",-1,"W",-1,-1,-1,0,0,"INFO"]

{"sheet":"Alt B MDI-X","index":3,"n_rows":103,"n_cols":10,"rows_kept":103,"cut":false,"hidden":false,"merged":[[93,0,93,3],[47,0,47,1],[47,2,47,3],[57,0,57,1],[57,2,57,3],[67,0,67,1],[67,2,67,3],[34,0,34,1],[34,2,34,3],[3,0,3,1],[5,3,5,4],[5,6,5,7],[8,0,8,1],[8,2,8,3]]}
["PDA-600 AT TEST REPORT",null,null,"Coverage:","ALT A","MDI","Type-1","Software Version:","2.4.0.6"]
[null," 4/23/2025","17:31:21",null,"ALT B","MDI-X","Type-2 PHY","PDA Firmware:",2.08]
["Product Tested:",null,"Cycles:","Color Key:",null,null,"Type-2 LLDP","Report Ver:",{"$f":"ReportVersion","v":2.11}]
["EW7489ZI7_ES1",null,1,"PASS","FAIL","WARN","INFO","Serial Number","604A0196"]
[]
[]
[]
[]
["Detection & Classification",null,"PSE Emulation:",null,"Pairs:","B","Polarity:","MDI-X","Det_Cycles:",3]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"Rdet",25.36,"kohm",25.36,25.36,25.36,23.7,26.3,"P"]
[null,"Rdet_final",25.28,"kohm",25.28,25.28,25.28,23.7,26.3,"P"]
[null,"Rdet_unpwr",">99.00","kohm",99,99,99,"<12.00",">45.00","P"]
[null,"Rdet_at_Vmin",24.9,"kohm",24.9,24.9,24.9,23.7,26.3,"P"]
[null,"Rdet_at_Vmax",25.7,"kohm",25.7,25.7,25.7,23.7,26.3,"P"]
[null,"Rdet_Voffset",0.7,"VDC",0.7,0.7,0.7,0,1.9,"P"]
[null,"Cdet",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
[null,"Cdet_final",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
[null,"1 Event Classification"]
[null,"Iclass",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
[null,"ClassNum",4,null,4,4,"-",0,4,"P"]
[null,"Tclass",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
[null,"ClassStability",1,null,null,null,null,1,1,"P"]
[null,"Iclass_at_Vmin",40.1,"mA",40.1,40.1,40.1,36,44,"P"]
[null,"Iclass_at_Vmax",39.6,"mA",39.6,39.6,39.6,36,44,"P"]
[null,"2 Event Classification"]
[null,"Iclass_event1",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
[null,"Iclass_event2",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
[null,"MarkI",1.38,"mA",1.38,1.38,1.38,0.25,4,"P"]
[null,"ClassNum2",4,null,4,4,"-",0,4,"P"]
[null,"Tclass_event1",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
[null,"Tclass_event2",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
[null,"ClassStability_event1",1,null,null,null,null,1,1,"P"]
[null,"ClassStability_event2",1,null,null,null,null,1,1,"P"]
["Power-Up / Down"]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"InrushI_1",158.5,"mA",158.5,158.5,158.5,0,400,"P"]
[null,"InrushI_2",159.69999999999999,"mA",159.69999999999999,159.69999999999999,159.69999999999999,0,400,"P"]
[null,"IlimMinViolation",0,null,0,0,"-",0,0,"P"]
[null,"Pmax_Tdelay",0.6,"W",0.6,0.6,0.6,0,14.4,"P"]
[null,"Inrush_delayed",0,null,0,0,"-",0,0,"P"]
[null,"Von",38,"VDC",38,38,38,30,42,"P"]
[null,"Voff",35.799999999999997,"VDC",35.799999999999997,35.799999999999997,35.799999999999997,30,42,"P"]
[null,"Vhyst",2.2999999999999998,"VDC",2.2999999999999998,2.2999999999999998,2.2999999999999998,2.8,12,"WARN"]
[null,"BackfeedV",0,"VDC",0,0,0,0,2.8,"P"]
[null,"ClassRecover",0,null,0,0,"-",0,0,"P"]
[null,"SigRecoverTime",0,"sec",0,0,0,0,30,"P"]
["MDI Powered Type-1",null,"PSE Emulation:",null,"On Time:","10 sec","Off Time:","10 sec","Vport:",42]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"MinI_1",9.1,"mA",9.1,9.1,9.1,0,342,"P"]
[null,"MaxI_1",99.2,"mA",99.2,99.2,99.2,10,342,"P"]
[null,"Vport_1",42.2,"VDC",42.2,42.2,42.2,37,57,"INFO"]
[null,"Ppeak_1",4.1900000000000004,"W",4.1900000000000004,4.1900000000000004,4.1900000000000004,0,14.4,"P"]
[null,"Pavg_1",2.4900000000000002,"W",2.4900000000000002,2.4900000000000002,2.4900000000000002,0,13,"P"]
[null,"MPSViolation_1",0,null,0,0,"-",0,0,"P"]
[null,"TcutWindowViolation_1",0,null,0,0,"-",0,0,"P"]
[null,"DutyCycleViolation_1",0,null,0,0,"-",0,0,"P"]
["MDI Powered Type-2 PHY",null,"PSE Emulation:",null,"On Time:","10 sec","Off Time:","10 sec","Vport:",43.5]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"MinI_2",9.1,"mA",9.1,9.1,9.1,0,649.29999999999995,"P"]
[null,"MaxI_2",62.1,"mA",62.1,62.1,62.1,10,649.29999999999995,"P"]
[null,"Vport_2",43.6,"VDC",43.6,43.6,43.6,42.5,57,"INFO"]
[null,"Ppeak_2",2.7,"W",2.7,2.7,2.7,0,28.31,"P"]
[null,"Pavg_2",2.5,"W",2.5,2.5,2.5,0,25.5,"P"]
[null,"MPSViolation_2",0,null,0,0,"-",0,0,"P"]
[null,"TcutWindowViolation_2",0,null,0,0,"-",0,0,"P"]
[null,"DutyCycleViolation_2",0,null,0,0,"-",0,0,"P"]
["MDI Powered Type-2 LLDP",null,"PSE Emulation:",null,"On Time:","60 sec","Off Time:","10 sec","Vport:",43.5]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"MinI_PreAlloc",9.1,"mA",9.1,9.1,9.1,0,330.4,"P"]
[null,"MaxI_PreAlloc",114.8,"mA",114.8,114.8,114.8,10,330.4,"P"]
[null,"Vport_PreAlloc",43.7,"VDC",43.7,43.7,43.7,42.5,57,"INFO"]
[null,"Ppeak_PreAlloc",5.0199999999999996,"W",5.0199999999999996,5.0199999999999996,5.0199999999999996,0,14.4,"P"]
[null,"Pavg_PreAlloc",2.74,"W",2.74,2.74,2.74,0,13,"P"]
[null,"MPSViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
[null,"TcutWindowViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
[null,"DutyCycleViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
[null,"MinI_PostAlloc",-1,"mA",-1,-1,-1,0,0,"NA"]
[null,"MaxI_PostAlloc",-1,"mA",-1,-1,-1,10,0,"NA"]
[null,"Vport_PostAlloc",-1,"VDC",-1,-1,-1,0,57,"INFO"]
[null,"Ppeak_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"Pavg_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"MPSViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
[null,"TcutWindowViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
[null,"DutyCycleViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
[null,"MinI_AfterThrottle",-1,"mA",-1,-1,-1,0,0,"NA"]
[null,"MaxI_AfterThrottle",-1,"mA",-1,-1,-1,10,0,"NA"]
[null,"Vport_AfterThrottle",-1,"VDC",-1,-1,-1,0,57,"INFO"]
[null,"Ppeak_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"Pavg_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"MPSViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
[null,"TcutWindowViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
[null,"DutyCycleViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["PD LLDP Protocol Characteristics"]
[null,"Parameter                   Cycle:",1,"Units","Min.","Max.","Average","Low Lim.","High Lim.","P/F"]
[null,"TimeToLink",-1,"sec",-1,-1,-1,null,null,"N/A"]
[null,"LinkSpeed",-1,"rate","-","-","-",null,null,"N/A"]
[null,"FirstReqTime",-1,"sec",-1,-1,-1,null,null,"N/A"]
[null,"PowerRequest",-1,"W",-1,-1,-1,0.1,25.5,"F"]
[null,"PDAckTime",-1,"sec",-1,-1,-1,0,10,"NA"]
[null,"AllocPowerEchoed",-1,"W",-1,-1,-1,0,0,"NA"]
[null,"ThrottleAckTime",-1,"sec",-1,-1,-1,0,0,"F"]
[null,"ThrottlePowerReq",-1,"W",-1,-1,-1,0,0,"INFO"]

{"sheet":"Note!","index":4,"n_rows":92,"n_cols":6,"rows_kept":92,"cut":false,"hidden":false,"merged":[[27,4,28,4],[1,1,1,4],[5,4,6,4],[5,3,6,3],[10,4,11,4],[10,3,11,3],[12,4,13,4],[18,4,19,4],[22,4,23,4],[24,4,25,4],[14,2,15,2],[14,3,15,3],[14,4,15,4],[5,5,6,5],[10,5,11,5],[7,2,8,2],[7,3,8,3],[7,4,8,4],[7,5,8,5],[57,5,72,5],[85,5,88,5],[12,5,25,5],[32,5,34,5],[27,5,30,5],[39,5,46,5],[48,5,55,5]]}
[]
[null,"PD Conformance Test Suite Parameters"]
[]
[null,"Parameter","Description","Units","Acceptance Criteria (802.3at references)","PICS"]
[null,"Detection & Classification"]
[null,"Rdet","Detection resistance (2.7 to 10.1 V band) from a single probe.","KW","23.7 to 26.3\n802.3at Table 33-14  ","PD7              PD8             PD11"]
[null,"Rdet_final","Detection resistance after multiple detection and classification probing sequences.  Evaluate response to PSE's that probe repeatedly prior to power-up."]
[null,"Rdet_at_Vmin","Detection resistance at different chords in the 2.7 to 10.1 V band. (not supported by PDA-602A)","KW","\n802.3at Table 33-14  ","PD10 (partial)"]
[null,"Rdet_at_Vmax"]
[null,"Rdet_unpwr","Non-valid detection resistance presented by the unpowered pairset.","KW","< 12 or > 45 \n802.3at para. 33.3.4, Table 33-15\n","PD9"]
[null,"Cdet","Detection capacitance (2.7 to 10.1 V band)","mF","0.05 to 0.12 \n802.3at Table 33-14\n","PD8          PD11"]
[null,"Cdet_final","Detection capacitance after multiple detection and classification probing sequences.  Evaluate response to PSE's that probe repeatedly prior to power-up."]
[null,"Iclass","Classification current signature, 1 event classification.","mA","0-4, 9-12, 17-20, 26-30, or 36-44\n0, 1, 2, 3, or 4  (respectively)\n","PD12      PD13      PD14 (partial)      PD15      PD16      PD17      PD18      PD19 (partial)      PD20      PD21      PD22      PD23      PD42"]
[null,"ClassNum","PD Class determined from Iclass","PD Class"]
[null,"Iclass_at_Vmin","Classification current signature at low and high edge of 14.5 - 20.5 V band. (not supported by PDA-602A)","mA","0-4, 9-12, 17-20, 26-30, or 36-44                                          802.3at Tables 33-16, 33-17"]
[null,"Iclass_at_Vmax"]
[null,"Tclass","Time from when Vport = 15.5VDC until class current reaches valid level","seconds","< 0.005\n802.3at 33.3.7.8 & Table 33-18\n"]
[null,"ClassStability","Class current remains in valid range during classification period that ranges from 6-75 msec","flag (1 or 0)","All class samples = Iclass\n802.3at para. 33.3.7.8 \n"]
[null,"Iclass_event1","Classification current signature during 1st Classification pulse, 2-Event classification.","mA","0-4, 9-12, 17-20, 26-30, or 36-44\n802.3at Table 33-16 \n"]
[null,"Iclass_event2","Classification current signature during 2nd Classification pulse, 2-Event classification.","mA"]
[null,"MarkI","Current drawn during mark region of 2-Event classification.","mA","0.25 to 4\n802.3at  Table 33-17\n"]
[null,"ClassNum2","PD Class determined from Iclass during 2-Event classification.","PD_Class","0, 1, 2, 3, or 4"]
[null,"Tclass_event1","Time from when Vport = 15.5VDC until class current reaches valid level, during 1st Classification pulse, 2-Event classification","seconds","< 0.005\n802.3at 33.3.7.8 & Table 33-18"]
[null,"Tclass_event2","Time from when Vport = 15.5VDC until class current reaches valid level, during 2nd Classification pulse, 2-Event classification","seconds"]
[null,"ClassStability_event1","Class current remains in valid range during classification period, 1st class pulse.  ","flag (1 or 0)","All class samples = Iclass\n802.3at para. 33.3.7.8"]
[null,"ClassStability_event2","Class current remains in valid range during classification period, 2nd class pulse.  ","flag (1 or 0)"]
[null,"Power-Up / Down"]
[null,"InrushI_1","Highest current drawn during the first 50 msec after power on. Power on is preceeded by a 1 event classification.","mA","< 400mA\nA PD may draw more than 400mA if it presents capacitive load, Cport < 180uF.  Because Cport cannot be measured, out-of-limit performance is flagged with WARN, not FAIL.\n802.3at Table 33-18 & para. 33.3.7.3.","PD30       PD31"]
[null,"InrushI_2\n(Type-2 testing)","Highest current drawn during the first 50 msec after power on. Power on is preceeded by a 2 event classification.","mA"]
[null,"Pmax_Tdelay\n(Type-2 testing)","Highest power consumed during the period from 50 msec to 80 msec after power-up that is preceded by 2-Event classification.","watts","< 14.4\nA Type-2 PD must not draw a peak power exceeding Type-1 PD maximum peak power of 14.4W during 30msec between end of inrush and Tdelay.\n802.3at para. 33.3.7.3.\n"]
[null,"Inrush_delayed","Flags a PD behavior where the start of inrush is delayed by more than 1ms after power-up and where inrush level (>400mA) may require current limiting by a PSE.  PD’s that delay inrush and exceed 400mA may not experience 450mA current limiting by a PSE that applies the “legacy_powerup” exception.  See 802.3at, para. 3.2.4.4.","flag (1 or 0)","flag= 0 if;\nInrush Current < 400 mA  \nor \nInrush Current (@ > 1 msec)  < Current (@ < 1 msec)"]
[null,"IlimMinViolation","Flags a PD behavior where the DUT draws >400mA after TInrush has completed, when the PD is powered following 1 event classification. This may cause current limiting by a PSE, and the resulting reduction in voltage could cause the PD to not successfully power on. (this check was added based on an interop problem case)","flag (1 or 0)","flag= 0 if Current > 400 mA during the 1.5 second interval starting at the completion of TInrush.\n","PD33"]
[null,"Von","Voltage at which PD starts to draw load current","VDC","30 to 42,  802.3at Table 33-18","PD25       PD27      PD28"]
[null,"Voff","Voltage at which PD stops drawing load current","VDC","> 30,   802.3at Table 33-18. WARN if > 37VDC, based on the lowest voltage that a Type 1 PSE could provide."]
[null,"Vhyst","Hysteresis band between Von and Voff.","VDC","Provided for information purposes. There is no explicit value for hysteresis specified in Table 33-18, but the need for hysteresis is implied by 802.3at para. 33.3.7.1 (startup oscillation)."]
[null,"BackfeedV","Voltage present on the unpowered pair with Vport_PD max applied. Unpowered pair is terminated with 100kΩ.","VDC","0 to 2.8\n802.3at Table 33-18, para. 33.3.7.9","PD43"]
[null,"ClassRecover","Flag indicating that PD classification signature following power removal and PD restoration of a potentially acceptable detection signature (i.e. between 15KW and 33KW) does not match expected PD classification signature.","flag (1 or 0)","A value of \"1\" will be reported with a WARN status because PSE's will possibly mis-classify this PD following power-removal events."]
[null,"SigRecoverTime","Time to restore expected PD classification signature if ClassRecover is reported as \"1\".   Otherwise, vaue reported is \"0 sec\".  Measured from PD shutdown.","seconds","A PD need not present a valid classification signature until that PD first presents a valid detection signature, so there is no clear specification time limit."]
[null,"MDI Powered Type-1","PD-under-test powered to Type-1 Vport with 1-Event Classification"]
[null,"MinI_1","Minimum current drawn by the PD while powered on at Type-1 VPort_PD","mA","0 to (Pclass_PD / VPort_PD)\n802.3at para. 33.3.7.4, Table 33-18","PD24  (partial)  PD26       PD29       PD32       PD33       PD34 (partial)       PD35       PD37       **only if MPS low pwr    PD44       PD45"]
[null,"MaxI_1","Maximum current drawn by the PD while powered on at Type-1 Vport_PD.  The maximum current must exceed Iport_mps.","mA","10 to (Pclass_PD / VPort_PD)\n802.3at para. 33.3.7.4, Table 33-18\nIport_mps > 10, 802.3at para. 33.3.8"]
[null,"Vport_1","Vport level at the point where the MaxI_1 occurs.","V","VPort_PD should conform to ranges in\n802.3at Table 33-18"]
[null,"Ppeak_1","Maximum instantaneous power consumed by the PD while powered on at Type-1 Vport_PD","watts","< PPeak_PD (for PD Classification)\n802.3at Table 33-18, para. 33.3.7.4"]
[null,"Pavg_1","Average power (1 second moving window) consumed by the PD while powered on a Type-1 Vport_PD","watts","< Pclass_PD (for PD Classification)\n802.3at Table 33-18, para. 33.3.7.2"]
[null,"MPSViolation_1","Flag indicating PD did not satisfy DC Maintain Power Signature (MPS) and will be potentially subject to shutdown by a PSE using DC MPS method.","flag (1 or 0)","In order to stay powered, the PD must draw > 10mA for a time period > 75 msec out of every 325 msec time interval.  802.3at para. 33.3.8"]
[null,"TcutWindowViolation_1","Flag indicating that PD power draw exceeded Pclass_PD for longer than Tcut_min (50 msec).  PD is at risk of overload shutdown by PSE.","flag (1 or 0)","In order to stay powered, transient loads may not exceed Pclass_PD for time duration > Tcut_min, or 50 msec.  802.3at para. 33.3.7.4."]
[null,"DutyCycleViolation_1","Flag indicating that PD power draw is exceeding Pclass_PD for greater than 5% of the time.   PD is at risk of overload shutdown by PSE.","flag (1 or 0)","In order to stay powered, transient loads may not exceed Pclass_PD for > 5% duty cycle. 802.3at para. 33.3.7.4."]
[null,"MDI Powered Type-2","PD-under-test powered to Type-2 Vport with 2-Event Classification"]
[null,"MinI_2","Minimum current drawn by the PD while powered on at Type-2 Vport_PD prior to LLDP power allocation.","mA","0 to (25.5W / VPort_PD)\n802.3at para. 33.3.7.4, Table 33-18","PD24  (partial)  PD26       PD29       PD32       PD33       PD34 (partial)       PD35       PD37       **only if MPS low pwr    PD44       PD45"]
[null,"MaxI_2","Maximum current drawn by the PD while powered  on at Type-2 Vport_PD prior to LLDP power allocation.  The maximum current must exceed Iport_mps.","mA","10 to (25.5W / VPort_PD)\n802.3at para. 33.3.7.4, Table 33-18\nIport_mps > 10, 802.3at para. 33.3.8"]
[null,"Vport_2","Vport level at the point where the MaxI_2 occurs.","V","VPort_PD should conform to ranges in\n802.3at Table 33-18"]
[null,"Ppeak_2","Maximum instantaneous power consumed by the PD while powered on at Type-2 VPort_PD","watts","< 28.3 \n802.3at Table 33-18, para. 33.3.7.4"]
[null,"Pavg_2","Average power (1 second moving window) consumed by the PD while powered on a Type-2 VPort_PD","watts","< 25.5\n802.3at Table 33-18, para. 33.3.7.2"]
[null,"MPSViolation_2","Flag indicating PD did not satisfy DC Maintain Power Signature (MPS) and will be potentially subject to shutdown by a PSE using DC MPS method.","flag (1 or 0)","In order to stay powered, the PD must draw > 10mA for a time period > 75 msec out of every 325 msec time interval.  802.3at para. 33.3.8."]
[null,"TcutWindowViolation_2","Flag indicating that PD power draw exceeded 25.5W for longer than Tcut_min (50 msec).  PD is at risk of overload shutdown by PSE.","flag (1 or 0)","In order to stay powered, transient loads may not exceed 25.5W for time duration > Tcut_min, or 50 msec.  802.3at para. 33.3.7.4."]
[null,"DutyCycleViolation_2","Flag indicating that PD power draw is exceeding 25.5W for greater than 5% of the time.   PD is at risk of overload shutdown by PSE.","flag (1 or 0)","In order to stay powered, transient loads may not exceed 25.5W for > 5% duty cycle. 802.3at para. 33.3.7.4."]
[null,"MDI Powered Type-2 LLDP","PD-under-test powered to Type-2 Vport with 1-Event Classification and subsequent LLDP Negotiation"]
[null,"MinI_PreAlloc","Minimum current drawn by the PD while powered on at Type-2 Vport_PD prior to LLDP power allocation.","mA","0 to (13W / VPort_PD)\n802.3at para. 33.3.3.5, Table 33-18","PD24  (partial)  PD26       PD29       PD32       PD33       PD34 (partial)       PD35       PD37       PD44       PD45       DLL4       DLL7       DLL9       DLL11"]
[null,"MaxI_PreAlloc","Maximum current drawn by the PD while powered  on at Type-2 Vport_PD prior to LLDP power allocation.  The maximum current must exceed Iport_mps.","mA","10 to (13W / VPort_PD)\n802.3at para. 33.3.3.5, Table 33-18\nIport_mps > 10, 802.3at para. 33.3.8"]
[null,"Vport_PreAlloc","Vport level at the point where the MaxI_PreAlloc occurs.","V","VPort_PD should conform to ranges in\n802.3at Table 33-18"]
[null,"Ppeak_PreAlloc","Maximum power consumed by the PD while powered on at Type-2 Vport prior to LLDP power allocation.","watts","< 14.4 \n802.3at Table 33-18, para. 33.3.3.5"]
[null,"Pavg_PreAlloc","Average power (1 second moving window) consumed by the PD while powered on at Type-2 Vport prior to LLDP power allocation.","watts","< 25.5\n802.3at Table 33-18, para. 33.3.3.5"]
[null,"MPSViolation_PreAlloc","Flag indicating PD did not satisfy DC Maintain Power Signature (MPS) and will be potentially subject to shutdown by a PSE using DC MPS method.  Measured before LLDP power allocation.","flag (1 or 0)","In order to stay powered, the PD must draw > 10mA for a time period > 75 msec out of every 325 msec time interval.  802.3at para. 33.3.8."]
[null,"TcutWindowViolation_PreAlloc","Flag indicating that PD power draw exceeded 13W for longer than Tcut_min (50 msec).  PD is at risk of overload shutdown by PSE.  Measured before LLDP power allocation.","flag (1 or 0)","In order to stay powered, transient loads may not exceed 13W for time duration > Tcut_min, or 50 msec.  802.3at para. 33.3.7.4."]
[null,"DutyCycleViolation_PreAlloc","Flag indicating that PD power draw is exceeding 13W for greater than 5% of the time.   PD is at risk of overload shutdown by PSE.  Measured before LLDP power allocation.","flag (1 or 0)","In order to stay powered, transient loads may not exceed 13W for > 5% duty cycle. 802.3at para. 33.3.7.4."]
[null,"MinI_PostAlloc","Minimum current drawn by the PD while powered on at Type-2 Vport_PD following LLDP power allocation.","mA","0 to (Pclass_PD / VPort_PD)\n802.3at para. 33.3.7.4, Table 33-18"]
[null,"MaxI_PostAlloc","Maximum current drawn by the PD while powered  on at Type-2 Vport_PD following LLDP power allocation.","mA","10 to (Pclass_PD / VPort_PD)\n802.3at para. 33.3.7.4, Table 33-18\nIport_mps > 10, 802.3at para. 33.3.8"]
[null,"Vport_PostAlloc","Vport level at the point where the MaxI_PostAlloc occurs.","V","VPort_PD should conform to ranges in\n802.3at Table 33-18"]
[null,"Ppeak_PostAlloc","Maximum power consumed by the PD while powered on at Type-2 Vport_PD following LLDP power allocation.","watts","< Ppeak_PD \n802.3at Table 33-18, para. 33.3.3.5"]
[null,"Pavg_PostAlloc","Average power (1 second moving window) consumed by the PD while powered on at Type-2 Vport_PD following LLDP power allocation.","watts","< Pclass_PD\n802.3at Table 33-18, para. 33.3.3.5"]
[null,"MPSViolation_PostAlloc","Flag indicating PD did not satisfy DC Maintain Power Signature (MPS) and will be potentially subject to shutdown by a PSE using DC MPS method.  Measured after LLDP power allocation.","flag (1 or 0)","In order to stay powered, the PD must draw > 10mA for a time period > 75 msec out of every 325 msec time interval.  802.3at para. 33.3.8."]
[null,"WindowViolation_PostAlloc","Flag indicating that PD power draw exceeded Pclass_PD for longer than Tcut_min (50 msec).  PD is at risk of overload shutdown by PSE.  Measured after LLDP power allocation.","flag (1 or 0)","In order to stay powered, transient loads may not exceed Pclass_PD for time duration > Tcut_min, or 50 msec.  802.3at para. 33.3.7.4."]
[null,"DutyCycleViolation_PostAlloc","Flag indicating that PD power draw is exceeding Pclass_PD for greater than 5% of the time.   PD is at risk of overload shutdown by PSE.  Measured after LLDP power allocation.","flag (1 or 0)","In order to stay powered, transient loads may not exceed 13W for > 5% duty cycle. 802.3at para. 33.3.7.4.\n"]
[null,"MinI_AfterThrottle","Minimum current drawn by the PD while powered on at Type-2 Vport_PD and following allocation reduction (or power demotion) by PSE.","mA","0 to (13W / VPort_PD)  \nINFO limit - not a required behavior - 802.3at para. 33.6.3.5"]
[null,"MaxI_AfterThrottle","Maximum current drawn by the PD while powered on at Type-2 Vport_PD and following allocation reduction (or power demotion) by PSE.","mA","10 to (13W / VPort_PD)\nINFO limit - not a required behavior - 802.3at para. 33.6.3.5\nIport_mps > 10, 802.3at para. 33.3.8"]
[null,"Vport_AfterThrottle","Vport level at the point where the MaxI_AfterThrottle occurs.","V","VPort_PD should conform to ranges in\n802.3at Table 33-18"]
[null,"Ppeak_AfterThrottle","Maximum power consumed by the PD while powered on at Type-2 Vport_PD and following allocation reduction (or power demotion) by PSE.","watts","< 14.4 \nINFO limit - not a required behavior - 802.3at para. 33.6.3.5"]
[null,"Pavg_AfterThrottle","Average power (1 second moving window) consumed by the PD while powered on at Type-2 Vport_PD and following allocation reduction (or power demotion) by PSE.","watts","< 25.5\nINFO limit - not a required behavior - 802.3at para. 33.6.3.5"]
[null,"MPSViolation_AfterThrottle","Flag indicating PD did not satisfy DC Maintain Power Signature (MPS) and will be potentially subject to shutdown by a PSE using DC MPS method.  Measured after LLDP power demotion.","flag (1 or 0)","In order to stay powered, the PD must draw > 10mA for a time period > 75 msec out of every 325 msec time interval.  802.3at para. 33.3.8."]
[null,"TcutWindowViolation_AfterThrottle","Flag indicating that PD power draw exceeded 13W for longer than Tcut_min (50 msec).  PD is at risk of overload shutdown by PSE.  Measured after LLDP power demotion.","flag (1 or 0)","In order to stay powered, transient loads may not exceed 13W for time duration > Tcut_min, or 50 msec.  802.3at para. 33.3.7.4."]
[null,"DutyCycleViolation_AfterThrottle","Flag indicating that PD power draw is exceeding 13W for greater than 5% of the time.   PD is at risk of overload shutdown by PSE.  Measured after LLDP power demotion.","flag (1 or 0)","In order to stay powered, transient loads may not exceed 13W for > 5% duty cycle. 802.3at para. 33.3.7.4."]
[null,"PD LLDP Protocol Parameters","PD-under-test powered to Type-2 Vport with 1-Event Classification and subsequent LLDP Negotiation"]
[null,"TimeToLink","Length of time from power-up until LAN link was established.  Reports ‘-1’ if no link established.","seconds","Information parameter (INFO)."]
[null,"LinkSpeed","Speed of the LAN link.  Reports ‘-1’ if no link established.","10 | 100 | 1000","Information parameter (INFO)."]
[null,"FirstReqTime","Length of time after power-up until first LLDP Power-via-MDI request received.","seconds","Information parameter (INFO).   802.3at requires that a Type-2 PD should link and initiate LLDP within 5 minutes of power-up."]
[null,"PowerRequest","Contents of the PD requested power value field in the Power-via-MDI TLV.","watts","0.1 to 25.5\n802.3 Clause 79.3.2.5","DLL2       DLL3       DLL4       DLL9       DLL11"]
[null,"PDAckTime","Length of time for transmission of an updated LLDPDU after an LLDPDU with a new PSE allocated power value is received by the PD.","seconds","< 10\n802.3at para. 33.6.2"]
[null,"AllocPowerEchoed","Contents of the PSE allocated power value from the LLDPDU acknowledgement sent by the PD.","watts","= Allocated power value sent by PDA-600 – this will be same as PowerRequest so long as PowerRequest is valid value.."]
[null,"ThrottleAckTime","The length of time it takes the PD to acknowledge receiving the new alloc value.","seconds","< 10 seconds\n802.3at para. 33.6.2"]
[null,"ThrottlePowerReq","The PD requested power value field in the LLDPDU containing the Throttle Ack.","watts","Information parameter (INFO).  A PD is not required to alter its power request after power demotion."]
[]
[null,"Report Version",2.11,null,null,"2022-11-03"]

{"sheet":"raw_data","index":5,"n_rows":448,"n_cols":12,"rows_kept":448,"cut":false,"hidden":false,"merged":[]}
["PDA-600 Conformance Test Results"]
["Date"," 4/23/2025","Time","17:31:21","SN","'604A0196","SW","2.4.0.6","FW",2.08,"HW",4]
["CSV version",2.1,"ID","EW7489ZI7_ES1"]
["PASSIVE_QUADS","PDA_ALT_A_MDI","PDA_ALT_A_MDIX","PDA_ALT_B_MDI","PDA_ALT_B_MDIX"]
["ACTIVE_QUADS","PDA_ALT_A_MDI","PDA_ALT_A_MDIX","PDA_ALT_B_MDI","PDA_ALT_B_MDIX"]
["PASSIVE TESTS"]
["PDA_ALT_A_MDI",1,"units","min","max","avg","low","high","status"]
["Rdet",25.33,"kohm",25.33,25.33,25.33,23.7,26.3,"P"]
["Rdet_final",25.28,"kohm",25.28,25.28,25.28,23.7,26.3,"P"]
["Rdet_unpwr",">99.00","kohm",99,99,99,"<12.00",">45.00","P"]
["Rdet_at_Vmin",24.5,"kohm",24.5,24.5,24.5,23.7,26.3,"P"]
["Rdet_at_Vmax",25.58,"kohm",25.58,25.58,25.58,23.7,26.3,"P"]
["Rdet_Voffset",0.7,"VDC",0.7,0.7,0.7,0,1.9,"P"]
["Cdet",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
["Cdet_final",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
["NumMultiCycles",3,null,null,null,null,null,null,"INFO"]
["Iclass",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
["ClassNum",4,null,4,4,"-",0,4,"P"]
["Tclass",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
["Iclass_avg",40.200000000000003,"mA",40.200000000000003,40.200000000000003,40.200000000000003,36,44,"P"]
["Iclass_min",40,"mA",40,40,40,36,44,"INFO"]
["Iclass_max",40.299999999999997,"mA",40.299999999999997,40.299999999999997,40.299999999999997,36,44,"INFO"]
["Iclass_at_Vmin",39.6,"mA",39.6,39.6,39.6,36,44,"P"]
["Iclass_at_Vmax",39.4,"mA",39.4,39.4,39.4,36,44,"P"]
["Iclass_event1",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
["Iclass_event2",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
["MarkI",1.31,"mA",1.31,1.31,1.31,0.25,4,"P"]
["ClassNum2",4,null,4,4,"-",0,4,"P"]
["Tclass_event1",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
["Iclass_avg_event1",40.299999999999997,"mA",40.299999999999997,40.299999999999997,40.299999999999997,36,44,"P"]
["Iclass_min_event1",40.200000000000003,"mA",40.200000000000003,40.200000000000003,40.200000000000003,36,44,"INFO"]
["Iclass_max_event1",40.5,"mA",40.5,40.5,40.5,36,44,"INFO"]
["Tclass_event2",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
["Iclass_avg_event2",40.200000000000003,"mA",40.200000000000003,40.200000000000003,40.200000000000003,36,44,"P"]
["Iclass_min_event2",40.1,"mA",40.1,40.1,40.1,36,44,"INFO"]
["Iclass_max_event2",40.4,"mA",40.4,40.4,40.4,36,44,"INFO"]
["PDA_ALT_A_MDIX",1,"units","min","max","avg","low","high","status"]
["Rdet",25.3,"kohm",25.3,25.3,25.3,23.7,26.3,"P"]
["Rdet_final",25.33,"kohm",25.33,25.33,25.33,23.7,26.3,"P"]
["Rdet_unpwr",">99.00","kohm",99,99,99,"<12.00",">45.00","P"]
["Rdet_at_Vmin",24.74,"kohm",24.74,24.74,24.74,23.7,26.3,"P"]
["Rdet_at_Vmax",25.66,"kohm",25.66,25.66,25.66,23.7,26.3,"P"]
["Rdet_Voffset",0.7,"VDC",0.7,0.7,0.7,0,1.9,"P"]
["Cdet",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
["Cdet_final",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
["NumMultiCycles",3,null,null,null,null,null,null,"INFO"]
["Iclass",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
["ClassNum",4,null,4,4,"-",0,4,"P"]
["Tclass",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
["Iclass_avg",40.299999999999997,"mA",40.299999999999997,40.299999999999997,40.299999999999997,36,44,"P"]
["Iclass_min",40.200000000000003,"mA",40.200000000000003,40.200000000000003,40.200000000000003,36,44,"INFO"]
["Iclass_max",40.4,"mA",40.4,40.4,40.4,36,44,"INFO"]
["Iclass_at_Vmin",39.9,"mA",39.9,39.9,39.9,36,44,"P"]
["Iclass_at_Vmax",39.5,"mA",39.5,39.5,39.5,36,44,"P"]
["Iclass_event1",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
["Iclass_event2",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
["MarkI",1.31,"mA",1.31,1.31,1.31,0.25,4,"P"]
["ClassNum2",4,null,4,4,"-",0,4,"P"]
["Tclass_event1",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
["Iclass_avg_event1",40.4,"mA",40.4,40.4,40.4,36,44,"P"]
["Iclass_min_event1",40.200000000000003,"mA",40.200000000000003,40.200000000000003,40.200000000000003,36,44,"INFO"]
["Iclass_max_event1",40.5,"mA",40.5,40.5,40.5,36,44,"INFO"]
["Tclass_event2",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
["Iclass_avg_event2",40.200000000000003,"mA",40.200000000000003,40.200000000000003,40.200000000000003,36,44,"P"]
["Iclass_min_event2",40.1,"mA",40.1,40.1,40.1,36,44,"INFO"]
["Iclass_max_event2",40.4,"mA",40.4,40.4,40.4,36,44,"INFO"]
["PDA_ALT_B_MDI",1,"units","min","max","avg","low","high","status"]
["Rdet",25.28,"kohm",25.28,25.28,25.28,23.7,26.3,"P"]
["Rdet_final",25.26,"kohm",25.26,25.26,25.26,23.7,26.3,"P"]
["Rdet_unpwr",">99.00","kohm",99,99,99,"<12.00",">45.00","P"]
["Rdet_at_Vmin",24.9,"kohm",24.9,24.9,24.9,23.7,26.3,"P"]
["Rdet_at_Vmax",25.76,"kohm",25.76,25.76,25.76,23.7,26.3,"P"]
["Rdet_Voffset",0.7,"VDC",0.7,0.7,0.7,0,1.9,"P"]
["Cdet",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
["Cdet_final",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
["NumMultiCycles",3,null,null,null,null,null,null,"INFO"]
["Iclass",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
["ClassNum",4,null,4,4,"-",0,4,"P"]
["Tclass",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
["Iclass_avg",40.1,"mA",40.1,40.1,40.1,36,44,"P"]
["Iclass_min",40,"mA",40,40,40,36,44,"INFO"]
["Iclass_max",40.200000000000003,"mA",40.200000000000003,40.200000000000003,40.200000000000003,36,44,"INFO"]
["Iclass_at_Vmin",39.4,"mA",39.4,39.4,39.4,36,44,"P"]
["Iclass_at_Vmax",39.700000000000003,"mA",39.700000000000003,39.700000000000003,39.700000000000003,36,44,"P"]
["Iclass_event1",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
["Iclass_event2",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
["MarkI",1.38,"mA",1.38,1.38,1.38,0.25,4,"P"]
["ClassNum2",4,null,4,4,"-",0,4,"P"]
["Tclass_event1",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
["Iclass_avg_event1",40.1,"mA",40.1,40.1,40.1,36,44,"P"]
["Iclass_min_event1",39.9,"mA",39.9,39.9,39.9,36,44,"INFO"]
["Iclass_max_event1",40.200000000000003,"mA",40.200000000000003,40.200000000000003,40.200000000000003,36,44,"INFO"]
["Tclass_event2",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
["Iclass_avg_event2",40,"mA",40,40,40,36,44,"P"]
["Iclass_min_event2",39.700000000000003,"mA",39.700000000000003,39.700000000000003,39.700000000000003,36,44,"INFO"]
["Iclass_max_event2",40.200000000000003,"mA",40.200000000000003,40.200000000000003,40.200000000000003,36,44,"INFO"]
["PDA_ALT_B_MDIX",1,"units","min","max","avg","low","high","status"]
["Rdet",25.36,"kohm",25.36,25.36,25.36,23.7,26.3,"P"]
["Rdet_final",25.28,"kohm",25.28,25.28,25.28,23.7,26.3,"P"]
["Rdet_unpwr",">99.00","kohm",99,99,99,"<12.00",">45.00","P"]
["Rdet_at_Vmin",24.9,"kohm",24.9,24.9,24.9,23.7,26.3,"P"]
["Rdet_at_Vmax",25.7,"kohm",25.7,25.7,25.7,23.7,26.3,"P"]
["Rdet_Voffset",0.7,"VDC",0.7,0.7,0.7,0,1.9,"P"]
["Cdet",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
["Cdet_final",0.11,"uF",0.11,0.11,0.11,0.05,0.12,"P"]
["NumMultiCycles",3,null,null,null,null,null,null,"INFO"]
["Iclass",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
["ClassNum",4,null,4,4,"-",0,4,"P"]
["Tclass",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
["Iclass_avg",40.1,"mA",40.1,40.1,40.1,36,44,"P"]
["Iclass_min",39.9,"mA",39.9,39.9,39.9,36,44,"INFO"]
["Iclass_max",40.200000000000003,"mA",40.200000000000003,40.200000000000003,40.200000000000003,36,44,"INFO"]
["Iclass_at_Vmin",40.1,"mA",40.1,40.1,40.1,36,44,"P"]
["Iclass_at_Vmax",39.6,"mA",39.6,39.6,39.6,36,44,"P"]
["Iclass_event1",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
["Iclass_event2",39.799999999999997,"mA",39.799999999999997,39.799999999999997,39.799999999999997,36,44,"P"]
["MarkI",1.38,"mA",1.38,1.38,1.38,0.25,4,"P"]
["ClassNum2",4,null,4,4,"-",0,4,"P"]
["Tclass_event1",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
["Iclass_avg_event1",40.1,"mA",40.1,40.1,40.1,36,44,"P"]
["Iclass_min_event1",39.9,"mA",39.9,39.9,39.9,36,44,"INFO"]
["Iclass_max_event1",40.299999999999997,"mA",40.299999999999997,40.299999999999997,40.299999999999997,36,44,"INFO"]
["Tclass_event2",5.0000000000000001E-4,"sec",5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-4,5.0000000000000001E-3,"P"]
["Iclass_avg_event2",40,"mA",40,40,40,36,44,"P"]
["Iclass_min_event2",39.9,"mA",39.9,39.9,39.9,36,44,"INFO"]
["Iclass_max_event2",40.299999999999997,"mA",40.299999999999997,40.299999999999997,40.299999999999997,36,44,"INFO"]
["ACTIVE TESTS"]
["PDA_ALT_A_MDI",1,"units","min","max","avg","low","high","status"]
["PRE-POWER"]
["InrushI_1",176.8,"mA",176.8,176.8,176.8,0,400,"P"]
["InrushI_2",145,"mA",145,145,145,0,400,"P"]
["IlimMinViolation",0,null,0,0,"-",0,0,"P"]
["Pmax_Tdelay",0.6,"W",0.6,0.6,0.6,0,14.4,"P"]
["Inrush_delayed",0,null,0,0,"-",0,0,"P"]
["Von",37.799999999999997,"VDC",37.799999999999997,37.799999999999997,37.799999999999997,30,42,"P"]
["Voff",35.6,"VDC",35.6,35.6,35.6,30,42,"P"]
["Vhyst",2.2999999999999998,"VDC",2.2999999999999998,2.2999999999999998,2.2999999999999998,2.8,12,"WARN"]
["BackfeedV",0,"VDC",0,0,0,0,2.8,"P"]
["ClassRecover",0,null,0,0,"-",0,0,"P"]
["SigRecoverTime",0,"sec",0,0,0,0,30,"P"]
["OffTime",10,"sec",null,null,null,null,null,"INFO"]
["PhyOnTime",10,"sec",null,null,null,null,null,"INFO"]
["VportType1",42,"VDC",null,null,null,null,null,"INFO"]
["VportPHY",43.5,"VDC",null,null,null,null,null,"INFO"]
["TYPE1"]
["MinI_1",9.3000000000000007,"mA",9.3000000000000007,9.3000000000000007,9.3000000000000007,0,343.7,"P"]
["MaxI_1",92.3,"mA",92.3,92.3,92.3,10,343.7,"P"]
["Vport_1",42,"VDC",42,42,42,37,57,"INFO"]
["Ppeak_1",3.87,"W",3.87,3.87,3.87,0,14.4,"P"]
["PeakViolation_1",0,null,0,0,"-",0,0,"P"]
["Pavg_1",2.4700000000000002,"W",2.4700000000000002,2.4700000000000002,2.4700000000000002,0,13,"P"]
["PclassViolation_1",0,null,0,0,"-",0,0,"P"]
["MPSViolation_1",0,null,0,0,"-",0,0,"P"]
["TcutWindowViolation_1",0,null,0,0,"-",0,0,"P"]
["DutyCycleViolation_1",0,null,0,0,"-",0,0,"P"]
["TYPE2 PHY"]
["MinI_2",9.6,"mA",9.6,9.6,9.6,0,652.20000000000005,"P"]
["MaxI_2",61.5,"mA",61.5,61.5,61.5,10,652.20000000000005,"P"]
["Vport_2",43.4,"VDC",43.4,43.4,43.4,42.5,57,"INFO"]
["Ppeak_2",2.67,"W",2.67,2.67,2.67,0,28.31,"P"]
["PeakViolation_2",0,null,0,0,"-",0,0,"P"]
["Pavg_2",2.4900000000000002,"W",2.4900000000000002,2.4900000000000002,2.4900000000000002,0,25.5,"P"]
["PclassViolation_2",0,null,0,0,"-",0,0,"P"]
["MPSViolation_2",0,null,0,0,"-",0,0,"P"]
["TcutWindowViolation_2",0,null,0,0,"-",0,0,"P"]
["DutyCycleViolation_2",0,null,0,0,"-",0,0,"P"]
["TYPE2 LLDP"]
["LLDPOnTime",60,"sec",null,null,null,null,null,"INFO"]
["VportLLDP",43.5,"VDC",null,null,null,null,null,"INFO"]
["MinI_PreAlloc",9.4,"mA",9.4,9.4,9.4,0,331.8,"P"]
["MaxI_PreAlloc",89.9,"mA",89.9,89.9,89.9,10,331.8,"P"]
["Vport_PreAlloc",43.5,"VDC",43.5,43.5,43.5,42.5,57,"INFO"]
["Ppeak_PreAlloc",3.91,"W",3.91,3.91,3.91,0,14.4,"P"]
["PeakViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["Pavg_PreAlloc",2.72,"W",2.72,2.72,2.72,0,13,"P"]
["PclassViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["MPSViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["TcutWindowViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["DutyCycleViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["MinI_PostAlloc",-1,"mA",-1,-1,-1,0,0,"NA"]
["MaxI_PostAlloc",-1,"mA",-1,-1,-1,10,0,"NA"]
["Vport_PostAlloc",-1,"VDC",-1,-1,-1,0,57,"INFO"]
["Ppeak_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
["PeakViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["Pavg_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
["PclassViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["MPSViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["TcutWindowViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["DutyCycleViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["TimeToLink",-1,"sec",-1,-1,-1,null,null,"N/A"]
["LinkSpeed",-1,"rate","-","-","-",null,null,"N/A"]
["FirstReqTime",-1,"sec",-1,-1,-1,null,null,"N/A"]
["PowerRequest",-1,"W",-1,-1,-1,0.1,25.5,"F"]
["PDAckTime",-1,"sec",-1,-1,-1,0,10,"NA"]
["AllocPowerEchoed",-1,"W",-1,-1,-1,0,0,"NA"]
["ThrottleAckTime",-1,"sec",-1,-1,-1,0,0,"F"]
["ThrottlePowerReq",-1,"W",-1,-1,-1,0,0,"INFO"]
["MinI_AfterThrottle",-1,"mA",-1,-1,-1,0,0,"NA"]
["MaxI_AfterThrottle",-1,"mA",-1,-1,-1,10,0,"NA"]
["Vport_AfterThrottle",-1,"VDC",-1,-1,-1,0,57,"INFO"]
["Ppeak_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
["PeakViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["Pavg_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
["PclassViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["MPSViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["TcutWindowViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["DutyCycleViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["PDA_ALT_A_MDIX",1,"units","min","max","avg","low","high","status"]
["PRE-POWER"]
["InrushI_1",144.6,"mA",144.6,144.6,144.6,0,400,"P"]
["InrushI_2",147.19999999999999,"mA",147.19999999999999,147.19999999999999,147.19999999999999,0,400,"P"]
["IlimMinViolation",0,null,0,0,"-",0,0,"P"]
["Pmax_Tdelay",0.6,"W",0.6,0.6,0.6,0,14.4,"P"]
["Inrush_delayed",0,null,0,0,"-",0,0,"P"]
["Von",37.9,"VDC",37.9,37.9,37.9,30,42,"P"]
["Voff",35.700000000000003,"VDC",35.700000000000003,35.700000000000003,35.700000000000003,30,42,"P"]
["Vhyst",2.1,"VDC",2.1,2.1,2.1,2.8,12,"WARN"]
["BackfeedV",0.1,"VDC",0.1,0.1,0.1,0,2.8,"P"]
["ClassRecover",0,null,0,0,"-",0,0,"P"]
["SigRecoverTime",0,"sec",0,0,0,0,30,"P"]
["OffTime",10,"sec",null,null,null,null,null,"INFO"]
["PhyOnTime",10,"sec",null,null,null,null,null,"INFO"]
["VportType1",42,"VDC",null,null,null,null,null,"INFO"]
["VportPHY",43.5,"VDC",null,null,null,null,null,"INFO"]
["TYPE1"]
["MinI_1",9.6,"mA",9.6,9.6,9.6,0,341.9,"P"]
["MaxI_1",90.7,"mA",90.7,90.7,90.7,10,341.9,"P"]
["Vport_1",42.3,"VDC",42.3,42.3,42.3,37,57,"INFO"]
["Ppeak_1",3.83,"W",3.83,3.83,3.83,0,14.4,"P"]
["PeakViolation_1",0,null,0,0,"-",0,0,"P"]
["Pavg_1",2.5,"W",2.5,2.5,2.5,0,13,"P"]
["PclassViolation_1",0,null,0,0,"-",0,0,"P"]
["MPSViolation_1",0,null,0,0,"-",0,0,"P"]
["TcutWindowViolation_1",0,null,0,0,"-",0,0,"P"]
["DutyCycleViolation_1",0,null,0,0,"-",0,0,"P"]
["TYPE2 PHY"]
["MinI_2",9.6,"mA",9.6,9.6,9.6,0,649,"P"]
["MaxI_2",61.4,"mA",61.4,61.4,61.4,10,649,"P"]
["Vport_2",43.6,"VDC",43.6,43.6,43.6,42.5,57,"INFO"]
["Ppeak_2",2.68,"W",2.68,2.68,2.68,0,28.31,"P"]
["PeakViolation_2",0,null,0,0,"-",0,0,"P"]
["Pavg_2",2.5099999999999998,"W",2.5099999999999998,2.5099999999999998,2.5099999999999998,0,25.5,"P"]
["PclassViolation_2",0,null,0,0,"-",0,0,"P"]
["MPSViolation_2",0,null,0,0,"-",0,0,"P"]
["TcutWindowViolation_2",0,null,0,0,"-",0,0,"P"]
["DutyCycleViolation_2",0,null,0,0,"-",0,0,"P"]
["TYPE2 LLDP"]
["LLDPOnTime",60,"sec",null,null,null,null,null,"INFO"]
["VportLLDP",43.5,"VDC",null,null,null,null,null,"INFO"]
["MinI_PreAlloc",9.5,"mA",9.5,9.5,9.5,0,330.2,"P"]
["MaxI_PreAlloc",88.3,"mA",88.3,88.3,88.3,10,330.2,"P"]
["Vport_PreAlloc",43.7,"VDC",43.7,43.7,43.7,42.5,57,"INFO"]
["Ppeak_PreAlloc",3.86,"W",3.86,3.86,3.86,0,14.4,"P"]
["PeakViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["Pavg_PreAlloc",2.74,"W",2.74,2.74,2.74,0,13,"P"]
["PclassViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["MPSViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["TcutWindowViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["DutyCycleViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["MinI_PostAlloc",-1,"mA",-1,-1,-1,0,0,"NA"]
["MaxI_PostAlloc",-1,"mA",-1,-1,-1,10,0,"NA"]
["Vport_PostAlloc",-1,"VDC",-1,-1,-1,0,57,"INFO"]
["Ppeak_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
["PeakViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["Pavg_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
["PclassViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["MPSViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["TcutWindowViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["DutyCycleViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["TimeToLink",-1,"sec",-1,-1,-1,null,null,"N/A"]
["LinkSpeed",-1,"rate","-","-","-",null,null,"N/A"]
["FirstReqTime",-1,"sec",-1,-1,-1,null,null,"N/A"]
["PowerRequest",-1,"W",-1,-1,-1,0.1,25.5,"F"]
["PDAckTime",-1,"sec",-1,-1,-1,0,10,"NA"]
["AllocPowerEchoed",-1,"W",-1,-1,-1,0,0,"NA"]
["ThrottleAckTime",-1,"sec",-1,-1,-1,0,0,"F"]
["ThrottlePowerReq",-1,"W",-1,-1,-1,0,0,"INFO"]
["MinI_AfterThrottle",-1,"mA",-1,-1,-1,0,0,"NA"]
["MaxI_AfterThrottle",-1,"mA",-1,-1,-1,10,0,"NA"]
["Vport_AfterThrottle",-1,"VDC",-1,-1,-1,0,57,"INFO"]
["Ppeak_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
["PeakViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["Pavg_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
["PclassViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["MPSViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["TcutWindowViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["DutyCycleViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["PDA_ALT_B_MDI",1,"units","min","max","avg","low","high","status"]
["PRE-POWER"]
["InrushI_1",157.19999999999999,"mA",157.19999999999999,157.19999999999999,157.19999999999999,0,400,"P"]
["InrushI_2",164.5,"mA",164.5,164.5,164.5,0,400,"P"]
["IlimMinViolation",0,null,0,0,"-",0,0,"P"]
["Pmax_Tdelay",0.6,"W",0.6,0.6,0.6,0,14.4,"P"]
["Inrush_delayed",0,null,0,0,"-",0,0,"P"]
["Von",37.799999999999997,"VDC",37.799999999999997,37.799999999999997,37.799999999999997,30,42,"P"]
["Voff",35.5,"VDC",35.5,35.5,35.5,30,42,"P"]
["Vhyst",2.2999999999999998,"VDC",2.2999999999999998,2.2999999999999998,2.2999999999999998,2.8,12,"WARN"]
["BackfeedV",0,"VDC",0,0,0,0,2.8,"P"]
["ClassRecover",0,null,0,0,"-",0,0,"P"]
["SigRecoverTime",0,"sec",0,0,0,0,30,"P"]
["OffTime",10,"sec",null,null,null,null,null,"INFO"]
["PhyOnTime",10,"sec",null,null,null,null,null,"INFO"]
["VportType1",42,"VDC",null,null,null,null,null,"INFO"]
["VportPHY",43.5,"VDC",null,null,null,null,null,"INFO"]
["TYPE1"]
["MinI_1",9,"mA",9,9,9,0,344.2,"P"]
["MaxI_1",98.4,"mA",98.4,98.4,98.4,10,344.2,"P"]
["Vport_1",42,"VDC",42,42,42,37,57,"INFO"]
["Ppeak_1",4.13,"W",4.13,4.13,4.13,0,14.4,"P"]
["PeakViolation_1",0,null,0,0,"-",0,0,"P"]
["Pavg_1",2.4700000000000002,"W",2.4700000000000002,2.4700000000000002,2.4700000000000002,0,13,"P"]
["PclassViolation_1",0,null,0,0,"-",0,0,"P"]
["MPSViolation_1",0,null,0,0,"-",0,0,"P"]
["TcutWindowViolation_1",0,null,0,0,"-",0,0,"P"]
["DutyCycleViolation_1",0,null,0,0,"-",0,0,"P"]
["TYPE2 PHY"]
["MinI_2",9.1,"mA",9.1,9.1,9.1,0,653.20000000000005,"P"]
["MaxI_2",62.4,"mA",62.4,62.4,62.4,10,653.20000000000005,"P"]
["Vport_2",43.3,"VDC",43.3,43.3,43.3,42.5,57,"INFO"]
["Ppeak_2",2.7,"W",2.7,2.7,2.7,0,28.31,"P"]
["PeakViolation_2",0,null,0,0,"-",0,0,"P"]
["Pavg_2",2.4900000000000002,"W",2.4900000000000002,2.4900000000000002,2.4900000000000002,0,25.5,"P"]
["PclassViolation_2",0,null,0,0,"-",0,0,"P"]
["MPSViolation_2",0,null,0,0,"-",0,0,"P"]
["TcutWindowViolation_2",0,null,0,0,"-",0,0,"P"]
["DutyCycleViolation_2",0,null,0,0,"-",0,0,"P"]
["TYPE2 LLDP"]
["LLDPOnTime",60,"sec",null,null,null,null,null,"INFO"]
["VportLLDP",43.5,"VDC",null,null,null,null,null,"INFO"]
["MinI_PreAlloc",9.3000000000000007,"mA",9.3000000000000007,9.3000000000000007,9.3000000000000007,0,332.4,"P"]
["MaxI_PreAlloc",115.6,"mA",115.6,115.6,115.6,10,332.4,"P"]
["Vport_PreAlloc",43.5,"VDC",43.5,43.5,43.5,42.5,57,"INFO"]
["Ppeak_PreAlloc",5.0199999999999996,"W",5.0199999999999996,5.0199999999999996,5.0199999999999996,0,14.4,"P"]
["PeakViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["Pavg_PreAlloc",2.72,"W",2.72,2.72,2.72,0,13,"P"]
["PclassViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["MPSViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["TcutWindowViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["DutyCycleViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["MinI_PostAlloc",-1,"mA",-1,-1,-1,0,0,"NA"]
["MaxI_PostAlloc",-1,"mA",-1,-1,-1,10,0,"NA"]
["Vport_PostAlloc",-1,"VDC",-1,-1,-1,0,57,"INFO"]
["Ppeak_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
["PeakViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["Pavg_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
["PclassViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["MPSViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["TcutWindowViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["DutyCycleViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["TimeToLink",-1,"sec",-1,-1,-1,null,null,"N/A"]
["LinkSpeed",-1,"rate","-","-","-",null,null,"N/A"]
["FirstReqTime",-1,"sec",-1,-1,-1,null,null,"N/A"]
["PowerRequest",-1,"W",-1,-1,-1,0.1,25.5,"F"]
["PDAckTime",-1,"sec",-1,-1,-1,0,10,"NA"]
["AllocPowerEchoed",-1,"W",-1,-1,-1,0,0,"NA"]
["ThrottleAckTime",-1,"sec",-1,-1,-1,0,0,"F"]
["ThrottlePowerReq",-1,"W",-1,-1,-1,0,0,"INFO"]
["MinI_AfterThrottle",-1,"mA",-1,-1,-1,0,0,"NA"]
["MaxI_AfterThrottle",-1,"mA",-1,-1,-1,10,0,"NA"]
["Vport_AfterThrottle",-1,"VDC",-1,-1,-1,0,57,"INFO"]
["Ppeak_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
["PeakViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["Pavg_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
["PclassViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["MPSViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["TcutWindowViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["DutyCycleViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["PDA_ALT_B_MDIX",1,"units","min","max","avg","low","high","status"]
["PRE-POWER"]
["InrushI_1",158.5,"mA",158.5,158.5,158.5,0,400,"P"]
["InrushI_2",159.69999999999999,"mA",159.69999999999999,159.69999999999999,159.69999999999999,0,400,"P"]
["IlimMinViolation",0,null,0,0,"-",0,0,"P"]
["Pmax_Tdelay",0.6,"W",0.6,0.6,0.6,0,14.4,"P"]
["Inrush_delayed",0,null,0,0,"-",0,0,"P"]
["Von",38,"VDC",38,38,38,30,42,"P"]
["Voff",35.799999999999997,"VDC",35.799999999999997,35.799999999999997,35.799999999999997,30,42,"P"]
["Vhyst",2.2999999999999998,"VDC",2.2999999999999998,2.2999999999999998,2.2999999999999998,2.8,12,"WARN"]
["BackfeedV",0,"VDC",0,0,0,0,2.8,"P"]
["ClassRecover",0,null,0,0,"-",0,0,"P"]
["SigRecoverTime",0,"sec",0,0,0,0,30,"P"]
["OffTime",10,"sec",null,null,null,null,null,"INFO"]
["PhyOnTime",10,"sec",null,null,null,null,null,"INFO"]
["VportType1",42,"VDC",null,null,null,null,null,"INFO"]
["VportPHY",43.5,"VDC",null,null,null,null,null,"INFO"]
["TYPE1"]
["MinI_1",9.1,"mA",9.1,9.1,9.1,0,342,"P"]
["MaxI_1",99.2,"mA",99.2,99.2,99.2,10,342,"P"]
["Vport_1",42.2,"VDC",42.2,42.2,42.2,37,57,"INFO"]
["Ppeak_1",4.1900000000000004,"W",4.1900000000000004,4.1900000000000004,4.1900000000000004,0,14.4,"P"]
["PeakViolation_1",0,null,0,0,"-",0,0,"P"]
["Pavg_1",2.4900000000000002,"W",2.4900000000000002,2.4900000000000002,2.4900000000000002,0,13,"P"]
["PclassViolation_1",0,null,0,0,"-",0,0,"P"]
["MPSViolation_1",0,null,0,0,"-",0,0,"P"]
["TcutWindowViolation_1",0,null,0,0,"-",0,0,"P"]
["DutyCycleViolation_1",0,null,0,0,"-",0,0,"P"]
["TYPE2 PHY"]
["MinI_2",9.1,"mA",9.1,9.1,9.1,0,649.29999999999995,"P"]
["MaxI_2",62.1,"mA",62.1,62.1,62.1,10,649.29999999999995,"P"]
["Vport_2",43.6,"VDC",43.6,43.6,43.6,42.5,57,"INFO"]
["Ppeak_2",2.7,"W",2.7,2.7,2.7,0,28.31,"P"]
["PeakViolation_2",0,null,0,0,"-",0,0,"P"]
["Pavg_2",2.5,"W",2.5,2.5,2.5,0,25.5,"P"]
["PclassViolation_2",0,null,0,0,"-",0,0,"P"]
["MPSViolation_2",0,null,0,0,"-",0,0,"P"]
["TcutWindowViolation_2",0,null,0,0,"-",0,0,"P"]
["DutyCycleViolation_2",0,null,0,0,"-",0,0,"P"]
["TYPE2 LLDP"]
["LLDPOnTime",60,"sec",null,null,null,null,null,"INFO"]
["VportLLDP",43.5,"VDC",null,null,null,null,null,"INFO"]
["MinI_PreAlloc",9.1,"mA",9.1,9.1,9.1,0,330.4,"P"]
["MaxI_PreAlloc",114.8,"mA",114.8,114.8,114.8,10,330.4,"P"]
["Vport_PreAlloc",43.7,"VDC",43.7,43.7,43.7,42.5,57,"INFO"]
["Ppeak_PreAlloc",5.0199999999999996,"W",5.0199999999999996,5.0199999999999996,5.0199999999999996,0,14.4,"P"]
["PeakViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["Pavg_PreAlloc",2.74,"W",2.74,2.74,2.74,0,13,"P"]
["PclassViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["MPSViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["TcutWindowViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["DutyCycleViolation_PreAlloc",0,null,0,0,"-",0,0,"P"]
["MinI_PostAlloc",-1,"mA",-1,-1,-1,0,0,"NA"]
["MaxI_PostAlloc",-1,"mA",-1,-1,-1,10,0,"NA"]
["Vport_PostAlloc",-1,"VDC",-1,-1,-1,0,57,"INFO"]
["Ppeak_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
["PeakViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["Pavg_PostAlloc",-1,"W",-1,-1,-1,0,0,"NA"]
["PclassViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["MPSViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["TcutWindowViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["DutyCycleViolation_PostAlloc",-1,null,-1,-1,"-",0,0,"NA"]
["TimeToLink",-1,"sec",-1,-1,-1,null,null,"N/A"]
["LinkSpeed",-1,"rate","-","-","-",null,null,"N/A"]
["FirstReqTime",-1,"sec",-1,-1,-1,null,null,"N/A"]
["PowerRequest",-1,"W",-1,-1,-1,0.1,25.5,"F"]
["PDAckTime",-1,"sec",-1,-1,-1,0,10,"NA"]
["AllocPowerEchoed",-1,"W",-1,-1,-1,0,0,"NA"]
["ThrottleAckTime",-1,"sec",-1,-1,-1,0,0,"F"]
["ThrottlePowerReq",-1,"W",-1,-1,-1,0,0,"INFO"]
["MinI_AfterThrottle",-1,"mA",-1,-1,-1,0,0,"NA"]
["MaxI_AfterThrottle",-1,"mA",-1,-1,-1,10,0,"NA"]
["Vport_AfterThrottle",-1,"VDC",-1,-1,-1,0,57,"INFO"]
["Ppeak_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
["PeakViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["Pavg_AfterThrottle",-1,"W",-1,-1,-1,0,0,"NA"]
["PclassViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["MPSViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["TcutWindowViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["DutyCycleViolation_AfterThrottle",-1,null,-1,-1,"-",0,0,"NA"]
["END"]