{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["2S1P-ZY-1212"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"2S1P-ZY-1212","index":0,"n_rows":266,"n_cols":5,"rows_kept":266,"cut":false,"hidden":false,"merged":[]}
["* Texas Instruments Data Flash File"]
["* File created Wed Dec 14 11:38:50 2022"]
["*"]
["* Device Number 542"]
["* Firmware Version 2.01"]
["* Build Number not available"]
["* Order Number not available"]
["*"]
["* bqz Device Number 0542"]
["* bqz Firmware Version 2.01"]
["* bqz Build Number 1"]
["*"]
["* Field Order: Class name"," Subclass name"," Parameter name"," Parameter Value"," Display Units"]
["Calibration","Data","CC Gain",5.1150000000000002,"mOhm"]
["Calibration","Data","CC Delta",5.093,"mOhm"]
["Calibration","Data","CC Offset",-1507,"-"]
["Calibration","Data","Board Offset",-1,"Counts"]
["Calibration","Data","Int Temp Offset",-0.3,"簞C"]
["Calibration","Data","Ext Temp Offset",-0.3,"簞C"]
["Calibration","Data","Pack V Offset",6,"mV"]
["Calibration","Current","Filter",239,"Num"]
["Calibration","Current","Deadband",5,"mA"]
["Calibration","Current","CC Deadband",17,"Counts"]
["Configuration","Charge","Charging Voltage",4200,"mV"]
["Configuration","Charge Termination","Taper Current",150,"mA"]
["Configuration","Charge Termination","Min Taper Capacity",100,"mAh"]
["Configuration","Charge Termination","Taper Voltage",100,"mV"]
["Configuration","Charge Termination","Current Taper Window",40,"s"]
["Configuration","Charge Termination","TCA Set %",-1,"%"]
["Configuration","Charge Termination","TCA Clear %",99,"%"]
["Configuration","Charge Termination","FC Set %",-1,"%"]
["Configuration","Charge Termination","FC Clear %",99,"%"]
["Configuration","Charge Termination","DODatEOC Delta T",5,"簞C"]
["Configuration","JEITA","T1 Temp",0,"簞C"]
["Configuration","JEITA","T2 Temp",10,"簞C"]
["Configuration","JEITA","T3 Temp",45,"簞C"]
["Configuration","JEITA","T4 Temp",50,"簞C"]
["Configuration","JEITA","T5 Temp",60,"簞C"]
["Configuration","JEITA","Temp Hys",3,"簞C"]
["Configuration","JEITA","T1-T2 Chg Voltage",4200,"mV"]
["Configuration","JEITA","T2-T3 Chg Voltage",4200,"mV"]
["Configuration","JEITA","T3-T4 Chg Voltage",4150,"mV"]
["Configuration","JEITA","T4-T5 Chg Voltage",4100,"mV"]
["Configuration","JEITA","T1-T2 Chg Current",35,"%"]
["Configuration","JEITA","T2-T3 Chg Current",50,"%"]
["Configuration","JEITA","T3-T4 Chg Current",50,"%"]
["Configuration","JEITA","T4-T5 Chg Current",50,"%"]
["Configuration","Registers","Pack Configuration","297f","Flag"]
["Configuration","Registers","Pack Configuration B",83,"Flag"]
["Configuration","Registers","Pack Configuration C","b9","Flag"]
["Configuration","Registers","Pack Configuration D",57,"Flag"]
["Configuration","HDQ","Host Interrupt Tries",3,"Num"]
["Configuration","Power","Flash Update OK Voltage",2400,"mV"]
["Configuration","Power","Sleep Current",15,"mA"]
["Configuration","Power","Hibernate Current",8,"mA"]
["Configuration","Power","Hibernate Voltage",2550,"mV"]
["Configuration","Power","FS Wait",120,"s"]
["Configuration","Lifetime Data","Lifetime Max Temp",116.2,"簞C"]
["Configuration","Lifetime Data","Lifetime Min Temp",-18.8,"簞C"]
["Configuration","Lifetime Data","Lifetime Max Pack Voltage",4197,"mV"]
["Configuration","Lifetime Data","Lifetime Min Pack Voltage",2412,"mV"]
["Configuration","Lifetime Data","Lifetime Max Chg Current",2022,"mA"]
["Configuration","Lifetime Data","Lifetime Max Dsg Current",-6935,"mA"]
["Configuration","Lifetime Temp Samples","LT Flash Cnt",0,"Num"]
["Configuration","Lifetime Resolution","LT Temp Res",1,"簞C"]
["Configuration","Lifetime Resolution","LT V Res",25,"mV"]
["Configuration","Lifetime Resolution","LT Cur Res",100,"mA"]
["Configuration","Lifetime Resolution","LT Update Time",60,"s"]
["Configuration","Safety","OT Chg",55,"簞C"]
["Configuration","Safety","OT Chg Time",5,"s"]
["Configuration","Safety","OT Chg Recovery",50,"簞C"]
["Configuration","Safety","OT Dsg",60,"簞C"]
["Configuration","Safety","OT Dsg Time",5,"s"]
["Configuration","Safety","OT Dsg Recovery",55,"簞C"]
["Configuration","Manufacturer Data","Pack Lot Code",0,"Hex"]
["Configuration","Manufacturer Data","PCB Lot Code",0,"Hex"]
["Configuration","Manufacturer Data","Firmware Version",0,"Hex"]
["Configuration","Manufacturer Data","Hardware Revision",0,"Hex"]
["Configuration","Manufacturer Data","Cell Revision",0,"Hex"]
["Configuration","Manufacturer Data","DF Config Version",0,"Hex"]
["Configuration","Integrity Data","All DF Checksum",0,"Hex"]
["Configuration","Integrity Data","Static Chem DF Checksum","7abb","Hex"]
["Configuration","Integrity Data","Static DF Checksum",0,"Hex"]
["Configuration","Data","Design Voltage",3600,"mV"]
["Configuration","Data","Cycle Count",2,"Num"]
["Configuration","Data","CC Threshold",2475,"mAh"]
["Configuration","Data","Design Capacity",2475,"mAh"]
["Configuration","Data","Design Energy",8910,"mWh"]
["Configuration","Data","SOH Load I",-7000,"mA"]
["Configuration","Data","TDD SOH Percent",80,"%"]
["Configuration","Data","ISD Current",10,"hourrate"]
["Configuration","Data","ISD I Filter",127,"Num"]
["Configuration","Data","Min ISD Time",7,"hour"]
["Configuration","Data","Design Energy Scale",1,"Num"]
["Configuration","Discharge","SOC1 Set Threshold",248,"mAh"]
["Configuration","Discharge","SOC1 Clear Threshold",371,"mAh"]
["Configuration","Discharge","SOCF Set Threshold",50,"mAh"]
["Configuration","Discharge","SOCF Clear Threshold",124,"mAh"]
["Configuration","Discharge","BL Set Volt Threshold",2500,"mV"]
["Configuration","Discharge","BL Set Volt Time",2,"s"]
["Configuration","Discharge","BL Clear Volt Threshold",2600,"mV"]
["Configuration","Discharge","BH Set Volt Threshold",4300,"mV"]
["Configuration","Discharge","BH Volt Time",2,"s"]
["Configuration","Discharge","BH Clear Volt Threshold",4200,"mV"]
["Gas Gauging","Current Thresholds","Dsg Current Threshold",60,"mA"]
["Gas Gauging","Current Thresholds","Chg Current Threshold",75,"mA"]
["Gas Gauging","Current Thresholds","Quit Current",40,"mA"]
["Gas Gauging","Current Thresholds","Dsg Relax Time",60,"s"]
["Gas Gauging","Current Thresholds","Chg Relax Time",60,"s"]
["Gas Gauging","Current Thresholds","Max IR Correct",400,"mV"]
["Gas Gauging","State","Qmax Cell 0",2630,"mAh"]
["Gas Gauging","State","Update Status",6,"Hex"]
["Gas Gauging","State","V at Chg Term",4197,"mV"]
["Gas Gauging","State","Avg I Last Run",-498,"mA"]
["Gas Gauging","State","Avg P Last Run",-1699,"pwr"]
["Gas Gauging","State","Delta Voltage",3,"mV"]
["Gas Gauging","State","T Rise",50,"Num"]
["Gas Gauging","State","T Time Constant",1000,"Num"]
["Gas Gauging","IT Cfg","Load Select",1,"Num"]
["Gas Gauging","IT Cfg","Load Mode",1,"Num"]
["Gas Gauging","IT Cfg","Max Res Factor",15,"Num"]
["Gas Gauging","IT Cfg","Min Res Factor",5,"Num"]
["Gas Gauging","IT Cfg","Ra Filter",800,"Num"]
["Gas Gauging","IT Cfg","Res V Drop",50,"mV"]
["Gas Gauging","IT Cfg","Fast Qmax Start DOD %",92,"%"]
["Gas Gauging","IT Cfg","Fast Qmax End DOD %",96,"%"]
["Gas Gauging","IT Cfg","Fast Qmax Start Volt Delta",200,"mV"]
["Gas Gauging","IT Cfg","Fast Qmax Current Threshold",4,"hourrate"]
["Gas Gauging","IT Cfg","Qmax Capacity Err",1.5,"%"]
["Gas Gauging","IT Cfg","Max Qmax Change",30,"%"]
["Gas Gauging","IT Cfg","Terminate Voltage",2800,"mV"]
["Gas Gauging","IT Cfg","Term V Delta",200,"mV"]
["Gas Gauging","IT Cfg","ResRelax Time",500,"s"]
["Gas Gauging","IT Cfg","User Rate-mA",0,"mA"]
["Gas Gauging","IT Cfg","User Rate-Pwr",0,"pwr"]
["Gas Gauging","IT Cfg","Reserve Cap-mAh",0,"mAh"]
["Gas Gauging","IT Cfg","Reserve Energy",0,"egy"]
["Gas Gauging","IT Cfg","Max DeltaV",200,"mV"]
["Gas Gauging","IT Cfg","Min DeltaV",0,"mV"]
["Gas Gauging","IT Cfg","Max Sim Rate",1,"hourrate"]
["Gas Gauging","IT Cfg","Min Sim Rate",20,"hourrate"]
["Gas Gauging","IT Cfg","Ra Max Delta",20,"mOhm"]
["Gas Gauging","IT Cfg","Trace Resistance",0,"mOhm"]
["Gas Gauging","IT Cfg","Downstream Resistance",0,"mOhm"]
["Gas Gauging","IT Cfg","Qmax Max Delta %",5,"%"]
["Gas Gauging","IT Cfg","Qmax Bound %",130,"%"]
["Gas Gauging","IT Cfg","DeltaV Max Delta",10,"mV"]
["Gas Gauging","IT Cfg","Max Res Scale",5000,"Num"]
["Gas Gauging","IT Cfg","Min Res Scale",200,"Num"]
["Gas Gauging","IT Cfg","Fast Scale Start SOC",10,"%"]
["Gas Gauging","IT Cfg","Fast Scale Load Select",3,"Num"]
["Gas Gauging","IT Cfg","Charge Hys V Shift",40,"mV"]
["Gas Gauging","IT Cfg","RaScl OCV Rst Temp Thresh",15,"簞C"]
["Gas Gauging","IT Cfg","Max Allowed Current",8500,"mA"]
["Gas Gauging","IT Cfg","Max Current Pulse Duration",10,"s"]
["Gas Gauging","IT Cfg","Max Current Interrupt Step",500,"mA"]
["Gas Gauging","IT Cfg","Predict Outside Temp Time",2000,"s"]
["Gas Gauging","IT Cfg","Termination Voltage Valid Time",10,"s"]
["Security","Codes","Sealed to Unsealed MSB",3029,"Hex"]
["Security","Codes","Sealed to Unsealed LSB",2,"Hex"]
["Security","Codes","Unsealed to Full MSB","ffff","Hex"]
["Security","Codes","Unsealed to Full LSB","ffff","Hex"]
["Security","Codes","Authen Key3 MSB",123,"Hex"]
["Security","Codes","Authen Key3 LSB",4567,"Hex"]
["Security","Codes","Authen Key2 MSB","89ab","Hex"]
["Security","Codes","Authen Key2 LSB","cdef","Hex"]
["Security","Codes","Authen Key1 MSB","fedc","Hex"]
["Security","Codes","Authen Key1 LSB","ba98","Hex"]
["Security","Codes","Authen Key0 MSB",7654,"Hex"]
["Security","Codes","Authen Key0 LSB",3210,"Hex"]
["System Data","Manufacturer Info","Block A 0",0,"Hex"]
["System Data","Manufacturer Info","Block A 1",0,"Hex"]
["System Data","Manufacturer Info","Block A 2",0,"Hex"]
["System Data","Manufacturer Info","Block A 3",0,"Hex"]
["System Data","Manufacturer Info","Block A 4",0,"Hex"]
["System Data","Manufacturer Info","Block A 5",0,"Hex"]
["System Data","Manufacturer Info","Block A 6",0,"Hex"]
["System Data","Manufacturer Info","Block A 7",0,"Hex"]
["System Data","Manufacturer Info","Block A 8",0,"Hex"]
["System Data","Manufacturer Info","Block A 9",0,"Hex"]
["System Data","Manufacturer Info","Block A 10",0,"Hex"]
["System Data","Manufacturer Info","Block A 11",0,"Hex"]
["System Data","Manufacturer Info","Block A 12",0,"Hex"]
["System Data","Manufacturer Info","Block A 13",0,"Hex"]
["System Data","Manufacturer Info","Block A 14",0,"Hex"]
["System Data","Manufacturer Info","Block A 15",0,"Hex"]
["System Data","Manufacturer Info","Block A 16",0,"Hex"]
["System Data","Manufacturer Info","Block A 17",0,"Hex"]
["System Data","Manufacturer Info","Block A 18",0,"Hex"]
["System Data","Manufacturer Info","Block A 19",0,"Hex"]
["System Data","Manufacturer Info","Block A 20",0,"Hex"]
["System Data","Manufacturer Info","Block A 21",0,"Hex"]
["System Data","Manufacturer Info","Block A 22",0,"Hex"]
["System Data","Manufacturer Info","Block A 23",0,"Hex"]
["System Data","Manufacturer Info","Block A 24",0,"Hex"]
["System Data","Manufacturer Info","Block A 25",0,"Hex"]
["System Data","Manufacturer Info","Block A 26",0,"Hex"]
["System Data","Manufacturer Info","Block A 27",0,"Hex"]
["System Data","Manufacturer Info","Block A 28",0,"Hex"]
["System Data","Manufacturer Info","Block A 29",0,"Hex"]
["System Data","Manufacturer Info","Block A 30",0,"Hex"]
["System Data","Manufacturer Info","Block A 31",0,"Hex"]
["System Data","Manufacturer Info","Block B 0",1,"Hex"]
["System Data","Manufacturer Info","Block B 1",0,"Hex"]
["System Data","Manufacturer Info","Block B 2",0,"Hex"]
["System Data","Manufacturer Info","Block B 3",0,"Hex"]
["System Data","Manufacturer Info","Block B 4",0,"Hex"]
["System Data","Manufacturer Info","Block B 5",0,"Hex"]
["System Data","Manufacturer Info","Block B 6",0,"Hex"]
["System Data","Manufacturer Info","Block B 7",0,"Hex"]
["System Data","Manufacturer Info","Block B 8",0,"Hex"]
["System Data","Manufacturer Info","Block B 9",0,"Hex"]
["System Data","Manufacturer Info","Block B 10",0,"Hex"]
["System Data","Manufacturer Info","Block B 11",0,"Hex"]
["System Data","Manufacturer Info","Block B 12",0,"Hex"]
["System Data","Manufacturer Info","Block B 13",0,"Hex"]
["System Data","Manufacturer Info","Block B 14",0,"Hex"]
["System Data","Manufacturer Info","Block B 15",0,"Hex"]
["System Data","Manufacturer Info","Block B 16",0,"Hex"]
["System Data","Manufacturer Info","Block B 17",0,"Hex"]
["System Data","Manufacturer Info","Block B 18",0,"Hex"]
["System Data","Manufacturer Info","Block B 19",0,"Hex"]
["System Data","Manufacturer Info","Block B 20",0,"Hex"]
["System Data","Manufacturer Info","Block B 21",0,"Hex"]
["System Data","Manufacturer Info","Block B 22",0,"Hex"]
["System Data","Manufacturer Info","Block B 23",0,"Hex"]
["System Data","Manufacturer Info","Block B 24",0,"Hex"]
["System Data","Manufacturer Info","Block B 25",0,"Hex"]
["System Data","Manufacturer Info","Block B 26",0,"Hex"]
["System Data","Manufacturer Info","Block B 27",0,"Hex"]
["System Data","Manufacturer Info","Block B 28",0,"Hex"]
["System Data","Manufacturer Info","Block B 29",0,"Hex"]
["System Data","Manufacturer Info","Block B 30",0,"Hex"]
["System Data","Manufacturer Info","Block B 31",0,"Hex"]
["Ra Tables","Ra0 Table","Ra Flag",0,"-"]
["Ra Tables","Ra0 Table","Ra 0",108,"2^-10ohm"]
["Ra Tables","Ra0 Table","Ra 1",108,"2^-10ohm"]
["Ra Tables","Ra0 Table","Ra 2",131,"2^-10ohm"]
["Ra Tables","Ra0 Table","Ra 3",132,"2^-10ohm"]
["Ra Tables","Ra0 Table","Ra 4",136,"2^-10ohm"]
["Ra Tables","Ra0 Table","Ra 5",140,"2^-10ohm"]
["Ra Tables","Ra0 Table","Ra 6",172,"2^-10ohm"]
["Ra Tables","Ra0 Table","Ra 7",199,"2^-10ohm"]
["Ra Tables","Ra0 Table","Ra 8",223,"2^-10ohm"]
["Ra Tables","Ra0 Table","Ra 9",287,"2^-10ohm"]
["Ra Tables","Ra0 Table","Ra 10",205,"2^-10ohm"]
["Ra Tables","Ra0 Table","Ra 11",268,"2^-10ohm"]
["Ra Tables","Ra0 Table","Ra 12",305,"2^-10ohm"]
["Ra Tables","Ra0 Table","Ra 13",912,"2^-10ohm"]
["Ra Tables","Ra0 Table","Ra 14",1531,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra Flag",55,"-"]
["Ra Tables","Ra0x Table","Ra 0",108,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra 1",108,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra 2",131,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra 3",141,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra 4",145,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra 5",150,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra 6",184,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra 7",213,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra 8",238,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra 9",307,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra 10",219,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra 11",286,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra 12",326,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra 13",974,"2^-10ohm"]
["Ra Tables","Ra0x Table","Ra 14",1635,"2^-10ohm"]