**I2C1 Debug**

1. I2C addresses selection:

A close up of a list

AI-generated content may be incorrect.

1. Read register 0x00 by Linux tool i2ctranster

**Path: PC -> USB -> CH347 -> I2C -> TPS65988DK**

A screenshot of a computer

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.

A screen shot of a computer

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.

A screen shot of a computer

AI-generated content may be incorrect.

1. Sweep I2C address

A screenshot of a computer

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.

1. Test registers 0x03/0x07 by ‘Application Custom Tool’

A screenshot of a computer

AI-generated content may be incorrect.

A screenshot of a computer error message

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.