**I2C1 Debug**

1. I2C addresses selection:



1. Read register 0x00 by Linux tool i2ctranster

**Path: PC -> USB -> CH347 -> I2C -> TPS65988DK**













1. Sweep I2C address





1. Test registers 0x03/0x07 by ‘Application Custom Tool’





