**Instruction’s firmware update MSP-EXP430F5529LP**

1. Install Java.
2. Run file “Setup\_PMICUSB2ANYLaunchpadFirmware\_2.7.0.0.exe”.
3. Run “MSP430\_USB\_Firmware\_Upgrade\_Example-1.3.1.2-Setup”
4. Run “BSL\_USB\_GUI.exe” from folder C:\ti\msp\MSP430USBFW\_1\_3\_1\_2\MSP430USBFW.
5. Choose “Select Firmare”.
6. Browse to file “USB2ANY\_2.7.0.0\_LP.txt” at folder “C:\Program Files (x86)\Texas Instruments\PMIC USB2ANY Launchpad Firmware”
7. Press and hold on “MSP-EXP430F5529LP” button S5 “BSL”.
8. Connect USB to PC.
9. Press “Update Firmware”.
10. When finish below is the result.

Graphical user interface, application

Description automatically generated