("FILE_TYPE"	"PMAP File"
    ("devices"
        ("R")
        ("D_D1")
        ("C")
        ("VPULSE")
        ("CESR_7")
        ("LDCR")
        ("IPULSE")
    )
    ("instances"
        ("R3"
            ("device_name"	"R")
            ("pspice_path"	"R_R3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"10k")
                    ("pspice_param"	"VALUE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("D1"
            ("device_name"	"D_D1")
            ("pspice_path"	"D_D1")
            ("level"	"0")
            ("model_params"
                ("AREA"
                    ("value"	"")
                    ("pspice_param"	"AREA")
                )
            )
        )
        ("R1"
            ("device_name"	"R")
            ("pspice_path"	"R_R1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"10k")
                    ("pspice_param"	"VALUE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("R2"
            ("device_name"	"R")
            ("pspice_path"	"R_R2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"69.8k")
                    ("pspice_param"	"VALUE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("C3"
            ("device_name"	"C")
            ("pspice_path"	"C_C3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"330p")
                    ("pspice_param"	"VALUE")
                )
                ("MAX_TEMP"
                    ("value"	"CTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"CSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("KNEE"
                    ("value"	"CBMAX")
                    ("pspice_param"	"KNEE")
                )
                ("CURRENT"
                    ("value"	"CIMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("VOLTAGE"
                    ("value"	"CMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("Rs"
            ("device_name"	"R")
            ("pspice_path"	"R_Rs")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"10m")
                    ("pspice_param"	"VALUE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("VIN"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_VIN")
            ("level"	"0")
            ("model_params"
                ("PER"
                    ("value"	"3")
                    ("pspice_param"	"PER")
                )
                ("TF"
                    ("value"	"40u")
                    ("pspice_param"	"TF")
                )
                ("TD"
                    ("value"	"40u")
                    ("pspice_param"	"TD")
                )
                ("V1"
                    ("value"	"0")
                    ("pspice_param"	"V1")
                )
                ("V2"
                    ("value"	"5")
                    ("pspice_param"	"V2")
                )
                ("TR"
                    ("value"	"40u")
                    ("pspice_param"	"TR")
                )
                ("PW"
                    ("value"	"1")
                    ("pspice_param"	"PW")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
            )
        )
        ("C2"
            ("device_name"	"CESR_7")
            ("pspice_path"	"X_C2")
            ("level"	"0")
            ("model_params"
                ("C"
                    ("value"	"10u")
                    ("pspice_param"	"C")
                )
                ("ESR"
                    ("value"	"4.6m")
                    ("pspice_param"	"ESR")
                )
            )
        )
        ("L1"
            ("device_name"	"LDCR")
            ("pspice_path"	"X_L1")
            ("level"	"0")
            ("model_params"
                ("L"
                    ("value"	"33u")
                    ("pspice_param"	"L")
                )
                ("DCR"
                    ("value"	"80m")
                    ("pspice_param"	"DCR")
                )
                ("IC"
                    ("value"	"")
                    ("pspice_param"	"IC")
                )
            )
        )
        ("C1"
            ("device_name"	"CESR_7")
            ("pspice_path"	"X_C1")
            ("level"	"0")
            ("model_params"
                ("C"
                    ("value"	"20u")
                    ("pspice_param"	"C")
                )
                ("ESR"
                    ("value"	"2.3m")
                    ("pspice_param"	"ESR")
                )
            )
        )
        ("Iload"
            ("device_name"	"IPULSE")
            ("pspice_path"	"I_Iload")
            ("level"	"0")
            ("model_params"
                ("DC"
                    ("value"	"0Adc")
                    ("pspice_param"	"DC")
                )
                ("AC"
                    ("value"	"0Aac")
                    ("pspice_param"	"AC")
                )
                ("PW"
                    ("value"	"750u")
                    ("pspice_param"	"PW")
                )
                ("TR"
                    ("value"	"10u")
                    ("pspice_param"	"TR")
                )
                ("I2"
                    ("value"	"0.03")
                    ("pspice_param"	"I2")
                )
                ("I1"
                    ("value"	"0")
                    ("pspice_param"	"I1")
                )
                ("TD"
                    ("value"	"700u")
                    ("pspice_param"	"TD")
                )
                ("TF"
                    ("value"	"10u")
                    ("pspice_param"	"TF")
                )
                ("PER"
                    ("value"	"1500u")
                    ("pspice_param"	"PER")
                )
            )
        )
    )
)
