	Kernel Driver

	(Replace Linux native kernel driver with the newer version)
platform/broadcom/sonic-platform-modules-accton/stn-a2/modules/lm25066.c

	Create Device Instance

	echo lm5066i 0x58 > /sys/bus/i2c/devices/i2c-20/new_device
echo lm5066i 0x58 > /sys/bus/i2c/devices/i2c-21/new_device

	Path
	Access
	Description

	
	
	Value

	/sys/class/hwmon/hwmon[8-9]/

	
	curr1_average
	ro
	Average measured input current

	
	
	
	0h read_avg_iin

	
	curr1_input
	ro
	Measured input current

	
	
	
	0h mfr_read_iin

	
	curr1_label
	ro
	"iin"

	
	
	
	

	
	curr1_max
	r/w
	Maximum input current

	
	
	
	

	
	curr1_max_alarm
	r/w
	Input current high alarm

	
	
	
	Default: N/A

	
	in1_average
	ro
	Average measured input voltage

	
	
	
	0h read_avg_vin

	
	in1_input
	ro
	Measured input voltage

	
	
	
	0h read_vin

	
	in1_label
	ro
	"vin"

	
	
	
	10V to 80V

	
	in1_max
	r/w
	Maximum input voltage

	
	
	
	

	
	in1_max_alarm
	r/w
	Input voltage high alarm

	
	
	
	

	
	in1_min
	r/w
	Minimum input voltage

	
	
	
	

	
	in1_min_alarm
	r/w
	Input voltage low alarm

	
	
	
	

	
	in2_input
	ro
	Measured voltage on VAUX pin

	
	
	
	0h read_vaux

	
	in2_label
	ro
	"vmon"

	
	
	
	

	
	in3_average
	ro
	Average measured output voltage

	
	
	
	0h read_avg_vout

	
	in3_input
	ro
	Measured output voltage

	
	
	
	0h read_vout

	
	in3_label
	ro
	"vout1"

	
	
	
	10V to 80V

	
	in3_min
	r/w
	Minimum output voltage

	
	
	
	

	
	in3_min_alarm
	r/w
	Output voltage low alarm

	
	
	
	

	
	power1_alarm
	r/w
	Input power alarm

	
	
	
	Default: N/A

	
	power1_average
	ro
	Average measured input power

	
	
	
	0h read_avg_pin

	
	power1_input
	ro
	Measured input power

	
	
	
	0h read_pin

	
	power1_input_highest
	ro
	Historical maximum power

	
	
	
	0h read_pin_peak

	
	power1_label
	ro
	"pin"

	
	
	
	

	
	power1_max
	r/w
	Maximum input power limit

	
	
	
	

	
	power1_reset_history
	r/wo
	Write any value to reset maximum power history

	
	
	
	N/A

	
	temp1_crit
	r/w
	Critical high temperature

	
	
	
	

	
	temp1_crit_alarm
	r/w
	Chip temperature critical high alarm

	
	
	
	

	
	temp1_input
	ro
	Measured temperature

	
	
	
	-40o C to 125o C, 190h read_temperature_1

	
	temp1_max
	r/w
	Maximum temperature

	
	
	
	

	
	temp1_max_alarm
	r/w
	Chip temperature high alarm
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	root@sonic:/sys/bus/i2c/devices/20-0058# ls
driver  hwmon  modalias  name  power  subsystem  uevent
root@sonic:/sys/bus/i2c/devices/20-0058# cat name
lm5066i
root@sonic:/sys/bus/i2c/devices/20-0058# cd hwmon
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon# ls
hwmon8
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon# cd hwmon8
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# ls
curr1_average    in1_max        in3_min               power1_max
curr1_input      in1_max_alarm  in3_min_alarm         power1_reset_history
curr1_label      in1_min        name                  subsystem
curr1_max        in1_min_alarm  power                 temp1_crit
curr1_max_alarm  in2_input      power1_alarm          temp1_crit_alarm
device           in2_label      power1_average        temp1_input
in1_average      in3_average    power1_input          temp1_max
in1_input        in3_input      power1_input_highest  temp1_max_alarm
in1_label        in3_label      power1_label          uevent
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat curr1_average
464
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat curr1_input
497
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat curr1_label
iin
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat curr1_max
1724
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat curr1_max_alarm
0
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat in1_average
4232
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat in1_input
4232
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat in1_label
vin
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat in1_max
5553
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat in1_max_alarm
0
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat in1_min
30
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat in1_min_alarm
0
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat name
lm5066i
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat power1_alarm
0
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat power1_average
27042915
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat power1_input
27630805
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat power1_input_highest
57613168
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat power1_label
pin
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat power1_max
152263374
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat power1_reset_history
2351557
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat temp1_crit
15937
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat temp1_crit_alarm
0
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat temp1_input
9312
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat temp1_max
15937
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cat temp1_max_alarm
0
root@sonic:/sys/bus/i2c/devices/20-0058/hwmon/hwmon8# cd ../../../21-0058
root@sonic:/sys/bus/i2c/devices/21-0058# cat name
lm5066i
root@sonic:/sys/bus/i2c/devices/21-0058# cd hwmon
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon# ls
hwmon9
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon# cd hwmon9
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# ls
curr1_average    in1_max        in3_min               power1_max
curr1_input      in1_max_alarm  in3_min_alarm         power1_reset_history
curr1_label      in1_min        name                  subsystem
curr1_max        in1_min_alarm  power                 temp1_crit
curr1_max_alarm  in2_input      power1_alarm          temp1_crit_alarm
device           in2_label      power1_average        temp1_input
in1_average      in3_average    power1_input          temp1_max
in1_input        in3_input      power1_input_highest  temp1_max_alarm
in1_label        in3_label      power1_label          uevent
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat curr1_average
1306
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat curr1_input
1340
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat curr1_label
iin
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat curr1_max
1724
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat curr1_max_alarm
0
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat in1_average
4210
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat in1_input
4210
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat in1_label
vin
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat in1_max
5553
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat in1_max_alarm
0
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat in1_min
30
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat in1_min_alarm
0
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat in2_input
896
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat in2_label
vmon
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat in3_average
4106
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat in3_input
4106
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat in3_label
vout1
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat in3_min
-108
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat in3_min_alarm
0
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat name
lm5066i
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat power1_alarm
0
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat power1_average
71134626
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat power1_input
71134626
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat power1_input_highest
115814226
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat power1_label
pin
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat power1_max
152263374
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat power1_reset_history
2351557
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat temp1_crit
15937
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat temp1_crit_alarm
0
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat temp1_input
10625
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat temp1_max
15937
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cat temp1_max_alarm
0
root@sonic:/sys/bus/i2c/devices/21-0058/hwmon/hwmon9# cd /sys/bus/i2c/devices/
root@sonic:/sys/bus/i2c/devices# 
root@sonic:/sys/bus/i2c/devices# cd 19-0034
root@sonic:/sys/bus/i2c/devices/19-0034# ls
driver  hwmon  modalias  name  power  subsystem  uevent
root@sonic:/sys/bus/i2c/devices/19-0034# cat name
ucd90160a
root@sonic:/sys/bus/i2c/devices/19-0034# cd hwmon
root@sonic:/sys/bus/i2c/devices/19-0034/hwmon# ls
hwmon10
root@sonic:/sys/bus/i2c/devices/19-0034/hwmon# cd hwmon10
root@sonic:/sys/bus/i2c/devices/19-0034/hwmon/hwmon10# ls
device            in14_crit_alarm   in2_label        in6_lcrit_alarm
in10_crit         in14_input        in2_lcrit        in6_max
in10_crit_alarm   in14_label        in2_lcrit_alarm  in6_max_alarm
in10_input        in14_lcrit        in2_max          in6_min
in10_label        in14_lcrit_alarm  in2_max_alarm    in6_min_alarm
in10_lcrit        in14_max          in2_min          in7_crit
in10_lcrit_alarm  in14_max_alarm    in2_min_alarm    in7_crit_alarm
in10_max          in14_min          in3_crit         in7_input
in10_max_alarm    in14_min_alarm    in3_crit_alarm   in7_label
in10_min          in15_crit         in3_input        in7_lcrit
in10_min_alarm    in15_crit_alarm   in3_label        in7_lcrit_alarm
in11_crit         in15_input        in3_lcrit        in7_max
in11_crit_alarm   in15_label        in3_lcrit_alarm  in7_max_alarm
in11_input        in15_lcrit        in3_max          in7_min
in11_label        in15_lcrit_alarm  in3_max_alarm    in7_min_alarm
in11_lcrit        in15_max          in3_min          in8_crit
in11_lcrit_alarm  in15_max_alarm    in3_min_alarm    in8_crit_alarm
in11_max          in15_min          in4_crit         in8_input
in11_max_alarm    in15_min_alarm    in4_crit_alarm   in8_label
in11_min          in16_crit         in4_input        in8_lcrit
in11_min_alarm    in16_crit_alarm   in4_label        in8_lcrit_alarm
in12_crit         in16_input        in4_lcrit        in8_max
in12_crit_alarm   in16_label        in4_lcrit_alarm  in8_max_alarm
in12_input        in16_lcrit        in4_max          in8_min
in12_label        in16_lcrit_alarm  in4_max_alarm    in8_min_alarm
in12_lcrit        in16_max          in4_min          in9_crit
in12_lcrit_alarm  in16_max_alarm    in4_min_alarm    in9_crit_alarm
in12_max          in16_min          in5_crit         in9_input
in12_max_alarm    in16_min_alarm    in5_crit_alarm   in9_label
in12_min          in1_crit          in5_input        in9_lcrit
in12_min_alarm    in1_crit_alarm    in5_label        in9_lcrit_alarm
in13_crit         in1_input         in5_lcrit        in9_max
in13_crit_alarm   in1_label         in5_lcrit_alarm  in9_max_alarm
in13_input        in1_lcrit         in5_max          in9_min
in13_label        in1_lcrit_alarm   in5_max_alarm    in9_min_alarm
in13_lcrit        in1_max           in5_min          name
in13_lcrit_alarm  in1_max_alarm     in5_min_alarm    power
in13_max          in1_min           in6_crit         subsystem
in13_max_alarm    in1_min_alarm     in6_crit_alarm   temp1_alarm
in13_min          in2_crit          in6_input        temp1_input
in13_min_alarm    in2_crit_alarm    in6_label        uevent
in14_crit         in2_input         in6_lcrit
root@sonic:/sys/bus/i2c/devices/19-0034/hwmon/hwmon10# cat in4_max
5500
root@sonic:/sys/bus/i2c/devices/19-0034/hwmon/hwmon10#




