
**** 07/23/24 10:28:21 ***** PSpice 17.4.0 (23 July 2022) ***** ID# 0 ********

 ** Profile: "LM5157_EVM_STEADY-trans"  [ d:\snvmc64b\lm5157_pspice_trans\lm5157_trans-pspicefiles\lm5157_evm_steady\trans.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "trans.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "../../../lm5157_trans_evm.lib" 
.LIB "../../../lm5157_trans.lib" 
* From [PSPICE NETLIST] section of C:\Users\i0316\AppData\Roaming\SPB_Data\cdssetup\OrCAD_PSpice\17.4.0\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 300u 297u 20n 
.OPTIONS ADVCONV
.OPTIONS ITL1= 400
.OPTIONS ITL2= 50
.PROBE64 V(alias(*)) I(alias(*)) 
.INC "..\LM5157_EVM_STEADY.net" 



**** INCLUDING LM5157_EVM_STEADY.net ****
* source LM5157_TRANS
C_C3         BIAS 0  1000p  TC=0,0 
X_C12         VOUT 0 CESR PARAMS:  C=4.7u  ESR=2m X=1  IC={SS*12}
C_C10         BIAS 0  10u  TC=0,0 
C_C8         BIAS 0  10u  TC=0,0 
X_C2         BIAS 0 CESR PARAMS:  C=22u  ESR=5m X=1  IC={SS*10}
R_R17         FB 0  4.53k TC=0,0 
C_C22         BIAS 0  100n  TC=0,0 
X_C18         VOUT 0 CESR PARAMS:  C=100n  ESR=1m X=1  IC={SS*12}
R_R16         RT 0  9.53k TC=0,0 
R_R19         N16795152 0  2.61k TC=0,0 
C_C7         BIAS 0  10u  TC=0,0 
X_C13         VOUT 0 CESR PARAMS:  C=4.7u  ESR=2m X=1  IC={SS*12}
R_R14         N16794793 FB  49.9k TC=0,0 
C_C6         BIAS 0  10u  TC=0,0 
C_C9         BIAS 0  10u  TC=0,0 
R_RLOAD         VOUT 0  {12/1.6} TC=0,0 
X_C16         VOUT 0 CESR PARAMS:  C=4.7u  ESR=2m X=1  IC={SS*12}
X_C15         VOUT 0 CESR PARAMS:  C=4.7u  ESR=2m X=1  IC={SS*12}
R_R5         VCC PGOOD  100k TC=0,0 
R_R12         N16794793 VOUT  10 TC=0,0 
C_C25         COMP N16795152  10n  TC=0,0 
R_R9         UVLO BIAS  61.9k TC=0,0 
X_C11         VOUT 0 CESR PARAMS:  C=4.7u  ESR=2m X=1  IC={SS*12}
X_C14         VOUT 0 CESR PARAMS:  C=4.7u  ESR=2m X=1  IC={SS*12}
X_U1         0 BIAS COMP UVLO 0 FB 0 N24942 0 0 PGOOD RT SS SW SW SW N16780257
+  LM5157_TRANS PARAMS: FAST_HICCUP={FAST_HICCUP} SS={SS} LM51571={LM51571}
X_L2         BIAS SW LDCR PARAMS: L=1.5u DCR=0.01
C_C5         BIAS 0  0.01u  TC=0,0 
C_C4         BIAS 0  0.1u  TC=0,0 
C_C24         SS 0  22n IC={SS*1} TC=0,0 
C_C26         COMP 0  100p  TC=0,0 
X_C17         VOUT 0 CESR PARAMS:  C=100n  ESR=1m X=1  IC={SS*12}
R_R15         0 UVLO  71.5k TC=0,0 
V_VIN         BIAS 0 6
C_C21         VCC 0  1u IC={SS*5} TC=0,0 
R_R20         N16780257 VCC  5 TC=0,0 
D_D1         SW VOUT D_D1 
.PARAM  ss=1 lm51571=0 fast_hiccup=1

**** RESUMING trans.cir ****
.END

ERROR(ORPSIM-16587): Cannot simulate circuit because there are more than 250 devices, which exceeds the limit for PSpice A/D Basics. To simulate this circuit, upgrade to a higher license.


ABORTING SIMULATION
**** 07/23/24 10:28:21 ***** PSpice 17.4.0 (23 July 2022) ***** ID# 0 ********

 ** Profile: "LM5157_EVM_STEADY-trans"  [ d:\snvmc64b\lm5157_pspice_trans\lm5157_trans-pspicefiles\lm5157_evm_steady\trans.sim ] 


 ****     JOB STATISTICS SUMMARY


******************************************************************************



Node counts:
  Top level (NUNODS)                =          14
  External (NCNODS)                 =         366
  Total (NUMNOD)                    =         385

Total device count (NUMEL)          =          25
  Capacitors (C)                    =          13
  Diodes (D)                        =           1
  VCVS (E)                          =           0
  CCCS (F)                          =           0
  VCCS (G)                          =           0
  CCVS (H)                          =           0
  Current Sources (I)               =           0
  Inductors (L)                     =           0
  Resistors (R)                     =          10
  VSwitches (S)                     =           0
  Voltage Sources (V)               =           1

Number of subcircuits (X)           =          11

Matrix statistics:
  Matrix size (NSTOP)               =         589
  Initial no. elements (NTTAR)      =        1463
  No. elements w/ fillin (NTTBR)    =        1463
  No. fillins (IFILL)               =           0
  No. overflows (NTTOV)             =           0
  No. LU operations (IOPS)          =           0
  Percent sparsity (PERSPA)         =      99.578

Analysis statistics:
  No. total time points (NUMTTP)    =           0
  No. rejected time points (NUMRTP) =           0
  No. iterations (NUMNIT)           =           0

Load Threads                        =           1

Runtime statistics:                       Seconds      Iterations
  Matrix load                       =        0.00
  Matrix solution                   =        0.00               1
  Readin                            =         .03
  General setup                     =        0.00
  CMI setup                     =        0.00
  Setup                             =        0.00
  DC sweep                          =        0.00               0
  Bias point                        =        0.00               0
  AC and noise                      =        0.00               0
  Total transient analysis          =        0.00
  Output                            =        0.00
  Overhead                          =         .14
  Total job time (using Solver 1)   =         .22
