
**** 08/01/24 00:26:01 **** PSpice 23.1.0 (30 January 2024) *** ID# 0 ********

 ** Profile: "Flyback-tran"  [ C:\Users\a0489390\Downloads\LM5157_PSPICE_TRANS\lm5157_trans-pspicefiles\flyback\tran.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "tran.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "../../../lm5157_trans_evm.lib" 
.LIB "../../../lm5157_trans.lib" 
* From [PSPICE NETLIST] section of C:\cds_spb_home\cdssetup\OrCAD_PSpiceTIPSpice_Install\23.1.0\PSpice.ini file:
.lib "nom_pspti.lib" 
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 20ms 0 20n 
.OPTIONS ADVCONV
.OPTIONS FILEMODELSEARCH
.OPTIONS ABSTOL= 1.0n
.OPTIONS GMIN= 1p
.OPTIONS ITL1= 1000
.OPTIONS ITL2= 100
.OPTIONS ITL4= 100
.PROBE64 V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\Flyback.net" 



**** INCLUDING Flyback.net ****
* source LM5157_TRANS
R_R16         RT 0  109.5k TC=0,0 
R_R19         N05413 0  31k TC=0,0 
R_R17         FB 0  2.27k TC=0,0 
R_R9         UVLO BIAS  166.67k TC=0,0 
C_C8         BIAS 0  100n  TC=0,0 
D_D3         N04107 N04389 D_D1 
C_C6         BIAS 0  22u  TC=0,0 
C_C24         SS 0  80n IC={0*1} TC=0,0 
Kn_K1         L_L1 L_L2 
+ L_L3 L_L4 
+ L_L5  0.995
C_C4         BIAS 0  22u  TC=0,0 
V_VIN         BIAS 0  
+PULSE 0 12 0 100us 100u 1 2
X_C14         VOUT1 0 CESR PARAMS:  C=10u  ESR=26.45m X=1  IC=0
X_C15         VOUT1 0 CESR PARAMS:  C=1u  ESR=26.45m X=1  IC={0}
X_C16         VOUT1 0 CESR PARAMS:  C=1u  ESR=26.45m X=1  IC={0*12}
X_C17         VOUT1 0 CESR PARAMS:  C=100n  ESR=1m X=1  IC={0*12}
L_L1         N04113 BIAS  30u  
L_L2         N12648 0  90u  
X_U1         0 BIAS COMP UVLO 0 FB MODE N04813 0 0 PGOOD RT SS N04107 N04107
+  N04107 VCC LM5157_TRANS PARAMS: FAST_HICCUP={FAST_HICCUP} SS={SS} LM51571=
+ {LM51571}
R_R23         N04113 N04107  1m TC=0,0 
R_R14         VOUT1 FB  49.9k TC=0,0 
R_R5         VCC PGOOD  49.9k TC=0,0 
R_R15         0 UVLO  71.43k TC=0,0 
C_C22         BIAS 0  100n  TC=0,0 
C_C27         0 VCC  1u  TC=0,0 
C_C25         COMP N05413  23n  TC=0,0 
D_D4         N12652 VOUT1 D_D1 
R_R33         N12652 N12648  1m TC=0,0 
C_C11         0 VOUT2  1u  TC=0,0 
D_D1         VSEC2 VOUT2 D_D1 
R_R24         VSEC2 N13065  1m TC=0,0 
L_L3         N13065 0  90u  
C_C10         0 VOUT2  36u  TC=0,0 
C_C13         0 VOUT2  100n  TC=0,0 
C_C12         0 VOUT2  1u  TC=0,0 
C_C38         0 VOUT3  20u  TC=0,0 
D_D5         VSEC3 VOUT3 D_D1 
C_C41         0 VOUT3  100n  TC=0,0 
L_L4         N15115 0  90u  
C_C39         0 VOUT3  1u  TC=0,0 
C_C40         0 VOUT3  1u  TC=0,0 
R_R34         VSEC3 N15115  1m TC=0,0 
D_D6         VSEC4 VOUT4 D_D1 
R_R35         VSEC4 N16046  1m TC=0,0 
L_L5         N16046 0  90u  
C_C42         0 VOUT4  20u  TC=0,0 
C_C45         0 VOUT4  100n  TC=0,0 
C_C43         0 VOUT4  1u  TC=0,0 
C_C44         0 VOUT4  1u  TC=0,0 
R_Rload2         0 VOUT3  {23/0.075} TC=0,0 
R_Rload1         0 VOUT2  {23/0.15} TC=0,0 
R_Rload3         0 VOUT4  {23/0.075} TC=0,0 
R_RLOAD         VOUT1 0  23/0.1 TC=0,0 
R_R36         MODE 0  100k TC=0,0 
C_C46         FB 0  0n IC={0} TC=0,0 
--------------------$
ERROR(ORPSIM-16144): Value may not be 0
C_C47         COMP 0  313p  TC=0,0 
D_D9         BIAS N04389 PLVA650A/PLP 
Q_Q1         0 SS COMP BD202
.IC         V(VOUT2 )=0
.IC         V(VOUT3 )=0
.IC         V(VOUT4 )=0
.PARAM  ss=1 lm51571=0 fast_hiccup=1

**** RESUMING tran.cir ****
.END
