Mode pin to ground

