1. **Before add waiting instruction between ‘set\_pwm 0 ’ and ‘set\_pwm 255’**



**Engine 1 begin**

**Engine 2 begin**

t=0.08s T\_delay= 311.899ms



t=0.12s T\_delay=309.611ms



t=0.24s T\_delay=309.611ms

1. After add waiting instruction（wait 360ms） between ‘set\_pwm 0 ’ and ‘set\_pwm 255’



t=0.08s normal

1. **Reference program code**

