`

Input(1.2A)

LP8868-X

BOOST TOPOLOGY

Vf LED=3.2V

7LB LED

5 HB LED

GND