



Note: R20 & R21 were hand soldered externally. Tested 2.0V.


Top layer.



Layer 2 (GND)



Layer 3 (PWR)



Layer 4

