- Preliminary Steps
  - Compliance Suite Settings
    - Save Mode: Save all
    - Capture Raw File: Disabled
    - Capture Power Measurement: Disabled
    - VBus and CC Self-Test: Disabled
    - CC Voltage Calibration: Disabled
  - Analyzing Vendor Information File (VIF)...
  - Making debounce values intermediate file...
  - Teledyne LeCroy USB Compliance Suite Version: 7.82 Build 1187
  - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\Variables.ginc ...
  - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\Variables.inc ...
  - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\VendorInformation.inc ...
  - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\VendorInformationExtra.inc ...
  - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\VendorInformation.ginc ...
  - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\VendorInformationExtra.ginc ...
  - CVS_Manager_Class was created
  - CVS_Manager_Class::Initialize::Number of connected boards: 1
  - Argument(1)=26648
  - Argument(2)=0
  - Board_Class was created
  - Board_Class::ReadBoardInfo() for serial number #26648
  - Creating Automation Object ...
  - Binding Voyager #0 with Serial #26648
  - Board_Class::OpenConnection() [CVS_0]
  - Board Name=Voyager M310e
  - BoardID=161
  - BoardRev=9
  - Serial=#26648
  - CVS_Manager_Class::Release()::Number of connected boards: 1
  - Board_Class::CloseConnection()::AutomationObj.SetAnalyzerParameters(1,0)
  - Board_Class::CloseConnection() Successfully for CVS_0 to #26648
  - Board_Class was destroyed
  - CVS_Manager_Class was destroyed
  - Determine Cable type : Voyager serial number #26648 pass
    - Teledyne LeCroy USB Compliance Suite Version: 7.82 Build 1187
    - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\Variables.ginc ...
    - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\Variables.inc ...
    - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\VendorInformation.inc ...
    - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\VendorInformationExtra.inc ...
    - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\VendorInformation.ginc ...
    - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\VendorInformationExtra.ginc ...
    - VIF initiated successfully!
    - CVS_Manager_Class was created
    - CVS_Manager_Class::Initialize::Number of connected boards: 1
    - Argument(1)=26648
    - Argument(2)=0
    - Board_Class was created
    - Board_Class::ReadBoardInfo() for serial number #26648
    - Creating Automation Object ...
    - Binding Voyager #0 with Serial #26648
    - Board_Class::OpenConnection() [CVS_0]
    - Board Name=Voyager M310e
    - BoardID=161
    - BoardRev=9
    - Serial=#26648
    - VIF Extraction
      - Extracting from component "1" of file "C:\Users\Administrator\Desktop\Vendor_Info_File_v3.32VIF 1-20897_20250318.xml" ...
      - VIF_Product_Type = 0
      - PD_Port_Type = 0
      - Connector_Type = 2
      - USB_PD_Support = YES
      - Type_C_State_Machine = 1
      - Captive_Cable = NO
      - Captive_Cable_Is_eMarked = 0xFF *
      - USB4_Supported = NO
      - Type_C_Can_Act_As_Device = NO
      - Type_C_Is_Alt_Mode_Adapter = NO
      - Device_Supports_USB_Data = 0xFF *
      - Device_Speed = 0XFF *
      - Device_Max_USB2_Speed = 0XFF *
      - USB4_Max_Speed = 0XFF *
      - Type_C_Can_Act_As_Host = NO
      - Host_Supports_USB_Data = 0XFF *
      - Host_Speed = 0XFF *
      - Type_C_Port_On_Hub = NO
      - Type_C_Supports_Audio_Accessory = NO
      - Type_C_Supports_Vconn_Powered_Accessory = 0XFF *
      - Type_C_Is_Debug_Target_SRC = 0XFF *
      - Type_C_Is_Debug_Target_SNK = NO
      - Type_C_Implements_Try_SRC = 0XFF *
      - Type_C_Implements_Try_SNK = 0XFF *
      - Host_Is_Embedded = 0XFF *
    - Successfully finished VIF Extraction.
    - UpdateVariableInFile::3
    - Update AnalyzerID in file VendorInformation.ginc to 18
    - UpdateVariableInFile::3
    - Update AnalyzerID in file VendorInformation.inc to 18
    - UpdateVariableInFile::17
    - Update BOARD_REV in file VendorInformation.ginc to 9
    - UpdateVariableInFile::17
    - Update BOARD_REV in file VendorInformation.inc to 9
    - The test conditions are met and test is applicable to run.
    - Test_Class::RunCableDetection() for CVS_0
    - Running "Cable Detection" module to check the connected Cable and PUT...
    - RunModule_Class::Create_CaptureTask(0,C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Common\TC_CableDetection.rec,C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Common\TC_CableDetection.updg,,E:\M310e workspace\MITEK-CORPORATION-0-MITEK-CORPORATION-0-0\20250409_135956\USB Power Delivery\PreliminaryTC_CableDetection_cvs0.usb)
    - RunModule_Class::ConfigModule(0,14,8000)
    - RunModule_Class::ConfigModule::GENERATION_WAIT_TIME -> 8000
    - RunModule_Class::ConfigModule(0,16,True)
    - RunModule_Class::ConfigModule::GENERATION_FAIL_IGNORANCE -> True
    - RunModule_Class::ConfigModule(0,12,GetCableDetectionVseValues)
    - RunModule_Class::ConfigModule::EXTRACT_VERIFIED_RESULTS -> GetCableDetectionVseValues
    - RunModule_Class::Run_Single(0)
    - Capture_Class::Run() on CVS_0
    - Board_Class::SetSyncGUID [{6D3087F7-39C8-45AF-B3EA-E7C444823ABC}]
    - Board_Class::SetAnalyzerParameters (1, 3)
    - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Common\TC_CableDetection.rec: Starting Recording
    - RecordingOptions::ApplySettings()
    - RecordingOptions::ApplyTraceSettings()::[TC_CableDetection_cvs0.usb]
    - RecordingOptions::ApplySettings()::SetTraceFileName ->E:\M310e workspace\MITEK-CORPORATION-0-MITEK-CORPORATION-0-0\20250409_135956\USB Power Delivery\Preliminary\01_TC_CableDetection_cvs0.usb
    - RecordingOptions::ApplyGeneralSettings()
    - RecordingOptions::ApplyCapturePowerMeasurement()
    - RecordingOptions::ApplyRecordingBufferSize()
    - RecordingOptions::ApplyExtTriggerInRecOption()
    - RecordingOptions::ApplyExtTriggerOutRecOption():: No change was applied!
    - RecordingOptions::ApplyExerciserConnectedName()::[MITEK-CORPORATION-0-MITEK-CORPORATION-0-0][]
    - RecordingOptions::ApplyCaptureRawFile()
    - RecordingOptions::ApplyTypeCSettings()
    - RecordingOptions::ApplyCaptureCC_Traffic()
    - RecordingOptions::ApplyTypeCRoleSides()
    - RecordingOptions::ApplyUncertainSettingsTypeC()
    - Board_Class::StartRecording()
    - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Common\TC_CableDetection.updg: Starting PD Generation
    - Waiting... [maximum 8000 ms]
    - Board_Class::WaitForPDGenerationIdle() for CVS_0 : Serial#26648 wait_time_msec=8000
    - Stopping PD Generation
    - Waiting for Trigger...
    - Analyzer Trigged... 3764 ms
    - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Common\TC_CableDetection.rec: Stopping Recording at 3876 ms
    - Board_Class::StopRecordingAndWaitForTrace()
    - Board_Class::SetSyncGUID []
    - Trace is ready... 6328 ms
    - Check_Class::Verify() on Trace from CVS_0
    - Check_Class::Verify()::ErrorCode from relevant CVS = 0:
    - Check_Class::Verify()::Executing AlwaysApplicable
    - UpdateVariableInFile::3
    - Update CVS_ID in file CVS_Parameters.inc to 18
    - UpdateVariableInFile::2
    - Update ERROR_ON_READING_CURRENT in file CVS_Parameters.inc to 20000
    - Making a copy from Intermediate folder to E:\M310e workspace\MITEK-CORPORATION-0-MITEK-CORPORATION-0-0\20250409_135956\USB Power Delivery\Preliminary\Debug\0
    - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Common\TC_CableDetection.vse: Running Verification Script
    - Running Verification script : TC_CableDetection.vse
    - Running GetCableDetectionVseValues
    - CableDetection::Extracetd from VSE : PUT_Connected = YES
    - CableDetection::Extracetd from VSE : ConnectedCableType = VConn Pass-Thru
    - CableDetection::Extracetd from VSE : CableDirection = NORMAL
    - Verification Result: PASSED
    - Capture_Class::UpdateTraceFileName(1)
    - E:\M310e workspace\MITEK-CORPORATION-0-MITEK-CORPORATION-0-0\20250409_135956\USB Power Delivery\Preliminary\01_TC_CableDetection_cvs0.usb: Saving trace file
    - Trace captured.
    - CableDetection_Class::Run_CableDetection::Result of Run_Single(0) = 1
    - UpdateVariableInFile::3
    - Update DETECTED_CABLE_TYPE in file CableVariables.ginc to 2
    - UpdateVariableInFile::3
    - Update DETECTED_CABLE_TYPE in file CableVariables.inc to 2
    - UpdateVariableInFile::8
    - Update PUT_CONNECTED in file CableVariables.ginc to YES
    - UpdateVariableInFile::8
    - Update PUT_CONNECTED in file CableVariables.inc to YES
    - UpdateVariableInFile::8
    - Update CABLE_DIRECTION in file CableVariables.ginc to NORMAL
    - UpdateVariableInFile::8
    - Update CABLE_DIRECTION in file CableVariables.inc to NORMAL
    - Test_Class::Run_CableOrientation() for CVS_0
    - Test_Class::Run_CableOrientation()::Set default CC line to CC_LINE_1 and Result to PASS because we cannot run the orientation according to the VIF
    - CableDetection_Class::SaveOrientationResults()
    - UpdateVariableInFile::2
    - Update bMaxPacketSize in file CableVariables.ginc to 64
    - UpdateVariableInFile::2
    - Update BOS_Length in file CableVariables.ginc to 64
    - UpdateVariableInFile::2
    - Update IS_USB2_STARTED in file CableVariables.ginc to 0
    - UpdateVariableInFile::8
    - Update DEFAULT_CC_LINE in file CableVariables.ginc to CC_LINE_1
    - UpdateVariableInFile::8
    - Update DEFAULT_CC_LINE in file CableVariables.inc to CC_LINE_1
    - TC_CableDetection : Finished
      - CVS_Manager_Class::Release()::Number of connected boards: 1
      - Board_Class::CloseConnection()::AutomationObj.SetAnalyzerParameters(1,0)
      - Board_Class::CloseConnection() Successfully for CVS_0 to #26648
      - Board_Class was destroyed
      - CVS_Manager_Class was destroyed
- TEST.PD.PROT.SNK.09 Atomic Message Sequence - PS_RDY FAIL
  - Teledyne LeCroy USB Compliance Suite Version: 7.82 Build 1187
  - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\Variables.ginc ...
  - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\Variables.inc ...
  - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\VendorInformation.inc ...
  - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\VendorInformationExtra.inc ...
  - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\VendorInformation.ginc ...
  - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Intermediate\VendorInformationExtra.ginc ...
  - VIF initiated successfully!
  - CVS_Manager_Class was created
  - CVS_Manager_Class::Initialize::Number of connected boards: 1
  - Argument(1)=26648
  - Argument(2)=0
  - Board_Class was created
  - Board_Class::ReadBoardInfo() for serial number #26648
  - Creating Automation Object ...
  - Binding Voyager #0 with Serial #26648
  - Board_Class::OpenConnection() [CVS_0]
  - Board Name=Voyager M310e
  - BoardID=161
  - BoardRev=9
  - Serial=#26648
  - VIF Extraction
    - Extracting from component "1" of file "C:\Users\Administrator\Desktop\Vendor_Info_File_v3.32VIF 1-20897_20250318.xml" ...
    - UpdateVariableInFile::2
    - Update Snk_PPS_Counter in file Variables.ginc to 0
    - UpdateVariableInFile::2
    - Update Snk_PPS_Counter in file Variables.inc to 0
    - UpdateVariableInFile::2
    - Update Snk_EPR_Counter in file Variables.ginc to 0
    - UpdateVariableInFile::2
    - Update Snk_EPR_Counter in file Variables.inc to 0
    - UpdateVariableInFile::2
    - Update Snk_Null_PDOs in file Variables.ginc to 0
    - UpdateVariableInFile::2
    - Update Snk_Null_PDOs in file Variables.inc to 0
    - VIF_Product_Type = 0
    - PD_Port_Type = 0
    - Connector_Type = 2
    - USB_PD_Support = YES
    - Captive_Cable = NO
    - Captive_Cable_Is_eMarked = 0xFF *
    - PD_Specification_Revision = 2
    - Accepts_PR_Swap_As_Src = 0XFF *
    - USB_Suspend_May_Be_Cleared = 0XFF *
    - Unconstrained_Power = NO
    - USB_Comms_Capable = NO
    - DR_Swap_To_UFP_Supported = NO
    - Port_Source_Power_Type = 0XFF *
    - Num_Src_PDOs = 0XFF *
    - PD_Power_As_Source = 0XFF *
    - Accepts_PR_Swap_As_Snk = 0XFF *
    - Requests_PR_Swap_As_Src = 0XFF *
    - Requests_PR_Swap_As_Snk = 0XFF *
    - DR_Swap_To_DFP_Supported = NO
    - Unchunked_Extended_Messages_Supported = YES
    - Num_Snk_PDOs = 3
    - PD_Power_As_Sink = 45000
    - No_USB_Suspend_May_Be_Set = YES
    - Higher_Capability_Set = YES
    - Num_Swappable_Battery_Slots = 0
    - Num_Fixed_Batteries = 1
    - VCONN_Swap_To_On_Supported = NO
    - VCONN_Swap_To_Off_Supported = NO
    - Attempts_Discov_SOP = NO
    - Modal_Operation_Supported_SOP = NO
    - FR_Swap_Reqd_Type_C_Current_As_Initial_Source = 0
    - Master_Port = 0XFF *
    - Has_Invariant_PDOs = 0XFF *
    - SOP_P_Capable = NO
    - EPR_Supported_As_Src = 0XFF *
    - EPR_Supported_As_Snk = NO
    - PD_Spec_Revision_Major = 3
    - PD_Spec_Revision_Minor = 1
    - PD_Spec_Version_Major = 1
    - PD_Spec_Version_Minor = 8
    - Type_C_State_Machine = 1
    - Type_C_Supports_Audio_Accessory = NO
    - Type_C_Supports_Vconn_Powered_Accessory = 0XFF *
    - Type_C_Is_Debug_Target_SRC = 0XFF *
    - Type_C_Is_Debug_Target_SNK = NO
    - Type_C_Implements_Try_SRC = 0XFF *
    - Type_C_Implements_Try_SNK = 0XFF *
    - Host_Is_Embedded = 0XFF *
    - Snk_PDO_Supply_Type1 = 0
    - Snk_PDO_Voltage1 = 100
    - Snk_PDO_Op_Current1 = 300
    - Snk_PDO_Supply_Type2 = 0
    - Snk_PDO_Voltage2 = 180
    - Snk_PDO_Op_Current2 = 300
    - Snk_PDO_Supply_Type3 = 0
    - Snk_PDO_Voltage3 = 300
    - Snk_PDO_Op_Current3 = 300
  - Successfully finished VIF Extraction.
  - UpdateVariableInFile::3
  - Update AnalyzerID in file VendorInformation.ginc to 18
  - UpdateVariableInFile::3
  - Update AnalyzerID in file VendorInformation.inc to 18
  - UpdateVariableInFile::17
  - Update BOARD_REV in file VendorInformation.ginc to 9
  - UpdateVariableInFile::17
  - Update BOARD_REV in file VendorInformation.inc to 9
  - The test conditions are met and test is applicable to run.
  - Test_Class::IsCableMatched(VConn Pass-Thru)
  - PUT_CONNECTED = YES
  - DETECTED_CABLE_TYPE = VConn Pass-Thru
  - CABLE_DIRECTION = NORMAL
  - IS_USB2_STARTED = 0
  - Cable is matched.
  - Successfully detected device role (0x2) according to the provided VIF.
  - Test_Class::CheckTheCable()::UserFunctions(1): PD_CapabilityFunctionGenerator()
  - Test_Class::IsReadyToRun()::result = 1
  - AddCondition:MaxConditionCounter = 1
  - AddCondition:MaxConditionCounter = 2
  - Test_Class::ConnectToBoards()
  - Board_Class::OpenConnection() --> Already opened!
  - Test Preliminary procedures has started.
  - Calibrating VBUS current on Voyager (0) #26648 ...
  - Test Preliminary procedures has done.
  - Rev2Snk fail
    - Power Delivery Link initialization on Voyager #26648 : Running Generation
    - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Common\InitPDLink.updg: Starting PD Generation
    - Waiting... [maximum 8000 ms]
    - Board_Class::WaitForPDGenerationIdle() for CVS_0 : Serial#26648 wait_time_msec=8000
    - Stopping PD Generation
    - UpdateVariableInFile::8
    - Update ConditionID in file Variables.inc to "Rev2Snk"
    - UpdateVariableInFile::2
    - Update ConditionNumber in file Variables.ginc to 0
    - UpdateVariableInFile::2
    - Update TestPdRevision in file Variables.inc to 1
    - UpdateVariableInFile::8
    - Update SPEC_REV in file VendorInformation.ginc to PD_SPEC_REVISION_2
    - UpdateVariableInFile::2
    - Update Tester_RolePort in file VendorInformationExtra.inc to 2
    - UpdateVariableInFile::2
    - Update Tester_RolePort in file VendorInformationExtra.ginc to 2
    - UpdateVariableInFile::2
    - Update UUT_RolePort in file VendorInformationExtra.inc to 0
    - UpdateVariableInFile::2
    - Update UUT_RolePort in file VendorInformationExtra.ginc to 0
    - UpdateVariableInFile::2
    - Update SwapRequired in file Variables.inc to 0
    - UpdateVariableInFile::2
    - Update SwapRequired in file Variables.ginc to 0
    - UpdateVariableInFile::2
    - Update CaptiveCableBringUP in file Variables.inc to 0
    - UpdateVariableInFile::2
    - Update CaptiveCableBringUP in file Variables.ginc to 0
    - Running AtStart_func: CheckVconnApplicability(this)
    - Running CheckToEndCondition_func: Do_Return_False_with_One_param of Item #0
    - Capture_Class::Run() on CVS_0
    - Board_Class::SetSyncGUID [{9C691D69-FFE1-43AE-9A33-E5D33D3FE8D2}]
    - Board_Class::SetAnalyzerParameters (1, 0)
    - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\REC\USB Power Delivery - USBIF\Protocol Specific Tests\TEST.PD.PROT.SNK.9.rec: Starting Recording
    - RecordingOptions::ApplySettings()
    - RecordingOptions::ApplyTraceSettings()::[TEST.PD.PROT.SNK.9_Rev2Snk.usb]
    - RecordingOptions::ApplySettings()::SetTraceFileName ->E:\M310e workspace\MITEK-CORPORATION-0-MITEK-CORPORATION-0-0\20250409_135956\USB Power Delivery\TEST.PD.PROT.SNK.9\01_TEST.PD.PROT.SNK.9_Rev2Snk.usb
    - RecordingOptions::ApplyGeneralSettings()
    - RecordingOptions::ApplyCapturePowerMeasurement()
    - RecordingOptions::ApplyRecordingBufferSize()
    - RecordingOptions::ApplyExtTriggerInRecOption()
    - RecordingOptions::ApplyExtTriggerOutRecOption():: No change was applied!
    - RecordingOptions::ApplyExerciserConnectedName()::[MITEK-CORPORATION-0-MITEK-CORPORATION-0-0][]
    - RecordingOptions::ApplyCaptureRawFile()
    - RecordingOptions::ApplyTypeCSettings()
    - RecordingOptions::ApplyCaptureCC_Traffic()
    - RecordingOptions::ApplyTypeCRoleSides()
    - ApplyTypeCRoleSides()::RO_SETTING_TC_EXERCISER_ROLE = 4
    - ApplyTypeCRoleSides()::RO_SETTING_TC_DEVICE_ROLE = 2
    - RecordingOptions::ApplyUncertainSettingsTypeC()
    - Board_Class::StartRecording()
    - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\GEN\USB Power Delivery - USBIF\Protocol Specific Tests\TEST.PD.PROT.SNK.9.UPDg: Starting PD Generation
    - Waiting... [maximum 15000 ms]
    - Board_Class::WaitForPDGenerationIdle() for CVS_0 : Serial#26648 wait_time_msec=15000
    - Stopping PD Generation
    - Waiting for Trigger...
    - Analyzer Trigged... 11732 ms
    - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\REC\USB Power Delivery - USBIF\Protocol Specific Tests\TEST.PD.PROT.SNK.9.rec: Stopping Recording at 11844 ms
    - Board_Class::StopRecordingAndWaitForTrace()
    - Board_Class::SetSyncGUID []
    - Trace is ready... 14396 ms
    - Running CheckToEndCondition_func: Do_Return_False_with_One_param of Item #1
    - COMMON.PROC.BU.2#1 pass
      - Saving COMMON.PROC.BU.2#1 in the file Variables.inc
      - UpdateVariableInFile::8
      - Update VerificationID in file Variables.inc to "COMMON.PROC.BU.2#1"
      - Saving VID_List array in the file Variables.inc
      - UpdateVariableInFile::8204
      - Update VID_List in file Variables.inc to maximum 0 elements
      - Relevant CVS found on item 0
      - Check_Class::Verify() on Trace from CVS_0
      - Check_Class::Verify()::ErrorCode from relevant CVS = 0:
      - Check_Class::Verify()::Check if any Bring-up has failed.
      - Check_Class::Verify()::Executing AlwaysApplicable
      - UpdateVariableInFile::3
      - Update CVS_ID in file CVS_Parameters.inc to 18
      - UpdateVariableInFile::2
      - Update ERROR_ON_READING_CURRENT in file CVS_Parameters.inc to 20000
      - Making a copy from Intermediate folder to E:\M310e workspace\MITEK-CORPORATION-0-MITEK-CORPORATION-0-0\20250409_135956\USB Power Delivery\TEST.PD.PROT.SNK.9\Debug\1_c1v1
      - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\VSE\USB Power Delivery - USBIF\Protocol Specific Tests\TEST.PD.PROT.SNK.9.vse: Running Verification Script
      - Running Verification script : TEST.PD.PROT.SNK.9.vse
      - Running Do_Nothing_Sub_with_One_param
      - Verification Result: PASSED
      - Running CheckToEndCondition_func: Do_Return_False_with_One_param of Item #2
    - TEST.PD.PROT.SNK.9#1 pass
      - Saving TEST.PD.PROT.SNK.9#1 in the file Variables.inc
      - UpdateVariableInFile::8
      - Update VerificationID in file Variables.inc to "TEST.PD.PROT.SNK.9#1"
      - Saving VID_List array in the file Variables.inc
      - UpdateVariableInFile::8204
      - Update VID_List in file Variables.inc to maximum 0 elements
      - Relevant CVS found on item 0
      - Check_Class::Verify() on Trace from CVS_0
      - Check_Class::Verify()::ErrorCode from relevant CVS = 0:
      - Check_Class::Verify()::Check if any Bring-up has failed.
      - Check_Class::Verify()::Executing AlwaysApplicable
      - UpdateVariableInFile::3
      - Update CVS_ID in file CVS_Parameters.inc to 18
      - UpdateVariableInFile::2
      - Update ERROR_ON_READING_CURRENT in file CVS_Parameters.inc to 20000
      - Making a copy from Intermediate folder to E:\M310e workspace\MITEK-CORPORATION-0-MITEK-CORPORATION-0-0\20250409_135956\USB Power Delivery\TEST.PD.PROT.SNK.9\Debug\1_c1v2
      - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\VSE\USB Power Delivery - USBIF\Protocol Specific Tests\TEST.PD.PROT.SNK.9.vse: Running Verification Script
      - Running Verification script : TEST.PD.PROT.SNK.9.vse
      - Running Do_Nothing_Sub_with_One_param
      - Verification Result: PASSED
      - Running CheckToEndCondition_func: Do_Return_False_with_One_param of Item #3
    - TEST.PD.PROT.SNK.9#2 fail
      - Saving TEST.PD.PROT.SNK.9#2 in the file Variables.inc
      - UpdateVariableInFile::8
      - Update VerificationID in file Variables.inc to "TEST.PD.PROT.SNK.9#2"
      - Saving VID_List array in the file Variables.inc
      - UpdateVariableInFile::8204
      - Update VID_List in file Variables.inc to maximum 0 elements
      - Relevant CVS found on item 0
      - Check_Class::Verify() on Trace from CVS_0
      - Check_Class::Verify()::ErrorCode from relevant CVS = 0:
      - Check_Class::Verify()::Check if any Bring-up has failed.
      - Check_Class::Verify()::Executing AlwaysApplicable
      - UpdateVariableInFile::3
      - Update CVS_ID in file CVS_Parameters.inc to 18
      - UpdateVariableInFile::2
      - Update ERROR_ON_READING_CURRENT in file CVS_Parameters.inc to 20000
      - Making a copy from Intermediate folder to E:\M310e workspace\MITEK-CORPORATION-0-MITEK-CORPORATION-0-0\20250409_135956\USB Power Delivery\TEST.PD.PROT.SNK.9\Debug\1_c1v3
      - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\VSE\USB Power Delivery - USBIF\Protocol Specific Tests\TEST.PD.PROT.SNK.9.vse: Running Verification Script
      - Running Verification script : TEST.PD.PROT.SNK.9.vse
      - Running Do_Nothing_Sub_with_One_param
      - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\VSE\USB Power Delivery - USBIF\Protocol Specific Tests\TEST.PD.PROT.SNK.9.vse.Txt ...
      - Error(0x00000273): The UUT did not send a Hard Reset.
      - Verification Result: FAILED
      - E:\M310e workspace\MITEK-CORPORATION-0-MITEK-CORPORATION-0-0\20250409_135956\USB Power Delivery\TEST.PD.PROT.SNK.9\01_TEST.PD.PROT.SNK.9_Rev2Snk_FAIL.usb: Saving trace file
      - Trace captured.
      - Running ProcessResult:
  - Rev3ChkdSnk fail
    - Power Delivery Link initialization on Voyager #26648 : Running Generation
    - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\Common\InitPDLink.updg: Starting PD Generation
    - Waiting... [maximum 8000 ms]
    - Board_Class::WaitForPDGenerationIdle() for CVS_0 : Serial#26648 wait_time_msec=8000
    - Stopping PD Generation
    - UpdateVariableInFile::8
    - Update ConditionID in file Variables.inc to "Rev3ChkdSnk"
    - UpdateVariableInFile::2
    - Update ConditionNumber in file Variables.ginc to 0
    - UpdateVariableInFile::2
    - Update TestPdRevision in file Variables.inc to 2
    - UpdateVariableInFile::8
    - Update SPEC_REV in file VendorInformation.ginc to PD_SPEC_REVISION_3
    - UpdateVariableInFile::2
    - Update Tester_RolePort in file VendorInformationExtra.inc to 2
    - UpdateVariableInFile::2
    - Update Tester_RolePort in file VendorInformationExtra.ginc to 2
    - UpdateVariableInFile::2
    - Update UUT_RolePort in file VendorInformationExtra.inc to 0
    - UpdateVariableInFile::2
    - Update UUT_RolePort in file VendorInformationExtra.ginc to 0
    - UpdateVariableInFile::2
    - Update SwapRequired in file Variables.inc to 0
    - UpdateVariableInFile::2
    - Update SwapRequired in file Variables.ginc to 0
    - UpdateVariableInFile::2
    - Update CaptiveCableBringUP in file Variables.inc to 0
    - UpdateVariableInFile::2
    - Update CaptiveCableBringUP in file Variables.ginc to 0
    - Running AtStart_func: CheckVconnApplicability(this)
    - Running CheckToEndCondition_func: Do_Return_False_with_One_param of Item #0
    - Capture_Class::Run() on CVS_0
    - Board_Class::SetSyncGUID [{6484744A-9AE9-4B4F-B00F-4B6B086F661F}]
    - Board_Class::SetAnalyzerParameters (1, 0)
    - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\REC\USB Power Delivery - USBIF\Protocol Specific Tests\TEST.PD.PROT.SNK.9.rec: Starting Recording
    - RecordingOptions::ApplySettings()
    - RecordingOptions::ApplyTraceSettings()::[TEST.PD.PROT.SNK.9_Rev3ChkdSnk.usb]
    - RecordingOptions::ApplySettings()::SetTraceFileName ->E:\M310e workspace\MITEK-CORPORATION-0-MITEK-CORPORATION-0-0\20250409_135956\USB Power Delivery\TEST.PD.PROT.SNK.9\02_TEST.PD.PROT.SNK.9_Rev3ChkdSnk.usb
    - RecordingOptions::ApplyGeneralSettings()
    - RecordingOptions::ApplyCapturePowerMeasurement()
    - RecordingOptions::ApplyRecordingBufferSize()
    - RecordingOptions::ApplyExtTriggerInRecOption()
    - RecordingOptions::ApplyExtTriggerOutRecOption():: No change was applied!
    - RecordingOptions::ApplyExerciserConnectedName()::[MITEK-CORPORATION-0-MITEK-CORPORATION-0-0][]
    - RecordingOptions::ApplyCaptureRawFile()
    - RecordingOptions::ApplyTypeCSettings()
    - RecordingOptions::ApplyCaptureCC_Traffic()
    - RecordingOptions::ApplyTypeCRoleSides()
    - ApplyTypeCRoleSides()::RO_SETTING_TC_EXERCISER_ROLE = 4
    - ApplyTypeCRoleSides()::RO_SETTING_TC_DEVICE_ROLE = 2
    - RecordingOptions::ApplyUncertainSettingsTypeC()
    - Board_Class::StartRecording()
    - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\GEN\USB Power Delivery - USBIF\Protocol Specific Tests\TEST.PD.PROT.SNK.9.UPDg: Starting PD Generation
    - Waiting... [maximum 15000 ms]
    - Board_Class::WaitForPDGenerationIdle() for CVS_0 : Serial#26648 wait_time_msec=15000
    - Stopping PD Generation
    - Waiting for Trigger...
    - Analyzer Trigged... 11784 ms
    - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\REC\USB Power Delivery - USBIF\Protocol Specific Tests\TEST.PD.PROT.SNK.9.rec: Stopping Recording at 11892 ms
    - Board_Class::StopRecordingAndWaitForTrace()
    - Board_Class::SetSyncGUID []
    - Trace is ready... 14484 ms
    - Running CheckToEndCondition_func: Do_Return_False_with_One_param of Item #1
    - COMMON.PROC.BU.2#1 pass
      - Saving COMMON.PROC.BU.2#1 in the file Variables.inc
      - UpdateVariableInFile::8
      - Update VerificationID in file Variables.inc to "COMMON.PROC.BU.2#1"
      - Saving VID_List array in the file Variables.inc
      - UpdateVariableInFile::8204
      - Update VID_List in file Variables.inc to maximum 0 elements
      - Relevant CVS found on item 0
      - Check_Class::Verify() on Trace from CVS_0
      - Check_Class::Verify()::ErrorCode from relevant CVS = 0:
      - Check_Class::Verify()::Check if any Bring-up has failed.
      - Check_Class::Verify()::Executing AlwaysApplicable
      - UpdateVariableInFile::3
      - Update CVS_ID in file CVS_Parameters.inc to 18
      - UpdateVariableInFile::2
      - Update ERROR_ON_READING_CURRENT in file CVS_Parameters.inc to 20000
      - Making a copy from Intermediate folder to E:\M310e workspace\MITEK-CORPORATION-0-MITEK-CORPORATION-0-0\20250409_135956\USB Power Delivery\TEST.PD.PROT.SNK.9\Debug\2_c2v1
      - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\VSE\USB Power Delivery - USBIF\Protocol Specific Tests\TEST.PD.PROT.SNK.9.vse: Running Verification Script
      - Running Verification script : TEST.PD.PROT.SNK.9.vse
      - Running Do_Nothing_Sub_with_One_param
      - Verification Result: PASSED
      - Running CheckToEndCondition_func: Do_Return_False_with_One_param of Item #2
    - TEST.PD.PROT.SNK.9#1 pass
      - Saving TEST.PD.PROT.SNK.9#1 in the file Variables.inc
      - UpdateVariableInFile::8
      - Update VerificationID in file Variables.inc to "TEST.PD.PROT.SNK.9#1"
      - Saving VID_List array in the file Variables.inc
      - UpdateVariableInFile::8204
      - Update VID_List in file Variables.inc to maximum 0 elements
      - Relevant CVS found on item 0
      - Check_Class::Verify() on Trace from CVS_0
      - Check_Class::Verify()::ErrorCode from relevant CVS = 0:
      - Check_Class::Verify()::Check if any Bring-up has failed.
      - Check_Class::Verify()::Executing AlwaysApplicable
      - UpdateVariableInFile::3
      - Update CVS_ID in file CVS_Parameters.inc to 18
      - UpdateVariableInFile::2
      - Update ERROR_ON_READING_CURRENT in file CVS_Parameters.inc to 20000
      - Making a copy from Intermediate folder to E:\M310e workspace\MITEK-CORPORATION-0-MITEK-CORPORATION-0-0\20250409_135956\USB Power Delivery\TEST.PD.PROT.SNK.9\Debug\2_c2v2
      - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\VSE\USB Power Delivery - USBIF\Protocol Specific Tests\TEST.PD.PROT.SNK.9.vse: Running Verification Script
      - Running Verification script : TEST.PD.PROT.SNK.9.vse
      - Running Do_Nothing_Sub_with_One_param
      - Verification Result: PASSED
      - Running CheckToEndCondition_func: Do_Return_False_with_One_param of Item #3
    - TEST.PD.PROT.SNK.9#2 fail
      - Saving TEST.PD.PROT.SNK.9#2 in the file Variables.inc
      - UpdateVariableInFile::8
      - Update VerificationID in file Variables.inc to "TEST.PD.PROT.SNK.9#2"
      - Saving VID_List array in the file Variables.inc
      - UpdateVariableInFile::8204
      - Update VID_List in file Variables.inc to maximum 0 elements
      - Relevant CVS found on item 0
      - Check_Class::Verify() on Trace from CVS_0
      - Check_Class::Verify()::ErrorCode from relevant CVS = 0:
      - Check_Class::Verify()::Check if any Bring-up has failed.
      - Check_Class::Verify()::Executing AlwaysApplicable
      - UpdateVariableInFile::3
      - Update CVS_ID in file CVS_Parameters.inc to 18
      - UpdateVariableInFile::2
      - Update ERROR_ON_READING_CURRENT in file CVS_Parameters.inc to 20000
      - Making a copy from Intermediate folder to E:\M310e workspace\MITEK-CORPORATION-0-MITEK-CORPORATION-0-0\20250409_135956\USB Power Delivery\TEST.PD.PROT.SNK.9\Debug\2_c2v3
      - C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\VSE\USB Power Delivery - USBIF\Protocol Specific Tests\TEST.PD.PROT.SNK.9.vse: Running Verification Script
      - Running Verification script : TEST.PD.PROT.SNK.9.vse
      - Running Do_Nothing_Sub_with_One_param
      - Deleting file C:\Users\Public\Documents\LeCroy\USBCompliance\Scripts\VSE\USB Power Delivery - USBIF\Protocol Specific Tests\TEST.PD.PROT.SNK.9.vse.Txt ...
      - Error(0x00000273): The UUT did not send a Hard Reset.
      - Verification Result: FAILED
      - E:\M310e workspace\MITEK-CORPORATION-0-MITEK-CORPORATION-0-0\20250409_135956\USB Power Delivery\TEST.PD.PROT.SNK.9\02_TEST.PD.PROT.SNK.9_Rev3ChkdSnk_FAIL.usb: Saving trace file
      - Trace captured.
      - Running ProcessResult:
      - Test_Class::DisconnectFromBoards()
      - Board_Class::CloseConnection()::AutomationObj.SetAnalyzerParameters(1,0)
      - Board_Class::CloseConnection() Successfully for CVS_0 to #26648
  - TEST.PD.PROT.SNK.9 : Finished
    - CVS_Manager_Class::Release()::Number of connected boards: 1
    - Board_Class::CloseConnection() --> Already Closed!
    - Board_Class was destroyed
    - CVS_Manager_Class was destroyed
  - Test Elapsed Time: 0 minute(s) and 58 seconds