{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["LM(2)5118 Calculator","Bill of Materials","Bode Plots","Worksheet","Graph"],"not_rendered":{"charts":12,"images":1,"macros":0,"external_links":0,"defined_names":95,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"LM(2)5118 Calculator","index":0,"n_rows":113,"n_cols":7,"rows_kept":113,"cut":false,"hidden":false,"merged":[]}
["LM(2)5118 Quick Start Component Calculator",null,null,null,"Version 2.01"]
["Revision date:  April 2014"]
[]
[]
[]
[" Step 1 - Application Requirements"]
[null,null,"Vout (V)",null,12]
[" Enter design requirements in the shaded cells",null,"Vin(min) (V)",null,8]
[null,null,"Vin(max) (V)",null,36]
[null,null,"Maximum Average Load Current Iout (A)",null,6]
[null,null,"Ripple Current as % of Maximum Load Current (%)",null,0.4]
[null,null,"Effciency of Converter (%)",null,0.8]
[null,null,"VCCX Voltage (V)",null,0]
[null,null,"Vin at start of  Transition to Buck-Boost Mode (V)",null,{"$f":"1.33*Vout","v":15.96}]
[null,null,"Buck-Boost Mode Operation",null,{"$f":"IF(Vinmin<1.4*Vout,\"YES\",\"NO\")","v":"YES"}]
[]
[null,null,"Recommended Controller IC",null,{"$f":"IF(E15 = \"NO\", \"LM5116\", \"LM5118\")","v":"LM5118"}]
[]
["Step 2 - Switching Frequency"]
[null,null,"Maximum Possible Switching Frequency (kHz)",null,{"$f":"IF(Fmax<610,Fmax,500)","v":500}]
[{"$f":"IF(E21>=E20,\"Violation of Minimum On-Time or Max Frequency\",\"\")","v":""},null,"Switching Frequency (kHz)",null,294]
[{"$f":"IF(E21>=E20,\"Reduce Switching Frequency\",\"\")","v":""},null,"Timing Resistor, Rt (kW)",null,{"$f":"6.4*10^3/Fsw-3.02","v":18.748707482993197}]
[{"$f":"IF(Dviolate<DMaximumAll,\"Check Switching Frequency or Decrease Vin\",\"\")","v":""}]
["Step 3 - Inductor Value"]
[null,null,"Calculated Buck Mode Inductor Value, Lb (µH)",null,{"$f":"IF(Vinmax>E14,((Vout*(Vinmax-Vout))/(Vinmax*Fsw*(Ripple*Iout)))*1000,\"NA\")","v":11.337868480725623}]
[null,null,"Calculated Buck-Boost Mode Inductor Value, Lb-b (µH)",null,{"$f":"IF(BuckBoostMode=\"YES\",(((Vinmin)*Vout)/((Vinmin+Vout)*Fsw*Ripple*Iout))*1000,\"NA\")","v":6.8027210884353737}]
[null,null,"Actual Chosen Inductor Value, L (µH)",null,4.7]
[null,null,"Inductor Tolerance (%)",null,0.2]
[]
["Step 4 - Calculate Output and Inductor Currents Based on Chosen Inductor"]
[null,null,"Buck mode Ripple Current at Vin(max), ΔI (A)",null,{"$f":"IF(Vinmax>E14,((Vout*(Vinmax-Vout))/(Vinmax*L*Fsw))*1000,\"NA\")","v":5.7895498624981903}]
[null,null,"Buck-Boost Ripple Current at Vin(min), ΔI (A)",null,{"$f":"(Vout*Vinmin)/(Fsw*L*(Vout+Vinmin))*1000","v":3.4737299174989147}]
[null,null,"Buck-Boost Ripple Current at Vin=Vout, ΔI (A) ",null,{"$f":"IF(Vinmax>=Vout,(Vout*Vout)/((Vout+Vout)*Fsw*L)*1000,\"NA\")","v":4.3421623968736425}]
[null,null,"Buck mode Ripple Current at Vin(max), Including inductor tolerance, ΔI (A)",null,{"$f":"IrippleBuck/(1-L_tol)","v":7.2369373281227372}]
[null,null,"Buck-Boost Ripple Current at Vin(min), Including inductor tolerance, ΔI (A)",null,{"$f":"IrippleBB/(1-L_tol)","v":4.3421623968736434}]
[null,null,"Buck Average Inductor Current at Vin(max), Including Effciency (A)",null,{"$f":"Iout/Eff","v":7.5}]
[null,null,"Buck-Boost Average Inductor Current at Vin(min), Including Effciency (A)",null,{"$f":"((Vout+Vinmin)/Vinmin)*(Iout/Eff)","v":18.75}]
[null,null,"Buck-Mode Peak Inductor Current, Ip(b) (A)",null,{"$f":"IF(Vinmax>E14,ILavgBuck+E34/2,\"NA\")","v":11.118468664061368}]
[null,null,"Buck-Boost Mode Peak Inductor Current, Ip(b-b) (A)",null,{"$f":"IF(BuckBoostMode=\"YES\",ILavgBB+E35/2,\"NA\")","v":20.921081198436823}," "]
[]
["Step 5 - Sense Resistor"]
[null,null,"Current Limit Margin (% beyond Max Load) (%)",null,0.1]
[null,null,"Buck Mode K Factor (K)",null,{"$f":"1+(10/(Vinmax-Vout))","v":1.4166666666666667}]
[null,null,"Selected Buck Mode K Factor (K)",null,1.1599999999999999]
[null,null,"Buck-Boost Mode K Factor (K)",null,{"$f":"1+(10/Vinmin)","v":2.25}]
[null,null,"Selected Buck-Boost Mode K Factor (K)",null,3]
[null,null,"Current Sense Resistor, Rs (mW)",null,{"$f":"IF((2.5*(1-E42))/(10*(ILavgBB+(IrippleBB*KBB)/2))*1000<(1.25*(1-E42))/(10*(ILavgBuck+(IrippleBuck*KBuck)/2))*1000,(2.5*(1-E42))/(10*(ILavgBB+(IrippleBB*KBB)/2))*1000,(1.25*(1-E42))/(10*(ILavgBuck+(IrippleBuck*KBuck)/2))*1000)","v":9.3904179408766577}," "]
[null,null,"Closest Standard Value, Rs (mW)",null,7]
[]
["Step 6 - Ramp Capacitor"]
[null,null,"Cramp (pF)",null,{"$f":"(L*5*10^-6)/(10*Rs)*10^9","v":335.71428571428567}]
[null,null,"Closest Smaller Standard Value, Cramp (pF)",null,470]
[null,null,"Rramp (kW)",null,{"$f":"IF(Vout>20,7/(Vout*5*10^-6-50*10^-6)*10^-3,\"NA\")","v":"NA"}]
[]
["Step 7 - Current Limits"]
[null,null,"Buck Mode Peak Inductor Current Limit (A)",null,{"$f":"IF(ILPeakLimitBuck<IpeakBuck,\"Error\",ILPeakLimitBuck)","v":16.134062540923157}]
[null,null,"Buck-Boost Mode Peak Inductor Current Limit (A)",null,{"$f":"IF(ILPeakLimitBB<IpeakBB,\"Error\",ILPeakLimitBB)","v":32.612741145090254}]
[]
["Step 9 - Output Capacitors (Based on Worst Case Conditions for Each Mode)"]
[null,null,"Target output ripple (mV)",null,50]
[null,null,"Buck-Boost Duty cycle at Vin(min) (%)",null,{"$f":"Vout/(Vinmin+Vout)","v":0.6}]
[null,null,"Buck-Boost RMS Ripple Current in Output Cap (A)",null,{"$f":"SQRT(-(DBB*Iout^2)/(DBB-1))","v":7.3484692283495336}]
[null,null,"Minimum COUT output Capacitor Value (µF)",null,{"$f":"Iout*Vout/(Vinmin+Vout)/(Fsw*DeltaVout)*1000000","v":244.89795918367346}]
[null,null,"Required COUT ESR (mW)",null,{"$f":"DeltaVout/(Iout/(1-E61)+IrippleBB/2)","v":2.9874173044493451}]
[null,null,"Chosen COUT output capacitor value (µF)",null,660]
[null,null,"Actual COUT ESR (mW)",null,14]
[null,null,"Buck Mode Output Ripple Voltage (mV)",null,{"$f":"IF(Vinmax<BuckMode,\"NA\",Coutesr*((Iout/(1-E61)+(IrippleBB/2))))","v":234.31610942249239}]
[]
["Step 10 - Input Capacitors (Based on Worst Case Conditions for Each Mode)"]
[null,null,"Buck-Boost RMS Input Ripple Current (A)",null,{"$f":"(Iout/(1-DBB))*SQRT(DBB*(1-DBB))","v":7.3484692283495336}]
[null,null,"Buck-Boost Mode Peak to Peak Current Ripple in Input Cap (A)",null,{"$f":"IpeakBB","v":20.921081198436823}]
[null,null,"Buck Mode RMS input Ripple Current (A)",null,{"$f":"IF(Vinmax<BuckMode,\"NA\",Iout*0.5)","v":3}]
[null,null,"Buck Mode Peak to Peak Current Ripple in Input Cap (A)",null,{"$f":"IpeakBuck","v":11.118468664061368}]
[null,null,"Initial Input Capacitor Value(μF)",null,{"$f":"E39/2/Fsw*1000","v":35.580070065368751}]
[null,null,"Chosen CIN Input Capacitor Value (µF)",null,30]
[]
["Step 11 - Feedback Resistors"]
[null,null,"Rfb2 (W)",null,8760]
[null,null,"Rfb1 (W)",null,{"$f":"_Rfb2/((Vout/1.23)-1)","v":1000.4456824512536}]
[]
["Step 12 - Chb & Cvcc Capacitor"]
[null,null,"High-side MOSFET Qg at VGS=10V (nC)",null,46]
[null,null,"Minimum Bootstrap Capacitor Chb (µF)",null,{"$f":"E82*10^-3/(0.05*7)","v":0.13142857142857142}]
[null,null,"Chosen Value for Chb (µF)",null,0.1]
[null,null,"Minimum VCC Bypass Capacitor Cvcc (µF)",null,{"$f":"10*E84","v":1}]
[]
["Step 13 - Error Amplifier Compensation"]
[null,null,"Right Half Plane Zero Frequency (kHz)",null,{"$f":"((Rout*(1-DBB)^2)/(2*PI()*L*DBB*10^-6))/1000","v":18.060135386314371}]
[null,null,"Capacitor ESR Zero Frequency (kHz)",null,{"$f":"1/(Cout*Coutesr*2*PI()*10^-6)","v":17.224560940681314}]
[null,null,"Capacitor Pole Frequency (kHz)",null,{"$f":"(1+DBB)/(2*PI()*Cout*Rout*10^-3)","v":0.19291508253563075}]
[null,null,"Bandwidth (kHz)",null,{"$f":"fmodRzero/4","v":4.5150338465785929}]
[null,null,"Selected Bandwith (kHz)",null,1.95]
[null,null,"Target Compensation Zero (kHz)",null,{"$f":"fcutoff/10","v":0.19500000000000001}]
[null,null,"Target Compensation Pole (kHz)",null,{"$f":"fmodRzero","v":18.060135386314371}]
[null,null,"Cpole (nF)",null,{"$f":"fcompZero/(fcompPole*_Rfb2*CompGain)*10^9","v":0.71586301285304299}]
[null,null,"Select Nearest Standard Cpole Value (nF)",null,0.22]
[null,null,"Czero (nF)",null,{"$f":"((1/(CompGain*_Rfb2))-E95*10^-9)*10^9","v":65.584562270125716},null," "]
[null,null,"Select Nearest Standard Czero Value (nF)",null,100]
[null,null,"Rcomp (W)",null,{"$f":"1/(fcompZero*2*3.14*E97*10^-9)","v":12450.996774480813}]
[null,null,"Select nearest Standard Rcomp Value (W)",null,10000]
[]
["Step 14 - Soft Start capacitor"]
[null,null,"Choose soft-start time (ms)",null,12]
[null,null,"Soft Start Capacitor Value (nF)",null,{"$f":"(E103*10^(-5))/1.23*10^6","v":97.560975609756113}]
[]
["Step 15 - UVLO Threshold and Hiccup Mode Restart"]
[null,null,"Minimum Value of Resistor Ruv1  (kW)",null,{"$f":"Vinmax","v":36}]
[null,null,"Chosen Value of  Ruv1 (kW)",null,75]
[null,null,"Desired Undervoltage Threshold (V)",null,4]
[null,null,"Ruv2 Value (kW)",null,{"$f":"1.23*E108/(E109+5*E108*10^(-3)-1.23)","v":29.332273449920507}]
[null,null,"Choose off-time of hiccup duty cycle (µs)",null,723]
[null,null,"Vin voltage for desired hiccup mode off-time  (V)  ",null,12]
[null,null,"Hiccup Mode Off-time Capacitor Value Cr (nF)",null,{"$f":"-(E111*(E110+E108))/(E110*E108*LN(1-((0.98*(E110+E108))/(E110*E112))))","v":99.917863427169848}]

{"sheet":"Bill of Materials","index":1,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[null,"LM5118 List of Components"]
[]
[null,"Component","Description","Value","Minimum Rating"]
[null,"L","Inductor",{"$f":"L","v":4.7},{"$f":"ILPeakLimitBB","v":32.612741145090254}]
[null,"Cin ","Input capacitor",{"$f":"Cin","v":30},{"$f":"Vinmax","v":36}]
[null,"Cramp","Ramp capacitor",{"$f":"Cramp","v":470},16]
[null,"Css","Soft start capacitor",{"$f":"Css","v":97.560975609756113},6]
[null,"Cout","Output capacitor",{"$f":"Cout","v":660},{"$f":"Vout","v":12}]
[null,"Cr","UVLO filter capacitor",{"$f":"Cr","v":99.917863427169848},16]
[null,"Cpole","Compensation capacitor",{"$f":"Cpole","v":0.22},6]
[null,"Czero","Compensation capacitor",{"$f":"Czero","v":100},6]
[null,"Cvcc","VCC bypass capacitor",{"$f":"Cvcc","v":1},12]
[null,"Chb","HB-SW bypass capacitor",{"$f":"Chb","v":0.1},{"$f":"MAX(Vccx,VCC)","v":7}]
[null,"Rfb1","Feedback resistor",{"$f":"_Rfb1","v":1000.4456824512536},"1/16 W"]
[null,"Rfb2","Feedback resistor",{"$f":"_Rfb2","v":8760},"1/16 W"]
[null,"Ruv1","UVLO divider resistor",{"$f":"_Ruv1","v":75},{"$f":"IF(AND(Vinmax^2/(_Ruv2*1000)<0.05,Vinmax<=50),\"1/16W\",\"1/8W\")","v":"1/16W"}]
[null,"Ruv2","UVLO divider resistor",{"$f":"_Ruv2","v":29.332273449920507},"1/16 W"]
[null,"Rs","Sense resistor",{"$f":"Rs","v":7},{"$f":"IF(PRS_BB>PRS_B,PRS_BB,PRS_B)","v":2.4609375}]
[null,"Rt","Oscillator timing resistor",{"$f":"Rt","v":18.748707482993197},"1/16 W"]
[null,"Rramp","Optional ramp resistor",{"$f":"Rramp","v":"NA"},{"$f":"IF(D20=\"NA\",\"-\",\"1/16 W\")","v":"-"}]
[null,"Rcomp","Compensation resistor",{"$f":"Rcomp/1000","v":10},"1/16 W"]

{"sheet":"Bode Plots","index":2,"n_rows":24,"n_cols":24,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
["Buck-Boost Mode",null,null,null,null,null,null,null,null,null,null,null,"Buck Mode "]
[null,"Frequency (Hz)","Frequency (rad/sec)","Modulator\nGain\n(dB)","Modulator\nPhase\n(deg)","Error Amplifier Gain\n(dB)","Error Amplifier Phase (deg)","Overall Loop\nGain\n(dB)","Loop\nPhase\n(deg)",null,null,null,null,"Frequency (Hz)","Frequency (rad/sec)","Modulator\nGain\n(dB)","Modulator\nPhase\n(deg)","Error Amplifier Gain\n(dB)","Error Amplifier Phase (deg)","Overall Loop\nGain\n(dB)","Loop\nPhase\n(deg)"]
[null,0.1,{"$f":"2*PI()*B3","v":0.62831853071795862},{"$f":"20*LOG(AmBB*IMABS(IMDIV(IMPRODUCT(COMPLEX(1,-C3/wrBB),COMPLEX(1,C3/wzBB)),COMPLEX(1,C3/wpBB))))","v":17.077438119765777},{"$f":"IMARGUMENT(IMDIV(IMPRODUCT(COMPLEX(1,-C3/wrBB),COMPLEX(1,C3/wzBB)),COMPLEX(1,C3/wpBB)))*(180/PI())","v":-2.968460733987114E-2},{"$f":"20*LOG(Afb*IMABS(IMDIV(IMDIV(COMPLEX(1,C3/wzea),COMPLEX(1,C3/wpea)),COMPLEX(0,C3))))","v":65.167234255864258},{"$f":"IMARGUMENT(IMDIV(IMDIV(COMPLEX(-1,-C3/wzea),COMPLEX(1,C3/wpea)),COMPLEX(0,C3)))*(180/PI())","v":90.035920969120099},{"$f":"D3+F3","v":82.244672375630032},{"$f":"E3+G3","v":90.006236361780225},null,"Modulator - Buck-Boost",null,null,0.1,{"$f":"2*PI()*N3","v":0.62831853071795862},{"$f":"20*LOG(Amb*IMABS(IMDIV(COMPLEX(1,O3/wzb),COMPLEX(1,O3/wpb))))","v":29.11863612575198},{"$f":"IMARGUMENT(IMDIV(COMPLEX(1,O3/wzb),COMPLEX(1,O3/wpb)))*(180/PI())","v":-4.7187349104116545E-2},{"$f":"20*LOG(Afb*IMABS(IMDIV(IMDIV(COMPLEX(1,O3/wzea),COMPLEX(1,O3/wpea)),COMPLEX(0,O3))))","v":65.167234255864258},{"$f":"IMARGUMENT(IMDIV(IMDIV(COMPLEX(-1,-O3/wzea),COMPLEX(1,O3/wpea)),COMPLEX(0,O3)))*(180/PI())","v":90.035920969120099},{"$f":"P3+R3","v":94.285870381616235},{"$f":"Q3+S3","v":89.988733620015978},null,"Modulator - Buck"]
[null,0.2,{"$f":"2*PI()*B4","v":1.2566370614359172},17.077434619759181,-5.9369198718979402E-2,59.146639486132344,90.071841909815774,76.224074105891532,90.012472711096791,null,"rad/sec","Hz",null,0.2,{"$f":"2*PI()*N4","v":1.2566370614359172},29.118627164036802,-9.4374632833040525E-2,59.146639486132344,90.071841909815774,{"$f":"P4+R4","v":88.265266650169139},{"$f":"Q4+S4","v":89.977467276982736},null,"rad/sec","Hz"]
[null,0.5,{"$f":"2*PI()*B5","v":3.1415926535897931},17.077410119791928,-0.1484227174851773,51.187875317355811,90.179604277114805,68.265285437147739,90.03118155962963,"wp",{"$f":"(1+DBB)/(Cout*10^-6*Rout)","v":1212.1212121212122},{"$f":"K5/(2*PI())","v":192.91508253563075},null,0.5,{"$f":"2*PI()*N5","v":3.1415926535897931},29.118564432548343,-0.23593543802806247,51.187875317355811,90.179604277114805,80.306439749904158,89.94366883908674,"wz",{"$f":"1/(Cout*10^-6*Coutesr*10^-3)","v":108225.10822510823},{"$f":"W5/(2*PI())","v":17224.560940681313}]
[null,1,{"$f":"2*PI()*B6","v":6.2831853071795862},17.077322621037737,-0.29684343991358075,45.167403989725628,90.359205001277289,62.244726610763365,90.062361561363701,"wr",{"$f":"(Rout*(1-DBB)^2)/(L*10^-6*DBB)","v":113475.17730496457},{"$f":"K6/(2*PI())","v":18060.13538631437},null,1,{"$f":"2*PI()*N6","v":6.2831853071795862},29.118340398915514,-0.471862704561752,45.167403989725628,90.359205001277289,74.285744388641149,89.887342296715531,"wp",{"$f":"1/(Cout*10^-6*Rout)","v":757.57575757575762},{"$f":"W6/(2*PI())","v":120.5719265847692}]
[null,2,{"$f":"2*PI()*B7","v":12.566370614359172},17.076972643657108,-0.59367092033782365,39.147318380975598,90.718381581460264,56.224291024632706,90.124710661122435,"wz",{"$f":"1/(Cout*10^-6*Coutesr*10^-3)","v":108225.10822510823},{"$f":"K7/(2*PI())","v":17224.560940681313},null,2,{"$f":"2*PI()*N7","v":12.566370614359172},29.117444379946843,-0.94366004728413533,39.147318380975598,90.718381581460264,68.264762760922437,89.774721534176123,null,"Gain","dB"]
[null,5,31.415926535897931,17.074523591737222,-1.4838981177932415,31.19211663488095,91.795456867043569,48.266640226618172,90.311558749250324,null,"Gain","dB",null,5,31.415926535897931,29.111177418504447,-2.3580074175939743,31.19211663488095,91.795456867043569,60.3032940533854,89.437449449449588,"Am",{"$f":"Rout/Ri","v":28.571428571428569},{"$f":"20*LOG(Amb)","v":29.118639112994487}]
[null,10,62.831853071795862,17.065788239840117,-2.9658051511418293,25.184343963072347,93.587371165669651,42.250132202912468,90.621566014527815,"Am",{"$f":"(Rout/Ri)*((1-DBB)/(1+DBB))","v":7.1428571428571423},{"$f":"20*LOG(K9)","v":17.07743928643524},null,10,62.831853071795862,29.088868955997999,-4.7078848621668286,25.184343963072347,93.587371165669651,54.273212919070346,88.87948630350283]
[null,20,125.66370614359172,17.031021564655408,-5.9157771578508829,19.21467747306524,97.146650578629419,36.245699037720648,91.230873420778536,null,null,null,null,20,125.66370614359172,29.000763778534271,-9.3517162422901237,19.21467747306524,97.146650578629419,48.215441251599515,87.794934336339296]
[null,50,314.15926535897933,16.795152762166058,-14.522579693213222,11.596605997032363,107.40108142553261,28.391758759198421,92.878501732319393,null,"Error Amp",null,null,50,314.15926535897933,28.429518219723494,-22.356987984875538,11.596605997032363,107.40108142553261,40.026124216755861,85.044093440657065,null,"Error Amp"]
[null,100,628.31853071795865,16.044129484796294,-27.385153424915408,6.6122943956471172,122.06288154296811,22.656423880443413,94.677728118052698,null,"rad/sec","Hz",null,100,628.31853071795865,26.845390537980727,-39.339012667804596,6.6122943956471172,122.06288154296811,33.457684933627846,82.723868875163518,null,"rad/sec","Hz"]
[null,200,1256.6370614359173,13.908795119879416,-46.00225094251315,3.2613432008160665,141.3300608619584,17.170138320695482,95.327809919445258,"wpea",{"$f":"(Czero*10^-9+Cpole*10^-9)/(Cpole*10^-9*Czero*10^-9*Rcomp)","v":455545.45454545453},{"$f":"wpea/(2*PI())","v":72502.310893953414},null,200,1256.6370614359173,23.377189225203434,-58.250671150438542,3.2613432008160665,141.3300608619584,26.638532426019502,83.079389711519866,"wpea",{"$f":"(Czero*10^-9+Cpole*10^-9)/(Cpole*10^-9*Czero*10^-9*Rcomp)","v":455545.45454545453},{"$f":"wpea/(2*PI())","v":72502.310893953414}]
[null,500,3141.5926535897929,8.2096586841259569,-68.824993013422713,1.5497632941141855,161.94808840003472,9.7594219782401428,93.123095386612007,"wzea",{"$f":"1/(Czero*10^-9*Rcomp)","v":1000},{"$f":"wzea/(2*PI())","v":159.15494309189535},null,500,3141.5926535897929,16.522347214882551,-74.779581180469378,1.5497632941141855,161.94808840003472,18.072110508996737,87.168507219565342,"wzea",{"$f":"1/(Czero*10^-9*Rcomp)","v":1000},{"$f":"wzea/(2*PI())","v":159.15494309189535}]
[null,1000,6283.1853071795858,2.6539781752749461,-78.927510461167969,1.2386416944375231,170.16672760285019,3.892619869712469,91.239217141682218,null,"Gain","dB",null,1000,6283.1853071795858,10.69549529154034,-79.80225472241186,1.2386416944375231,170.16672760285019,11.934136985977863,90.364472880438328,null,"Gain","dB"]
[null,2000,12566.370614359172,-3.164959309600079,-84.186545351745991,1.1549417060357816,173.87001255798802,-2.0100176035642976,89.683467206242028,"Afb",{"$f":"1/(_Rfb2*(Czero*10^-9+Cpole*10^-9))","v":1139.0466088759979},{"$f":"20*LOG(K16)","v":61.130829908509227},null,2000,12566.370614359172,4.7653694759202985,-79.926902972889323,1.1549417060357816,173.87001255798802,5.9203111819560803,93.943109585098696,"Afb",{"$f":"1/(_Rfb2*(Czero*10^-9+Cpole*10^-9))","v":1139.0466088759979},{"$f":"20*LOG(W16)","v":61.130829908509227}]
[null,5000,31415.926535897932,-10.52901044026704,-87.078229851577987,1.1146221828675738,174.23177339951653,-9.4143882573994659,87.15354354793854,null,null,null,null,5000,31415.926535897932,-2.8870100279751423,-72.431491977526164,1.1146221828675738,174.23177339951653,-1.7723878451075685,101.80028142199036]
[null,10000,62831.853071795864,-14.793959657312467,-87.730357031613337,1.0500867573513109,171.23512021688691,-13.743872899961156,83.504763185273575,null,null,null,null,10000,62831.853071795864,-7.9955681442348752,-59.171199970493035,1.0500867573513109,171.23512021688691,-6.9454813868835643,112.06392024639388]
[null,20000,125663.70614359173,-16.052882541524745,-88.101059824064734,0.81259866390427882,164.12237113549972,-15.240283877620467,76.021311311434985,null,null,null,null,20000,125663.70614359173,-11.569790122207671,-40.390544729119839,0.81259866390427882,164.12237113549972,-10.757191458303392,123.73182640637988]
[null,50000,314159.26535897929,-12.07366822379603,-88.927459675793386,-0.5587947119299872,145.22618731350858,-12.632462935726018,56.298727637715189,null,null,null,null,50000,314159.26535897929,-13.492389121086232,-18.870214917685242,-0.5587947119299872,145.22618731350858,-14.05118383301622,126.35597239582333]
[null,100000,628318.53071795858,-6.8062699058734024,-89.425172722180605,-3.4966954602366762,125.85179074391938,-10.30296536611008,36.426618021738776,null,null,null,null,100000,628318.53071795858,-13.852431921115109,-9.7039661423808603,-3.4966954602366762,125.85179074391938,-17.349127381351785,116.14782460153852]
[null,200000,1256637.0614359172,-0.98466138515520241,-89.707208068325912,-8.2189481607955912,109.88057126531295,-9.2036095459507941,20.17336319698704,null,null,null,null,200000,1256637.0614359172,-13.94730832007234,-4.8877860390789012,-8.2189481607955912,109.88057126531295,-22.166256480867929,104.99278522623405]
[null,500000,3141592.653589793,6.9175924804276576,-89.882262865919387,-15.731902214845437,98.232408772276969,-8.8143097344177797,8.3501459063575822,null,null,null,null,500000,3141592.653589793,-13.97424944004076,-1.9591925295656851,-15.731902214845437,98.232408772276969,-29.706151654886199,96.273216242711285]
[null,1000000,6283185.307179586,12.9300841438062,-89.941086790219828,-21.684902263918055,94.137701631651652,-8.7548181201118549,4.1966148414318241,null,null,null,null,1000000,6283185.307179586,-13.978111852203119,-0.9798888016390398,-21.684902263918055,94.137701631651652,-35.663014116121175,93.157812830012617]

{"sheet":"Worksheet","index":3,"n_rows":89,"n_cols":6,"rows_kept":89,"cut":false,"hidden":true,"merged":[]}
[]
[null,null,null,null,"10 is buck","10 is buck-boost"]
[]
[null,{"$f":"IF(Vout>0.7*Vin_nominal,\"Buck-Boost Mode\",\"Buck Mode\")","v":{"$error":"#NAME?"}},null,"Vin","Vout"]
[null,null,null,null,12]
[null,null,null,20,{"$f":"IF(E5<0.7*D6,10,0)","v":10},{"$f":"IF(E5>0.7*D6,10,0)","v":0}]
[null,null,null,19,{"$f":"IF(E5<0.7*D7,10,0)","v":10},{"$f":"IF(E5>0.7*D7,10,0)","v":0}]
[null,null,null,18,{"$f":"IF(E5<0.7*D8,10,0)","v":10},{"$f":"IF(E5>0.7*D8,10,0)","v":0}]
[null,null,null,17,{"$f":"IF(E5<0.7*D9,10,0)","v":0},{"$f":"IF(E5>0.7*D9,10,0)","v":10}]
[null,null,null,16,{"$f":"IF(E5<0.7*D10,10,0)","v":0},{"$f":"IF(E5>0.7*D10,10,0)","v":10}]
[null,null,null,14,{"$f":"IF(E7<0.7*D11,10,0)","v":0},{"$f":"IF(E5>0.7*D11,10,0)","v":10}]
[null,null,null,13,{"$f":"IF(E8<0.7*D12,10,0)","v":0},{"$f":"IF(E5>0.7*D12,10,0)","v":10}]
[null,null,null,12,{"$f":"IF(E5<0.7*D13,10,0)","v":0},{"$f":"IF(E5>0.7*D13,10,0)","v":10}]
[null,null,null,11,{"$f":"IF(E5<0.7*D14,10,0)","v":0},{"$f":"IF(E5>0.7*D14,10,0)","v":10}]
[null,null,null,10,{"$f":"IF(E5<0.7*D15,10,0)","v":0},{"$f":"IF(E5>0.7*D15,10,0)","v":10}]
[]
[null,null,null,null,12]
[null,null,13,75,{"$f":"E17/0.7","v":17.142857142857142},{"$f":"E18","v":17.142857142857142}]
[null,null,13,74,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,73,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,72,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,71,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,70,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,{"$f":"D23-1","v":69},{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,68,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,67,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,66,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,65,{"$f":"E17/0.7","v":17.142857142857142}]
[null,null,13,64,17.142857142857142]
[null,null,13,63,17.142857142857142]
[null,null,13,62,17.142857142857142]
[null,null,13,61,17.142857142857142]
[null,null,13,60,17.142857142857142]
[null,null,13,{"$f":"D33-1","v":59},17.142857142857142]
[null,null,13,58,17.142857142857142]
[null,null,13,57,17.142857142857142]
[null,null,13,56,17.142857142857142]
[null,null,13,55,17.142857142857142]
[null,null,13,54,17.142857142857142]
[null,null,13,53,17.142857142857142]
[null,null,13,52,17.142857142857142]
[null,null,13,51,17.142857142857142]
[null,null,13,50,17.142857142857142]
[null,null,13,49,17.142857142857142]
[null,null,13,48,17.142857142857142]
[null,null,13,47,17.142857142857142]
[null,null,13,46,17.142857142857142]
[null,null,13,45,17.142857142857142]
[null,null,13,44,17.142857142857142]
[null,null,13,43,17.142857142857142]
[null,null,13,42,17.142857142857142]
[null,null,13,41,17.142857142857142]
[null,null,13,40,17.142857142857142]
[null,null,13,39,17.142857142857142]
[null,null,13,38,17.142857142857142]
[null,null,13,37,17.142857142857142]
[null,null,13,36,17.142857142857142]
[null,null,13,35,17.142857142857142]
[null,null,13,34,17.142857142857142]
[null,null,13,33,17.142857142857142]
[null,null,13,32,17.142857142857142]
[null,null,13,31,17.142857142857142]
[null,null,13,30,17.142857142857142]
[null,null,13,29,17.142857142857142]
[null,null,13,28,17.142857142857142]
[null,null,13,27,17.142857142857142]
[null,null,13,26,17.142857142857142]
[null,null,13,25,17.142857142857142]
[null,null,13,24,17.142857142857142]
[null,null,13,23,17.142857142857142]
[null,null,13,22,17.142857142857142]
[null,null,13,21,17.142857142857142]
[null,null,13,20,17.142857142857142]
[null,null,13,19,17.142857142857142]
[null,null,13,18,17.142857142857142]
[null,null,13,17,17.142857142857142]
[null,null,13,16,17.142857142857142]
[null,null,13,15,17.142857142857142]
[null,null,13,14,17.142857142857142]
[null,null,13,13,17.142857142857142]
[null,null,13,12,17.142857142857142]
[null,null,13,11,17.142857142857142]
[null,null,13,10,17.142857142857142]
[null,null,13,9,17.142857142857142]
[null,null,13,8,17.142857142857142]
[null,null,13,7,17.142857142857142]
[null,null,13,6,17.142857142857142]
[null,null,13,5,17.142857142857142]
[null,null,13,4,17.142857142857142]

{"sheet":"Graph","index":4,"n_rows":13,"n_cols":13,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[null,null,"Vinmin","Vinmax","Lower ts limit","Upper ts limit","Lo B-B Voltage","Hi B-B voltage","Lower Buck","Upper Buck"]
[]
[]
[null,null,{"$f":"Vinmin","v":8},{"$f":"Vinmax","v":36},{"$f":"1.15*Vout","v":13.799999999999999},{"$f":"Vout/0.75","v":16},{"$f":"Vinmin","v":8},{"$f":"E7","v":13.799999999999999},{"$f":"Vout/0.75","v":16},{"$f":"Vinmax","v":36},null,{"$f":"Vout","v":12},{"$f":"Vin_nominal","v":{"$error":"#NAME?"}}]
[null,null,"Buck-Boost",null,null,null,5,{"$f":"IF(Vinmax<H7,Vinmax,H7)","v":13.799999999999999}]
[null,null,"Graph-Trans",null,null,{"$f":"IF(Vinmax>F7,F7,IF(Vinmax>E7,Vinmax,0))","v":16}]
[null,null,"Offset-Trans",null,null,{"$f":"F9-H8","v":2.2000000000000011}]
[]
[null,"NEW ","Buck",null,null,null,null,{"$f":"IF(Vinmax>F7,Vinmax,0)","v":36}]
[null,"Offset","Offset-Buck",null,null,null,null,{"$f":"H12-F7","v":20}]