
**** 02/25/21 19:39:13 ******* PSpice 17.4.0 (Nov 2018) ******* ID# 0 ********

 ** Profile: "EVM_switching_tb-trans"  [ E:\File1\Girish UCC21750\1_1\ucc21750_trans-pspicefiles\evm_switching_tb\trans.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "trans.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "C:/Cadence/PSpiceTI/tools/lib/ti2/UCC21750_TRANS.lib" 
.LIB "C:/Cadence/PSpiceTI/tools/lib/ON/ONSEMI_SiCMOSFET_1200_pspice.txt" 
* From [PSPICE NETLIST] section of C:\SPB_Data\cdssetup\OrCAD_PSpiceTIPSpice_Install\17.4.0\PSpice.ini file:
.lib "nom_pspti.lib" 
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 1m 0 100u 
.OPTIONS ADVCONV
.OPTIONS ABSTOL= 1.0n
.OPTIONS ITL2= 40
.OPTIONS ITL4= 40
.OPTIONS VNTOL= 1.0m
.OPTIONS DMFACTOR= 0.001
.AUTOCONVERGE ITL1=1000 ITL2=1000 ITL4=1000 RELTOL=0.05 ABSTOL=1.0E-6 VNTOL=.001 PIVTOL=1.0E-10 
.PROBE64 N([N16779135])
.PROBE64 N([N16779212])
.INC "..\EVM_switching_tb.net" 



**** INCLUDING EVM_switching_tb.net ****
* source UCC21750_TRANS
R_R5         RDY VCC  5k TC=0,0 
C_C2         N16764291 N16764231  10u  TC=0,0 
V_V7         VCC 0  
+PWL 0 0 10u 3.3 50u 3.3 
V_V2         IN+ 0  
+PULSE 0 3.3 0 5ns 5ns 16us 20us
R_R3         FLTB VCC  5k TC=0,0 
R_R8         OC N16764291  1k TC=0,0 
V_V8         N16764231 N16764291  
+PWL 0 0 15u 20 95u 20 105u 20 
V_V11         AIN N16764291 2.5
R_R14         0 APWM  200k TC=0,0 
V_V5         N16766688 0  
+PWL 0 5 45u 5 45.1u 5 48u 5 48.1u 5 
R_R12         OUTL N16768175  2 TC=0,0 
R_R13         N16781649 N16768175  2 TC=0,0 
C_C4         VCC 0  10u  
C_C5         VCC 0  1u  
X_U1         RDY IN+ 0 N16781649 OUTL N16766688 AIN APWM N16768175 N16764291
+  VCC N16764231 N16764291 FLTB OC 0 UCC21750_TRANS
X_L1    N16764291 N16779135 EVM_switching_tb_L1 
C_C6         N16779212 N16779135  0.5u  TC=0,0 
R_R15         N16779212 N16779135  600 TC=0,0 
V_V12         N16779093 N16779212 750
R_R16         N16764291 N16768175  10k TC=0,0 
V_V13         AIN N16779212 2.5
V_V17         IN+ 0  
+PULSE 3.3 0 0 5ns 5ns 16us 20us
R_R17         OC N16779212  1k TC=0,0 
X_U2         RDY IN+ 0 N16785386 OUTL N16785315 AIN APWM N16785398 N16779212
+  VCC N16785447 N16779212 FLTB OC 0 UCC21750_TRANS
R_R22         N16785386 N16785398  2 TC=0,0 
R_R21         RDY VCC  5k TC=0,0 
V_V16         N16785315 0  
+PWL 0 5 45u 5 45.1u 5 48u 5 48.1u 5 
C_C10         N16779212 N16785447  10u  TC=0,0 
R_R23         OUTL N16785398  2 TC=0,0 
V_V15         VCC 0  
+PWL 0 0 10u 3.3 50u 3.3 
R_R24         N16779212 N16785398  10k TC=0,0 
C_C8         VCC 0  10u  
C_C9         VCC 0  1u  
R_R18         0 APWM  200k TC=0,0 
V_V18         N16785447 N16779212  
+PWL 0 0 15u 20 95u 20 105u 20 
R_R19         FLTB VCC  5k TC=0,0 
X_X1         N16779093 N16768175 N16764291 NTHL020N120SC1_3p
X_X2         N16764291 N16785398 N16779212 NTHL020N120SC1_3p

.subckt EVM_switching_tb_L1 1 2  
L_L1         1 _SR L_L1 1.5mH  
.model         L_L1 IND L=1 DEV=10%     
RRDC_L1         _SR 2 0.140   
.ends EVM_switching_tb_L1

**** RESUMING trans.cir ****
.END

ERROR(ORPSIM-15143): Voltage source and/or inductor loop involving X_U2.E_E158. You may break the loop by adding a series resistance
